General information                                                             
Total Memory Size:                                                              8 GBytes

Current Performance Settings                                                    
Maximum Supported Memory Clock:                                                 666.7 MHz
Current Memory Clock:                                                           665.7 MHz
Current Timing (tCAS-tRCD-tRP-tRAS):                                            9-9-9-24
Memory Runs At:                                                                 Dual-Channel

Command Rate:                                                                   2T
Read to Read Delay (tRD_RD) Different Rank:                                     1T
Read to Read Delay (tRD_RD) Different DIMM:                                     3T
Write to Write Delay (tWR_WR) Different Rank:                                   3T
Write to Write Delay (tWR_WR) Different DIMM:                                   3T
Read to Write Delay (tRD_WR) Same Rank:                                         3T
Read to Write Delay (tRD_WR) Different Rank:                                    3T
Read to Write Delay (tRD_WR) Different DIMM:                                    3T
Write to Read Delay (tWR_RD) Same Rank (tWTR):                                  5T
Write to Read Delay (tWR_RD) Different Rank:                                    1T
Write to Read Delay (tWR_RD) Different DIMM:                                    1T
Read to Precharge Delay (tRTP):                                                 5T
Write to Precharge Delay (tWTP):                                                21T
Write Recovery Time (tWR):                                                      10T
RAS# to RAS# Delay (tRRD):                                                      4T
Refresh Cycle Time (tRFC):                                                      107T
Four Activate Window (tFAW):                                                    20T
