System Report

Date | Mi 25 Sep 2019 14:05:19 CEST
--- | ---
OS Version | 10.14.6
OS Build | 18G95
Model Name | iMac Pro
Model Identifier | iMacPro1,1
Processor | Intel(R) Core(TM) i9-9900K CPU @ 3.60GHz
Total Number of Cores | 8
Memory | 32 GB
Graphics Card(s) | Radeon RX 580
Bootloader | Clover - UEFI r5033
| AppleHDA | is loaded

AppleALC | 1.3.9
--- | ---
FakeSMC | 1800
IntelMausiEthernet | 2.5.0d0
Lilu | 1.3.7
USBInjectAll | 0.7.1

FakeSMC_ACPISensors | EFI/CLOVER/kexts/Other
--- | ---
AppleALC | EFI/CLOVER/kexts/Other
FakeSMC_CPUSensors | EFI/CLOVER/kexts/Other
EnergyDriver | /Library/Extensions
FakeSMC | EFI/CLOVER/kexts/Other
FakeSMC_GPUSensors | EFI/CLOVER/kexts/Other
IntelMausiEthernet | EFI/CLOVER/kexts/Other
FakeSMC_LPCSensors | EFI/CLOVER/kexts/Other
Lilu | EFI/CLOVER/kexts/Other
FakeSMC_SMMSensors | EFI/CLOVER/kexts/Other
USBInjectAll | EFI/CLOVER/kexts/Other

Sleep On Power Button | 1
--- | ---
hibernatefile | /dev/null
proximitywake | 0
powernap | 0
gpuswitch | 2
networkoversleep | 0
disksleep | 10
sleep | 3 (sleep prevented by sharingd, useractivityd)
hibernatemode | 0
ttyskeepawake | 1
displaysleep | 3
tcpkeepalive | 1
womp | 0

Vendor | Device | Sub Ven | Sub Dev | Vendor Name | Device Name
--- | --- | --- | --- | --- | ---
8086 | 3E30 | 1043 | 8694 | Intel Corporation | 8th Gen Core 8-core Desktop Processor Host Bridge/DRAM Registers (Coffee Lake S)
8086 | 1901 | 0000 | 0000 | Intel Corporation | Xeon E3-1200 v5/E3-1500 v5/6th Gen Core Processor PCIe Controller (x16)
8086 | A36D | 1043 | 8694 | Intel Corporation | Cannon Lake PCH USB 3.1 xHCI Host Controller
8086 | A36F | 1043 | 8694 | Intel Corporation | Cannon Lake PCH Shared SRAM
8086 | A360 | 1043 | 8694 | Intel Corporation | Cannon Lake PCH HECI Controller
8086 | A352 | 1043 | 8694 | Intel Corporation | Cannon Lake PCH SATA AHCI Controller
8086 | A340 | 0000 | 0000 | Intel Corporation | Cannon Lake PCH PCI Express Root Port #17
8086 | A338 | 0000 | 0000 | Intel Corporation | Cannon Lake PCH PCI Express Root Port #1
8086 | A33D | 0000 | 0000 | Intel Corporation | Cannon Lake PCH PCI Express Root Port #6
8086 | A330 | 0000 | 0000 | Intel Corporation | Cannon Lake PCH PCI Express Root Port #9
8086 | A305 | 1043 | 8694 | Intel Corporation | Z390 Chipset LPC/eSPI Controller
8086 | A348 | 1043 | 8724 | Intel Corporation | Cannon Lake PCH cAVS
8086 | A323 | 1043 | 8694 | Intel Corporation | Cannon Lake PCH SMBus Controller
8086 | A324 | 1043 | 8694 | Intel Corporation | Cannon Lake PCH SPI Controller
8086 | 15BC | 1043 | 8672 | Intel Corporation | Ethernet Connection (7) I219-V
1002 | 67DF | 148C | 2378 | Advanced Micro Devices, Inc. (AMD/ATI) | Ellesmere (Radeon RX 470/480/570/570X/580/580X/590)
1002 | AAF0 | 148C | AAF0 | Advanced Micro Devices, Inc. (AMD/ATI) | Ellesmere HDMI Audio (Radeon RX 470/480 / 570/580/590)
1D6A | 87B1 | 16B8 | 7300 | Aquantia Corp. | AQC107 NBase-T/IEEE 802.3bz Ethernet Controller (AQtion)
14E4 | 43A0 | 106B | 0112 | Broadcom Inc. and subsidiaries | BCM4360 802.11ac Wireless Network Adapter
15B7 | 5002 | 15B7 | 5002 | Sandisk Corp | WD Black 2018/PC SN720 NVMe SSD