+-o HDEF@1F,3  <class IOPCIDevice, id 0x1000003b7, registered, matched, active, busy 0 (226 ms), retain 11>
    {
      "acpi-device" = "IOACPIPlatformDevice is not serializable"
      "IOPCIMSIMode" = Yes
      "assigned-addresses" = <10fb0082c000000000000200000000000040000020fb0082c0000000000000000000000000000100>
      "vendor-id" = <86800000>
      "class-code" = <00030400>
      "subsystem-vendor-id" = <43100000>
      "IOName" = "pci8086,a2f0"
      "AFGLowPowerState" = <03000000>
      "pcidebug" = "0:31:3"
      "layout-id" = <07000000>
      "IOServiceDEXTEntitlements" = (("com.apple.developer.driverkit.transport.pci"))
      "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
      "built-in" = <00>
      "IOPCIResourced" = Yes
      "AAPL,slot-name" = "Built In"
      "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
      "IODeviceMemory" = (({"address"=824633851904,"length"=16384}),({"address"=824633720832,"length"=65536}))
      "PinConfigurations" = <f0111141104011012010010130600101402001015090a09060908102703081018040210229e6e74090604501>
      "name" = "Audio Controller"
      "subsystem-id" = <24870000>
      "acpi-pmcap-offset" = 80
      "model" = <"Apple High Definition Audio Controller">
      "alc-layout-id" = <07000000>
      "MaximumBootBeepVolumeAlt" = <7f>
      "device_type" = <"Audio Controller">
      "compatible" = <"pci8086,0C0C","HDEF">
      "IOReportLegendPublic" = Yes
      "reg" = <00fb00000000000000000000000000000000000010fb00020000000000000000000000000040000020fb000200000000000000000000000000000100>
      "MaximumBootBeepVolume" = <01>
      "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="HDEF 1"})
      "device-id" = <f0a20000>
      "revision-id" = <00000000>
      "IOInterruptSpecifiers" = (<1000000007000000>,<0d00000000000100>)
      "acpi-path" = "IOACPIPlane:/_SB/PC00@0/CAVS@1f0003"
    }
    

+-o ALZA@e0000  <class IORegistryEntry, id 0x1000002f6, retain 4>
    {
      "acpi-device" = "IOACPIPlatformDevice is not serializable"
      "acpi-path" = "IOACPIPlane:/_SB/PC00@0/ALZA@e0000"
    }
    

+-o HDAU@0,1  <class IOPCIDevice, id 0x1000003d7, registered, matched, active, busy 0 (18 ms), retain 11>
    {
      "acpi-device" = "IOACPIPlatformDevice is not serializable"
      "IOPCIMSIMode" = Yes
      "assigned-addresses" = <1001c382000000000000dad80000000000400000>
      "vendor-id" = <02100000>
      "class-code" = <00030400>
      "subsystem-vendor-id" = <02100000>
      "IOPCIExpressLinkCapabilities" = 4197636
      "hda-gfx" = <"onboard-1">
      "IOName" = "pci1002,ab38"
      "pcidebug" = "195:0:1"
      "IOChildIndex" = 2
      "layout-id" = <07000000>
      "IOPCIExpressLinkStatus" = 4356
      "pci-aspm-default" = 2
      "IOPCIExpressCapabilities" = 18
      "IOServiceDEXTEntitlements" = (("com.apple.developer.driverkit.transport.pci"))
      "IOInterruptControllers" = ("io-apic-3","IOPCIMessagedInterruptController")
      "built-in" = <00>
      "IOPCIResourced" = Yes
      "AAPL,slot-name" = "Built In"
      "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
      "IODeviceMemory" = (({"address"=3638165504,"length"=16384}))
      "acpi-pmcap-offset" = 80
      "name" = "HDMI Controller"
      "subsystem-id" = <38ab0000>
      "model" = <"Apple HDMI Audio Controller">
      "device_type" = <"HDMI Controller">
      "compatible" = <"pci1002,ab38","pciclass,040300","HDAU">
      "IOReportLegendPublic" = Yes
      "reg" = <0001c300000000000000000000000000000000001001c30200000000000000000000000000400000>
      "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="HDAU 1"})
      "device-id" = <38ab0000>
      "revision-id" = <00000000>
      "IOInterruptSpecifiers" = (<0400000007000000>,<1b00000000000100>)
      "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2A@0/SL05@ffff/EGP1@0/HDAU@1"
    }
    

