Dumped from libSMC.dylib as of 10.14 beta 7 (6.200.5)

Dumping keys for m87...
 Set 0 has 24 keys:
 [    ] type [sp7s] 73703738 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [sp7s] 73703738 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [  9]: NB 1.05V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: NB 1.05V Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: GPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 14]: GPU Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [ 15]: NB 1.25V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: NB 1.25V Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 19]: GPU Frame Buffer Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 20]: GPU Frame Buffer Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 21]: NB 1.8V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 22]: NB 1.8V Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 23]: HP Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 12 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(Th1H)
 [TG0H] type [sp7s] 73703738 len [ 2] idx [  5]: NB Proximity Temp(TG0H)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  6]: Heat Pipe Temp(Th2H)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [  7]: Airport Temp (TW0P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  8]: Palm Rest Temp(Ts0P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: Charger Prox Temp(Tm0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [ 10]: Fan Target Temp(TTF0)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU Prox Temp(TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Die Temp(TG0D)
 [    ] type [sp7s] 73703738 len [ 2] idx [ 16]: Battery Temp
Dumping keys for m88...
 Set 0 has 24 keys:
 [    ] type [sp7s] 73703738 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [sp7s] 73703738 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [  9]: NB 1.05V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: NB 1.05V Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: GPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 14]: GPU Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [ 15]: NB 1.25V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: NB 1.25V Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 19]: GPU Frame Buffer Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 20]: GPU Frame Buffer Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 21]: NB 1.8V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 22]: NB 1.8V Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 23]: HP Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 12 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(Th1H)
 [TG0H] type [sp7s] 73703738 len [ 2] idx [  5]: NB Proximity Temp(TG0H)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  6]: Heat Pipe Temp(Th2H)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [  7]: Airport Temp (TW0P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  8]: Palm Rest Temp(Ts0P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: Charger Prox Temp(Tm0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [ 10]: Fan Target Temp(TTF0)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU Prox Temp(TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Die Temp(TG0D)
 [    ] type [sp7s] 73703738 len [ 2] idx [ 16]: Battery Temp
Dumping keys for m98...
 Set 0 has 27 keys:
 [    ] type [spns] 73706E38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [spns] 73706E38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [ 12]: GPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: GPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 14]: GPU Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [ 15]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: MCP DDR Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 17]: CPU 1.05V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 18]: CPU 1.05V Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 19]: GPU Frame Buffer Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 20]: GPU Frame Buffer Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 21]: CPU High Side Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 22]: CPU High Side Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 23]: HP Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 18 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(Th2H)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  5]: MCP Prox Temp(TN0P)
 [TG0H] type [sp7s] 73703738 len [ 2] idx [  6]: Heat Pipe Temp(TG0H)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Pipe Syth Temp(Ts0S)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  8]: Palm Rest Temp(Ts0P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: Batt Charger Prox Temp(Tm0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [ 10]: Fan Target Temp(TTF0)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU Prox Temp(TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Die Digital Temp(TG0D)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [ 13]: GPU Die Analog Temp(TG0T)
 [TG1H] type [sp7s] 73703738 len [ 2] idx [ 14]: Heat Pipe Temp2(TG1H)
 [TB3T] type [sp7s] 73703738 len [ 2] idx [ 15]: Battery Ambient Temp (TB3T)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 16]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 17]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 18]: Battery Thermistor 1(TB2T)
Dumping keys for m98a...
 Set 0 has 27 keys:
 [    ] type [spns] 73706E38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [spns] 73706E38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [ 12]: GPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: GPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 14]: GPU Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [ 15]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: MCP DDR Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 17]: CPU 1.05V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 18]: CPU 1.05V Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 19]: GPU Frame Buffer Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 20]: GPU Frame Buffer Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 21]: CPU High Side Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 22]: CPU High Side Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 23]: HP Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 18 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(Th2H)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  5]: MCP Prox Temp(TN0P)
 [TG0H] type [sp7s] 73703738 len [ 2] idx [  6]: Heat Pipe Temp(TG0H)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Pipe Syth Temp(Ts0S)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  8]: Palm Rest Temp(Ts0P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: Batt Charger Prox Temp(Tm0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [ 10]: Fan Target Temp(TTF0)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU Prox Temp(TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Die Digital Temp(TG0D)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [ 13]: GPU Die Analog Temp(TG0T)
 [TG1H] type [sp7s] 73703738 len [ 2] idx [ 14]: Heat Pipe Temp2(TG1H)
 [TB3T] type [sp7s] 73703738 len [ 2] idx [ 15]: Battery Ambient Temp (TB3T)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 16]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 17]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 18]: Battery Thermistor 1(TB2T)
Dumping keys for K20...
 Set 0 has 27 keys:
 [    ] type [spns] 73706E38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [spns] 73706E38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [ 12]: GPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: GPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 14]: GPU Voltage
 [    ] type [spns] 73706E38 len [ 2] idx [ 15]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: MCP DDR Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 17]: CPU 1.05V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 18]: CPU 1.05V Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 19]: GPU Frame Buffer Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 20]: GPU Frame Buffer Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 21]: CPU High Side Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 22]: CPU High Side Current
 [    ] type [spns] 73706E38 len [ 2] idx [ 23]: HP Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 18 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(Th2H)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  5]: MCP Prox Temp(TN0P)
 [TG0H] type [sp7s] 73703738 len [ 2] idx [  6]: Heat Pipe Temp(TG0H)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Pipe Syth Temp(Ts0S)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  8]: Palm Rest Temp(Ts0P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: Batt Charger Prox Temp(Tm0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [ 10]: Fan Target Temp(TTF0)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU Prox Temp(TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Die Digital Temp(TG0D)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [ 13]: GPU Die Analog Temp(TG0T)
 [TG1H] type [sp7s] 73703738 len [ 2] idx [ 14]: Heat Pipe Temp2(TG1H)
 [TB3T] type [sp7s] 73703738 len [ 2] idx [ 15]: Battery Ambient Temp (TB3T)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 16]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 17]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 18]: Battery Thermistor 1(TB2T)
Dumping keys for K19...
 Set 0 has 40 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 12]: GPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: GPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 14]: GPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 15]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 17]: CPU 1.05V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 18]: CPU 1.05V Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 19]: GPU 1.8V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 20]: GPU 1.8V Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 21]: CPU High Side Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 22]: CPU High Sdie Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 23]: Heatpipe Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 24]: ODD Voltage
 [    ] type [fp4f] 66703463 len [ 2] idx [ 25]: ODD Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 26]: ODD Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 27]: Airport Voltage
 [    ] type [fp4f] 66703463 len [ 2] idx [ 28]: Airport Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 29]: Airport Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 30]: HDD Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 31]: HDD Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 32]: DIMM Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 33]: DIMM Power
 [    ] type [fp2f] 66703265 len [ 2] idx [ 34]: Backlight Input Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 35]: Backlight Input Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 36]: Backlight Output Voltage
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 18 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(Th1H)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP die temp (TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  5]: MCP prox temp (TN0P)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  6]: Heat Pipe Temp(Th2H)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Pipe Synthetic Temp(Ts0S)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  8]: Palm Rest Temp(Ts0P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: Charger Prox Temp(Tm0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [ 10]: Fan Target Temp(TTF0)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU Prox Temp(TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Die Digital Temp(TG0D)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [ 13]: GPU Die Analog Temp(TG0T)
 [    ] type [sp7s] 73703738 len [ 2] idx [ 14]: Not Connected
 [TB3T] type [sp7s] 73703738 len [ 2] idx [ 15]: Battery Temp(TB3T)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 16]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 17]: Battery Thermistor Temp 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 18]: Battery Thermistor Temp 1(TB2T)
Dumping keys for K19I...
 Set 0 has 40 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 12]: GPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: GPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 14]: GPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 15]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 17]: CPU 1.05V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 18]: CPU 1.05V Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 19]: GPU 1.8V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 20]: GPU 1.8V Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 21]: CPU High Side Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 22]: CPU High Sdie Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 23]: Heatpipe Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 24]: ODD Voltage
 [    ] type [fp4f] 66703463 len [ 2] idx [ 25]: ODD Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 26]: ODD Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 27]: Airport Voltage
 [    ] type [fp4f] 66703463 len [ 2] idx [ 28]: Airport Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 29]: Airport Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 30]: HDD Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 31]: HDD Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 32]: DIMM Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 33]: DIMM Power
 [    ] type [fp2f] 66703265 len [ 2] idx [ 34]: Backlight Input Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 35]: Backlight Input Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 36]: Backlight Output Voltage
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 18 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(Th1H)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP die temp (TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  5]: MCP prox temp (TN0P)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  6]: Heat Pipe Temp(Th2H)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Pipe Synthetic Temp(Ts0S)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  8]: Palm Rest Temp(Ts0P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: Charger Prox Temp(Tm0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [ 10]: Fan Target Temp(TTF0)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU Prox Temp(TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Die Digital Temp(TG0D)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [ 13]: GPU Die Analog Temp(TG0T)
 [    ] type [sp7s] 73703738 len [ 2] idx [ 14]: Not Connected
 [TB3T] type [sp7s] 73703738 len [ 2] idx [ 15]: Battery Temp(TB3T)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 16]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 17]: Battery Thermistor Temp 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 18]: Battery Thermistor Temp 1(TB2T)
Dumping keys for K17...
 Set 0 has 54 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [PP0R] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power (PP0R)
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [PC0C] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power (PC0C)
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [PN0R] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power (PN0R)
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [PG0C] type [fpof] 66706F38 len [ 2] idx [ 12]: GPU Power (PG0C)
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: GPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 14]: GPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 15]: CPU DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: CPU DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 17]: 1.05V S0 Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 18]: 1.05V S0 Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 19]: GPU 1.8V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 20]: GPU 1.8V Current
 [PC0R] type [fpof] 66706F38 len [ 2] idx [ 21]: CPU High Side Power (PC0R)
 [    ] type [fp4f] 66703463 len [ 2] idx [ 22]: CPU High Sdie Current
 [PHPC] type [fpof] 66706F38 len [ 2] idx [ 23]: Heatpipe Power (PHPC)
 [    ] type [fp4f] 66703463 len [ 2] idx [ 24]: ODD Voltage
 [    ] type [fp4f] 66703463 len [ 2] idx [ 25]: ODD Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 26]: ODD Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 27]: Airport Voltage
 [    ] type [fp4f] 66703463 len [ 2] idx [ 28]: Airport Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 29]: Airport Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 30]: HDD Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 31]: HDD Power
 [    ] type [fp2f] 66703265 len [ 2] idx [ 34]: Backlight Input Power
 [    ] type [fpof] 66706F38 len [ 2] idx [ 35]: Backlight Input Current
 [    ] type [fp6f] 66703661 len [ 2] idx [ 36]: Backlight Output Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 37]: S3 1.5V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 38]: S3 1.5V Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 39]: S5 3.3V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 40]: S5 3.3V Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 41]: S0 VTT PCH Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 42]: S0 VTT PCH Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 43]: PCH Core Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 44]: PCH Core Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 45]: S3 3.3V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 46]: S3 3.3V Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 47]: S0 5V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 48]: S0 5V Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 49]: S0 3.3V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 50]: S0 3.3V Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 51]: GPU 1.1V Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 52]: GPU 1.1V Current
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 18 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  3]: Right Fin Stack Temp(Th1H)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [  4]: GPU Die Analog Temp(TG0T)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [  5]: Right Fin Stack Temp(TG0D)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [  6]: Right Fin Stack Temp(TG0P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  7]: Palm Rest Temp(Ts0P)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  8]: Left Fin Stack Temp(Th2H)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: Battery Charger Prox Temp(Tm0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 10]: Heat Pipe Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 12]: Battery Thermistor Temp 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 13]: Battery Thermistor Temp 1(TB2T)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 14]: Max of CPU Core vs. Mem Ctlr/IG PECI Temps(TC1C)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 15]: PCH Die Temp(TPCD)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU Core PECI Temp(TC0C)
 [TMCD] type [sp7s] 73703738 len [ 2] idx [ 17]: Memory Controller/Integrated Graphics PECI Temp(TMCD)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [ 18]: PCH Prox Temp(TP0P)
Dumping keys for K18...
 Set 0 has 39 keys:
 [    ] type [sp7s] 73703738 len [ 2] idx [  1]: DCIn Power
 [    ] type [sp3s] 73703363 len [ 2] idx [  2]: DCIn Current
 [    ] type [sp7s] 73703738 len [ 2] idx [  3]: PBus Power
 [    ] type [sp4s] 73703462 len [ 2] idx [  4]: PBus Current
 [    ] type [sp4s] 73703462 len [ 2] idx [  5]: PBus Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Power
 [    ] type [sp6s] 73703639 len [ 2] idx [  7]: CPU Current
 [    ] type [sp1s] 73703165 len [ 2] idx [  8]: CPU Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [  9]: NB Int GPU Power
 [    ] type [sp6s] 73703639 len [ 2] idx [ 10]: NB Int GPU Current
 [    ] type [sp1s] 73703165 len [ 2] idx [ 11]: NB Int GPU Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU Power
 [    ] type [sp6s] 73703639 len [ 2] idx [ 13]: GPU Current
 [    ] type [sp1s] 73703165 len [ 2] idx [ 14]: GPU Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU DDR Power
 [    ] type [sp6s] 73703639 len [ 2] idx [ 16]: CPU DDR Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 17]: 1.05V S0 Power
 [    ] type [sp6s] 73703639 len [ 2] idx [ 18]: 1.05V S0 Current
 [    ] type [sp1s] 73703165 len [ 2] idx [ 37]: 1.05V S0 Voltage
 [    ] type [sp7s] 73703738 len [ 2] idx [ 19]: GPU 1.8V Power
 [    ] type [sp6s] 73703639 len [ 2] idx [ 20]: GPU 1.8V Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU High Side Power
 [    ] type [sp4s] 73703462 len [ 2] idx [ 22]: CPU High Sdie Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 23]: Heatpipe Power
 [    ] type [sp5s] 73703561 len [ 2] idx [ 24]: ODD Voltage
 [    ] type [sp2s] 73703264 len [ 2] idx [ 25]: ODD Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 26]: ODD Power
 [    ] type [fp4f] 66703463 len [ 2] idx [ 27]: Airport Voltage
 [    ] type [sp2s] 73703264 len [ 2] idx [ 28]: Airport Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 29]: Airport Power
 [    ] type [sp4s] 73703462 len [ 2] idx [ 30]: HDD Current
 [    ] type [sp7s] 73703738 len [ 2] idx [ 31]: HDD Power
 [    ] type [sp7s] 73703738 len [ 2] idx [ 34]: Backlight Input Power
 [    ] type [sp2s] 73703264 len [ 2] idx [ 35]: Backlight Input Current
 [    ] type [sp6s] 73703639 len [ 2] idx [ 36]: Backlight Output Voltage
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 17 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  3]: Right Fin Stack Temp(Th1H)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [  4]: GPU Die Analog Temp(TG0T)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [  5]: Right Fin Stack Temp(TG0D)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [  6]: Right Fin Stack Temp(TG0P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  7]: Palm Rest Temp(Ts0P)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  8]: Left Fin Stack Temp(Th2H)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: Battery Charger Prox Temp(Tm0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 10]: Heat Pipe Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 12]: Battery Thermistor Temp 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 13]: Battery Thermistor Temp 1(TB2T)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 14]: Max of CPU Core vs. Mem Ctlr/IG PECI Temps(TC1C)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 15]: PCH Die Temp(TPCD)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU Core PECI Temp(TC0C)
 [TMCD] type [sp7s] 73703738 len [ 2] idx [ 17]: Memory Controller/Integrated Graphics PECI Temp(TMCD)
Dumping keys for D2...
 Set 0 has 60 keys:
 [PHPC] type [sp8s] 73703837 len [ 2] idx [  1]: HP Power (Watts) (PHPC)
 [PC0R] type [sp8s] 73703837 len [ 2] idx [  2]: CPU Computing High Side Power (Watts) (PC0R)
 [PG0R] type [sp8s] 73703837 len [ 2] idx [  3]: Ext GPU Ext GPU High Side Power (Watts) (PG0R)
 [PO0R] type [sp8s] 73703837 len [ 2] idx [  4]: Other High Side Power   (Watts) (PO0R)
 [PDTR] type [sp8s] 73703837 len [ 2] idx [  5]: DC-In total power  (Watts) (PDTR)
 [PPBR] type [sp9s] 73703936 len [ 2] idx [  6]: PBus on battery power (Watts) (PPBR)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [  7]: HDD Power  (Watts) (PHDC)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [  8]: CPU Core Power (Watts) (PC0C)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [  9]: DDR Power (Watts) (PM0R)
 [PC1C] type [sp8s] 73703837 len [ 2] idx [ 10]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PN0R] type [sp7s] 73703738 len [ 2] idx [ 11]: NB Int GPU Power (Watts) (PN0R)
 [PC2C] type [sp8s] 73703837 len [ 2] idx [ 12]: CPU VCCSA Power (Watts) (PC2C)
 [PG0C] type [sp7s] 73703738 len [ 2] idx [ 13]: Ext GPU Power (Watts) (PG0C)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 14]: Backlight Input Power   (Watts) (PBLC)
 [PG3C] type [sp7s] 73703738 len [ 2] idx [ 15]: Ext GPU 1.35V Power (Watts) (PG3C)
 [PTPR] type [sp8s] 73703837 len [ 2] idx [ 16]: T25 - Track Pad Power (Watts) (PTPR)
 [PSBC] type [sp8s] 73703837 len [ 2] idx [ 17]: PCH core Power (DEBUG) (Watts) (PSBC)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 18]: Airport Power   (watts) (PAPC)
 [PHSC] type [sp7s] 73703738 len [ 2] idx [ 19]: Thunderbolt Power (Watts) (PHSC)
 [PG1C] type [sp7s] 73703738 len [ 2] idx [ 20]: Ext GPU 1.8V Power (DEBUG) (Watts) (PG1C)
 [PC3C] type [sp8s] 73703837 len [ 2] idx [ 21]: CPU DDR Power (Watts) (PC3C)
 [PLDC] type [sp8s] 73703837 len [ 2] idx [ 22]: LCD Driver Power (Watts) (PLDC)
 [PG2C] type [sp7s] 73703738 len [ 2] idx [ 23]: Ext GPU 1.0V Power  (DEBUG) (Watts) (PG2C)
 [VC0C] type [sp1s] 73703165 len [ 2] idx [ 24]: CPU Core voltage. (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 25]: CPU Core current. (Amps) (IC0C)
 [IG0R] type [sp4s] 73703462 len [ 2] idx [ 26]: Ext GPU High Side current. (Amps) (IG0R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 27]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp3s] 73703363 len [ 2] idx [ 28]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 29]: PBus rail voltage. (Volts) (VP0R)
 [IHDC] type [sp4s] 73703462 len [ 2] idx [ 30]: HDD Current  (Amps) (IHDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 31]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp4s] 73703462 len [ 2] idx [ 32]: CPU Computing High Side current. (Amps) (IC0R)
 [IO0R] type [sp4s] 73703462 len [ 2] idx [ 33]: Other High Side current.  (Amps) (IO0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 34]: DDR current. (Amps) (IM0C)
 [IC1C] type [sp6s] 73703639 len [ 2] idx [ 35]: VCCIO 1.05V S0  current. (Amps) (IC1C)
 [VN0C] type [sp1s] 73703165 len [ 2] idx [ 36]: NB Int GPU voltage. (Volts) (VN0C)
 [IC2C] type [sp6s] 73703639 len [ 2] idx [ 37]: VCCSA S0  current. (Amps) (IC2C)
 [VG0C] type [sp1s] 73703165 len [ 2] idx [ 38]: Ext GPU Core voltage. (Volts) (VG0C)
 [IG0C] type [sp6s] 73703639 len [ 2] idx [ 39]: Ext GPU Core current. (Amps) (IG0C)
 [VBLC] type [sp6s] 73703639 len [ 2] idx [ 40]: Backlight Output Voltage.  (Volts) (VBLC)
 [IBLC] type [sp1s] 73703165 len [ 2] idx [ 41]: Backlight Current.  (Amps) (IBLC)
 [IN0C] type [sp6s] 73703639 len [ 2] idx [ 42]: NB Int GPU current. (Amps) (IN0C)
 [IG3C] type [sp4s] 73703462 len [ 2] idx [ 43]: Ext GPU  1.35 V current. (Amps) (IG3C)
 [ITPC] type [sp4s] 73703462 len [ 2] idx [ 44]: T25 - Track Pad Current  (Amps) (ITPC)
 [ISBC] type [sp4s] 73703462 len [ 2] idx [ 45]: PCH core  Current (Amps) (ISBC)
 [IAPC] type [sp4s] 73703462 len [ 2] idx [ 46]: Airport Current (Amps) (IAPC)
 [IHSC] type [sp4s] 73703462 len [ 2] idx [ 47]: Thunderbolt Current  (Amps) (IHSC)
 [IG1C] type [sp4s] 73703462 len [ 2] idx [ 48]: Ext GPU 1.8V current. (DEBUG) (Amps) (IG1C)
 [VCRP] type [sp7s] 73703738 len [ 2] idx [ 49]: CPU Ripple voltage. (DEBUG) (Volts) (VCRP)
 [IC3C] type [sp4s] 73703462 len [ 2] idx [ 50]: CPU DDR Current (Debug)  (Amps) (IC3C)
 [ILDC] type [sp4s] 73703462 len [ 2] idx [ 51]: LCD Driver Current (Debug)  (Amps) (ILDC)
 [IG2C] type [sp4s] 73703462 len [ 2] idx [ 52]: Ext GPU 1.0V current. (DEBUG) (Amps) (IG2C)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 38 keys:
 [PCPT] type [sp8s] 73703837 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp8s] 73703837 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp8s] 73703837 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [  4]: CPU PECI die temp  (DegC) (TCXC)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  5]: CPU proximity temp (DegC) (TC0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [  6]: PCH Proxmity temp (DegC) (TP0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [  7]: DCIn Air flow Temperature (DegC) (Ta0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  8]: Right Fin stack temp (DegC) (Th1H)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [  9]: GPU Die Analog temp (DegC) (TG0D)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 10]: GPU proximity temp (DegC) (TG0P)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [ 11]: Left Fin stack temp (DegC) (Th2H)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 12]: Dimm Proximity temp(DegC) (TM0P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 13]: Airport Temp (DegC) (TW0P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 14]: Palm Rest Temp (DegC) (Ts0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 15]: PCH Die temp (DegC) (TPCD)
 [TS0P] type [sp7s] 73703738 len [ 2] idx [ 16]: Speaker Proximity Temp (DegC) (TS0P)
 [TS0D] type [sp7s] 73703738 len [ 2] idx [ 17]: Speaker Remote Temp (DegC) (TS0D)
 [TS1P] type [sp7s] 73703738 len [ 2] idx [ 18]: Speaker Proximity 2 Temp (DegC) (TS1P)
 [TS1D] type [sp7s] 73703738 len [ 2] idx [ 19]: Speaker Remote 2 Temp (DegC) (TS1D)
 [MST1] type [sp8s] 73703837 len [ 2] idx [ 20]: Audio ScratchPad register (MST1)
 [MST2] type [sp8s] 73703837 len [ 2] idx [ 21]: Audio ScratchPad2 register (MST2)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 22]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 23]: CPU die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU PECI die temp Trend (DegC) (TCTD)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TMBS] type [sp7s] 73703738 len [ 2] idx [ 26]: DIMM Bandwidth Estimate (DegC) (TMBS)
 [TM0S] type [sp7s] 73703738 len [ 2] idx [ 27]: Synthetic DIMM Estimate(DegC) (TM0S)
 [Ts1S] type [sp7s] 73703738 len [ 2] idx [ 28]: Synthetic Top skin (DegC) (Ts1S)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 29]: SSD Temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 30]: SSD Temp B  (DegC) (TH0B)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [PSTR] type [sp8s] 73703837 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [si1s] 73693136 len [ 2] idx [243]: Battery Actual current. (A) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (V) (B0AV)
Dumping keys for J15...
 Set 0 has 58 keys:
 [PHPC] type [sp8s] 73703837 len [ 2] idx [  1]: HP Power (Watts) (PHPC)
 [PC0R] type [sp9s] 73703936 len [ 2] idx [  2]: CPU Computing High Side Power (Watts) (PC0R)
 [PG0R] type [sp8s] 73703837 len [ 2] idx [  3]: Ext GPU High Side Power (Watts) (PG0R)
 [PO0R] type [sp8s] 73703837 len [ 2] idx [  4]: Other High Side Power   (Watts) (PO0R)
 [PO0R] type [sp8s] 73703837 len [ 2] idx [  5]: Other High Side Power   (Watts) (PO0R)
 [PDTR] type [sp8s] 73703837 len [ 2] idx [  6]: DC-In total power  (Watts) (PDTR)
 [PPBR] type [sp9s] 73703936 len [ 2] idx [  7]: PBus on battery power (Watts) (PPBR)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [  8]: SSD Power  (Watts) (PHDC)
 [PC0C] type [spas] 73706135 len [ 2] idx [  9]: CPU Core Package Power (Watts) (PC0C)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [ 10]: DDR Power (Watts) (PM0R)
 [PC3C] type [sp8s] 73703837 len [ 2] idx [ 11]: CPU DDR Power (Watts) (PC3C)
 [PG0C] type [sp7s] 73703738 len [ 2] idx [ 12]: Ext GPU Power (Watts) (PG0C)
 [PG1C] type [sp7s] 73703738 len [ 2] idx [ 13]: Ext GPU Frame Buffer Power  (Watts) (PG1C)
 [PG2C] type [sp7s] 73703738 len [ 2] idx [ 14]: Ext GPU 1.05V Power (Watts) (PG2C)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 15]: Backlight Input Power   (Watts) (PBLC)
 [PSBC] type [sp8s] 73703837 len [ 2] idx [ 16]: PCH core Power (Watts) (PSBC)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 17]: Airport Power   (watts) (PAPC)
 [PHSC] type [sp7s] 73703738 len [ 2] idx [ 18]: Thunderbolt Power (Watts) (PHSC)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 19]: CPU Package Core voltage. (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 20]: CPU Package Core current. (Amps) (IC0C)
 [IG0R] type [sp4s] 73703462 len [ 2] idx [ 21]: Ext GPU High Side current. (Amps) (IG0R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 22]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp4s] 73703462 len [ 2] idx [ 23]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 24]: PBus rail voltage. (Volts) (VP0R)
 [IHDC] type [sp4s] 73703462 len [ 2] idx [ 25]: SSD Current  (Amps) (IHDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 26]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 27]: CPU Computing High Side current. (Amps) (IC0R)
 [IO0R] type [sp4s] 73703462 len [ 2] idx [ 28]: Other High Side current.  (Amps) (IO0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 29]: DDR current. (Amps) (IM0C)
 [IC3C] type [sp6s] 73703639 len [ 2] idx [ 30]: CPU DDR Current  (Amps) (IC3C)
 [ILDC] type [sp1s] 73703165 len [ 2] idx [ 31]: LCD Panel Current  (Amps) (ILDC)
 [VG0C] type [sp1s] 73703165 len [ 2] idx [ 32]: Ext GPU Core voltage. (Volts) (VG0C)
 [IG0C] type [sp6s] 73703639 len [ 2] idx [ 33]: Ext GPU Core current. (Amps) (IG0C)
 [VBLC] type [sp6s] 73703639 len [ 2] idx [ 34]: Backlight Output Boosted Voltage.  (Volts) (VBLC)
 [IBLC] type [sp1s] 73703165 len [ 2] idx [ 35]: LCD Backlight Current.  (Amps) (IBLC)
 [VG1C] type [sp2s] 73703264 len [ 2] idx [ 36]: Ext GPU Frame Buffer Voltage. (Volts) (VG1C)
 [IG1C] type [sp6s] 73703639 len [ 2] idx [ 37]: Ext GPU Frame Buffer current.  (Amps) (IG1C)
 [IG2C] type [sp4s] 73703462 len [ 2] idx [ 38]: Ext GPU 1.05V current. (Amps) (IG2C)
 [ISBC] type [sp4s] 73703462 len [ 2] idx [ 39]: PCH core  Current (Amps) (ISBC)
 [IAPC] type [sp4s] 73703462 len [ 2] idx [ 40]: Airport Current (Amps) (IAPC)
 [IHSC] type [sp4s] 73703462 len [ 2] idx [ 41]: Thunderbolt Current  (Amps) (IHSC)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [PZ1F] type [sp8s] 73703837 len [ 2] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [sp8s] 73703837 len [ 2] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [ui1u] 75693136 len [ 2] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [sp8s] 73703837 len [ 2] idx [226]: Zone 1 Filtered Power (PZ2F)
 [PZ2E] type [sp8s] 73703837 len [ 2] idx [227]: Zone 1 Target Power (PZ2E)
 [PZ2T] type [ui1u] 75693136 len [ 2] idx [228]: Zone 1 Abstract Throttle (PZ2T)
 [PZ3F] type [sp8s] 73703837 len [ 2] idx [229]: Zone 1 Filtered Power (PZ3F)
 [PZ3E] type [sp8s] 73703837 len [ 2] idx [230]: Zone 1 Target Power (PZ3E)
 [PZ3T] type [ui1u] 75693136 len [ 2] idx [231]: Zone 1 Abstract Throttle (PZ3T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 41 keys:
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  1]: Palm Rest Temp (DegC) (Ts0P)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [  2]: CPU PECI die temp  (DegC) (TCXC)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  3]: CPU proximity temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  4]: Dimm Proximity temp(DegC) (TM0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [  5]: PCH Proxmity temp (DegC) (TP0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [  6]: DCIn Air flow Temperature (DegC) (Ta0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [  7]: GPU Die Analog temp (DegC) (TG0D)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  8]: Right Fin stack temp (DegC) (Th1H)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  9]: Left Fin stack temp (DegC) (Th2H)
 [TG1d] type [sp7s] 73703738 len [ 2] idx [ 10]: GPU digital die temp Raw (without offset) (DegC) (TG1d)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 11]: Airport Temp (DegC) (TW0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 12]: PCH Die temp (DegC) (TPCD)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC3C] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU Core 2 temp (PECI) (DegC) (TC3C)
 [TC4C] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU Core 3 temp (PECI) (DegC) (TC4C)
 [PCPT] type [sp8s] 73703837 len [ 2] idx [ 17]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp8s] 73703837 len [ 2] idx [ 18]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp8s] 73703837 len [ 2] idx [ 19]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 20]: Synthetic bottom skin (DegC) (Ts0S)
 [Ts1S] type [sp7s] 73703738 len [ 2] idx [ 21]: Synthetic Top skin (DegC) (Ts1S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 23]: CPU PECI die temp Trend (DegC) (TCTD)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TMBS] type [sp7s] 73703738 len [ 2] idx [ 25]: DIMM Bandwidth Estimate (DegC) (TMBS)
 [TM0S] type [sp7s] 73703738 len [ 2] idx [ 26]: Synthetic DIMM Estimate(DegC) (TM0S)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 27]: SSD Temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 28]: SSD Temp B  (DegC) (TH0B)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 29]: GPU proximity temp (DegC) (TG0P)
 [TG1D] type [sp7s] 73703738 len [ 2] idx [ 30]: GPU digital die temp (DegC) (TG1D)
 [TG1F] type [sp7s] 73703738 len [ 2] idx [ 31]: GPU digital die temp filtered (DegC) (TG1F)
 [TaSP] type [sp7s] 73703738 len [ 2] idx [ 32]: DCIn Air flow Adjusted Temperature (DegC) (TaSP)
 [TH0V] type [sp7s] 73703738 len [ 2] idx [ 33]: SSD Temp B Foreign Drive Prediction   (DegC) (TH0V)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [PSTR] type [sp8s] 73703837 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for J45...
 Set 0 has 41 keys:
 [PC0C] type [spas] 73706135 len [ 2] idx [  1]: CPU Core Package Power (Includes Integrated Graphics Power) (Watts) (PC0C)
 [PDTR] type [sp8s] 73703837 len [ 2] idx [  2]: DC-In total power  (Watts) (PDTR)
 [PPBR] type [sp9s] 73703936 len [ 2] idx [  3]: PBus on battery power (Watts) (PPBR)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [  4]: SSD Power  (Watts) (PHDC)
 [PC0R] type [sp9s] 73703936 len [ 2] idx [  5]: CPU Computing High Side Power (Watts) (PC0R)
 [PO3R] type [sp8s] 73703837 len [ 2] idx [  6]: Other 3.3V High Side Power   (Watts) (PO3R)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [  7]: DDR Power (Watts) (PM0R)
 [PC3C] type [sp8s] 73703837 len [ 2] idx [  8]: CPU DDR Power (Watts) (PC3C)
 [PO5R] type [sp8s] 73703837 len [ 2] idx [  9]: Other 5V High Side Power   (Watts) (PO5R)
 [PLDC] type [sp8s] 73703837 len [ 2] idx [ 10]: LCD Panel Power (Watts) (PLDC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 11]: Backlight Input Power   (Watts) (PBLC)
 [PCMC] type [sp8s] 73703837 len [ 2] idx [ 12]: S2 Camera Power (Watts) (PCMC)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 13]: Airport Power   (Watts) (PAPC)
 [PHSC] type [sp7s] 73703738 len [ 2] idx [ 14]: Thunderbolt Power (Watts) (PHSC)
 [PTPC] type [sp8s] 73703837 len [ 2] idx [ 15]: T101 Boost/PBus Accuator Power (Watts) (PTPC)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 16]: CPU Package Core Voltage. (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 17]: CPU Package Core current. (Amps) (IC0C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 18]: DC In Voltage. (Volts) (VD0R)
 [ID0R] type [sp4s] 73703462 len [ 2] idx [ 19]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 20]: PBus rail Voltage. (Volts) (VP0R)
 [IHDC] type [sp4s] 73703462 len [ 2] idx [ 21]: SSD Current  (Amps) (IHDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 22]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 23]: CPU Computing High Side current. (Amps) (IC0R)
 [IO3R] type [sp4s] 73703462 len [ 2] idx [ 24]: Other 3.3V High Side current.  (Amps) (IO3R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 25]: DDR current. (Amps) (IM0C)
 [IC3C] type [sp6s] 73703639 len [ 2] idx [ 26]: CPU DDR Current  (Amps) (IC3C)
 [ILDC] type [sp1s] 73703165 len [ 2] idx [ 27]: LCD Panel Current  (Amps) (ILDC)
 [IO5R] type [sp4s] 73703462 len [ 2] idx [ 28]: Other 5V High Side current.  (Amps) (IO5R)
 [VTPC] type [sp6s] 73703639 len [ 2] idx [ 29]: T101 Boost/PBus Accuator Voltage. (Volts) (VTPC)
 [IBLC] type [sp1s] 73703165 len [ 2] idx [ 30]: LCD Backlight Current.  (Amps) (IBLC)
 [ICMC] type [sp4s] 73703462 len [ 2] idx [ 31]: S2 Camera Current  (Amps) (ICMC)
 [ITPC] type [sp4s] 73703462 len [ 2] idx [ 32]: T101 Boost/PBus Accuator Current  (Amps) (ITPC)
 [IAPC] type [sp4s] 73703462 len [ 2] idx [ 33]: Airport Current (Amps) (IAPC)
 [IHSC] type [sp4s] 73703462 len [ 2] idx [ 34]: Thunderbolt Current  (Amps) (IHSC)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PTHC] type [fltf] 666C7420 len [ 4] idx [221]: HP Power Target (PTHC)
 [MSLT] type [fltf] 666C7420 len [ 4] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 36 keys:
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  1]: Palm Rest Temp (DegC) (Ts0P)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU proximity temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  3]: Dimm Proximity temp(DegC) (TM0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [  4]: PCH Proxmity temp (DegC) (TP0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [  5]: DCIn Air flow Temperature (DegC) (Ta0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  6]: Right Fin stack temp (DegC) (Th1H)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  7]: Left Fin stack temp (DegC) (Th2H)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [  9]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC3C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU Core 2 temp (PECI) (DegC) (TC3C)
 [TC4C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Core 3 temp (PECI) (DegC) (TC4C)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU PECI die temp  (DegC) (TCXC)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [PCPT] type [sp8s] 73703837 len [ 2] idx [ 15]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp8s] 73703837 len [ 2] idx [ 16]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp8s] 73703837 len [ 2] idx [ 17]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 18]: Airport Temp (DegC) (TW0P)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 19]: Drive0 (SSD Gumstick) OOB v3 raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 20]: Drive0 (SSD Gumstick) OOB v3 raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive0 (SSD Gumstick) OOB v3 raw temp C (DegC) (TH0c)
 [TH0x] type [sp7s] 73703738 len [ 2] idx [ 22]: Drive0 (SSD Gumstick) OOB v3 raw temp Max (DegC) (TH0x)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 23]: Synthetic bottom skin (DegC) (Ts0S)
 [Ts1S] type [sp7s] 73703738 len [ 2] idx [ 24]: Synthetic Top skin (DegC) (Ts1S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU die Virtual temp (DegC) (TC0E)
 [TM0S] type [sp7s] 73703738 len [ 2] idx [ 26]: Synthetic DIMM Estimate(DegC) (TM0S)
 [TMBS] type [sp7s] 73703738 len [ 2] idx [ 27]: DIMM Bandwidth Estimate (DegC) (TMBS)
 [TH0V] type [sp7s] 73703738 len [ 2] idx [ 28]: SSD Temp B Foreign Drive Prediction   (DegC) (TH0V)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [PSTR] type [sp8s] 73703837 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [si1s] 73693136 len [ 2] idx [243]: Battery Actual current. (A) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (V) (B0AV)
Dumping keys for J53...
 Set 0 has 44 keys:
 [VC0C] type [sp2s] 73703264 len [ 2] idx [  1]: CPU Package Core Voltage. (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [  2]: CPU Package Core current. (Amps) (IC0C)
 [ITPC] type [sp4s] 73703462 len [ 2] idx [  3]: T101 Accuator Current  (Amps) (ITPC)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [  4]: DC In Voltage. (Volts) (VD0R)
 [ID0R] type [sp4s] 73703462 len [ 2] idx [  5]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [  6]: PBus rail Voltage. (Volts) (VP0R)
 [IHDC] type [sp4s] 73703462 len [ 2] idx [  7]: SSD Current  (Amps) (IHDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [  8]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [  9]: CPU Computing High Side current. (Amps) (IC0R)
 [IO3R] type [sp4s] 73703462 len [ 2] idx [ 10]: Other 3.3V High Side current.  (Amps) (IO3R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 11]: DDR current. (Amps) (IM0C)
 [IC3C] type [sp6s] 73703639 len [ 2] idx [ 12]: CPU DDR Current  (Amps) (IC3C)
 [ILDC] type [sp1s] 73703165 len [ 2] idx [ 13]: LCD Panel Current  (Amps) (ILDC)
 [IO5R] type [sp4s] 73703462 len [ 2] idx [ 14]: Other 5V High Side current.  (Amps) (IO5R)
 [IBLC] type [sp1s] 73703165 len [ 2] idx [ 15]: LCD Backlight Current.  (Amps) (IBLC)
 [ICMC] type [sp4s] 73703462 len [ 2] idx [ 16]: S2 Camera Current  (Amps) (ICMC)
 [VTPC] type [sp6s] 73703639 len [ 2] idx [ 17]: T101 Accuator Voltage. (Volts) (VTPC)
 [IAPC] type [sp4s] 73703462 len [ 2] idx [ 18]: Airport Current (Amps) (IAPC)
 [IHSC] type [sp4s] 73703462 len [ 2] idx [ 19]: Thunderbolt Current  (Amps) (IHSC)
 [PC0C] type [spas] 73706135 len [ 2] idx [ 20]: CPU Core Package Power (Includes Integrated Graphics Power) (Watts) (PC0C)
 [PDTR] type [sp8s] 73703837 len [ 2] idx [ 21]: DC-In total power  (Watts) (PDTR)
 [PPBR] type [sp9s] 73703936 len [ 2] idx [ 22]: PBus on battery power (Watts) (PPBR)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [ 23]: SSD Power  (Watts) (PHDC)
 [PC0R] type [sp9s] 73703936 len [ 2] idx [ 24]: CPU Computing High Side Power (Watts) (PC0R)
 [PO3R] type [sp8s] 73703837 len [ 2] idx [ 25]: Other 3.3V High Side Power   (Watts) (PO3R)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [ 26]: DDR Power (Watts) (PM0R)
 [PC3C] type [sp8s] 73703837 len [ 2] idx [ 27]: CPU DDR Power (Watts) (PC3C)
 [PO5R] type [sp8s] 73703837 len [ 2] idx [ 28]: Other 5V High Side Power   (Watts) (PO5R)
 [PLDC] type [sp7s] 73703738 len [ 2] idx [ 29]: LCD Panel Power (Watts) (PLDC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 30]: Backlight Input Power   (Watts) (PBLC)
 [PCMC] type [sp8s] 73703837 len [ 2] idx [ 31]: S2 Camera Power (Watts) (PCMC)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 32]: Airport Power   (Watts) (PAPC)
 [PHSC] type [sp7s] 73703738 len [ 2] idx [ 33]: Thunderbolt Power (Watts) (PHSC)
 [PTPC] type [spas] 73706135 len [ 2] idx [ 34]: T101 Accuator Power (Watts) (PTPC)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [ 35]: HP Power (Watts) (PHPC)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 48 keys:
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  1]: Palm Rest Temp (DegC) (Ts0P)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU proximity temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  3]: Dimm Proximity temp(DegC) (TM0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [  4]: PCH Proxmity temp (DegC) (TP0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [  5]: DCIn Air flow Temperature (DegC) (Ta0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  6]: Right Fin stack temp (DegC) (Th1H)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  7]: Left Fin stack temp (DegC) (Th2H)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [  8]: PCH Die temp (DegC) (TPCD)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  9]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC3C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Core 2 temp (PECI) (DegC) (TC3C)
 [TC4C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core 3 temp (PECI) (DegC) (TC4C)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU PECI die temp  (DegC) (TCXC)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [PCPT] type [sp8s] 73703837 len [ 2] idx [ 16]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp8s] 73703837 len [ 2] idx [ 17]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp8s] 73703837 len [ 2] idx [ 18]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 19]: Airport Temp (DegC) (TW0P)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 20]: Drive0 (SSD Gumstick) OOB v3 raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive0 (SSD Gumstick) OOB v3 raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 22]: Drive0 (SSD Gumstick) OOB v3 raw temp C (DegC) (TH0c)
 [TH0x] type [sp7s] 73703738 len [ 2] idx [ 23]: Drive0 (SSD Gumstick) OOB v3 raw temp Max (DegC) (TH0x)
 [TCMc] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU eDRAM Hot Indicator(PECI) (DegC) (TCMc)
 [Ts1P] type [sp7s] 73703738 len [ 2] idx [ 25]: Palm Rest Temp 2 (DegC) (Ts1P)
 [TBXT] type [sp7s] 73703738 len [ 2] idx [ 26]: Battery temp (Same as TB0T) (DegC) (TBXT)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 27]: Synthetic bottom skin (DegC) (Ts0S)
 [Ts1S] type [sp7s] 73703738 len [ 2] idx [ 28]: Synthetic Top skin (DegC) (Ts1S)
 [IBAC] type [sp7s] 73703738 len [ 2] idx [ 29]: Battery Current (Amps) (IBAC)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 30]: CPU die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 31]: CPU PECI die temp Trend (DegC) (TCTD)
 [TCFC] type [ui1u] 75693136 len [ 2] idx [ 32]: CPU PECI die temp filter coeff (TCFC)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 33]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TM0S] type [sp7s] 73703738 len [ 2] idx [ 34]: Synthetic DIMM Estimate(DegC) (TM0S)
 [TaSP] type [sp7s] 73703738 len [ 2] idx [ 35]: DCIn Air flow Adjusted Temperature (DegC) (TaSP)
 [TH0V] type [sp7s] 73703738 len [ 2] idx [ 36]: SSD Temp B Foreign Drive Prediction   (DegC) (TH0V)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 37]: SSD Temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 38]: SSD Temp B  (DegC) (TH0B)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 39]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 40]: Drive 0 OOBv3 relative cooked temp Max Filtered (DegC) (TH0F)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [PSTR] type [sp8s] 73703837 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [si1s] 73693136 len [ 2] idx [243]: Battery Actual current. (A) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (V) (B0AV)
Dumping keys for J45G...
 Set 0 has 57 keys:
 [PC0C] type [spas] 73706135 len [ 2] idx [  1]: CPU Core Package Power (Includes Integrated Graphics Power) (Watts) (PC0C)
 [PG0R] type [sp8s] 73703837 len [ 2] idx [  2]: Ext GPU High Side Power (Watts) (PG0R)
 [PDTR] type [sp8s] 73703837 len [ 2] idx [  3]: DC-In total power  (Watts) (PDTR)
 [PPBR] type [sp9s] 73703936 len [ 2] idx [  4]: PBus on battery power (Watts) (PPBR)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [  5]: SSD Power  (Watts) (PHDC)
 [PC0R] type [sp9s] 73703936 len [ 2] idx [  6]: CPU Computing High Side Power (Watts) (PC0R)
 [PO3R] type [sp8s] 73703837 len [ 2] idx [  7]: Other 3.3V High Side Power   (Watts) (PO3R)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [  8]: DDR Power (Watts) (PM0R)
 [PC3C] type [sp8s] 73703837 len [ 2] idx [  9]: CPU DDR Power (Watts) (PC3C)
 [PLDC] type [sp8s] 73703837 len [ 2] idx [ 10]: LCD Panel Power (Watts) (PLDC)
 [PG0C] type [sp7s] 73703738 len [ 2] idx [ 11]: Ext GPU Power (Watts) (PG0C)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 12]: Backlight Input Power   (Watts) (PBLC)
 [PG1C] type [sp8s] 73703837 len [ 2] idx [ 13]: Ext GPU Frame Buffer Power  (Watts) (PG1C)
 [PG2C] type [sp7s] 73703738 len [ 2] idx [ 14]: Ext GPU 1.05V Power (Watts) (PG2C)
 [PCMC] type [sp8s] 73703837 len [ 2] idx [ 15]: S2 Camera Power (Watts) (PCMC)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 16]: Airport Power   (Watts) (PAPC)
 [PHSC] type [sp7s] 73703738 len [ 2] idx [ 17]: Thunderbolt Power (Watts) (PHSC)
 [PO5R] type [sp8s] 73703837 len [ 2] idx [ 18]: Other 5V High Side Power   (Watts) (PO5R)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 19]: CPU Package Core voltage. (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 20]: CPU Package Core current. (Amps) (IC0C)
 [IG0R] type [sp4s] 73703462 len [ 2] idx [ 21]: Ext GPU High Side current. (Amps) (IG0R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 22]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp4s] 73703462 len [ 2] idx [ 23]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 24]: PBus rail voltage. (Volts) (VP0R)
 [IHDC] type [sp4s] 73703462 len [ 2] idx [ 25]: SSD Current  (Amps) (IHDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 26]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 27]: CPU Computing High Side current. (Amps) (IC0R)
 [IO3R] type [sp4s] 73703462 len [ 2] idx [ 28]: Other 3.3V High Side current.  (Amps) (IO3R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 29]: DDR current. (Amps) (IM0C)
 [IC3C] type [sp6s] 73703639 len [ 2] idx [ 30]: CPU DDR Current  (Amps) (IC3C)
 [ILDC] type [sp1s] 73703165 len [ 2] idx [ 31]: LCD Panel Current  (Amps) (ILDC)
 [IO5R] type [sp4s] 73703462 len [ 2] idx [ 32]: Other 5V High Side current.  (Amps) (IO5R)
 [VG0C] type [sp1s] 73703165 len [ 2] idx [ 33]: Ext GPU Core voltage. (Volts) (VG0C)
 [IG0C] type [sp6s] 73703639 len [ 2] idx [ 34]: Ext GPU Core current. (Amps) (IG0C)
 [IBLC] type [sp1s] 73703165 len [ 2] idx [ 35]: LCD Backlight Current.  (Amps) (IBLC)
 [VG1C] type [sp2s] 73703264 len [ 2] idx [ 36]: Ext GPU Frame Buffer Voltage. (Volts) (VG1C)
 [IG1C] type [sp6s] 73703639 len [ 2] idx [ 37]: Ext GPU Frame Buffer current.  (Amps) (IG1C)
 [ICMC] type [sp4s] 73703462 len [ 2] idx [ 38]: S2 Camera Current  (Amps) (ICMC)
 [IG2C] type [sp4s] 73703462 len [ 2] idx [ 39]: Ext GPU 1.05V current. (Amps) (IG2C)
 [IAPC] type [sp4s] 73703462 len [ 2] idx [ 40]: Airport Current (Amps) (IAPC)
 [IHSC] type [sp2s] 73703264 len [ 2] idx [ 41]: Thunderbolt Current  (Amps) (IHSC)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PTHC] type [fltf] 666C7420 len [ 4] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [ui1u] 75693136 len [ 2] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [fltf] 666C7420 len [ 4] idx [226]: Zone 2 Filtered Power (PZ2F)
 [PZ2E] type [fltf] 666C7420 len [ 4] idx [227]: Zone 2 Target Power (PZ2E)
 [PZ2T] type [ui1u] 75693136 len [ 2] idx [228]: Zone 2 Abstract Throttle (PZ2T)
 [PZ3F] type [fltf] 666C7420 len [ 4] idx [229]: Zone 3 Filtered Power (PZ3F)
 [PZ3E] type [fltf] 666C7420 len [ 4] idx [230]: Zone 3 Target Power (PZ3E)
 [PZ3T] type [ui1u] 75693136 len [ 2] idx [231]: Zone 3 Abstract Throttle (PZ3T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 40 keys:
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  1]: Palm Rest Temp (DegC) (Ts0P)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU proximity temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  3]: Dimm Proximity temp(DegC) (TM0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [  4]: PCH Proxmity temp (DegC) (TP0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [  5]: DCIn Air flow Temperature (DegC) (Ta0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [  6]: GPU Die Analog temp (DegC) (TG0D)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  7]: Right Fin stack temp (DegC) (Th1H)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  8]: Left Fin stack temp (DegC) (Th2H)
 [TG1d] type [sp7s] 73703738 len [ 2] idx [  9]: GPU digital die temp Raw (without offset) (DegC) (TG1d)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC3C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core 2 temp (PECI) (DegC) (TC3C)
 [TC4C] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Core 3 temp (PECI) (DegC) (TC4C)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 14]: PCH Die temp (DegC) (TPCD)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU PECI die temp  (DegC) (TCXC)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [PCPT] type [sp8s] 73703837 len [ 2] idx [ 18]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp8s] 73703837 len [ 2] idx [ 19]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp8s] 73703837 len [ 2] idx [ 20]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 21]: Airport Temp (DegC) (TW0P)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 22]: Drive0 (SSD Gumstick) OOB v3 raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 23]: Drive0 (SSD Gumstick) OOB v3 raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 24]: Drive0 (SSD Gumstick) OOB v3 raw temp C (DegC) (TH0c)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 25]: Synthetic bottom skin (DegC) (Ts0S)
 [Ts1S] type [sp7s] 73703738 len [ 2] idx [ 26]: Synthetic Top skin (DegC) (Ts1S)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 27]: GPU proximity temp (DegC) (TG0P)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 28]: CPU die Virtual temp (DegC) (TC0E)
 [TM0S] type [sp7s] 73703738 len [ 2] idx [ 29]: Synthetic DIMM Estimate(DegC) (TM0S)
 [TMBS] type [sp7s] 73703738 len [ 2] idx [ 30]: DIMM Bandwidth Estimate (DegC) (TMBS)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 31]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH0V] type [sp7s] 73703738 len [ 2] idx [ 32]: SSD Temp B Foreign Drive Prediction   (DegC) (TH0V)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [PSTR] type [sp8s] 73703837 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [si1s] 73693136 len [ 2] idx [243]: Battery Actual current. (A) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (V) (B0AV)
Dumping keys for M96...
 Set 0 has 17 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  3]: DCIn Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  4]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  6]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  7]: CPU Power
 [    ] type [fpof] 66706F38 len [ 2] idx [ 10]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 11]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 12]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 15]: Zone Target Power
 [    ] type [fpof] 66706F38 len [ 2] idx [ 23]: Chipset Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 24]: Chipset VCore Current
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 14 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP die temp (TN0D)
 [TVFP] type [sp7s] 73703738 len [ 2] idx [  5]: Filtered Vent proximity (TVFP)
 [Th0P] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Spreader proximity temp (Th0P) 
 [TV0P] type [sp7s] 73703738 len [ 2] idx [  8]: Vent proximity temp (TV0P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  9]: Palm rest skin temp (Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 10]: Synthetic, bottom case, skin temp (Ts0S)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 11]: Wireless card temp (TW0P)
 [Tp0P] type [sp7s] 73703738 len [ 2] idx [ 12]: Power supply proximity temp (Tp0P)
 [Tp1P] type [sp7s] 73703738 len [ 2] idx [ 13]: Secondary power supply proximity (Tp1P)
 [TpFP] type [sp7s] 73703738 len [ 2] idx [ 14]: Filtered Power supply 1 proximity (TpFP)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 16]: Battery Temp (TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 17]: Battery Thermistor Temp 1 (TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 18]: Battery Thermistor Temp 2 (TB2T)
Dumping keys for M97...
 Set 0 has 18 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 15]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 23]: Heatpipe Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 14 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [THFH] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(THFH)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  5]: MCP Prox Temp(TN0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [  6]: Fan Target Temp(TTF0)
 [TG0H] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Pipe Temp(TG0H)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [  8]: Fan Target Temp(TTF0)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  9]: Palm Rest Temp(Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 10]: Bottom Case Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 12]: Battery Temp(TB0T)
 [TB3T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery Ambient Temp (TB3T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 13]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 14]: Battery Thermistor 1(TB2T)
Dumping keys for M97a...
 Set 0 has 18 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 15]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 23]: Heatpipe Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 14 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [THFH] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(THFH)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  5]: MCP Prox Temp(TN0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [  6]: Fan Target Temp(TTF0)
 [TG0H] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Pipe Temp(TG0H)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [  8]: Fan Target Temp(TTF0)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  9]: Palm Rest Temp(Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 10]: Bottom Case Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 12]: Battery Temp(TB0T)
 [TB3T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery Ambient Temp (TB3T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 13]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 14]: Battery Thermistor 1(TB2T)
Dumping keys for K24...
 Set 0 has 18 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 15]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 23]: Heatpipe Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 14 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [THFH] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(THFH)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  5]: MCP Prox Temp(TN0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [  6]: Fan Target Temp(TTF0)
 [TG0H] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Pipe Temp(TG0H)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [  8]: Fan Target Temp(TTF0)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  9]: Palm Rest Temp(Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 10]: Bottom Case Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 12]: Battery Temp(TB0T)
 [TB3T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery Ambient Temp (TB3T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 13]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 14]: Battery Thermistor 1(TB2T)
Dumping keys for K36b...
 Set 0 has 18 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 15]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 16]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 23]: Heatpipe Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 14 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [THFH] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Temp(THFH)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  5]: MCP Prox Temp(TN0P)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [  6]: Fan Target Temp(TTF0)
 [TG0H] type [sp7s] 73703738 len [ 2] idx [  7]: Heat Pipe Temp(TG0H)
 [TTF0] type [sp7s] 73703738 len [ 2] idx [  8]: Fan Target Temp(TTF0)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  9]: Palm Rest Temp(Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 10]: Bottom Case Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 12]: Battery Temp(TB0T)
 [TB3T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery Ambient Temp (TB3T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 13]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 14]: Battery Thermistor 1(TB2T)
Dumping keys for K84...
 Set 0 has 20 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 12]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 14]: CPU Highside Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 15]: CPU Highside Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 16]: Heatpipe Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 25 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  3]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Prox Temp(TN0P)
 [TN1D] type [sp7s] 73703738 len [ 2] idx [  5]: MCP Die2 Temp(TN1D)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [  6]: HDD Proximity Temp(TH0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  7]: Fin Stack Temp(Th1H)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  8]: Palm Rest Temp(Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  9]: Bottom Case Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 10]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 12]: Battery Thermistor 1(TB2T)
 [PZBL] type [sp7s] 73703738 len [ 2] idx [ 13]: Backlight Power(PZBL)
 [PZOD] type [sp7s] 73703738 len [ 2] idx [ 14]: ODD Power(PZOD)
 [PZAP] type [sp7s] 73703738 len [ 2] idx [ 15]: Airport Power(PZAP)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [ 16]: HDD Power(PZHD)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [ 17]: DIMM Power(PZHD)
 [VZOD] type [sp7s] 73703738 len [ 2] idx [ 18]: ODD Voltage(VZOD)
 [IZOD] type [sp7s] 73703738 len [ 2] idx [ 19]: ODD Current(IZOD)
 [VZAP] type [sp7s] 73703738 len [ 2] idx [ 20]: Airport Voltage(VZAP)
 [IZOP] type [sp7s] 73703738 len [ 2] idx [ 21]: Airport Current(IZOP)
 [IZHD] type [sp7s] 73703738 len [ 2] idx [ 22]: HDD Current(IZHD)
 [IZDM] type [sp7s] 73703738 len [ 2] idx [ 23]: DIMM Current(IZDM)
 [IZBL] type [sp7s] 73703738 len [ 2] idx [ 24]: Backlight Current(IZBL)
 [VZBL] type [sp7s] 73703738 len [ 2] idx [ 25]: Backlight Voltage(VZBL)
Dumping keys for K87...
 Set 0 has 20 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 12]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 14]: CPU Highside Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 15]: CPU Highside Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 16]: Heatpipe Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 25 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  3]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Prox Temp(TN0P)
 [TN1D] type [sp7s] 73703738 len [ 2] idx [  5]: MCP Die2 Temp(TN1D)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [  6]: HDD Proximity Temp(TH0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  7]: Fin Stack Temp(Th1H)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  8]: Palm Rest Temp(Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  9]: Bottom Case Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 10]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 12]: Battery Thermistor 1(TB2T)
 [PZBL] type [sp7s] 73703738 len [ 2] idx [ 13]: Backlight Power(PZBL)
 [PZOD] type [sp7s] 73703738 len [ 2] idx [ 14]: ODD Power(PZOD)
 [PZAP] type [sp7s] 73703738 len [ 2] idx [ 15]: Airport Power(PZAP)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [ 16]: HDD Power(PZHD)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [ 17]: DIMM Power(PZHD)
 [VZOD] type [sp7s] 73703738 len [ 2] idx [ 18]: ODD Voltage(VZOD)
 [IZOD] type [sp7s] 73703738 len [ 2] idx [ 19]: ODD Current(IZOD)
 [VZAP] type [sp7s] 73703738 len [ 2] idx [ 20]: Airport Voltage(VZAP)
 [IZOP] type [sp7s] 73703738 len [ 2] idx [ 21]: Airport Current(IZOP)
 [IZHD] type [sp7s] 73703738 len [ 2] idx [ 22]: HDD Current(IZHD)
 [IZDM] type [sp7s] 73703738 len [ 2] idx [ 23]: DIMM Current(IZDM)
 [IZBL] type [sp7s] 73703738 len [ 2] idx [ 24]: Backlight Current(IZBL)
 [VZBL] type [sp7s] 73703738 len [ 2] idx [ 25]: Backlight Voltage(VZBL)
Dumping keys for K69...
 Set 0 has 20 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 12]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 14]: CPU Highside Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 15]: CPU Highside Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 16]: Heatpipe Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 23 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  3]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Prox Temp(TN0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  5]: Fin Stack Temp(Th1H)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  6]: Palm Rest Temp(Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  7]: Bottom Case Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [  8]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [  9]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 10]: Battery Thermistor 1(TB2T)
 [PZBL] type [sp7s] 73703738 len [ 2] idx [ 11]: Backlight Power(PZBL)
 [PZOD] type [sp7s] 73703738 len [ 2] idx [ 12]: ODD Power(PZOD)
 [PZAP] type [sp7s] 73703738 len [ 2] idx [ 13]: Airport Power(PZAP)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [ 14]: HDD Power(PZHD)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [ 15]: DIMM Power(PZHD)
 [VZOD] type [sp7s] 73703738 len [ 2] idx [ 16]: ODD Voltage(VZOD)
 [IZOD] type [sp7s] 73703738 len [ 2] idx [ 17]: ODD Current(IZOD)
 [VZAP] type [sp7s] 73703738 len [ 2] idx [ 18]: Airport Voltage(VZAP)
 [IZOP] type [sp7s] 73703738 len [ 2] idx [ 19]: Airport Current(IZOP)
 [IZHD] type [sp7s] 73703738 len [ 2] idx [ 20]: HDD Current(IZHD)
 [IZDM] type [sp7s] 73703738 len [ 2] idx [ 21]: 1.5V S3 Current(IZDM)
 [IZBL] type [sp7s] 73703738 len [ 2] idx [ 22]: Backlight Current(IZBL)
 [VZBL] type [sp7s] 73703738 len [ 2] idx [ 23]: Backlight Voltage(VZBL)
Dumping keys for K6...
 Set 0 has 20 keys:
 [    ] type [fpof] 66706F38 len [ 2] idx [  1]: DCIn Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  2]: DCIn Current
 [    ] type [fpof] 66706F38 len [ 2] idx [  3]: PBus Power
 [    ] type [fp4f] 66703463 len [ 2] idx [  4]: PBus Current
 [    ] type [fp4f] 66703463 len [ 2] idx [  5]: PBus Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  6]: CPU Power
 [    ] type [fp6f] 66703661 len [ 2] idx [  7]: CPU Current
 [    ] type [fp2f] 66703265 len [ 2] idx [  8]: CPU Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [  9]: MCP VCore Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 10]: MCP VCore Current
 [    ] type [fp2f] 66703265 len [ 2] idx [ 11]: MCP VCore Voltage
 [    ] type [fpof] 66706F38 len [ 2] idx [ 12]: MCP DDR Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 13]: MCP DDR Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 14]: CPU Highside Power
 [    ] type [fp6f] 66703661 len [ 2] idx [ 15]: CPU Highside Current
 [    ] type [fpof] 66706F38 len [ 2] idx [ 16]: Heatpipe Power
 [    ] type [sp7s] 73703738 len [ 1] idx [240]: PLIMIT CPU
 [    ] type [sp7s] 73703738 len [ 1] idx [241]: PLIMIT GPU
 [    ] type [sp7s] 73703738 len [ 1] idx [242]: PLIMIT MEM
 [    ] type [sp7s] 73703738 len [ 1] idx [243]: PROCHOT
 Set 1 has 10 keys:
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Die Temp(TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Prox Temp(TC0P)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  3]: MCP Die Temp(TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  4]: MCP Prox Temp(TN0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  5]: Fin Stack Temp(Th1H)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  6]: Palm Rest Temp(Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  7]: Bottom Case Synthetic Temp(Ts0S)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [  8]: Battery Temp(TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [  9]: Battery Thermistor 0(TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 10]: Battery Thermistor 1(TB2T)
Dumping keys for K91F...
 Set 0 has 50 keys:
 [PC0C] type [sp9s] 73703936 len [ 2] idx [  1]: CPU Core Power (Watts) (PC0C)
 [PG0C] type [sp7s] 73703738 len [ 2] idx [  2]: Ext GPU Power (Watts) (PG0C)
 [PN0R] type [sp7s] 73703738 len [ 2] idx [  3]: NB Int GPU Power (Watts) (PN0R)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [  4]: DDR Power (Watts) (PM0R)
 [PC1C] type [sp8s] 73703837 len [ 2] idx [  5]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PC2C] type [sp8s] 73703837 len [ 2] idx [  6]: CPU VCCSA Power (Watts) (PC2C)
 [PD0R] type [sp8s] 73703837 len [ 2] idx [  7]: DC-In rail Power  (Watts) (PD0R)
 [PP0R] type [sp9s] 73703936 len [ 2] idx [  8]: PBus rail Power (Watts) (PP0R)
 [PC0R] type [sp8s] 73703837 len [ 2] idx [  9]: CPU Computing High Side Power (Watts) (PC0R)
 [PG0R] type [sp8s] 73703837 len [ 2] idx [ 10]: Ext GPU Ext GPU High Side Power (Watts) (PG0R)
 [PO0R] type [sp8s] 73703837 len [ 2] idx [ 11]: Other High Side Power   (Watts) (PO0R)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [ 12]: HP Power (Watts) (PHPC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 13]: Backlight Input Power  (DEBUG) (Watts) (PBLC)
 [PG1C] type [sp7s] 73703738 len [ 2] idx [ 14]: Ext GPU 1.8V Power  (DEBUG)  (Watts) (PG1C)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 15]: Airport Power  (DEBUG) (watts) (PAPC)
 [PG2C] type [sp7s] 73703738 len [ 2] idx [ 17]: Ext GPU 1.0V Power  (DEBUG) (Watts) (PG2C)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [ 18]: HDD Power  (DEBUG) (Watts) (PHDC)
 [PG3C] type [sp7s] 73703738 len [ 2] idx [ 19]: Ext GPU VRAM & I/O Power  (DEBUG) (Watts) (PG3C)
 [VC0C] type [sp1s] 73703165 len [ 2] idx [ 20]: CPU Core voltage. (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 21]: CPU Core current. (Amps) (IC0C)
 [VG0C] type [sp1s] 73703165 len [ 2] idx [ 22]: Ext GPU Core voltage. (Volts) (VG0C)
 [IG0C] type [sp6s] 73703639 len [ 2] idx [ 23]: Ext GPU Core current. (Amps) (IG0C)
 [IC0R] type [sp4s] 73703462 len [ 2] idx [ 24]: CPU Computing High Side current. (Amps) (IC0R)
 [IG0R] type [sp4s] 73703462 len [ 2] idx [ 25]: Ext GPU High Side current. (Amps) (IG0R)
 [IO0R] type [sp4s] 73703462 len [ 2] idx [ 26]: Other High Side current.  (Amps) (IO0R)
 [VN0R] type [sp1s] 73703165 len [ 2] idx [ 27]: NB Int GPU voltage. (Volts) (VN0R)
 [IN0C] type [sp6s] 73703639 len [ 2] idx [ 28]: NB Int GPU current. (Amps) (IN0C)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 29]: DDR current. (Amps) (IM0C)
 [IC1C] type [sp6s] 73703639 len [ 2] idx [ 30]: VCCIO 1.05V S0  current. (Amps) (IC1C)
 [IC2C] type [sp6s] 73703639 len [ 2] idx [ 31]: VCCSA S0  current. (Amps) (IC2C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 32]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp3s] 73703363 len [ 2] idx [ 33]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 34]: PBus rail voltage. (Volts) (VP0R)
 [IB0R] type [sp5s] 73703561 len [ 2] idx [ 35]: Battery Discharge Current MLB . (Amps) (IB0R)
 [IBLC] type [sp1s] 73703165 len [ 2] idx [ 36]: Backlight Current. (DEBUG) (Amps) (IBLC)
 [IG1C] type [sp5s] 73703561 len [ 2] idx [ 37]: Ext GPU  1.8 V current. (DEBUG) (Amps) (IG1C)
 [VCRP] type [sp5s] 73703561 len [ 2] idx [ 38]: CPU Ripple Voltage (DEBUG) (Volts) (VCRP)
 [IODC] type [sp4s] 73703462 len [ 2] idx [ 39]: ODD Current (DEBUG) (Amps) (IODC)
 [IG2C] type [sp4s] 73703462 len [ 2] idx [ 40]: Ext GPU 1.0V current. (DEBUG) (Amps) (IG2C)
 [IHDC] type [sp4s] 73703462 len [ 2] idx [ 41]: HDD Current (DEBUG) (Amps) (IHDC)
 [IG3C] type [sp4s] 73703462 len [ 2] idx [ 42]: Ext GPU VRAM & I/O current. (DEBUG) (Amps) (IG3C)
 [VBLC] type [sp6s] 73703639 len [ 2] idx [ 43]: Backlight Output Voltage. (DEBUG) (Volts) (VBLC)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 26 keys:
 [PCPT] type [sp8s] 73703837 len [ 2] idx [  1]: CPU total package power via PECI (Watts) (PCPT)
 [PCPC] type [sp8s] 73703837 len [ 2] idx [  2]: CPU core power via PECI (Watts) (PCPC)
 [PCPG] type [sp8s] 73703837 len [ 2] idx [  3]: CPU Gfx power via PECI (Watts) (PCPG)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Core PECI temp (DegC) (SIS! force bit 7) (TC0C)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  5]: CPU die temp (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  6]: CPU proximity temp (DegC) (TC0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [  7]: PCH Proxmity temp (DegC) (TP0P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  8]: Battery Charge Proximity temp (DegC) (Tm0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  9]: Right Fin stack temp (DegC) (Th1H)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 10]: GPU Die Analog temp (DegC) (TG0D)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU proximity temp (DegC) (TG0P)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [ 12]: Left Fin stack temp (DegC) (Th2H)
 [TG1D] type [sp7s] 73703738 len [ 2] idx [ 13]: GPU Die Digital temp (DegC) (TG1D)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 14]: Airport Temp (DegC) (TW0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [ 15]: T29 Proxmity temp (DegC) (THSP)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 16]: Palm Rest Temp (DegC) (Ts0P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 17]: Synthetic bottom skin (DegC) (Ts0S)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 18]: Max of CPU Core vs. Mem Ctlr/IG PECI temps (DegC) (SIS! force bit 5) (TC1C)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 19]: PCH Die temp (DegC) (SIS! force bit 6) (TPCD)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for K92...
 Set 0 has 63 keys:
 [PC0R] type [sp8s] 73703837 len [ 2] idx [  1]: CPU High Side Power (Watts) (PC0R)
 [PG0R] type [sp7s] 73703738 len [ 2] idx [  2]: Ext GPU Ext GPU High Side Power (Watts) (PG0R)
 [PB0R] type [sp8s] 73703837 len [ 2] idx [  3]: Battery Discharge Power MLB (IB0R * VP0R)  (Watts) (PB0R)
 [PC0C] type [sp8s] 73703837 len [ 2] idx [  4]: CPU core Power (Watts) (PC0C)
 [PG0C] type [sp7s] 73703738 len [ 2] idx [  5]: GPU core Power (Watts) (PG0C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  6]: NB Int GPU Power (Watts) (PN0C)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [  7]: DDR Power (Watts) (PM0R)
 [PC1C] type [sp8s] 73703837 len [ 2] idx [  8]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PC2C] type [sp8s] 73703837 len [ 2] idx [  9]: CPU VCCSA Power (Watts) (PC2C)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [ 10]: DCIN/Adapter rail Power (Watts) (PD0R)
 [PO0R] type [sp8s] 73703837 len [ 2] idx [ 11]: Other High Side Power   (Watts) (PO0R)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 12]: Backlight Power (DEBUG) (Watts) (PBLC)
 [PG1C] type [sp7s] 73703738 len [ 2] idx [ 13]: Ext GPU 1.8V Power  (DEBUG) (Watts) (PG1C)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 14]: Airport  Power (DEBUG) (Watts) (PAPC)
 [PG2C] type [sp7s] 73703738 len [ 2] idx [ 15]: Ext GPU 1.0V Power  (DEBUG) (Watts) (PG2C)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [ 16]: HDD Power (DEBUG) (Watts) (PHDC)
 [PG3C] type [sp7s] 73703738 len [ 2] idx [ 17]: Ext GPU VRAM & I/O Power  (DEBUG) (Watts) (PG3C)
 [PM1C] type [sp7s] 73703738 len [ 2] idx [ 18]: DDR 1.5V Power (DEBUG) (Watts) (PM1C)
 [PR0R] type [sp7s] 73703738 len [ 2] idx [ 19]: S0 5.0V Power (DEBUG) (Watts) (PR0R)
 [PR3R] type [sp7s] 73703738 len [ 2] idx [ 20]: S5 3.30V Power (DEBUG) (Watts) (PR3R)
 [PR2R] type [sp7s] 73703738 len [ 2] idx [ 21]: S3 5.0V Power (DEBUG) (Watts) (PR2R)
 [PR1R] type [sp7s] 73703738 len [ 2] idx [ 22]: S3 3.30V Power (DEBUG) (Watts) (PR1R)
 [PSBC] type [sp7s] 73703738 len [ 2] idx [ 23]: PCH core Power (DEBUG) (Watts) (PSBC)
 [VC0C] type [sp5s] 73703561 len [ 2] idx [ 24]: CPU Core Voltage (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU Core Current (Amps) (IC0C)
 [VG0C] type [sp5s] 73703561 len [ 2] idx [ 26]: GPU Core Voltage (Volts) (VG0C)
 [IG0C] type [sp5s] 73703561 len [ 2] idx [ 27]: Ext GPU Core Current (Amps) (IG0C)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 28]: CPU High Side Current (Amps) (IC0R)
 [IG0R] type [sp5s] 73703561 len [ 2] idx [ 29]: Ext GPU High Side Current. (Amps) (IG0R)
 [IO0R] type [sp5s] 73703561 len [ 2] idx [ 30]: Other High Side Current (Amps) (IO0R)
 [VN0C] type [sp5s] 73703561 len [ 2] idx [ 31]: GFX Voltage (Volts) (VN0C)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [ 32]: GFX core Current (Amps) (IN0C)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 33]: DDR3 Current (Amps) (IM0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 34]: CPU VCCIO Current (Amps) (IC1C)
 [IC2C] type [sp5s] 73703561 len [ 2] idx [ 35]: CPU VCCSA Current (Amps) (IC2C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 36]: Adapter Voltage (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 37]: DCIN/Adapter Current (Amps) (ID0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 38]: PBus Voltage  (Volts) (VP0R)
 [IB0R] type [sp5s] 73703561 len [ 2] idx [ 39]: Battery Discharge Current MLB  (Amps) (IB0R)
 [IBLC] type [sp5s] 73703561 len [ 2] idx [ 40]: Backlight  Current (DEBUG) (Amps) (IBLC)
 [IG1C] type [sp5s] 73703561 len [ 2] idx [ 41]: Ext GPU 1.8V Current (DEBUG) (Amps) (IG1C)
 [IAPC] type [sp5s] 73703561 len [ 2] idx [ 42]: Airport  Current (DEBUG) (Amps) (IAPC)
 [VCRP] type [sp5s] 73703561 len [ 2] idx [ 43]: CPU Ripple (Volts) (VCRP)
 [IG2C] type [sp5s] 73703561 len [ 2] idx [ 44]: Ext GPU 1.0V Current (DEBUG) (Amps) (IG2C)
 [IHDC] type [sp5s] 73703561 len [ 2] idx [ 45]: HDD  Current (DEBUG) (Amps) (IHDC)
 [IG3C] type [sp5s] 73703561 len [ 2] idx [ 46]: Ext GPU VRAM & I/O current Current (DEBUG) (Amps) (IG3C)
 [VBLC] type [sp6s] 73703639 len [ 2] idx [ 47]: Backlight  Voltage (DEBUG) (Volts) (VBLC)
 [IM1C] type [sp5s] 73703561 len [ 2] idx [ 48]: DDR 1.5V  Current (DEBUG) (Amps) (IM1C)
 [IR0C] type [sp5s] 73703561 len [ 2] idx [ 49]: S0 5.0V Current (DEBUG) (Amps) (IR0C)
 [IR3C] type [sp5s] 73703561 len [ 2] idx [ 50]: S5 3.30V Current (DEBUG) (Amps) (IR3C)
 [IR2C] type [sp5s] 73703561 len [ 2] idx [ 51]: S3 5.0V Current (DEBUG) (Amps) (IR2C)
 [IR1C] type [sp5s] 73703561 len [ 2] idx [ 52]: S3 3.30V Current (DEBUG) (Amps) (IR1C)
 [ISBC] type [sp5s] 73703561 len [ 2] idx [ 53]: PCH core  Current (DEBUG) (Amps) (ISBC)
 [VAPC] type [sp5s] 73703561 len [ 2] idx [ 54]: Airport  Voltage (DEBUG) (Volts) (VAPC)
 [VODC] type [sp5s] 73703561 len [ 2] idx [ 55]: ODD  Voltage (DEBUG) (Volts) (VODC)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 28 keys:
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [  1]: Synthetic bottom skin (DegC) (Ts0S)
 [PCPT] type [sp8s] 73703837 len [ 2] idx [  2]: CPU total package power via PECI (Watts) (PCPT)
 [PCPC] type [sp8s] 73703837 len [ 2] idx [  3]: CPU core power via PECI (Watts) (PCPC)
 [PCPG] type [sp8s] 73703837 len [ 2] idx [  4]: CPU Gfx power via PECI (Watts) (PCPG)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Core PECI temp (DegC) (TC0C)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  6]: CPU die temp (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  7]: CPU proximity temp (DegC) (TC0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [  8]: PCH Proximity temp (DegC) (TP0P)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [  9]: GPU proximity temp (DegC) (TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 10]: GPU Die Analog temp (DegC) (TG0D)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [ 11]: Left Fin stack temp (DegC) (Th2H)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [ 12]: Right Fin stack temp (DegC) (Th1H)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 13]: Palm Rest Temp (DegC) (Ts0P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 14]: Wireless card temp (DegC) (TW0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [ 15]: T29 proximity temp (DegC) (THSP)
 [TG1D] type [sp7s] 73703738 len [ 2] idx [ 16]: GPU Die Digital temp (DegC) (TG1D)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 17]: PCH Die temp (DegC) (TPCD)
 [FRD0] type [ui1u] 75693136 len [ 2] idx [ 18]: gasi16TmFastRawData array entry 0 (FRD0)
 [FRD1] type [ui1u] 75693136 len [ 2] idx [ 19]: gasi16TmFastRawData array entry 1 (FRD1)
 [FRD2] type [ui1u] 75693136 len [ 2] idx [ 20]: gasi16TmFastRawData array entry 2 (FRD2)
 [FRD3] type [ui1u] 75693136 len [ 2] idx [ 21]: gasi16TmFastRawData array entry 3 (FRD3)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for K90I...
 Set 0 has 24 keys:
 [PB0R] type [sp7s] 73703738 len [ 2] idx [  1]: Battery Discharge Power MLB (IB0R * VP0R)  (Watts) (PB0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [  2]: DCIN/Adapter Rail Power (Watts) (PD0R)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  3]: Load-side CPU Power (Watts) (PC0C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  4]: Load-side AXG Core Power (Watts) (PN0C)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  5]: High-Side Compute Power (Watts) (PC0R)
 [PO0R] type [sp7s] 73703738 len [ 2] idx [  6]: High-side 5v 3.3v Rail Power (Watts) (PO0R)
 [IC0C] type [sp6s] 73703639 len [ 2] idx [  7]: CPU Core Current (Amps) (IC0C)
 [VC0C] type [sp3s] 73703363 len [ 2] idx [  8]: CPU Core Voltage (Volts) (VC0C)
 [VN0R] type [sp3s] 73703363 len [ 2] idx [  9]: AGX Core Voltage (Volts) (VN0R)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [ 10]: AGX Core Current (Amps) (IN0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 11]: CPU VCCIO Current (Amps) (IC1C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 12]: Adapter Voltage (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 13]: DCIN/Adapter Current (Amps) (ID0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 14]: PBus Voltage  (Volts) (VP0R)
 [IB0R] type [sp5s] 73703561 len [ 2] idx [ 15]: Battery Discharge Current MLB (Amps) (IB0R)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 16]: CPU High Compute Current (IC0R)
 [IO0R] type [sp4s] 73703462 len [ 2] idx [ 17]: Other High Side current. (Amps) (IO0R)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp7s] 73703738 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 20 keys:
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Core PECI temp (DegC) (TC0C)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  5]: CPU die temp (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  6]: CPU proximity temp (DegC) (TC0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  7]: Fin stack temp (DegC) (Th1H)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [  8]: PCH proximity temp (DegC) (TP0P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [  9]: Airport Temp (DegC) (TW0P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 10]: Trackpad (DegC) (Ts0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 11]: PCH digital die temp (DegC) (SIS! force bit ) (TPCD)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 12]: Synthetic bottom skin (DegC) (Ts0S)
 [    ] type [sp7s] 73703738 len [ 2] idx [ 13]: Unused
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for K21...
 Set 0 has 31 keys:
 [PB0R] type [sp7s] 73703738 len [ 2] idx [  1]: Battery Discharge Power MLB (IB0R * VP0R)  (Watts) (PB0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [  2]: DCIN/Adapter rail Power (Watts) (PD0R)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  3]: CPU core Power (Watts) (PC0C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  4]: NB Int GPU Power (Watts) (PN0C)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  5]: CPU High Side Power (Watts) (PC0R)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [  6]: DDR Power (Watts) (PM0R)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [  7]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PZAP] type [sp7s] 73703738 len [ 2] idx [  8]: Airport  Power (DEBUG) (Watts) (PZAP)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [  9]: SSD Power (DEBUG) (Watts) (PZHD)
 [PZBL] type [sp7s] 73703738 len [ 2] idx [ 10]: Backlight Power (DEBUG) (Watts) (PZBL)
 [VC0C] type [sp5s] 73703561 len [ 2] idx [ 11]: CPU Core Voltage (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core Current (Amps) (IC0C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 13]: Adapter Voltage (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 14]: DCIN/Adapter Current (Amps) (ID0R)
 [VN0C] type [sp5s] 73703561 len [ 2] idx [ 15]: GFX Voltage (Volts) (VN0C)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [ 16]: GFX core Current (Amps) (IN0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 17]: CPU VCCIO Current (Amps) (IC1C)
 [IZBL] type [sp5s] 73703561 len [ 2] idx [ 18]: Backlight  Current (DEBUG) (Amps) (IZBL)
 [IZAP] type [sp5s] 73703561 len [ 2] idx [ 19]: Airport  Current (DEBUG) (Amps) (IZAP)
 [IZHD] type [sp5s] 73703561 len [ 2] idx [ 20]: SSD  Current (DEBUG) (Amps) (IZHD)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 21]: PBus Voltage  (Volts) (VP0R)
 [IB0R] type [sp5s] 73703561 len [ 2] idx [ 22]: Battery Discharge Current MLB  (Amps) (IB0R)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 23]: CPU High Side Current (Amps) (IC0R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [ 24]: DDR3 Current (Amps) (IM0R)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp7s] 73703738 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 33 keys:
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  4]: CPU proximity temp (DegC) (TC0P)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  5]: CPU die temp (DegC) (TC0D)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  6]: Memory proximity (DegC) (TM0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [  7]: air flow temp (DegC) (Ta0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  8]: Fin stack temp (DegC) (Th1H)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: MLB top side temp  (DegC) (Tm0P)
 [Tm1P] type [sp7s] 73703738 len [ 2] idx [ 10]: MLB bottom side temp  (DegC) (Tm1P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 11]: Palm Rest Temp (DegC) (Ts0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [ 12]: T29 proximity temp (DegC) (THSP)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU Core PECI temp (DegC) (TC0C)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 18]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 19]: CPU die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU PECI die temp Trend (DegC) (TCTD)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU PECI die temp max error filtered output used in TC0F=TC0E+TC0G (DegC) (TC0J)
 [VC1R] type [sp5s] 73703561 len [ 2] idx [ 23]: CPU High Side Voltage from EMC1704 (Volts) (VC1R)
 [IC1R] type [sp5s] 73703561 len [ 2] idx [ 24]: CPU High Side Current from EMC1704 (Amps) (IC1R)
 [PC1R] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU High Side Power from EMC1704 (Watts) (PC1R)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 26]: Hard Disk out-of-band virtual temperature (DegC) (TH0O)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 27]: Cooked and filtered SSD OOB temperature (SIT! force bit 7) (TH0F)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for K78...
 Set 0 has 31 keys:
 [PB0R] type [sp7s] 73703738 len [ 2] idx [  1]: Battery Discharge Power MLB (IB0R * VP0R)  (Watts) (PB0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [  2]: DCIN/Adapter rail Power (Watts) (PD0R)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  3]: CPU core Power (Watts) (PC0C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  4]: NB Int GPU Power (Watts) (PN0C)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  5]: CPU High Side Power (Watts) (PC0R)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [  6]: DDR Power (Watts) (PM0R)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [  7]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PZAP] type [sp7s] 73703738 len [ 2] idx [  8]: Airport  Power (DEBUG) (Watts) (PZAP)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [  9]: SSD Power (DEBUG) (Watts) (PZHD)
 [PZBL] type [sp7s] 73703738 len [ 2] idx [ 10]: Backlight Power (DEBUG) (Watts) (PZBL)
 [VC0C] type [sp5s] 73703561 len [ 2] idx [ 11]: CPU Core Voltage (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core Current (Amps) (IC0C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 13]: Adapter Voltage (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 14]: DCIN/Adapter Current (Amps) (ID0R)
 [VN0C] type [sp5s] 73703561 len [ 2] idx [ 15]: GFX Voltage (Volts) (VN0C)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [ 16]: GFX core Current (Amps) (IN0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 17]: CPU VCCIO Current (Amps) (IC1C)
 [IZBL] type [sp5s] 73703561 len [ 2] idx [ 18]: Backlight  Current (DEBUG) (Amps) (IZBL)
 [IZAP] type [sp5s] 73703561 len [ 2] idx [ 19]: Airport  Current (DEBUG) (Amps) (IZAP)
 [IZHD] type [sp5s] 73703561 len [ 2] idx [ 20]: SSD  Current (DEBUG) (Amps) (IZHD)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 21]: PBus Voltage  (Volts) (VP0R)
 [IB0R] type [sp5s] 73703561 len [ 2] idx [ 22]: Battery Discharge Current MLB  (Amps) (IB0R)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 23]: CPU High Side Current (Amps) (IC0R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [ 24]: DDR3 Current (Amps) (IM0R)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp7s] 73703738 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 33 keys:
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  4]: CPU proximity temp (DegC) (TC0P)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  5]: CPU die temp (DegC) (TC0D)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  6]: Memory proximity (DegC) (TM0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [  7]: air flow temp (DegC) (Ta0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  8]: Fin stack temp (DegC) (Th1H)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [  9]: MLB top side temp  (DegC) (Tm0P)
 [Tm1P] type [sp7s] 73703738 len [ 2] idx [ 10]: MLB bottom side temp  (DegC) (Tm1P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 11]: Palm Rest Temp (DegC) (Ts0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [ 12]: T29 proximity temp (DegC) (THSP)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU Core PECI temp (DegC) (TC0C)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 18]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 19]: CPU die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU PECI die temp Trend (DegC) (TCTD)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU PECI die temp max error filtered output used in TC0F=TC0E+TC0G (DegC) (TC0J)
 [VC1R] type [sp5s] 73703561 len [ 2] idx [ 23]: CPU High Side Voltage from EMC1704 (Volts) (VC1R)
 [IC1R] type [sp5s] 73703561 len [ 2] idx [ 24]: CPU High Side Current from EMC1704 (Amps) (IC1R)
 [PC1R] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU High Side Power from EMC1704 (Watts) (PC1R)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 26]: Hard Disk out-of-band virtual temperature (DegC) (TH0O)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 27]: Cooked and filtered SSD OOB temperature (SIT! force bit 7) (TH0F)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for J40G...
 Set 0 has 35 keys:
 [PHPC] type [sp7s] 73703738 len [ 2] idx [  1]: Average Thermal Control Power (SPS! force bit 13) (Watts) (PHPC)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  2]: Average CPU High side power (IC0R * VD0R) (SPS! force bit 10) (Watts) (PC0R)
 [PG0R] type [sp7s] 73703738 len [ 2] idx [  3]: Average GPU High side power (IG0R * VD0R) (SPS! force bit 10) (Watts) (PG0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [  4]: Average DC In rail power (ID0R * VD0R) (SPS! force bit 10) (Watts) (PD0R)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  5]: Average CPU Vcore power (IC0C * VC0C) (SPS! force bit 12) (Watts) (PC0C)
 [PN0R] type [sp7s] 73703738 len [ 2] idx [  6]: Average GFX Vcore power (IN0R * VN0R) (SPS! force bit 12) (Watts) (PN0R)
 [PG0C] type [sp7s] 73703738 len [ 2] idx [  7]: Average GPU Vcore power (IG0C * VG0C) (SPS! force bit 12) (Watts) (PG0C)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [  8]: Average Memory power (IM0C * 1.5V) (SPS! force bit 12) (Watts) (PM0C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [  9]: Average CPU VCCIO power (IC1C * 1.05V) (SPS! force bit 12) (Watts) (PC1C)
 [PD1R] type [sp7s] 73703738 len [ 2] idx [ 10]: Average CPU 1V5 power (ID1R * 1.5V) (SPS! force bit 10) (Watts) (PD1R)
 [PN1R] type [sp7s] 73703738 len [ 2] idx [ 11]: Average PCH 1V05 power (IN1R * 1.05V) (SPS! force bit 12) (Watts) (PN1R)
 [VC0C] type [sp1s] 73703165 len [ 2] idx [ 12]: CPU Vcore voltage. (SPS! force bit 1) (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 13]: CPU Vcore average current. (SPS! force bit 0) (Amps) (IC0C)
 [Vp0C] type [sp2s] 73703264 len [ 2] idx [ 14]: ACDC cooked temp (Volts) (Vp0C)
 [VG0C] type [sp1s] 73703165 len [ 2] idx [ 15]: GPU Vcore voltage. (SPS! force bit 8) (Volts) (VG0C)
 [IG0C] type [sp6s] 73703639 len [ 2] idx [ 16]: GPU Vcore average current. (SPS! force bit 0) (Amps) (IG0C)
 [VN0R] type [sp1s] 73703165 len [ 2] idx [ 17]: GFX Vcore voltage. (SPS! force bit 8) (Volts) (VN0R)
 [IN0R] type [sp6s] 73703639 len [ 2] idx [ 18]: GFX Vcore average current. (SPS! force bit 0) (Amps) (IN0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 19]: Memory average current. (SPS! force bit 2) (Amps) (IM0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 20]: CPU VCCIO current. (SPS! force bit 0) (Amps) (IC1C)
 [ID1R] type [sp5s] 73703561 len [ 2] idx [ 21]: CPU 1V5 average current. (SPS! force bit 3) (Amps) (ID1R)
 [VD0R] type [sp4s] 73703462 len [ 2] idx [ 22]: DC In voltage. (SPS! force bit 4) (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 23]: DC In Average current. (SPS! force bit 3) (Amps) (ID0R)
 [VC2C] type [sp0s] 73703066 len [ 2] idx [ 24]: CPU VCCSA voltage. (SPS! force bit 1) (Volts) (VC2C)
 [IC2C] type [sp5s] 73703561 len [ 2] idx [ 25]: CPU VCCSA current. (SPS! force bit 0) (Amps) (IC2C)
 [IC0R] type [sp4s] 73703462 len [ 2] idx [ 26]: CPU High side average current. (SPS! force bit 5) (Amps) (IC0R)
 [IG0R] type [sp3s] 73703363 len [ 2] idx [ 27]: GPU High side average current. (SPS! force bit 5) (Amps) (IG0R)
 [IN1R] type [sp5s] 73703561 len [ 2] idx [ 28]: PCH 1V05 average current. (SPS! force bit 7) (Amps) (IN1R)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 29 keys:
 [TC0d] type [sp7s] 73703738 len [ 2] idx [  1]: CPU die raw temp (DegC) (TC0d)
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  4]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSC] type [sp7s] 73703738 len [ 2] idx [  6]: CPU System Agent Core temp (PECI) (DegC) (TCSC)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Max Package Core temp (PECI) (DegC) (TCXC)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core 0 temp (PECI) (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  9]: CPU Core 1 temp (PECI) (DegC) (TC1C)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU PECI die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU PECI die temp Trend (DegC) (TCTD)
 [TCFC] type [ui1u] 75693136 len [ 2] idx [ 12]: CPU PECI die temp filter coeff (TCFC)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU PECI die temp max error filtered output (DegC) (TC0J)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU die temp (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU proximity temp (filtered) (DegC) (TC0P)
 [TG1D] type [sp7s] 73703738 len [ 2] idx [ 17]: GPU digital die temp (DegC) (TG1D)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 18]: GPU proximity temp (DegC) (TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 19]: GPU analog die temp (DegC) (TG0D)
 [TG0M] type [sp7s] 73703738 len [ 2] idx [ 20]: GFX memory temp (DegC) (TG0M)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [ 21]: PCH proximity temp (DegC) (TP0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 22]: PCH digital die temp (DegC) (TPCD)
 [TI0P] type [sp7s] 73703738 len [ 2] idx [ 23]: High Speed I/O proximity 0 temp (DegC) (TI0P)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 24]: HDD proximity temp (DegC) (TH0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 25]: Memory proximity temp (filtered) (DegC) (TM0P)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 26]: Ambient 0 temp (DegC) (TA0P)
 [TA1P] type [sp7s] 73703738 len [ 2] idx [ 27]: Ambient 1 temp (DegC) (TA1P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 28]: Airport Card temp (DegC) (TW0P)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
Dumping keys for J40I...
 Set 0 has 31 keys:
 [PHPC] type [sp7s] 73703738 len [ 2] idx [  1]: Average Thermal Control Power (SPS! force bit 13) (Watts) (PHPC)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  2]: Average CPU High side power (IC0R * VD0R) (SPS! force bit 10) (Watts) (PC0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [  3]: Average DC In rail power (ID0R * VD0R) (SPS! force bit 10) (Watts) (PD0R)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  4]: Average CPU Vcore power (IC0C * VC0C) (SPS! force bit 12) (Watts) (PC0C)
 [PN0R] type [sp7s] 73703738 len [ 2] idx [  5]: Average GFX Vcore power (IN0R * VN0R) (SPS! force bit 12) (Watts) (PN0R)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [  6]: Average Memory power (IM0C * 1.5V) (SPS! force bit 12) (Watts) (PM0C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [  7]: Average CPU VCCIO power (IC1C * 1.05V) (SPS! force bit 12) (Watts) (PC1C)
 [PD1R] type [sp7s] 73703738 len [ 2] idx [  8]: Average CPU 1V5 power (ID1R * 1.5V) (SPS! force bit 10) (Watts) (PD1R)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [  9]: Average CPU VCCSA power (IC2C * VC2C) (SPS! force bit 12) (Watts) (PC2C)
 [PN1R] type [sp7s] 73703738 len [ 2] idx [ 10]: Average PCH 1V05 power (IN1R * 1.05V) (SPS! force bit 12) (Watts) (PN1R)
 [VC0C] type [sp1s] 73703165 len [ 2] idx [ 11]: CPU Vcore voltage. (SPS! force bit 1) (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 12]: CPU Vcore average current. (SPS! force bit 0) (Amps) (IC0C)
 [Vp0C] type [sp2s] 73703264 len [ 2] idx [ 13]: ACDC cooked temp (Volts) (Vp0C)
 [VN0R] type [sp1s] 73703165 len [ 2] idx [ 14]: GFX Vcore voltage. (SPS! force bit 8) (Volts) (VN0R)
 [IN0R] type [sp6s] 73703639 len [ 2] idx [ 15]: GFX Vcore average current. (SPS! force bit 0) (Amps) (IN0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 16]: Memory average current. (SPS! force bit 2) (Amps) (IM0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 17]: CPU VCCIO current. (SPS! force bit 0) (Amps) (IC1C)
 [ID1R] type [sp5s] 73703561 len [ 2] idx [ 18]: CPU 1V5 average current. (SPS! force bit 3) (Amps) (ID1R)
 [VD0R] type [sp4s] 73703462 len [ 2] idx [ 19]: DC In voltage. (SPS! force bit 4) (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 20]: DC In Average current. (SPS! force bit 3) (Amps) (ID0R)
 [VC2C] type [sp0s] 73703066 len [ 2] idx [ 21]: CPU VCCSA voltage. (SPS! force bit 1) (Volts) (VC2C)
 [IC2C] type [sp5s] 73703561 len [ 2] idx [ 22]: CPU VCCSA current. (SPS! force bit 0) (Amps) (IC2C)
 [IC0R] type [sp4s] 73703462 len [ 2] idx [ 23]: CPU High side average current. (SPS! force bit 5) (Amps) (IC0R)
 [IN1R] type [sp5s] 73703561 len [ 2] idx [ 24]: PCH 1V05 average current. (SPS! force bit 7) (Amps) (IN1R)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 26 keys:
 [TC0d] type [sp7s] 73703738 len [ 2] idx [  1]: CPU die raw temp (DegC) (TC0d)
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  4]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSC] type [sp7s] 73703738 len [ 2] idx [  6]: CPU System Agent Core temp (PECI) (DegC) (TCSC)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Max Package Core temp (PECI) (DegC) (TCXC)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core 0 temp (PECI) (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  9]: CPU Core 1 temp (PECI) (DegC) (TC1C)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU PECI die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU PECI die temp Trend (DegC) (TCTD)
 [TCFC] type [ui1u] 75693136 len [ 2] idx [ 12]: CPU PECI die temp filter coeff (TCFC)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU PECI die temp max error filtered output (DegC) (TC0J)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU die temp (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU proximity temp (filtered) (DegC) (TC0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [ 17]: PCH proximity temp (DegC) (TP0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 18]: PCH digital die temp (DegC) (TPCD)
 [TI0P] type [sp7s] 73703738 len [ 2] idx [ 19]: High Speed I/O proximity 0 temp (DegC) (TI0P)
 [TI1P] type [sp7s] 73703738 len [ 2] idx [ 20]: High Speed I/O proximity 1 temp (DegC) (TI1P)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 21]: HDD proximity temp (DegC) (TH0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 22]: Memory proximity temp (filtered) (DegC) (TM0P)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 23]: Ambient 0 temp (DegC) (TA0P)
 [TA1P] type [sp7s] 73703738 len [ 2] idx [ 24]: Ambient 1 temp (DegC) (TA1P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 25]: Airport Card temp (DegC) (TW0P)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
Dumping keys for J40S...
 Set 0 has 31 keys:
 [PHPC] type [sp7s] 73703738 len [ 2] idx [  1]: Average Thermal Control Power (SPS! force bit 13) (Watts) (PHPC)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  2]: Average CPU High side power (IC0R * VD0R) (SPS! force bit 10) (Watts) (PC0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [  3]: Average DC In rail power (ID0R * VD0R) (SPS! force bit 10) (Watts) (PD0R)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  4]: Average CPU Vcore power (IC0C * VC0C) (SPS! force bit 12) (Watts) (PC0C)
 [PN0R] type [sp7s] 73703738 len [ 2] idx [  5]: Average GFX Vcore power (IN0R * VN0R) (SPS! force bit 12) (Watts) (PN0R)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [  6]: Average Memory power (IM0C * 1.5V) (SPS! force bit 12) (Watts) (PM0C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [  7]: Average CPU VCCIO power (IC1C * 1.05V) (SPS! force bit 12) (Watts) (PC1C)
 [PD1R] type [sp7s] 73703738 len [ 2] idx [  8]: Average CPU 1V5 power (ID1R * 1.5V) (SPS! force bit 10) (Watts) (PD1R)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [  9]: Average CPU VCCSA power (IC2C * VC2C) (SPS! force bit 12) (Watts) (PC2C)
 [PN1R] type [sp7s] 73703738 len [ 2] idx [ 10]: Average PCH 1V05 power (IN1R * 1.05V) (SPS! force bit 12) (Watts) (PN1R)
 [VC0C] type [sp1s] 73703165 len [ 2] idx [ 11]: CPU Vcore voltage. (SPS! force bit 1) (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 12]: CPU Vcore average current. (SPS! force bit 0) (Amps) (IC0C)
 [Vp0C] type [sp2s] 73703264 len [ 2] idx [ 13]: ACDC cooked temp (Volts) (Vp0C)
 [VN0R] type [sp1s] 73703165 len [ 2] idx [ 14]: GFX Vcore voltage. (SPS! force bit 8) (Volts) (VN0R)
 [IN0R] type [sp6s] 73703639 len [ 2] idx [ 15]: GFX Vcore average current. (SPS! force bit 0) (Amps) (IN0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 16]: Memory average current. (SPS! force bit 2) (Amps) (IM0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 17]: CPU VCCIO current. (SPS! force bit 0) (Amps) (IC1C)
 [ID1R] type [sp5s] 73703561 len [ 2] idx [ 18]: CPU 1V5 average current. (SPS! force bit 3) (Amps) (ID1R)
 [VD0R] type [sp4s] 73703462 len [ 2] idx [ 19]: DC In voltage. (SPS! force bit 4) (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 20]: DC In Average current. (SPS! force bit 3) (Amps) (ID0R)
 [VC2C] type [sp0s] 73703066 len [ 2] idx [ 21]: CPU VCCSA voltage. (SPS! force bit 1) (Volts) (VC2C)
 [IC2C] type [sp5s] 73703561 len [ 2] idx [ 22]: CPU VCCSA current. (SPS! force bit 0) (Amps) (IC2C)
 [IC0R] type [sp4s] 73703462 len [ 2] idx [ 23]: CPU High side average current. (SPS! force bit 5) (Amps) (IC0R)
 [IN1R] type [sp5s] 73703561 len [ 2] idx [ 24]: PCH 1V05 average current. (SPS! force bit 7) (Amps) (IN1R)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 28 keys:
 [TC0d] type [sp7s] 73703738 len [ 2] idx [  1]: CPU die raw temp (DegC) (TC0d)
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  4]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSC] type [sp7s] 73703738 len [ 2] idx [  6]: CPU System Agent Core temp (PECI) (DegC) (TCSC)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Max Package Core temp (PECI) (DegC) (TCXC)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core 0 temp (PECI) (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  9]: CPU Core 1 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU Core 2 temp (PECI) (DegC) (TC2C)
 [TC3C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Core 3 temp (PECI) (DegC) (TC3C)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU PECI die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU PECI die temp Trend (DegC) (TCTD)
 [TCFC] type [ui1u] 75693136 len [ 2] idx [ 14]: CPU PECI die temp filter coeff (TCFC)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU PECI die temp max error filtered output (DegC) (TC0J)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU die temp (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 18]: CPU proximity temp (filtered) (DegC) (TC0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [ 19]: PCH proximity temp (DegC) (TP0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 20]: PCH digital die temp (DegC) (TPCD)
 [TI0P] type [sp7s] 73703738 len [ 2] idx [ 21]: High Speed I/O proximity 0 temp (DegC) (TI0P)
 [TI1P] type [sp7s] 73703738 len [ 2] idx [ 22]: High Speed I/O proximity 1 temp (DegC) (TI1P)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 23]: HDD proximity temp (DegC) (TH0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 24]: Memory proximity temp (filtered) (DegC) (TM0P)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 25]: Ambient 0 temp (DegC) (TA0P)
 [TA1P] type [sp7s] 73703738 len [ 2] idx [ 26]: Ambient 1 temp (DegC) (TA1P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 27]: Airport Card temp (DegC) (TW0P)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
Dumping keys for K16...
 Set 0 has 33 keys:
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  1]: Average CPU Vcore Power (SPS! force bit 20) (Watts) (PC0C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  2]: Average MCP core Power (IN0C * VN0C) (SPS! force bit 23) (Watts) (PN0C)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [  3]: MCP Core Current(SPS! force bit 10) (Amps) (IN0C)
 [VN0C] type [sp1s] 73703165 len [ 2] idx [  4]: MCP Core Voltage (SPS! force bit 2) (Volts) (VN0C)
 [PN1C] type [sp7s] 73703738 len [ 2] idx [  5]: Average MCP memory Power (IN1C * 1.35V) (SPS! force bit 24) (Watts) (PN1C)
 [IN1C] type [sp3s] 73703363 len [ 2] idx [  6]: MCP DDR Current(SPS! force bit 11) (Amps) (IN1C)
 [VN1C] type [sp5s] 73703561 len [ 2] idx [  7]: MCP Memory Voltage (SPS! force bit 15) (Volts) (VN1C)
 [PB0R] type [sp7s] 73703738 len [ 2] idx [  8]: Average battery discharge power MLB (IB0R * VP0R) (SPS! force bit 21) (Watts) (PB0R)
 [IB0R] type [sp4s] 73703462 len [ 2] idx [  9]: Battery Discharge Current MLB (SPS! force bit 5) (Amps) (IB0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 10]: PBus Voltage (SPS! force bit 4) (Volts) (VP0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [ 11]: Average DCIN/Adapter rail Power (SPS! force bit 22) (Watts) (PD0R)
 [ID0R] type [sp3s] 73703363 len [ 2] idx [ 12]: DCIN/Adapter Current (SPS! force bit 3) (Amps) (ID0R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 13]: DC In Voltage (SPS! force bit 16) (Volts) (VD0R)
 [Pc0R] type [sp7s] 73703738 len [ 2] idx [ 14]: Average main chipset Power (Ic0R * VP0R) (SPS! force bit 25) (Watts) (Pc0R)
 [Ic0R] type [sp4s] 73703462 len [ 2] idx [ 15]: CSreg Current (SPS! force bit 12) (Amps) (Ic0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 16]: PBus Voltage (SPS! force bit 4) (Volts) (VP0R)
 [PZBL] type [sp7s] 73703738 len [ 2] idx [ 17]: LCD Backlight Power (IZBL * VP0R) (SPS! force bit 26) (Watts) (PZBL)
 [IZBL] type [sp0s] 73703066 len [ 2] idx [ 18]: LCD Backlight Current (SPS! force bit 7) (Amps) (IZBL)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 19]: PBus Voltage (SPS! force bit 4) (Volts) (VP0R)
 [PZAP] type [sp7s] 73703738 len [ 2] idx [ 20]: WIFI Power (IZAP * 3.3V) (SPS! force bit 27) (Watts) (PZAP)
 [IZAP] type [sp0s] 73703066 len [ 2] idx [ 21]: WLAN Current (SPS! force bit 8) (Amps) (IZAP)
 [VZAP] type [sp5s] 73703561 len [ 2] idx [ 22]: WIFI Voltage (SPS! force bit 17) (Volts) (VZAP)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [ 23]: SSD Power (IZHD * 3.3V) (SPS! force bit 28) (Watts) (PZHD)
 [IZHD] type [sp2s] 73703264 len [ 2] idx [ 24]: HDD Current (SPS! force bit 9) (Amps) (IZHD)
 [VZHD] type [sp5s] 73703561 len [ 2] idx [ 25]: SSD Voltage (SPS! force bit 18) (Volts) (VZHD)
 [PZDM] type [sp7s] 73703738 len [ 2] idx [ 26]: Memory Power (IZDM * 1.35V) (SPS! force bit 29) (Watts) (PZDM)
 [IZDM] type [sp5s] 73703561 len [ 2] idx [ 27]: 1V5S3 Current (SPS! force bit 6) (Amps) (IZDM)
 [VZDM] type [sp5s] 73703561 len [ 2] idx [ 28]: Memory Voltage (SPS! force bit 19) (Volts) (VZDM)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [ 29]: HP Power Target (PTHC)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [    ] type [ui8u] 75693820 len [ 1] idx [243]: Prochot
 Set 1 has 12 keys:
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  1]: Finstack proximity temp (SIT! force bit 14) (DegC) (Th1H)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Die temp (SIT! force bit 9) (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  3]: CPU proxmity temp (SIT! force bit 10) (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  4]: SSD proximity temp (SIU! force bit 0) (DegC) (TM0P)
 [TN1D] type [sp7s] 73703738 len [ 2] idx [  5]: MCP internal die temp (SIU! force bit 1) (DegC) (TN1D)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  6]: MCP89 Die temp (SIT! force bit 11) (DegC) (TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  7]: MCP89 Die temp (SIT! force bit 12) (DegC) (TN0P)
 [Tp0P] type [sp7s] 73703738 len [ 2] idx [  8]: MLB temp (SIT! force bit 15) (DegC) (Tp0P)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [  9]: Battery temp. (DegC) (TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 10]: Battery TS1 Temp (DegC) (TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery TS2 Temp (DegC) (TB2T)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 12]: Palm rest skin temp (SIT! force bit 13) (DegC) (Ts0P)
Dumping keys for K99...
 Set 0 has 33 keys:
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  1]: Average CPU Vcore Power (SPS! force bit 20) (Watts) (PC0C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  2]: Average MCP core Power (IN0C * VN0C) (SPS! force bit 23) (Watts) (PN0C)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [  3]: MCP Core Current(SPS! force bit 10) (Amps) (IN0C)
 [VN0C] type [sp1s] 73703165 len [ 2] idx [  4]: MCP Core Voltage (SPS! force bit 2) (Volts) (VN0C)
 [PN1C] type [sp7s] 73703738 len [ 2] idx [  5]: Average MCP memory Power (IN1C * 1.35V) (SPS! force bit 24) (Watts) (PN1C)
 [IN1C] type [sp3s] 73703363 len [ 2] idx [  6]: MCP DDR Current(SPS! force bit 11) (Amps) (IN1C)
 [VN1C] type [sp5s] 73703561 len [ 2] idx [  7]: MCP Memory Voltage (SPS! force bit 15) (Volts) (VN1C)
 [PB0R] type [sp7s] 73703738 len [ 2] idx [  8]: Average battery discharge power MLB (IB0R * VP0R) (SPS! force bit 21) (Watts) (PB0R)
 [IB0R] type [sp4s] 73703462 len [ 2] idx [  9]: Battery Discharge Current MLB (SPS! force bit 5) (Amps) (IB0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 10]: PBus Voltage (SPS! force bit 4) (Volts) (VP0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [ 11]: Average DCIN/Adapter rail Power (SPS! force bit 22) (Watts) (PD0R)
 [ID0R] type [sp3s] 73703363 len [ 2] idx [ 12]: DCIN/Adapter Current (SPS! force bit 3) (Amps) (ID0R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 13]: DC In Voltage (SPS! force bit 16) (Volts) (VD0R)
 [Pc0R] type [sp7s] 73703738 len [ 2] idx [ 14]: Average main chipset Power (Ic0R * VP0R) (SPS! force bit 25) (Watts) (Pc0R)
 [Ic0R] type [sp4s] 73703462 len [ 2] idx [ 15]: CSreg Current (SPS! force bit 12) (Amps) (Ic0R)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 16]: PBus Voltage (SPS! force bit 4) (Volts) (VP0R)
 [PZBL] type [sp7s] 73703738 len [ 2] idx [ 17]: LCD Backlight Power (IZBL * VP0R) (SPS! force bit 26) (Watts) (PZBL)
 [IZBL] type [sp0s] 73703066 len [ 2] idx [ 18]: LCD Backlight Current (SPS! force bit 7) (Amps) (IZBL)
 [VP0R] type [sp4s] 73703462 len [ 2] idx [ 19]: PBus Voltage (SPS! force bit 4) (Volts) (VP0R)
 [PZAP] type [sp7s] 73703738 len [ 2] idx [ 20]: WIFI Power (IZAP * 3.3V) (SPS! force bit 27) (Watts) (PZAP)
 [IZAP] type [sp0s] 73703066 len [ 2] idx [ 21]: WLAN Current (SPS! force bit 8) (Amps) (IZAP)
 [VZAP] type [sp5s] 73703561 len [ 2] idx [ 22]: WIFI Voltage (SPS! force bit 17) (Volts) (VZAP)
 [PZHD] type [sp7s] 73703738 len [ 2] idx [ 23]: SSD Power (IZHD * 3.3V) (SPS! force bit 28) (Watts) (PZHD)
 [IZHD] type [sp2s] 73703264 len [ 2] idx [ 24]: HDD Current (SPS! force bit 9) (Amps) (IZHD)
 [VZHD] type [sp5s] 73703561 len [ 2] idx [ 25]: SSD Voltage (SPS! force bit 18) (Volts) (VZHD)
 [PZDM] type [sp7s] 73703738 len [ 2] idx [ 26]: Memory Power (IZDM * 1.35V) (SPS! force bit 29) (Watts) (PZDM)
 [IZDM] type [sp5s] 73703561 len [ 2] idx [ 27]: 1V5S3 Current (SPS! force bit 6) (Amps) (IZDM)
 [VZDM] type [sp5s] 73703561 len [ 2] idx [ 28]: Memory Voltage (SPS! force bit 19) (Volts) (VZDM)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [ 29]: HP Power Target (PTHC)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [    ] type [ui8u] 75693820 len [ 1] idx [243]: Prochot
 Set 1 has 12 keys:
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  1]: Finstack proximity temp (SIT! force bit 14) (DegC) (Th1H)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Die temp (SIT! force bit 9) (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  3]: CPU proxmity temp (SIT! force bit 10) (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  4]: SSD proximity temp (SIU! force bit 0) (DegC) (TM0P)
 [TN1D] type [sp7s] 73703738 len [ 2] idx [  5]: MCP internal die temp (SIU! force bit 1) (DegC) (TN1D)
 [TN0D] type [sp7s] 73703738 len [ 2] idx [  6]: MCP89 Die temp (SIT! force bit 11) (DegC) (TN0D)
 [TN0P] type [sp7s] 73703738 len [ 2] idx [  7]: MCP89 Die temp (SIT! force bit 12) (DegC) (TN0P)
 [Tp0P] type [sp7s] 73703738 len [ 2] idx [  8]: MLB temp (SIT! force bit 15) (DegC) (Tp0P)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [  9]: Battery temp. (DegC) (TB0T)
 [TB1T] type [sp7s] 73703738 len [ 2] idx [ 10]: Battery TS1 Temp (DegC) (TB1T)
 [TB2T] type [sp7s] 73703738 len [ 2] idx [ 11]: Battery TS2 Temp (DegC) (TB2T)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 12]: Palm rest skin temp (SIT! force bit 13) (DegC) (Ts0P)
Dumping keys for J31...
 Set 0 has 48 keys:
 [PHPC] type [sp8s] 73703837 len [ 2] idx [  1]: Thermal control Power (Watts) (PHPC)
 [PC0R] type [sp8s] 73703837 len [ 2] idx [  2]: CPU Computing High Side Power (Watts) (PC0R)
 [PG0R] type [sp8s] 73703837 len [ 2] idx [  3]: Ext GPU Ext GPU High Side Power (Watts) (PG0R)
 [PO0R] type [sp7s] 73703738 len [ 2] idx [  4]: Other High Side Power   (Watts) (PO0R)
 [PPBR] type [sp8s] 73703837 len [ 2] idx [  5]: PBus on battery power (Watts) (PPBR)
 [PDTR] type [sp8s] 73703837 len [ 2] idx [  6]: DC-In total power  (Watts) (PDTR)
 [PCLT] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Package Total Power (SMC Load Sensors) (Watts) (PCLT)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core Power (Watts) (PC0C)
 [PG0C] type [sp7s] 73703738 len [ 2] idx [  9]: Ext GPU Power (Watts) (PG0C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [ 10]: Int GPU core Power (Watts) (PN0C)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [ 11]: DDR Power (Memory) (Watts) (PM0C)
 [PM1C] type [sp7s] 73703738 len [ 2] idx [ 12]: DDR Power (CPU & Memory) (Watts) (PM1C)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [ 13]: HDD Power  (Watts) (PHDC)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU VCCSA Power (Watts) (PC2C)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 16]: Airport Power   (watts) (PAPC)
 [PG1C] type [sp7s] 73703738 len [ 2] idx [ 17]: Ext GPU 1.8V Power  (Watts) (PG1C)
 [PG3C] type [sp7s] 73703738 len [ 2] idx [ 18]: Ext GPU 1.8V Power  (DEBUG) (Watts) (PG3C)
 [PHSP] type [sp7s] 73703738 len [ 2] idx [ 19]: T29 Power  (Watts) (PHSP)
 [PR1C] type [sp7s] 73703738 len [ 2] idx [ 20]: 3.3V S3.  (Amps) (PR1C)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 21]: Backlight Input Power   (Watts) (PBLC)
 [PG2C] type [sp7s] 73703738 len [ 2] idx [ 22]: Ext GPU 1.8V Power  (Watts) (PG2C)
 [VC0C] type [sp5s] 73703561 len [ 2] idx [ 23]: CPU Core voltage. (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU Core current. (Amps) (IC0C)
 [VN0C] type [sp5s] 73703561 len [ 2] idx [ 25]: Int GPU core voltage. (Volts) (VN0C)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [ 26]: Internal GPU core current. (Amps) (IN0C)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 27]: CPU Computing High Side current. (Amps) (IC0R)
 [IG0R] type [sp5s] 73703561 len [ 2] idx [ 28]: Ext GPU High Side current. (Amps) (IG0R)
 [IO0R] type [sp5s] 73703561 len [ 2] idx [ 29]: Other High Side current.  (Amps) (IO0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 30]: DDR 1.5V (Memory) current. (Amps) (IM0C)
 [IM1C] type [sp5s] 73703561 len [ 2] idx [ 31]: DDR 1.5V (CPU & Memory) current. (Amps) (IM1C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 32]: VCCIO  current. (Amps) (IC1C)
 [IC2C] type [sp5s] 73703561 len [ 2] idx [ 33]: VCCSA  current. (Amps) (IC2C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 34]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 35]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 36]: PBus rail voltage. (Volts) (VP0R)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 37]: PBus on battery current. (Amps) (IPBR)
 [VC2C] type [sp5s] 73703561 len [ 2] idx [ 38]: VCCSA voltage. (Volts) (VC2C)
 [VCRC] type [sp5s] 73703561 len [ 2] idx [ 39]: CPU Ripple voltage. (DEBUG) (Volts) (VCRC)
 [VG0C] type [sp5s] 73703561 len [ 2] idx [ 40]: Ext GPU Core voltage. (Volts) (VG0C)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 28 keys:
 [PCPT] type [sp8s] 73703837 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp8s] 73703837 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp8s] 73703837 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Core PECI temp (DegC) (SIS! force bit 7) (TCXC)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC3C] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Core 2 temp (PECI) (DegC) (TC3C)
 [TC4C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core 3 temp (PECI) (DegC) (TC4C)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  9]: CPU proximity temp (DegC) (TC0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [ 10]: PCH Proxmity temp (DegC) (TP0P)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 11]: Airflow temp (DegC) (TA0P)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU proximity temp (DegC) (TG0P)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 13]: GPU Die Analog temp (DegC) (TG0D)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [ 14]: Left Fin stack temp (DegC) (Th2H)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [ 15]: Right Fin stack temp (DegC) (Th1H)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 16]: Palm Rest Temp (DegC) (Ts0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 17]: Dimm Proximity temp(DegC) (SIS! force bit 1) (TM0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 18]: PCH Die temp (DegC) (SIS! force bit 6) (TPCD)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 19]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU die Virtual temp (DegC) (TC0E)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [PSTR] type [sp8s] 73703837 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for J30...
 Set 0 has 31 keys:
 [PHPC] type [sp7s] 73703738 len [ 2] idx [  1]: Thermal control Power (Watts) (PHPC)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Computing High Side Power (Watts) (PC0R)
 [PO0R] type [sp7s] 73703738 len [ 2] idx [  3]: Other High Side Power   (Watts) (PO0R)
 [PDTR] type [sp7s] 73703738 len [ 2] idx [  4]: DC-In total power  (Watts) (PDTR)
 [PPBR] type [sp7s] 73703738 len [ 2] idx [  5]: PBus on battery power (Watts) (PPBR)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [  6]: HDD Power  (Watts) (PHDC)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [  7]: DDR Power (Memory) (Watts) (PM0C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  9]: Int GPU core Power (Watts) (PN0C)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU VCCSA Power (Watts) (PC2C)
 [VC0C] type [sp5s] 73703561 len [ 2] idx [ 11]: CPU Core voltage. (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core current. (Amps) (IC0C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 13]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 14]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 15]: PBus rail voltage. (Volts) (VP0R)
 [IHDC] type [sp5s] 73703561 len [ 2] idx [ 16]: HDD/SSD Current  (Amps) (IHDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 17]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 18]: CPU Computing High Side current. (Amps) (IC0R)
 [IO0R] type [sp5s] 73703561 len [ 2] idx [ 19]: Other High Side current.  (Amps) (IO0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 20]: DDR 1.5V (Memory) current. (Amps) (IM0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 21]: VCCIO  current. (Amps) (IC1C)
 [VN0C] type [sp5s] 73703561 len [ 2] idx [ 22]: Int GPU core voltage. (Volts) (VN0C)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [ 23]: Internal GFX Core current. (Amps) (IN0C)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU Core Power (Watts) (PC0C)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp7s] 73703738 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 34 keys:
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Core PECI temp (DegC) (SIS! force bit 7) (TCXC)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  5]: Palm Rest Temp (DegC) (Ts0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  6]: Fin stack temp (DegC) (Th1H)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  7]: CPU proximity temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  8]: Dimm Proximity temp(DegC) (SIS! force bit 1) (TM0P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [  9]: Airport Temp (DegC) (TW0P)
 [TG1D] type [sp7s] 73703738 len [ 2] idx [ 10]: GPU digital die temp (DegC) (TG1D)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC3C] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Core 2 temp (PECI) (DegC) (TC3C)
 [TC4C] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Core 3 temp (PECI) (DegC) (TC4C)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 17]: Synthetic bottom skin (DegC) (Ts0S)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 18]: PCH Die temp (DegC) (TPCD)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 19]: CPU die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU PECI die temp Trend (DegC) (TCTD)
 [TCFC] type [ui1u] 75693136 len [ 2] idx [ 21]: CPU PECI die temp filter coeff (TCFC)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU PECI die temp max error filtered output (DegC) (TC0J)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 23]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 24]: Airflow temp (DegC) (TA0P)
 [TM0S] type [sp7s] 73703738 len [ 2] idx [ 25]: Synthetic DIMM Estimate(DegC) (SIS! force bit 1) (TM0S)
 [TMBS] type [sp7s] 73703738 len [ 2] idx [ 26]: DIMM Bandwidth Estimate (DegC) (SIS! force bit 1) (TMBS)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 27]: Cooked and filtered SSD OOB temperature (SIT! force bit 7) (TH0F)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for J11...
 Set 0 has 40 keys:
 [PHPC] type [sp7s] 73703738 len [ 2] idx [  1]: Thermal control Power (Watts) (PHPC)
 [PCLT] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Package Total Power (SMC Load Sensors) (Watts) (PCLT)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Computing High Side Power (Watts) (PC0R)
 [PO0R] type [sp7s] 73703738 len [ 2] idx [  4]: Other High Side Power   (Watts) (PO0R)
 [PPBR] type [sp7s] 73703738 len [ 2] idx [  5]: PBus on battery power (Watts) (PPBR)
 [PDTR] type [sp7s] 73703738 len [ 2] idx [  6]: DC-In total power  (Watts) (PDTR)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Core Power (Watts) (PC0C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  8]: Int GPU core Power (Watts) (PN0C)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [  9]: DDR Power (Memory) (Watts) (PM0R)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 11]: Airport Power   (watts) (PAPC)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [ 12]: SSD Power  (Watts) (PHDC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 13]: Backlight Input Power   (Watts) (PBLC)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU VCCSA Power (Watts) (PC2C)
 [PR1C] type [sp7s] 73703738 len [ 2] idx [ 15]: Other High Side current.  (Amps) (PR1C)
 [VC0C] type [sp5s] 73703561 len [ 2] idx [ 16]: CPU Core voltage. (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU Core current. (Amps) (IC0C)
 [VC2C] type [sp5s] 73703561 len [ 2] idx [ 18]: VCCSA voltage. (Volts) (VC2C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 19]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 20]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 21]: PBus rail voltage. (Volts) (VP0R)
 [IHDC] type [sp5s] 73703561 len [ 2] idx [ 22]: SSD Current  (Amps) (IHDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 23]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 24]: CPU Computing High Side current. (Amps) (IC0R)
 [IO0R] type [sp5s] 73703561 len [ 2] idx [ 25]: Other High Side current.  (Amps) (IO0R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [ 26]: DDR 1.5V (Memory) current. (Amps) (IM0R)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 27]: VCCIO  current. (Amps) (IC1C)
 [VN0C] type [sp5s] 73703561 len [ 2] idx [ 28]: Int GPU core voltage. (Volts) (VN0C)
 [IC2C] type [sp5s] 73703561 len [ 2] idx [ 29]: VCCSA  current. (Amps) (IC2C)
 [IR1C] type [sp5s] 73703561 len [ 2] idx [ 30]: Other High Side current.  (Amps) (IR1C)
 [IAPC] type [sp5s] 73703561 len [ 2] idx [ 31]: Airport Current (Amps) (IAPC)
 [IBLC] type [sp5s] 73703561 len [ 2] idx [ 32]: Backlight Current (Amps) (IBLC)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [ 33]: Internal GPU core current. (Amps) (IN0C)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp7s] 73703738 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 28 keys:
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Core PECI temp (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Core PECI temp (DegC) (TC0C)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core PECI temp (DegC) (TC0C)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  9]: CPU proximity temp (DegC) (TC0P)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU die temp (DegC) (TC0D)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 11]: Memory proximity (DegC) (TM0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [ 12]: air flow temp (DegC) (Ta0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [ 13]: Fin stack temp (DegC) (Th1H)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [ 14]: MLB top side temp  (DegC) (Tm0P)
 [Tm1P] type [sp7s] 73703738 len [ 2] idx [ 15]: MLB bottom side temp  (DegC) (Tm1P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 16]: Palm Rest Temp (DegC) (Ts0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [ 17]: T29 proximity temp (DegC) (THSP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 18]: PCH Die temp (DegC) (TPCD)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 19]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU die Virtual temp (DegC) (TC0E)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU PECI die temp max error filtered output used in TC0F=TC0E+TC0G (DegC) (TC0J)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for J13...
 Set 0 has 40 keys:
 [PHPC] type [sp7s] 73703738 len [ 2] idx [  1]: Thermal control Power (Watts) (PHPC)
 [PCLT] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Package Total Power (SMC Load Sensors) (Watts) (PCLT)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Computing High Side Power (Watts) (PC0R)
 [PO0R] type [sp7s] 73703738 len [ 2] idx [  4]: Other High Side Power   (Watts) (PO0R)
 [PPBR] type [sp7s] 73703738 len [ 2] idx [  5]: PBus on battery power (Watts) (PPBR)
 [PDTR] type [sp7s] 73703738 len [ 2] idx [  6]: DC-In total power  (Watts) (PDTR)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Core Power (Watts) (PC0C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  8]: Int GPU core Power (Watts) (PN0C)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [  9]: DDR Power (Memory) (Watts) (PM0R)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 11]: Airport Power   (watts) (PAPC)
 [PHDC] type [sp7s] 73703738 len [ 2] idx [ 12]: SSD Power  (Watts) (PHDC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 13]: Backlight Input Power   (Watts) (PBLC)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU VCCSA Power (Watts) (PC2C)
 [PR1C] type [sp7s] 73703738 len [ 2] idx [ 15]: Other High Side current.  (Amps) (PR1C)
 [VC0C] type [sp5s] 73703561 len [ 2] idx [ 16]: CPU Core voltage. (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU Core current. (Amps) (IC0C)
 [VC2C] type [sp5s] 73703561 len [ 2] idx [ 18]: VCCSA voltage. (Volts) (VC2C)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 19]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 20]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 21]: PBus rail voltage. (Volts) (VP0R)
 [IHDC] type [sp5s] 73703561 len [ 2] idx [ 22]: SSD Current  (Amps) (IHDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 23]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 24]: CPU Computing High Side current. (Amps) (IC0R)
 [IO0R] type [sp5s] 73703561 len [ 2] idx [ 25]: Other High Side current.  (Amps) (IO0R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [ 26]: DDR 1.5V (Memory) current. (Amps) (IM0R)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 27]: VCCIO  current. (Amps) (IC1C)
 [VN0C] type [sp5s] 73703561 len [ 2] idx [ 28]: Int GPU core voltage. (Volts) (VN0C)
 [IC2C] type [sp5s] 73703561 len [ 2] idx [ 29]: VCCSA  current. (Amps) (IC2C)
 [IR1C] type [sp5s] 73703561 len [ 2] idx [ 30]: Other High Side current.  (Amps) (IR1C)
 [IAPC] type [sp5s] 73703561 len [ 2] idx [ 31]: Airport Current (Amps) (IAPC)
 [IBLC] type [sp5s] 73703561 len [ 2] idx [ 32]: Backlight Current (Amps) (IBLC)
 [IN0C] type [sp5s] 73703561 len [ 2] idx [ 33]: Internal GPU core current. (Amps) (IN0C)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp7s] 73703738 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 28 keys:
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Core PECI temp (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Core PECI temp (DegC) (TC0C)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core PECI temp (DegC) (TC0C)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  9]: CPU proximity temp (DegC) (TC0P)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU die temp (DegC) (TC0D)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 11]: Memory proximity (DegC) (TM0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [ 12]: air flow temp (DegC) (Ta0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [ 13]: Fin stack temp (DegC) (Th1H)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [ 14]: MLB top side temp  (DegC) (Tm0P)
 [Tm1P] type [sp7s] 73703738 len [ 2] idx [ 15]: MLB bottom side temp  (DegC) (Tm1P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 16]: Palm Rest Temp (DegC) (Ts0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [ 17]: T29 proximity temp (DegC) (THSP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 18]: PCH Die temp (DegC) (TPCD)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 19]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU die Virtual temp (DegC) (TC0E)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU PECI die temp max error filtered output used in TC0F=TC0E+TC0G (DegC) (TC0J)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for J41...
 Set 0 has 48 keys:
 [PHPC] type [sp7s] 73703738 len [ 2] idx [  1]: Thermal control Power (Watts) (PHPC)
 [PCLT] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Package Total Power (SMC Load Sensors) (Watts) (PCLT)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Computing High Side Power (Watts) (PC0R)
 [PO0R] type [sp7s] 73703738 len [ 2] idx [  4]: Other High Side Power   (Watts) (PO0R)
 [PPBR] type [sp7s] 73703738 len [ 2] idx [  5]: PBus on battery power (Watts) (PPBR)
 [PDTR] type [sp7s] 73703738 len [ 2] idx [  6]: DC-In total power  (Watts) (PDTR)
 [PCS0] type [sp7s] 73703738 len [ 2] idx [  7]: Chipset lowside Power (Watts) (PCS0)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [  8]: Airport Power   (watts) (PAPC)
 [PSDC] type [sp7s] 73703738 len [ 2] idx [  9]: SSD Power  (Watts) (PSDC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 10]: Backlight Input Power   (Watts) (PBLC)
 [PB1R] type [sp7s] 73703738 len [ 2] idx [ 11]: Discrete BMON on battery power (Watts) (PB1R)
 [PM3C] type [sp7s] 73703738 len [ 2] idx [ 12]: DDR S3 Power. (Watts) (PM3C)
 [PR0C] type [sp7s] 73703738 len [ 2] idx [ 13]: 3.3V S0 power (Watts) (PR0C)
 [PR5C] type [sp7s] 73703738 len [ 2] idx [ 14]: 3.3V S5 power (Watts) (PR5C)
 [PS2C] type [sp7s] 73703738 len [ 2] idx [ 15]: S2 Camera power (Watts) (PS2C)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU DDR Power. (Watts) (PM0C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 17]: 1.05V S0 power (Watts) (PC1C)
 [PCS1] type [sp7s] 73703738 len [ 2] idx [ 18]: Chipset IMon Power (Watts) (PCS1)
 [VCS0] type [sp5s] 73703561 len [ 2] idx [ 19]: CPU Core voltage. (Volts) (VCS0)
 [ICS0] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU Core current. (Amps) (ICS0)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 21]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 22]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 23]: PBus rail voltage. (Volts) (VP0R)
 [ISDC] type [sp5s] 73703561 len [ 2] idx [ 24]: SSD Current  (Amps) (ISDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 25]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 26]: CPU Computing High Side current. (Amps) (IC0R)
 [IO0R] type [sp5s] 73703561 len [ 2] idx [ 27]: Other High Side current.  (Amps) (IO0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 28]: CPU DDR current. (Amps) (IM0C)
 [IR0C] type [sp5s] 73703561 len [ 2] idx [ 29]: 3.3V S0 current.  (Amps) (IR0C)
 [IAPC] type [sp5s] 73703561 len [ 2] idx [ 30]: Airport Current (Amps) (IAPC)
 [IBLC] type [sp5s] 73703561 len [ 2] idx [ 31]: Backlight Current (Amps) (IBLC)
 [IPB1] type [sp5s] 73703561 len [ 2] idx [ 32]: Discrete battery current. (Amps) (IPB1)
 [ILDC] type [sp5s] 73703561 len [ 2] idx [ 33]: LCD panel Current (Amps) (ILDC)
 [IM3C] type [sp5s] 73703561 len [ 2] idx [ 34]: DDR S3 current. (Amps) (IM3C)
 [IR5C] type [sp5s] 73703561 len [ 2] idx [ 35]: 3.3V S5 current.  (Amps) (IR5C)
 [IS2C] type [sp5s] 73703561 len [ 2] idx [ 36]: S2 Camera Current  (Amps) (IS2C)
 [VSDC] type [sp5s] 73703561 len [ 2] idx [ 37]: SD Card Voltage (Volts) (VSDC)
 [VC1C] type [sp5s] 73703561 len [ 2] idx [ 38]: 1.05 S0 voltage. (Volts) (VC1C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 39]: 1.05V S0 current. (Amps) (IC1C)
 [ICS1] type [sp7s] 73703738 len [ 2] idx [ 40]: CPU current from CPU IMON. (Amps) (ICS1)
 [VAPC] type [sp5s] 73703561 len [ 2] idx [ 41]: Wireless Voltage (Volts) (VAPC)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PTHC] type [fltf] 666C7420 len [ 4] idx [221]: HP Power Target (PTHC)
 [MSLT] type [fltf] 666C7420 len [ 4] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 29 keys:
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Core PECI temp (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [  8]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  9]: CPU proximity temp (DegC) (TC0P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 10]: Wireless proximity (DegC) (TW0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 11]: Memory proximity (DegC) (TM0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [ 12]: air flow temp (DegC) (Ta0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [ 13]: Fin stack temp (DegC) (Th1H)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [ 14]: MLB top side temp  (DegC) (Tm0P)
 [TCHP] type [sp7s] 73703738 len [ 2] idx [ 15]: Charger proximity temp  (DegC) (TCHP)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 16]: Trackpad Temp (DegC) (Ts0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [ 17]: T29 proximity temp (DegC) (THSP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 18]: PCH Die temp (DegC) (TPCD)
 [TS2P] type [sp7s] 73703738 len [ 2] idx [ 19]: S2 camera proximity temp (DegC) (TS2P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 20]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU die Virtual temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [si1s] 73693136 len [ 2] idx [243]: Battery Actual current. (A) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (V) (B0AV)
Dumping keys for J43...
 Set 0 has 48 keys:
 [PHPC] type [sp7s] 73703738 len [ 2] idx [  1]: Thermal control Power (Watts) (PHPC)
 [PCLT] type [sp7s] 73703738 len [ 2] idx [  2]: CPU Package Total Power (SMC Load Sensors) (Watts) (PCLT)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Computing High Side Power (Watts) (PC0R)
 [PO0R] type [sp7s] 73703738 len [ 2] idx [  4]: Other High Side Power   (Watts) (PO0R)
 [PPBR] type [sp7s] 73703738 len [ 2] idx [  5]: PBus on battery power (Watts) (PPBR)
 [PDTR] type [sp7s] 73703738 len [ 2] idx [  6]: DC-In total power  (Watts) (PDTR)
 [PCS0] type [sp7s] 73703738 len [ 2] idx [  7]: Chipset lowside Power (Watts) (PCS0)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [  8]: Airport Power   (watts) (PAPC)
 [PSDC] type [sp7s] 73703738 len [ 2] idx [  9]: SSD Power  (Watts) (PSDC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 10]: Backlight Input Power   (Watts) (PBLC)
 [PB1R] type [sp7s] 73703738 len [ 2] idx [ 11]: Discrete BMON on battery power (Watts) (PB1R)
 [PM3C] type [sp7s] 73703738 len [ 2] idx [ 12]: DDR S3 Power. (Watts) (PM3C)
 [PR0C] type [sp7s] 73703738 len [ 2] idx [ 13]: 3.3V S0 power (Watts) (PR0C)
 [PR5C] type [sp7s] 73703738 len [ 2] idx [ 14]: 3.3V S5 power (Watts) (PR5C)
 [PS2C] type [sp7s] 73703738 len [ 2] idx [ 15]: S2 Camera power (Watts) (PS2C)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU DDR Power. (Watts) (PM0C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 17]: 1.05V S0 power (Watts) (PC1C)
 [PCS1] type [sp7s] 73703738 len [ 2] idx [ 18]: Chipset IMon Power (Watts) (PCS1)
 [VCS0] type [sp5s] 73703561 len [ 2] idx [ 19]: CPU Core voltage. (Volts) (VCS0)
 [ICS0] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU Core current. (Amps) (ICS0)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 21]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 22]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 23]: PBus rail voltage. (Volts) (VP0R)
 [ISDC] type [sp5s] 73703561 len [ 2] idx [ 24]: SSD Current  (Amps) (ISDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 25]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 26]: CPU Computing High Side current. (Amps) (IC0R)
 [IO0R] type [sp5s] 73703561 len [ 2] idx [ 27]: Other High Side current.  (Amps) (IO0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 28]: CPU DDR current. (Amps) (IM0C)
 [IR0C] type [sp5s] 73703561 len [ 2] idx [ 29]: 3.3V S0 current.  (Amps) (IR0C)
 [IAPC] type [sp5s] 73703561 len [ 2] idx [ 30]: Airport Current (Amps) (IAPC)
 [IBLC] type [sp5s] 73703561 len [ 2] idx [ 31]: Backlight Current (Amps) (IBLC)
 [IPB1] type [sp5s] 73703561 len [ 2] idx [ 32]: Discrete battery current. (Amps) (IPB1)
 [ILDC] type [sp5s] 73703561 len [ 2] idx [ 33]: LCD panel Current (Amps) (ILDC)
 [IM3C] type [sp5s] 73703561 len [ 2] idx [ 34]: DDR S3 current. (Amps) (IM3C)
 [IR5C] type [sp5s] 73703561 len [ 2] idx [ 35]: 3.3V S5 current.  (Amps) (IR5C)
 [IS2C] type [sp5s] 73703561 len [ 2] idx [ 36]: S2 Camera Current  (Amps) (IS2C)
 [VSDC] type [sp5s] 73703561 len [ 2] idx [ 37]: SD Card Voltage (Volts) (VSDC)
 [VC1C] type [sp5s] 73703561 len [ 2] idx [ 38]: 1.05 S0 voltage. (Volts) (VC1C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 39]: 1.05V S0 current. (Amps) (IC1C)
 [ICS1] type [sp7s] 73703738 len [ 2] idx [ 40]: CPU current from CPU IMON. (Amps) (ICS1)
 [VAPC] type [sp5s] 73703561 len [ 2] idx [ 41]: Wireless Voltage (Volts) (VAPC)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PTHC] type [fltf] 666C7420 len [ 4] idx [221]: HP Power Target (PTHC)
 [MSLT] type [fltf] 666C7420 len [ 4] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 29 keys:
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Core PECI temp (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [  8]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  9]: CPU proximity temp (DegC) (TC0P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 10]: Wireless proximity (DegC) (TW0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 11]: Memory proximity (DegC) (TM0P)
 [Ta0P] type [sp7s] 73703738 len [ 2] idx [ 12]: air flow temp (DegC) (Ta0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [ 13]: Fin stack temp (DegC) (Th1H)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [ 14]: MLB top side temp  (DegC) (Tm0P)
 [TCHP] type [sp7s] 73703738 len [ 2] idx [ 15]: Charger proximity temp  (DegC) (TCHP)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [ 16]: Trackpad Temp (DegC) (Ts0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [ 17]: T29 proximity temp (DegC) (THSP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 18]: PCH Die temp (DegC) (TPCD)
 [TS2P] type [sp7s] 73703738 len [ 2] idx [ 19]: S2 camera proximity temp (DegC) (TS2P)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 20]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU die Virtual temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [si1s] 73693136 len [ 2] idx [243]: Battery Actual current. (A) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (V) (B0AV)
Dumping keys for D7...
 Set 0 has 34 keys:
 [IC0C] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Core low-side current (Amps) (IC0C)
 [IC0G] type [sp6s] 73703639 len [ 2] idx [  2]: CPU AXG  low-side current (Amps) (IC0G)
 [ID2R] type [sp6s] 73703639 len [ 2] idx [  3]: Power Supply 12V current (Amps) (ID2R)
 [IG0C] type [sp4s] 73703462 len [ 2] idx [  4]: GPU Core   high-side current (Amps) (IG0C)
 [IG0U] type [sp4s] 73703462 len [ 2] idx [  5]: GPU Uncore high-side current (Amps) (IG0U)
 [IH05] type [sp2s] 73703264 len [ 2] idx [  6]: HDD   5V low-side current (Amps) (IH05)
 [IH1R] type [sp2s] 73703264 len [ 2] idx [  7]: SSD 3.3V low-side current (Amps) (IH1R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [  8]: DIMM low-side current (Amps) (IM0R)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [  9]: CPU Core low-side power (Watts) (PC0C)
 [PC0G] type [sp9s] 73703936 len [ 2] idx [ 10]: CPU AXG  low-side power (Watts) (PC0G)
 [PCTR] type [sp9s] 73703936 len [ 2] idx [ 11]: CPU total power (PC0C + PC0G) (Watts) (PCTR)
 [PD2R] type [sp9s] 73703936 len [ 2] idx [ 12]: Power Supply 12V power (Watts) (PD2R)
 [PG0C] type [sp9s] 73703936 len [ 2] idx [ 13]: GPU Core   high-side power (Watts) (PG0C)
 [PG0U] type [sp9s] 73703936 len [ 2] idx [ 14]: GPU Uncore high-side power (Watts) (PG0U)
 [PGTR] type [sp9s] 73703936 len [ 2] idx [ 15]: GPU total power (PG0C + PG0U) (Watts) (PGTR)
 [PH0R] type [sp9s] 73703936 len [ 2] idx [ 16]: Drive 0 total (5V) low-side power (Watts) (PH0R)
 [PH1R] type [sp9s] 73703936 len [ 2] idx [ 17]: Drive 1 low-side power (Watts) (PH1R)
 [PM0R] type [sp9s] 73703936 len [ 2] idx [ 18]: DIMM low-side power (Watts) (PM0R)
 [PZ0G] type [sp9s] 73703936 len [ 2] idx [ 19]: Zone 0 average power (Watts) (PZ0G)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 20]: CPU Core low-side voltage (Volts) (VC0C)
 [VC0G] type [sp2s] 73703264 len [ 2] idx [ 21]: CPU AXG  low-side voltage (Volts) (VC0G)
 [VD2R] type [sp4s] 73703462 len [ 2] idx [ 22]: Power Supply 12V voltage (Volts) (VD2R)
 [VG0C] type [sp4s] 73703462 len [ 2] idx [ 23]: GPU Core   high-side voltage (Volts) (VG0C)
 [VG0U] type [sp4s] 73703462 len [ 2] idx [ 24]: GPU Uncore high-side voltage (Volts) (VG0U)
 [VH05] type [sp3s] 73703363 len [ 2] idx [ 25]: HDD   5V low-side voltage (Volts) (VH05)
 [VH1R] type [sp3s] 73703363 len [ 2] idx [ 26]: SSD 3.3V low-side voltage (Volts) (VH1R)
 [VM0R] type [sp2s] 73703264 len [ 2] idx [ 27]: DIMM low-side voltage (Volts) (VM0R)
 [PZ0F] type [sp9s] 73703936 len [ 2] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [sp9s] 73703936 len [ 2] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [ui1u] 75693136 len [ 2] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 48 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [Tb0p] type [sp7s] 73703738 len [ 2] idx [  2]: Backlight Controller proximity raw temp (DegC) (Tb0p)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Proximity raw temp (DegC) (TC0p)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [TG0p] type [sp7s] 73703738 len [ 2] idx [  6]: GPU 0 Proximity raw temp (DegC) (TG0p)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [  7]: Drive 0 (2.5) OOB v1 raw bit-mapped temp (TH0o)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [  8]: Drive 1 (2.5) OOB v1 raw bit-mapped temp (TH1o)
 [TL0p] type [sp7s] 73703738 len [ 2] idx [  9]: LCD unfiltered front-of-screen raw temp (DegC) (TL0p)
 [TL1p] type [sp7s] 73703738 len [ 2] idx [ 10]: LCD TCON Proximity raw temp (DegC) (TL1p)
 [TL2p] type [sp7s] 73703738 len [ 2] idx [ 11]: LCD IR target hotspot raw temp (DegC) (TL2p)
 [TL3p] type [spas] 73706135 len [ 2] idx [ 12]: LCD IR temp sensor die raw temp (DegC) (TL3p)
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [ 13]: MLB Proximity 0 raw temp (DegC) (Tm0p)
 [Tp2h] type [sp7s] 73703738 len [ 2] idx [ 14]: Power Supply T2 Secondary Heatsink raw temp (DegC) (Tp2h)
 [TS0p] type [sp7s] 73703738 len [ 2] idx [ 15]: Skin 0 raw temp (DegC) (TS0p)
 [VL3t] type [si1s] 73693136 len [ 2] idx [ 16]: LCD IR temp sensor voltage (Raw Register) (VL3t)
 [PCPC] type [sp9s] 73703936 len [ 2] idx [ 17]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp9s] 73703936 len [ 2] idx [ 18]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [PCPT] type [sp9s] 73703936 len [ 2] idx [ 19]: CPU package total power (PECI) (Watts) (PCPT)
 [PH0F] type [sp7s] 73703738 len [ 2] idx [ 20]: Drive 0 total (5V) filtered low-side power * 16 (Watts) (PH0F)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive 1 filtered low-side power * 16 (Watts) (PH1F)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 22]: Ambient cooked temp (DegC) (TA0P)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 23]: Ambient virtual temp (DegC) (TA0V)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU PECI Die filtered temp for fan control (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU PECI Die filtered and adjusted temp for power control (DegC) (TC0F)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 26]: GPU 0 Die cooked temp (DegC) (TG0D)
 [TG0E] type [sp7s] 73703738 len [ 2] idx [ 27]: GPU 0 Die filtered temp for fan control (DegC) (TG0E)
 [TG0F] type [sp7s] 73703738 len [ 2] idx [ 28]: GPU 0 Die filtered and adjusted temp for power control (DegC) (TG0F)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 29]: SSD 0 (2.5) OOB v3 relative filtered temp Max (DegC) (TH0F)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [ 30]: SSD 1 (Gumstick) OOB v3 relative filtered temp Max (DegC) (TH1F)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 31]: Drive 0 (2.5) OOB v1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 32]: Drive 1 (Gumstick) OOB v1 mapped temp (DegC) (TH1O)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 33]: Drive 0 (2.5) OOB v1 filtered temp (DegC) (TH0P)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 34]: SSD 0 (2.5) OOB v3 relative cooked temp Max (DegC) (TH0R)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 35]: Drive 1 (Gumstick) OOB v1 filtered temp (DegC) (TH1P)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 36]: SSD 1 (Gumstick) OOB v3 relative cooked   temp Max (DegC) (TH1R)
 [TL0P] type [sp7s] 73703738 len [ 2] idx [ 37]: LCD unfiltered front-of-screen cooked temp (DegC) (TL0P)
 [TL0V] type [sp7s] 73703738 len [ 2] idx [ 38]: LCD filtered right front-of-screen virtual temp (DegC) (TL0V)
 [TL1V] type [sp7s] 73703738 len [ 2] idx [ 39]: LCD TL1v-filtered center front-of-screen temp for color compensation (DegC) (TL1V)
 [TL1v] type [sp7s] 73703738 len [ 2] idx [ 40]: LCD filtered center front-of-screen temp that feeds TL1V (DegC) (TL1v)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 41]: DIMM virtual temp (DegC) (TM0V)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 42]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 43]: PCH Die cooked temp (DegC) (TPCD)
 [Tp2F] type [sp7s] 73703738 len [ 2] idx [ 44]: Power Supply T2 Secondary Heatsink filtered temp (DegC) (Tp2F)
 [Tp2H] type [sp7s] 73703738 len [ 2] idx [ 45]: Power Supply T2 Secondary Heatsink cooked temp (DegC) (Tp2H)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [ 46]: Skin 0 virtual temp (DegC) (TS0V)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp9s] 73703936 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for D7I...
 Set 0 has 27 keys:
 [IC0C] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Core low-side current (Amps) (IC0C)
 [IC0G] type [sp6s] 73703639 len [ 2] idx [  2]: CPU AXG  low-side current (Amps) (IC0G)
 [ID2R] type [sp6s] 73703639 len [ 2] idx [  3]: Power Supply 12V current (Amps) (ID2R)
 [IH05] type [sp2s] 73703264 len [ 2] idx [  4]: HDD   5V low-side current (Amps) (IH05)
 [IH1R] type [sp2s] 73703264 len [ 2] idx [  5]: SSD 3.3V low-side current (Amps) (IH1R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [  6]: DIMM low-side current (Amps) (IM0R)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [  7]: CPU Core low-side power (Watts) (PC0C)
 [PC0G] type [sp9s] 73703936 len [ 2] idx [  8]: CPU AXG  low-side power (Watts) (PC0G)
 [PCTR] type [sp9s] 73703936 len [ 2] idx [  9]: CPU total power (PC0C + PC0G) (Watts) (PCTR)
 [PD2R] type [sp9s] 73703936 len [ 2] idx [ 10]: Power Supply 12V power (Watts) (PD2R)
 [PH0R] type [sp9s] 73703936 len [ 2] idx [ 11]: Drive 0 total (5V) low-side power (Watts) (PH0R)
 [PH1R] type [sp9s] 73703936 len [ 2] idx [ 12]: Drive 1 low-side power (Watts) (PH1R)
 [PM0R] type [sp9s] 73703936 len [ 2] idx [ 13]: DIMM low-side power (Watts) (PM0R)
 [PZ0G] type [sp9s] 73703936 len [ 2] idx [ 14]: Zone 0 average power (Watts) (PZ0G)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 15]: CPU Core low-side voltage (Volts) (VC0C)
 [VC0G] type [sp2s] 73703264 len [ 2] idx [ 16]: CPU AXG  low-side voltage (Volts) (VC0G)
 [VD2R] type [sp4s] 73703462 len [ 2] idx [ 17]: Power Supply 12V voltage (Volts) (VD2R)
 [VH05] type [sp3s] 73703363 len [ 2] idx [ 18]: HDD   5V low-side voltage (Volts) (VH05)
 [VH1R] type [sp3s] 73703363 len [ 2] idx [ 19]: SSD 3.3V low-side voltage (Volts) (VH1R)
 [VM0R] type [sp2s] 73703264 len [ 2] idx [ 20]: DIMM low-side voltage (Volts) (VM0R)
 [PZ0F] type [sp9s] 73703936 len [ 2] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [sp9s] 73703936 len [ 2] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [ui1u] 75693136 len [ 2] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 45 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [Tb0p] type [sp7s] 73703738 len [ 2] idx [  2]: Backlight Controller proximity raw temp (DegC) (Tb0p)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Proximity raw temp (DegC) (TC0p)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [TG0p] type [sp7s] 73703738 len [ 2] idx [  6]: GPU 0 Proximity raw temp (DegC) (TG0p)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [  7]: Drive 0 (2.5) OOB v1 raw bit-mapped temp (TH0o)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [  8]: Drive 1 (2.5) OOB v1 raw bit-mapped temp (TH1o)
 [TL0p] type [sp7s] 73703738 len [ 2] idx [  9]: LCD unfiltered front-of-screen raw temp (DegC) (TL0p)
 [TL1p] type [sp7s] 73703738 len [ 2] idx [ 10]: LCD TCON Proximity raw temp (DegC) (TL1p)
 [TL2p] type [sp7s] 73703738 len [ 2] idx [ 11]: LCD IR target hotspot raw temp (DegC) (TL2p)
 [TL3p] type [spas] 73706135 len [ 2] idx [ 12]: LCD IR temp sensor die raw temp (DegC) (TL3p)
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [ 13]: MLB Proximity 0 raw temp (DegC) (Tm0p)
 [Tp2h] type [sp7s] 73703738 len [ 2] idx [ 14]: Power Supply T2 Secondary Heatsink raw temp (DegC) (Tp2h)
 [TS0p] type [sp7s] 73703738 len [ 2] idx [ 15]: Skin 0 raw temp (DegC) (TS0p)
 [VL3t] type [si1s] 73693136 len [ 2] idx [ 16]: LCD IR temp sensor voltage (Raw Register) (VL3t)
 [PCPC] type [sp9s] 73703936 len [ 2] idx [ 17]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp9s] 73703936 len [ 2] idx [ 18]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [PCPT] type [sp9s] 73703936 len [ 2] idx [ 19]: CPU package total power (PECI) (Watts) (PCPT)
 [PH0F] type [sp7s] 73703738 len [ 2] idx [ 20]: Drive 0 total (5V) filtered low-side power * 16 (Watts) (PH0F)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive 1 filtered low-side power * 16 (Watts) (PH1F)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 22]: Ambient cooked temp (DegC) (TA0P)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 23]: Ambient virtual temp (DegC) (TA0V)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU PECI Die filtered temp for fan control (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU PECI Die filtered and adjusted temp for power control (DegC) (TC0F)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 26]: SSD 0 (2.5) OOB v3 relative filtered temp Max (DegC) (TH0F)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [ 27]: SSD 1 (Gumstick) OOB v3 relative filtered temp Max (DegC) (TH1F)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 28]: Drive 0 (2.5) OOB v1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 29]: Drive 1 (Gumstick) OOB v1 mapped temp (DegC) (TH1O)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 30]: Drive 0 (2.5) OOB v1 filtered temp (DegC) (TH0P)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 31]: SSD 0 (2.5) OOB v3 relative cooked temp Max (DegC) (TH0R)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 32]: Drive 1 (Gumstick) OOB v1 filtered temp (DegC) (TH1P)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 33]: SSD 1 (Gumstick) OOB v3 relative cooked   temp Max (DegC) (TH1R)
 [TL0P] type [sp7s] 73703738 len [ 2] idx [ 34]: LCD unfiltered front-of-screen cooked temp (DegC) (TL0P)
 [TL0V] type [sp7s] 73703738 len [ 2] idx [ 35]: LCD filtered right front-of-screen virtual temp (DegC) (TL0V)
 [TL1V] type [sp7s] 73703738 len [ 2] idx [ 36]: LCD TL1v-filtered center front-of-screen temp for color compensation (DegC) (TL1V)
 [TL1v] type [sp7s] 73703738 len [ 2] idx [ 37]: LCD filtered center front-of-screen temp that feeds TL1V (DegC) (TL1v)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 38]: DIMM virtual temp (DegC) (TM0V)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 39]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 40]: PCH Die cooked temp (DegC) (TPCD)
 [Tp2F] type [sp7s] 73703738 len [ 2] idx [ 41]: Power Supply T2 Secondary Heatsink filtered temp (DegC) (Tp2F)
 [Tp2H] type [sp7s] 73703738 len [ 2] idx [ 42]: Power Supply T2 Secondary Heatsink cooked temp (DegC) (Tp2H)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [ 43]: Skin 0 virtual temp (DegC) (TS0V)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp9s] 73703936 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for D8...
 Set 0 has 49 keys:
 [IC0C] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Core low-side current (Amps) (IC0C)
 [IC0G] type [sp6s] 73703639 len [ 2] idx [  2]: CPU AXG  low-side current (Amps) (IC0G)
 [IC0I] type [sp2s] 73703264 len [ 2] idx [  3]: CPU I/O high-side current (Amps) (IC0I)
 [IC0M] type [sp2s] 73703264 len [ 2] idx [  4]: CPU Mem  low-side current (Amps) (IC0M)
 [IC0S] type [sp2s] 73703264 len [ 2] idx [  5]: CPU SA  high-side current (Amps) (IC0S)
 [ID2R] type [sp6s] 73703639 len [ 2] idx [  6]: Power Supply 12V  current (Amps) (ID2R)
 [IG0C] type [sp8s] 73703837 len [ 2] idx [  7]: GPU Core low-side current (Amps) (IG0C)
 [IG0F] type [sp3s] 73703363 len [ 2] idx [  8]: GPU FB  high-side current (Amps) (IG0F)
 [IH02] type [sp1s] 73703165 len [ 2] idx [  9]: HDD  12V low-side current (Amps) (IH02)
 [IH05] type [sp2s] 73703264 len [ 2] idx [ 10]: HDD   5V low-side current (Amps) (IH05)
 [IH1R] type [sp2s] 73703264 len [ 2] idx [ 11]: SSD 3.3V low-side current (Amps) (IH1R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [ 12]: DIMM     low-side current (Amps) (IM0R)
 [IN1R] type [sp3s] 73703363 len [ 2] idx [ 13]: PCH      low-side current (Amps) (IN1R)
 [IR1R] type [sp1s] 73703165 len [ 2] idx [ 14]: PCH/GPU/TBT 1.05V high-side current (Amps) (IR1R)
 [IW0R] type [sp2s] 73703264 len [ 2] idx [ 15]: Wifi     low-side current (Amps) (IW0R)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [ 16]: CPU Core low-side power (Watts) (PC0C)
 [PC0G] type [sp9s] 73703936 len [ 2] idx [ 17]: CPU AXG  low-side power (Watts) (PC0G)
 [PC0I] type [sp9s] 73703936 len [ 2] idx [ 18]: CPU I/O high-side power (Watts) (PC0I)
 [PC0M] type [sp9s] 73703936 len [ 2] idx [ 19]: CPU Mem  low-side power (Watts) (PC0M)
 [PC0S] type [sp9s] 73703936 len [ 2] idx [ 20]: CPU SA  high-side power (Watts) (PC0S)
 [PCTR] type [sp9s] 73703936 len [ 2] idx [ 21]: CPU total power (PC0C+PC0G+PC0I+PC0M+PC0S) (Watts) (PCTR)
 [PD2R] type [sp9s] 73703936 len [ 2] idx [ 22]: Power Supply 12V power (Watts) (PD2R)
 [PG0C] type [sp9s] 73703936 len [ 2] idx [ 23]: GPU Core       low-side power (Watts) (PG0C)
 [PG0F] type [sp9s] 73703936 len [ 2] idx [ 24]: GPU Frame Buf high-side power (Watts) (PG0F)
 [PGTR] type [sp9s] 73703936 len [ 2] idx [ 25]: GPU total power (PG0C + PG0F) (Watts) (PGTR)
 [PH02] type [sp9s] 73703936 len [ 2] idx [ 26]: Drive 0 12V low-side power (Watts) (PH02)
 [PH05] type [sp9s] 73703936 len [ 2] idx [ 27]: Drive 0  5V low-side power (Watts) (PH05)
 [PH0R] type [sp9s] 73703936 len [ 2] idx [ 28]: Drive 0 total power (PH02 + PH05) (Watts) (PH0R)
 [PH1R] type [sp9s] 73703936 len [ 2] idx [ 29]: Drive 1 low-side power (Watts) (PH1R)
 [PM0R] type [sp9s] 73703936 len [ 2] idx [ 30]: DIMM low-side power (Watts) (PM0R)
 [PN1R] type [sp9s] 73703936 len [ 2] idx [ 31]: PCH  low-side power (Watts) (PN1R)
 [PR1R] type [sp9s] 73703936 len [ 2] idx [ 32]: 1.05V high-side power (Watts) (PR1R)
 [PW0R] type [sp9s] 73703936 len [ 2] idx [ 33]: Wifi low-side power (Watts) (PW0R)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 34]: CPU Core low-side voltage (Volts) (VC0C)
 [VC0G] type [sp2s] 73703264 len [ 2] idx [ 35]: CPU AXG  low-side voltage (Volts) (VC0G)
 [VC0M] type [sp2s] 73703264 len [ 2] idx [ 36]: CPU Mem  low-side voltage (Volts) (VC0M)
 [VD2R] type [sp4s] 73703462 len [ 2] idx [ 37]: Power Supply 12V voltage (Volts) (VD2R)
 [VG0C] type [sp2s] 73703264 len [ 2] idx [ 38]: GPU Core low-side voltage (Volts) (VG0C)
 [VH05] type [sp3s] 73703363 len [ 2] idx [ 39]: HDD 5V   low-side voltage (Volts) (VH05)
 [VM0R] type [sp2s] 73703264 len [ 2] idx [ 40]: DIMM low-side voltage (Volts) (VM0R)
 [VN1R] type [sp2s] 73703264 len [ 2] idx [ 41]: PCH low-side voltage (Volts) (VN1R)
 [VR3R] type [sp3s] 73703363 len [ 2] idx [ 42]: 3.3V S0 rail voltage (Volts) (VR3R)
 [PZ0G] type [sp9s] 73703936 len [ 2] idx [220]: Zone 0 Power (PZ0G)
 [PZ0E] type [sp9s] 73703936 len [ 2] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [ui1u] 75693136 len [ 2] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 49 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [Tb0p] type [sp7s] 73703738 len [ 2] idx [  2]: Backlight Controller proximity raw temp (DegC) (Tb0p)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Proximity raw temp (DegC) (TC0p)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [TG0p] type [sp7s] 73703738 len [ 2] idx [  6]: GPU 0 Proximity raw temp (DegC) (TG0p)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [  7]: Drive 0 (2.5) OOB v1 raw bit-mapped temp (TH0o)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [  8]: Drive 1 (2.5) OOB v1 raw bit-mapped temp (TH1o)
 [TL0p] type [sp7s] 73703738 len [ 2] idx [  9]: LCD unfiltered front-of-screen raw temp (DegC) (TL0p)
 [TL1p] type [sp7s] 73703738 len [ 2] idx [ 10]: LCD TCON Proximity raw temp (DegC) (TL1p)
 [TL2p] type [sp7s] 73703738 len [ 2] idx [ 11]: LCD IR target hotspot raw temp (DegC) (TL2p)
 [TL3p] type [spas] 73706135 len [ 2] idx [ 12]: LCD IR temp sensor die raw temp (DegC) (TL3p)
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [ 13]: MLB Proximity 0 raw temp (DegC) (Tm0p)
 [Tm1p] type [sp7s] 73703738 len [ 2] idx [ 14]: MLB Proximity 1 raw temp (DegC) (Tm1p)
 [Tp2h] type [sp7s] 73703738 len [ 2] idx [ 15]: Power Supply T2 Secondary Heatsink raw temp (DegC) (Tp2h)
 [TS0p] type [sp7s] 73703738 len [ 2] idx [ 16]: Skin 0 raw temp (DegC) (TS0p)
 [VL3t] type [ui1u] 75693136 len [ 2] idx [ 17]: LCD IR temp sensor voltage (Raw Register) (VL3t)
 [PCPC] type [sp9s] 73703936 len [ 2] idx [ 18]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp9s] 73703936 len [ 2] idx [ 19]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [PCPT] type [sp9s] 73703936 len [ 2] idx [ 20]: CPU package total power (PECI) (Watts) (PCPT)
 [PH0F] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive 0 filtered total power (PH02 + PH05) * 16 (Watts) (PH0F)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 22]: Drive 1 filtered low-side power * 16 (Watts) (PH1F)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 23]: Ambient cooked temp (DegC) (TA0P)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 24]: Ambient virtual temp (DegC) (TA0V)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU PECI Die filtered temp for fan control (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 26]: CPU PECI Die filtered and adjusted temp for power control (DegC) (TC0F)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 27]: GPU 0 Die cooked temp (DegC) (TG0D)
 [TG0E] type [sp7s] 73703738 len [ 2] idx [ 28]: GPU 0 Die filtered temp for fan control (DegC) (TG0E)
 [TG0F] type [sp7s] 73703738 len [ 2] idx [ 29]: GPU 0 Die filtered and adjusted temp for power control (DegC) (TG0F)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 30]: SSD 0 (2.5) OOB v3 relative filtered temp Max (DegC) (TH0F)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [ 31]: SSD 1 (Gumstick) OOB v3 relative filtered temp Max (DegC) (TH1F)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 32]: Drive 0 (2.5) OOB v1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 33]: Drive 1 (Gumstick) OOB v1 mapped temp (DegC) (TH1O)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 34]: Drive 0 (2.5) OOB v1 filtered temp (DegC) (TH0P)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 35]: SSD 0 (2.5) OOB v3 relative cooked temp Max (DegC) (TH0R)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 36]: Drive 1 (Gumstick) OOB v1 filtered temp (DegC) (TH1P)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 37]: SSD 1 (Gumstick) OOB v3 relative cooked   temp Max (DegC) (TH1R)
 [TL0P] type [sp7s] 73703738 len [ 2] idx [ 38]: LCD unfiltered front-of-screen cooked temp (DegC) (TL0P)
 [TL0V] type [sp7s] 73703738 len [ 2] idx [ 39]: LCD filtered right front-of-screen virtual temp (DegC) (TL0V)
 [TL1V] type [sp7s] 73703738 len [ 2] idx [ 40]: LCD TL1v-filtered center front-of-screen temp for color compensation (DegC) (TL1V)
 [TL1v] type [sp7s] 73703738 len [ 2] idx [ 41]: LCD filtered center front-of-screen temp that feeds TL1V (DegC) (TL1v)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 42]: DIMM virtual temp (DegC) (TM0V)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 43]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 44]: PCH Die cooked temp (DegC) (TPCD)
 [Tp2F] type [sp7s] 73703738 len [ 2] idx [ 45]: Power Supply T2 Secondary Heatsink filtered temp (DegC) (Tp2F)
 [Tp2H] type [sp7s] 73703738 len [ 2] idx [ 46]: Power Supply T2 Secondary Heatsink cooked temp (DegC) (Tp2H)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [ 47]: Skin 0 virtual temp (DegC) (TS0V)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp9s] 73703936 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J50I...
 Set 0 has 38 keys:
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  1]: CPU High side power (IC0R * VD0R) (Watts) (PC0R)
 [PD0F] type [sp7s] 73703738 len [ 2] idx [  2]: Power supply power filtered then adjusted (Watts) (PD0F)
 [PD0E] type [sp7s] 73703738 len [ 2] idx [  3]: Power supply filtered power (Watts) (PD0E)
 [PDTR] type [sp7s] 73703738 len [ 2] idx [  4]: DC In rail power (ID0R * VD0R) (Watts) (PDTR)
 [PD0D] type [sp7s] 73703738 len [ 2] idx [  5]: Power Supply Power Trend (Watts) (PD0D)
 [PD0J] type [sp7s] 73703738 len [ 2] idx [  6]: Power supply max error filtered output (Watts) (PD0J)
 [PD0K] type [sp7s] 73703738 len [ 2] idx [  7]: Power supply filter coefficient (Watts) (PD0K)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Vcore power (IC0C * VC0C) (Watts) (PC0C)
 [PN0R] type [sp7s] 73703738 len [ 2] idx [  9]: GFX Vcore power (IN0R * VN0R) (Watts) (PN0R)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [ 10]: Memory power (IM0C * VM0R) (Watts) (PM0C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU VCCIO power (IC1C * 1.05V) (Watts) (PC1C)
 [PD1R] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU 1V5 power (ID1R * 1.5V) (Watts) (PD1R)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU VCCSA power (IC2C * VC2C) (Watts) (PC2C)
 [PN1R] type [sp7s] 73703738 len [ 2] idx [ 14]: PCH 1V05 power (IN1R * 1.05V) (Watts) (PN1R)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 15]: Airport power (IAPC * 3.3V) (Watts) (PAPC)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 16]: CPU Vcore voltage (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 17]: CPU Vcore current (Amps) (IC0C)
 [Vp0C] type [sp2s] 73703264 len [ 2] idx [ 18]: ACDC cooked temp (Volts) (Vp0C)
 [VN0R] type [sp2s] 73703264 len [ 2] idx [ 19]: GFX Vcore voltage (Volts) (VN0R)
 [IN0R] type [sp6s] 73703639 len [ 2] idx [ 20]: GFX Vcore current (Amps) (IN0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 21]: Memory current (Amps) (IM0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 22]: CPU VCCIO current (Amps) (IC1C)
 [ID1R] type [sp5s] 73703561 len [ 2] idx [ 23]: CPU 1V5 current (Amps) (ID1R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 24]: DC In voltage (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 25]: DC In current (Amps) (ID0R)
 [VC2C] type [sp2s] 73703264 len [ 2] idx [ 26]: CPU VCCSA voltage (Volts) (VC2C)
 [IC2C] type [sp5s] 73703561 len [ 2] idx [ 27]: CPU VCCSA current (Amps) (IC2C)
 [IC0R] type [sp4s] 73703462 len [ 2] idx [ 28]: CPU High side current (Amps) (IC0R)
 [IN1R] type [sp5s] 73703561 len [ 2] idx [ 29]: PCH 1V05 current (Amps) (IN1R)
 [PH1R] type [sp7s] 73703738 len [ 2] idx [ 30]: Drive 1 power (IH1R * 3.3V) (Watts) (PH1R)
 [PH2R] type [sp7s] 73703738 len [ 2] idx [ 31]: Drive 2 power (IH2R * 3.3V) (Watts) (PH2R)
 [PZ0F] type [sp7s] 73703738 len [ 2] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [sp7s] 73703738 len [ 2] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [ui1u] 75693136 len [ 2] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 41 keys:
 [TC0d] type [sp7s] 73703738 len [ 2] idx [  1]: CPU die raw temp (DegC) (TC0d)
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  4]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Gfx Core absolute cooked temp (PECI) (DegC) (TCGC)
 [TCSC] type [sp7s] 73703738 len [ 2] idx [  6]: CPU System Agent Core absolute cooked temp (PECI) (DegC) (TCSC)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Core 0 absolute cooked temp (PECI) (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core 1 absolute cooked temp (PECI) (DegC) (TC1C)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [  9]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU PECI die Virtual temp (DegC) (TC0E)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Max Package Core absolute cooked temp (PECI) (DegC) (TCXC)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU PECI die temp Trend (DegC) (TCTD)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU PECI die temp max error filtered output (DegC) (TC0J)
 [TCFC] type [ui1u] 75693136 len [ 2] idx [ 14]: CPU PECI die temp filter coeff (TCFC)
 [TM0S] type [sp7s] 73703738 len [ 2] idx [ 15]: Synthetic DIMM Estimate(DegC) (SIS! force bit 1) (TM0S)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 16]: Memory proximity temp (filtered) (DegC) (TM0P)
 [TMBS] type [sp7s] 73703738 len [ 2] idx [ 17]: DIMM Bandwidth Estimate (DegC) (SIS! force bit 1) (TMBS)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 18]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 19]: CPU proximity temp (filtered) (DegC) (TC0P)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 20]: Ambient 0 temp (DegC) (TA0P)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive 0 OOB v1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 22]: Drive 1 OOB v1 mapped temp (DegC) (TH1O)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 23]: SSD 0 OOB v3 absolute cooked temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 24]: SSD 0 OOB v3 absolute cooked temp B (DegC) (TH0B)
 [TH0C] type [sp7s] 73703738 len [ 2] idx [ 25]: SSD 0 OOB v3 absolute cooked temp C (DegC) (TH0C)
 [TH0X] type [sp7s] 73703738 len [ 2] idx [ 26]: SSD 0 OOB v3 cooked temp Max (DegC) (TH0X)
 [TH1A] type [sp7s] 73703738 len [ 2] idx [ 27]: SSD 1 OOB v3 absolute cooked temp A (DegC) (TH1A)
 [TH1B] type [sp7s] 73703738 len [ 2] idx [ 28]: SSD 1 OOB v3 absolute cooked temp B (DegC) (TH1B)
 [TH1C] type [sp7s] 73703738 len [ 2] idx [ 29]: SSD 1 OOB v3 absolute cooked temp C (DegC) (TH1C)
 [TH1X] type [sp7s] 73703738 len [ 2] idx [ 30]: SSD 1 OOB v3 cooked   temp Max (DegC) (TH1X)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [ 31]: CPU die temp (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 32]: CPU proximity temp (filtered) (DegC) (TC0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [ 33]: PCH proximity temp (DegC) (TP0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 34]: PCH digital die temp (DegC) (TPCD)
 [TI0P] type [sp7s] 73703738 len [ 2] idx [ 35]: High Speed I/O proximity 0 temp (DegC) (TI0P)
 [TI1P] type [sp7s] 73703738 len [ 2] idx [ 36]: High Speed I/O proximity 1 temp (DegC) (TI1P)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 37]: Ambient 0 temp (DegC) (TA0P)
 [TA1P] type [sp7s] 73703738 len [ 2] idx [ 38]: Ambient 1 temp (DegC) (TA1P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 39]: Airport Card temp (DegC) (TW0P)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J50S...
 Set 0 has 38 keys:
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  1]: CPU High side power (IC0R * VD0R) (Watts) (PC0R)
 [PD0F] type [sp7s] 73703738 len [ 2] idx [  2]: Power supply power filtered then adjusted (Watts) (PD0F)
 [PD0E] type [sp7s] 73703738 len [ 2] idx [  3]: Power supply filtered power (Watts) (PD0E)
 [PDTR] type [sp7s] 73703738 len [ 2] idx [  4]: DC In rail power (ID0R * VD0R) (Watts) (PDTR)
 [PD0D] type [sp7s] 73703738 len [ 2] idx [  5]: Power Supply Power Trend (Watts) (PD0D)
 [PD0J] type [sp7s] 73703738 len [ 2] idx [  6]: Power supply max error filtered output (Watts) (PD0J)
 [PD0K] type [sp7s] 73703738 len [ 2] idx [  7]: Power supply filter coefficient (Watts) (PD0K)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Vcore power (IC0C * VC0C) (Watts) (PC0C)
 [PN0R] type [sp7s] 73703738 len [ 2] idx [  9]: GFX Vcore power (IN0R * VN0R) (Watts) (PN0R)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [ 10]: Memory power (IM0C * VM0R) (Watts) (PM0C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU VCCIO power (IC1C * 1.05V) (Watts) (PC1C)
 [PD1R] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU 1V5 power (ID1R * 1.5V) (Watts) (PD1R)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU VCCSA power (IC2C * VC2C) (Watts) (PC2C)
 [PN1R] type [sp7s] 73703738 len [ 2] idx [ 14]: PCH 1V05 power (IN1R * 1.05V) (Watts) (PN1R)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 15]: Airport power (IAPC * 3.3V) (Watts) (PAPC)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 16]: CPU Vcore voltage (Volts) (VC0C)
 [IC0C] type [sp8s] 73703837 len [ 2] idx [ 17]: CPU Vcore current (Amps) (IC0C)
 [Vp0C] type [sp2s] 73703264 len [ 2] idx [ 18]: ACDC cooked temp (Volts) (Vp0C)
 [VN0R] type [sp2s] 73703264 len [ 2] idx [ 19]: GFX Vcore voltage (Volts) (VN0R)
 [IN0R] type [sp6s] 73703639 len [ 2] idx [ 20]: GFX Vcore current (Amps) (IN0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 21]: Memory current (Amps) (IM0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 22]: CPU VCCIO current (Amps) (IC1C)
 [ID1R] type [sp5s] 73703561 len [ 2] idx [ 23]: CPU 1V5 current (Amps) (ID1R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 24]: DC In voltage (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 25]: DC In current (Amps) (ID0R)
 [VC2C] type [sp2s] 73703264 len [ 2] idx [ 26]: CPU VCCSA voltage (Volts) (VC2C)
 [IC2C] type [sp5s] 73703561 len [ 2] idx [ 27]: CPU VCCSA current (Amps) (IC2C)
 [IC0R] type [sp4s] 73703462 len [ 2] idx [ 28]: CPU High side current (Amps) (IC0R)
 [IN1R] type [sp5s] 73703561 len [ 2] idx [ 29]: PCH 1V05 current (Amps) (IN1R)
 [PH1R] type [sp7s] 73703738 len [ 2] idx [ 30]: Drive 1 power (IH1R * 3.3V) (Watts) (PH1R)
 [PH2R] type [sp7s] 73703738 len [ 2] idx [ 31]: Drive 2 power (IH2R * 3.3V) (Watts) (PH2R)
 [PZ0F] type [sp7s] 73703738 len [ 2] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [sp7s] 73703738 len [ 2] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [ui1u] 75693136 len [ 2] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 43 keys:
 [TC0d] type [sp7s] 73703738 len [ 2] idx [  1]: CPU die raw temp (DegC) (TC0d)
 [PCPT] type [sp7s] 73703738 len [ 2] idx [  2]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [  3]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [  4]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Gfx Core absolute cooked temp (PECI) (DegC) (TCGC)
 [TCSC] type [sp7s] 73703738 len [ 2] idx [  6]: CPU System Agent Core absolute cooked temp (PECI) (DegC) (TCSC)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [  7]: CPU Core 0 absolute cooked temp (PECI) (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU Core 1 absolute cooked temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [  9]: CPU Core 2 absolute cooked temp (PECI) (DegC) (TC2C)
 [TC3C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU Core 3 absolute cooked temp (PECI) (DegC) (TC3C)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU PECI die Virtual temp (DegC) (TC0E)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Max Package Core absolute cooked temp (PECI) (DegC) (TCXC)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU PECI die temp Trend (DegC) (TCTD)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU PECI die temp max error filtered output (DegC) (TC0J)
 [TCFC] type [ui1u] 75693136 len [ 2] idx [ 16]: CPU PECI die temp filter coeff (TCFC)
 [TM0S] type [sp7s] 73703738 len [ 2] idx [ 17]: Synthetic DIMM Estimate(DegC) (SIS! force bit 1) (TM0S)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 18]: Memory proximity temp (filtered) (DegC) (TM0P)
 [TMBS] type [sp7s] 73703738 len [ 2] idx [ 19]: DIMM Bandwidth Estimate (DegC) (SIS! force bit 1) (TMBS)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 20]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU proximity temp (filtered) (DegC) (TC0P)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 22]: Ambient 0 temp (DegC) (TA0P)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 23]: Drive 0 OOB v1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 24]: Drive 1 OOB v1 mapped temp (DegC) (TH1O)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 25]: SSD 0 OOB v3 absolute cooked temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 26]: SSD 0 OOB v3 absolute cooked temp B (DegC) (TH0B)
 [TH0C] type [sp7s] 73703738 len [ 2] idx [ 27]: SSD 0 OOB v3 absolute cooked temp C (DegC) (TH0C)
 [TH0X] type [sp7s] 73703738 len [ 2] idx [ 28]: SSD 0 OOB v3 cooked temp Max (DegC) (TH0X)
 [TH1A] type [sp7s] 73703738 len [ 2] idx [ 29]: SSD 1 OOB v3 absolute cooked temp A (DegC) (TH1A)
 [TH1B] type [sp7s] 73703738 len [ 2] idx [ 30]: SSD 1 OOB v3 absolute cooked temp B (DegC) (TH1B)
 [TH1C] type [sp7s] 73703738 len [ 2] idx [ 31]: SSD 1 OOB v3 absolute cooked temp C (DegC) (TH1C)
 [TH1X] type [sp7s] 73703738 len [ 2] idx [ 32]: SSD 1 OOB v3 cooked   temp Max (DegC) (TH1X)
 [TC0D] type [sp7s] 73703738 len [ 2] idx [ 33]: CPU die temp (DegC) (TC0D)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 34]: CPU proximity temp (filtered) (DegC) (TC0P)
 [TP0P] type [sp7s] 73703738 len [ 2] idx [ 35]: PCH proximity temp (DegC) (TP0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 36]: PCH digital die temp (DegC) (TPCD)
 [TI0P] type [sp7s] 73703738 len [ 2] idx [ 37]: High Speed I/O proximity 0 temp (DegC) (TI0P)
 [TI1P] type [sp7s] 73703738 len [ 2] idx [ 38]: High Speed I/O proximity 1 temp (DegC) (TI1P)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 39]: Ambient 0 temp (DegC) (TA0P)
 [TA1P] type [sp7s] 73703738 len [ 2] idx [ 40]: Ambient 1 temp (DegC) (TA1P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 41]: Airport Card temp (DegC) (TW0P)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J64...
 Set 0 has 49 keys:
 [VC0C] type [sp2s] 73703264 len [ 2] idx [  1]: CPU core lowside voltage (Volts) . (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [  2]: CPU core lowside current (Amps) (IC0C)
 [VM0C] type [sp2s] 73703264 len [ 2] idx [  3]: 1.2V to CPU/MEM lowside voltage (Volts) . (VM0C)
 [IM0C] type [sp3s] 73703363 len [ 2] idx [  4]: 1.2V to CPU/MEM lowside current (Amps) (IM0C)
 [VM1C] type [sp2s] 73703264 len [ 2] idx [  5]: 1.8V S3 lowside voltage (Volts) . (VM1C)
 [IM1C] type [sp1s] 73703165 len [ 2] idx [  6]: 1.8V S3 lowside current (Amps) (IM1C)
 [VC1C] type [sp2s] 73703264 len [ 2] idx [  7]: 1.05V to CPU/PCH lowside voltage (Volts) . (VC1C)
 [IC1C] type [sp3s] 73703363 len [ 2] idx [  8]: 1.05V to CPU/PCH lowside current (Amps) (IC1C)
 [V50R] type [sp3s] 73703363 len [ 2] idx [  9]: 5V lowside voltage (Volts) (V50R)
 [I50R] type [sp5s] 73703561 len [ 2] idx [ 10]: 5V lowside current (Amps) (I50R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 11]: DCIN voltage (Volts) . (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 12]: DCIN highside current (Amps) (ID0R)
 [IC0R] type [sp3s] 73703363 len [ 2] idx [ 13]: CPU highside current (Amps) (IC0R)
 [IM0R] type [sp2s] 73703264 len [ 2] idx [ 14]: MEM highside current (Amps) (IM0R)
 [II0R] type [sp3s] 73703363 len [ 2] idx [ 15]: TBT IO highside current (Amps) (II0R)
 [VP0T] type [sp2s] 73703264 len [ 2] idx [ 16]: PSU cooked temperature represented as a voltage (Volts) (VP0T)
 [IAPC] type [sp2s] 73703264 len [ 2] idx [ 17]: WLAN lowside current (Amps) (IAPC)
 [IH0R] type [sp2s] 73703264 len [ 2] idx [ 18]: HDD1 lowside current (Amps) (IH0R)
 [IH1R] type [sp3s] 73703363 len [ 2] idx [ 19]: SSD lowside current (Amps) (IH1R)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU core lowside power (IC0C * VC0C) (Watts) (PC0C)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [ 21]: 1.2V to CPU/MEM lowside power (IM0C * VM0C) (Watts) (PM0C)
 [PM1C] type [sp7s] 73703738 len [ 2] idx [ 22]: 1.8V S3 lowside power (IM1C * VM1C) (Watts) (PM1C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 23]: 1.05V to CPU/PCH lowside power (IC1C * VC1C) (Watts) (PC1C)
 [P50R] type [sp7s] 73703738 len [ 2] idx [ 24]: 5V lowside power (I50R * V50R) (Watts) (P50R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [ 25]: DCIN highside power (ID0R * VD0R) (Watts) (PD0R)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [ 26]: CPU highside power (IC0R * VD0R) (Watts) (PC0R)
 [PM0R] type [sp7s] 73703738 len [ 2] idx [ 27]: MEM highside power (IM0R * VD0R) (Watts) (PM0R)
 [PI0R] type [sp7s] 73703738 len [ 2] idx [ 28]: TBT IO highside power (II0R * VD0R) (Watts) (PI0R)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 29]: WLAN lowside power (IAPC * 3.3V) (Watts) (PAPC)
 [PH0R] type [sp7s] 73703738 len [ 2] idx [ 30]: HDD1 lowside power (IH0R * V50R) (Watts) (PH0R)
 [PH1R] type [sp7s] 73703738 len [ 2] idx [ 31]: SSD lowside power (IH1R * 3.3V) (Watts) (PH1R)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [ 32]: Thermal Control Power (Watts) (PHPC)
 [PD0E] type [sp7s] 73703738 len [ 2] idx [ 33]: Power supply filtered power (Watts) (PD0E)
 [PD0D] type [sp7s] 73703738 len [ 2] idx [ 34]: Power Supply Power Trend (Watts) (PD0D)
 [PD0K] type [sp7s] 73703738 len [ 2] idx [ 35]: Power supply filter coefficient (Watts) (PD0K)
 [PD0J] type [sp7s] 73703738 len [ 2] idx [ 36]: Power supply max error filtered output (Watts) (PD0J)
 [PD0F] type [sp7s] 73703738 len [ 2] idx [ 37]: Power supply power filtered then adjusted (Watts) (PD0F)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [fltf] 666C7420 len [ 4] idx [226]: Zone 2 Filtered Power (PZ2F)
 [PZ2E] type [fltf] 666C7420 len [ 4] idx [227]: Zone 2 Target Power (PZ2E)
 [PZ2T] type [fltf] 666C7420 len [ 4] idx [228]: Zone 2 Abstract Throttle (PZ2T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 66 keys:
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [  1]: EMC1428 internal diode raw temp (DegC) (Tm0p)
 [Te0t] type [sp7s] 73703738 len [ 2] idx [  2]: TBT Thermal Diode raw temp (DegC) (Te0t)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU proximity raw temp (DegC) (TC0p)
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  4]: Ambient 1 raw temp (DegC) (TA0p)
 [TW0p] type [sp7s] 73703738 len [ 2] idx [  5]: Wifi proximity raw temp (DegC) (TW0p)
 [TA1p] type [sp7s] 73703738 len [ 2] idx [  6]: Ambient 2 raw temp (DegC) (TA1p)
 [TM0p] type [sp7s] 73703738 len [ 2] idx [  7]: LPDDR proximity raw temp (DegC) (TM0p)
 [TA2p] type [sp7s] 73703738 len [ 2] idx [  8]: Ambient 3 raw temp (DegC) (TA2p)
 [TPCd] type [sp7s] 73703738 len [ 2] idx [  9]: PCH digital die raw temp (DegC) (TPCd)
 [TCGc] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU Gfx Core absolute raw temp (PECI) (DegC) (TCGc)
 [TCSc] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU System Agent Core absolute raw temp (PECI) (DegC) (TCSc)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [TC0c] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Core 0 absolute raw temp (PECI) (DegC) (TC0c)
 [TC1c] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU Core 1 absolute raw temp (PECI) (DegC) (TC1c)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [ 16]: Drive 0 OOBv1 raw bit-mapped temp (TH0o)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [ 17]: Drive 0 OOBv1 raw bit-mapped temp (TH1o)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 18]: Drive 0 OOBv3 raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 19]: Drive 0 OOBv3 raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 20]: Drive 0 OOBv3 raw temp C (DegC) (TH0c)
 [TH1a] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive 1 OOBv3 raw temp A (DegC) (TH1a)
 [TH1b] type [sp7s] 73703738 len [ 2] idx [ 22]: Drive 1 OOBv3 raw temp B (DegC) (TH1b)
 [TH1c] type [sp7s] 73703738 len [ 2] idx [ 23]: Drive 1 OOBv3 raw temp C (DegC) (TH1c)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [ 24]: EMC1428 internal diode temp (DegC) (Tm0P)
 [Te0T] type [sp7s] 73703738 len [ 2] idx [ 25]: TBT Thermal Diode temp (DegC) (Te0T)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 26]: CPU proximity temp (filtered) (DegC) (TC0P)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 27]: Ambient 1 temp (DegC) (TA0P)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [ 28]: Wifi proximity temp (DegC) (TW0P)
 [TA1P] type [sp7s] 73703738 len [ 2] idx [ 29]: Ambient 2 temp (DegC) (TA1P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 30]: LPDDR proximity temp (filtered) (DegC) (TM0P)
 [TA2P] type [sp7s] 73703738 len [ 2] idx [ 31]: Ambient 3 temp (DegC) (TA2P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 32]: PCH digital die temp (DegC) (TPCD)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 33]: CPU Gfx Core absolute cooked temp (PECI) (DegC) (TCGC)
 [TCSC] type [sp7s] 73703738 len [ 2] idx [ 34]: CPU System Agent Core absolute cooked temp (PECI) (DegC) (TCSC)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [ 35]: CPU Max Package Core absolute cooked temp (PECI) (DegC) (TCXC)
 [PCPT] type [sp7s] 73703738 len [ 2] idx [ 36]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [ 37]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [ 38]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [ 39]: CPU Core 0 absolute cooked temp (PECI) (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 40]: CPU Core 1 absolute cooked temp (PECI) (DegC) (TC1C)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 41]: CPU PECI die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 42]: CPU PECI die temp Trend (DegC) (TCTD)
 [TCFC] type [ui1u] 75693136 len [ 2] idx [ 43]: CPU PECI die temp filter coeff (TCFC)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 44]: CPU PECI die temp max error filtered output (DegC) (TC0J)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 45]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [ 46]: Synthetic bottom skin (DegC) (TS0V)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 47]: Synthetic DIMM Estimate(DegC) (TM0V)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 48]: Drive 0 OOBv1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 49]: Drive 1 OOBv1 mapped temp (DegC) (TH1O)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 50]: Drive 0 OOBv3 absolute cooked temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 51]: Drive 0 OOBv3 absolute cooked temp B (DegC) (TH0B)
 [TH0C] type [sp7s] 73703738 len [ 2] idx [ 52]: Drive 0 OOBv3 absolute cooked temp C (DegC) (TH0C)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 53]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH1A] type [sp7s] 73703738 len [ 2] idx [ 54]: Drive 1 OOBv3 absolute cooked temp A (DegC) (TH1A)
 [TH1B] type [sp7s] 73703738 len [ 2] idx [ 55]: Drive 1 OOBv3 absolute cooked temp B (DegC) (TH1B)
 [TH1C] type [sp7s] 73703738 len [ 2] idx [ 56]: Drive 1 OOBv3 absolute cooked temp C (DegC) (TH1C)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 57]: Drive 1 OOBv3 relative cooked temp Max (DegC) (TH1R)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 58]: Drive 0 OOBv1 filtered temp (DegC) (TH0P)
 [PH0F] type [sp7s] 73703738 len [ 2] idx [ 59]: Drive 0 filtered total load-side power (PH02 + PH05) * 2 (Watts) (PH0F)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 60]: Drive 1 OOBv1 filtered temp (DegC) (TH1P)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 61]: Drive 1 filtered load-side power * 3 (Watts) (PH1F)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 62]: Drive 0 OOBv3 relative filtered temp Max (DegC) (TH0F)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [ 63]: Drive 1 OOBv3 relative filtered temp Max (DegC) (TH1F)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 64]: Ambient virtual temp (DegC) (TA0V)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for D1...
 Set 0 has 42 keys:
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Core Power (Watts) (PC0C)
 [PDTR] type [sp7s] 73703738 len [ 2] idx [  2]: DC-In total power  (Watts) (PDTR)
 [PPBR] type [sp7s] 73703738 len [ 2] idx [  3]: PBus on battery power (Watts) (PPBR)
 [PSDC] type [sp7s] 73703738 len [ 2] idx [  4]: SSD Power  (Watts) (PSDC)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Computing High Side Power (Watts) (PC0R)
 [PO0R] type [sp7s] 73703738 len [ 2] idx [  6]: Other High Side Power   (Watts) (PO0R)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [  7]: DDR Power (Memory) (Watts) (PM0C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [  8]: CPU VCCIO 1.05V S0 Power (Watts) (PC1C)
 [PN0C] type [sp7s] 73703738 len [ 2] idx [  9]: AXG core Power (Watts) (PN0C)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU VCCSA Power (Watts) (PC2C)
 [PLDC] type [sp8s] 73703837 len [ 2] idx [ 11]: LCD Driver Power (Watts) (PLDC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 12]: Backlight power (Watts) (PBLC)
 [PAPC] type [sp7s] 73703738 len [ 2] idx [ 13]: Airport power (Watts) (PAPC)
 [PHSP] type [sp7s] 73703738 len [ 2] idx [ 14]: Thunderbolt Power (Watts) (PHSP)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [ 15]: Thermal control Power (Watts) (PHPC)
 [VC0C] type [sp5s] 73703561 len [ 2] idx [ 16]: CPU Core voltage. (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU Core current. (Amps) (IC0C)
 [VD0R] type [sp6s] 73703639 len [ 2] idx [ 18]: DC In voltage. (Volts) (VD0R)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [ 19]: DC In rail current. (Amps) (ID0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 20]: PBus rail voltage. (Volts) (VP0R)
 [ISDC] type [sp5s] 73703561 len [ 2] idx [ 21]: SSD Gumstick 2 current. (Amps) (ISDC)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 22]: PBus on battery current. (Amps) (IPBR)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [ 23]: CPU Computing High Side current. (Amps) (IC0R)
 [IO0R] type [sp5s] 73703561 len [ 2] idx [ 24]: Other High Side current.  (Amps) (IO0R)
 [IM0C] type [sp5s] 73703561 len [ 2] idx [ 25]: DDR 1.3V (Memory) current. (Amps) (IM0C)
 [IC1C] type [sp5s] 73703561 len [ 2] idx [ 26]: VCCIO  current. (Amps) (IC1C)
 [VN0C] type [sp5s] 73703561 len [ 2] idx [ 27]: Int GPU core voltage. (Volts) (VN0C)
 [VC2C] type [sp2s] 73703264 len [ 2] idx [ 28]: CPU VCCSA Voltage. (Volts) (VC2C)
 [IC2C] type [sp4s] 73703462 len [ 2] idx [ 29]: VCCSA  current. (Amps) (IC2C)
 [ILDC] type [sp2s] 73703264 len [ 2] idx [ 30]: LCD Panel Current  (Amps) (ILDC)
 [VBLC] type [sp7s] 73703738 len [ 2] idx [ 31]: Backlight. (Volts) (VBLC)
 [IBLC] type [sp2s] 73703264 len [ 2] idx [ 32]: Backlight current. (Amps) (IBLC)
 [IN0C] type [sp7s] 73703738 len [ 2] idx [ 33]: Internal GFX Core current. (Amps) (IN0C)
 [IAPC] type [sp2s] 73703264 len [ 2] idx [ 34]: Airport current.  (Amps) (IAPC)
 [IHSP] type [sp3s] 73703363 len [ 2] idx [ 35]: Thunderbolt Current  (Amps) (IHSP)
 [PHPC] type [sp8s] 73703837 len [ 2] idx [220]: HP Power (PHPC)
 [PTHC] type [sp8s] 73703837 len [ 2] idx [221]: HP Power Target (PTHC)
 [MSLT] type [ui1u] 75693136 len [ 2] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 31 keys:
 [PCPT] type [sp8s] 73703837 len [ 2] idx [  1]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp8s] 73703837 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp8s] 73703837 len [ 2] idx [  3]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Core PECI temp (DegC) (SIS! force bit 7) (TCXC)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  5]: Palm Rest Temp (DegC) (Ts0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  6]: Right Fin stack temp (DegC) (Th1H)
 [Th2H] type [sp7s] 73703738 len [ 2] idx [  7]: Left Fin stack temp (DegC) (Th2H)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  8]: CPU proximity temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  9]: Dimm Proximity temp(DegC) () (TM0P)
 [TA1P] type [sp7s] 73703738 len [ 2] idx [ 10]: DCIN Airflow temp (DegC) (TA1P)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TC3C] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Core 2 temp (PECI) (DegC) (TC3C)
 [TC4C] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Core 3 temp (PECI) (DegC) (TC4C)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 17]: Synthetic bottom skin (DegC) (Ts0S)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 18]: CPU die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 19]: CPU PECI die temp Trend (SIS! force bit 5) (DegC) (TCTD)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 21]: PCH Die temp (DegC) (TPCD)
 [TM0S] type [sp7s] 73703738 len [ 2] idx [ 22]: Synthetic DIMM Estimate(DegC) () (TM0S)
 [TMBS] type [sp7s] 73703738 len [ 2] idx [ 23]: DIMM Bandwidth Estimate (DegC) (TMBS)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [F1Ac] type [fpef] 66706532 len [ 2] idx [221]: Fan1 Actual RPM(F1Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [ui1u] 75693136 len [ 2] idx [243]: Battery Actual current. (mA) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (mV) (B0AV)
Dumping keys for J44...
 Set 0 has 48 keys:
 [PPBR] type [sp7s] 73703738 len [ 2] idx [  1]: PBus (BMON) Batt Dischg Power (Watts) (PPBR)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Computing High Side Power (Watts) (PC0R)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [  9]: DDR Power CPU & MEM (Watts) (PM0C)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [ 21]: Battery current BMON. (Amps) (IPBR)
 [PP0R] type [sp7s] 73703738 len [ 2] idx [  2]: Batt Dischg Power Discrete (Watts) (PP0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [  3]: DC-In total power  (Watts) (PD0R)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Core (Watts) (PC0C)
 [PC2C] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Core IMON Power (Watts) (PC2C)
 [PO5R] type [sp7s] 73703738 len [ 2] idx [  7]: Other 5V High Side Power   (Watts) (PO5R)
 [PO3R] type [sp7s] 73703738 len [ 2] idx [  8]: Other 3.3V High Side Power   (Watts) (PO3R)
 [PCMC] type [sp7s] 73703738 len [ 2] idx [ 10]: S2 Camera Power (Watts) (PCMC)
 [PSDC] type [sp7s] 73703738 len [ 2] idx [ 11]: SSD Fixed 3.3V Power (Watts) (PSDC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 12]: Backlight Input Power   (Watts) (PBLC)
 [PLDC] type [sp7s] 73703738 len [ 2] idx [ 13]: LCD Panel Power (Watts) (PLDC)
 [PR3C] type [sp7s] 73703738 len [ 2] idx [ 14]: 3.3V in S0 Power(Watts) (PR3C)
 [PR5C] type [sp7s] 73703738 len [ 2] idx [ 15]: 5VV in S0 Power(Watts) (PR5C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 16]: DDR Power CPU (Watts) (PC1C)
 [PM1C] type [sp7s] 73703738 len [ 2] idx [ 17]: DDR Power CPU (Watts) (PM1C)
 [PHSC] type [sp7s] 73703738 len [ 2] idx [ 18]: Thunderbolt Power (Watts) (PHSC)
 [IC0R] type [sp4s] 73703462 len [ 2] idx [ 19]: CPU Computing High Side current. (Amps) (IC0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [ 20]: PBus rail Voltage. (Volts) (VP0R)
 [ID0R] type [sp4s] 73703462 len [ 2] idx [ 22]: DC In current AMON. (Amps) (ID0R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [ 23]: DC In Voltage. (Volts) (VD0R)
 [IP0R] type [sp4s] 73703462 len [ 2] idx [ 24]: Battery Current Discrete. (Amps) (IP0R)
 [IC0C] type [sp6s] 73703639 len [ 2] idx [ 25]: CPU Core Current. (Amps) (IC0C)
 [IO5R] type [sp4s] 73703462 len [ 2] idx [ 26]: Battery current BMON. (Amps) (IO5R)
 [IO3R] type [sp3s] 73703363 len [ 2] idx [ 27]: Current other 3.3V High. (Amps) (IO3R)
 [IM0C] type [sp4s] 73703462 len [ 2] idx [ 28]: CPU and MEM current. (Amps) (IM0C)
 [IBLC] type [sp1s] 73703165 len [ 2] idx [ 29]: Backlight Current (Amps) (IBLC)
 [ITPC] type [sp3s] 73703363 len [ 2] idx [ 30]: Trackpad Actuator Current (Amps) (ITPC)
 [ISDC] type [sp3s] 73703363 len [ 2] idx [ 31]: SSD Current (Amps) (ISDC)
 [IR3C] type [sp3s] 73703363 len [ 2] idx [ 32]: 3.3V S0 current. (Amps) (IR3C)
 [ICMC] type [sp1s] 73703165 len [ 2] idx [ 33]: Camera S2 Current (Amps) (ICMC)
 [VTPC] type [sp5s] 73703561 len [ 2] idx [ 34]: T101 Boost/PBus Accuator Voltage. (Volts) (VTPC)
 [IR5C] type [sp3s] 73703363 len [ 2] idx [ 35]: 5.0V S0 current. (Amps) (IR5C)
 [IM1C] type [sp2s] 73703264 len [ 2] idx [ 36]: CPU DDR current. (Amps) (IM1C)
 [IC1C] type [sp3s] 73703363 len [ 2] idx [ 37]: 1.05V PCH Core. (Amps) (IC1C)
 [VC0C] type [sp3s] 73703363 len [ 2] idx [ 38]: CPU Core Voltage. (Volts) (VC0C)
 [ILDC] type [sp1s] 73703165 len [ 2] idx [ 39]: LCD panel Current. (Amps) (ILDC)
 [IC2C] type [sp6s] 73703639 len [ 2] idx [ 40]: 1.05V CPU Core IMON. (Amps) (IC2C)
 [IHSC] type [sp2s] 73703264 len [ 2] idx [ 41]: Thunderbolt Current. (Amps) (IHSC)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PTHC] type [fltf] 666C7420 len [ 4] idx [221]: HP Power Target (PTHC)
 [MSLT] type [fltf] 666C7420 len [ 4] idx [222]: HP Power Throttle (MSLT)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 33 keys:
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 26]: Synthetic bottom skin (DegC) (Ts0S)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (V) (B0AV)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  1]: CPU proximity temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  2]: Dimm Proximity temp(DegC) (TM0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Proximity temp (DegC) (Th1H)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [  4]: Airflow temp (DegC) (TA0P)
 [TMLB] type [sp7s] 73703738 len [ 2] idx [  5]: Dimm Proximity temp(DegC) (TMLB)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  6]: Palm Rest Temp (DegC) (Ts0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [  7]: Thunderbolt Die temp (DegC) (THSP)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [  8]: Airport Temp (DegC) (TW0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [  9]: PCH Die temp (DegC) (TPCD)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU PECI die temp  (DegC) (TCXC)
 [PCPT] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 18]: Drive0 (SSD Gumstick) OOB v3 raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 19]: Drive0 (SSD Gumstick) OOB v3 raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 20]: Drive0 (SSD Gumstick) OOB v3 raw temp C (DegC) (TH0c)
 [TH0x] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive0 (SSD Gumstick) OOB v3 raw temp Max (DegC) (TH0x)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU die Virtual temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 23]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 24]: SSD Temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 25]: SSD Temp B  (DegC) (TH0B)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [si1s] 73693136 len [ 2] idx [243]: Battery Actual current. (A) (B0AC)
Dumping keys for J52...
 Set 0 has 53 keys:
 [IC0R] type [sp4s] 73703462 len [ 2] idx [  1]: CPU Computing High Side current. (Amps) (IC0R)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [  2]: PBus rail Voltage. (Volts) (VP0R)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [  3]: Battery current BMON. (Amps) (IPBR)
 [ID0R] type [sp4s] 73703462 len [ 2] idx [  4]: DC In current AMON. (Amps) (ID0R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [  5]: DC In Voltage. (Volts) (VD0R)
 [IP0R] type [sp4s] 73703462 len [ 2] idx [  6]: Battery Current Discrete. (Amps) (IP0R)
 [IC0C] type [sp6s] 73703639 len [ 2] idx [  7]: CPU Core Current. (Amps) (IC0C)
 [IO5R] type [sp3s] 73703363 len [ 2] idx [  8]: Battery current BMON. (Amps) (IO5R)
 [IO3R] type [sp3s] 73703363 len [ 2] idx [  9]: Current other 3.3V High. (Amps) (IO3R)
 [IM0C] type [sp4s] 73703462 len [ 2] idx [ 10]: CPU and MEM 1.2V DDR current. (Amps) (IM0C)
 [IBLC] type [sp1s] 73703165 len [ 2] idx [ 11]: Backlight Current (Amps) (IBLC)
 [ITPC] type [sp2s] 73703264 len [ 2] idx [ 12]: Trackpad Actuator Current (Amps) (ITPC)
 [IM2C] type [sp1s] 73703165 len [ 2] idx [ 13]: LPDDR current 1.8V. (Amps) (IM2C)
 [ISDC] type [sp2s] 73703264 len [ 2] idx [ 14]: SSD Current (Amps) (ISDC)
 [IR3C] type [sp2s] 73703264 len [ 2] idx [ 15]: 3.3V S0 current. (Amps) (IR3C)
 [ICMC] type [sp1s] 73703165 len [ 2] idx [ 16]: Camera S2 Current (Amps) (ICMC)
 [VTPC] type [sp5s] 73703561 len [ 2] idx [ 17]: T101 Accuator Voltage. (Volts) (VTPC)
 [IR5C] type [sp2s] 73703264 len [ 2] idx [ 18]: 5.0V S0 current. (Amps) (IR5C)
 [IM1C] type [sp1s] 73703165 len [ 2] idx [ 19]: LPDDR current 1.2V. (Amps) (IM1C)
 [IC1C] type [sp2s] 73703264 len [ 2] idx [ 20]: 1.05V PCH Core. (Amps) (IC1C)
 [VC0C] type [sp3s] 73703363 len [ 2] idx [ 21]: CPU Core Voltage. (Volts) (VC0C)
 [ILDC] type [sp1s] 73703165 len [ 2] idx [ 22]: LCD panel Current. (Amps) (ILDC)
 [IC2C] type [sp6s] 73703639 len [ 2] idx [ 23]: 1.05V CPU Core IMON. (Amps) (IC2C)
 [IHSC] type [sp2s] 73703264 len [ 2] idx [ 24]: Thunderbolt Current. (Amps) (IHSC)
 [PPBR] type [sp7s] 73703738 len [ 2] idx [ 25]: PBus (BMON) Batt Dischg Power (Watts) (PPBR)
 [PP0R] type [sp7s] 73703738 len [ 2] idx [ 26]: Batt Dischg Power Discrete (Watts) (PP0R)
 [PD0R] type [sp7s] 73703738 len [ 2] idx [ 27]: DC-In total power  (Watts) (PD0R)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [ 28]: CPU Computing High Side Power (Watts) (PC0R)
 [PC0C] type [sp7s] 73703738 len [ 2] idx [ 29]: CPU Core (Watts) (PC0C)
 [PO5R] type [sp7s] 73703738 len [ 2] idx [ 30]: Other 5V High Side Power   (Watts) (PO5R)
 [PO3R] type [sp7s] 73703738 len [ 2] idx [ 31]: Other 3.3V High Side Power   (Watts) (PO3R)
 [PM0C] type [sp7s] 73703738 len [ 2] idx [ 32]: DDR Power 1.2V CPU & MEM (Watts) (PM0C)
 [PM2C] type [sp7s] 73703738 len [ 2] idx [ 33]: DDR Power 1.8V CPU (Watts) (PM2C)
 [PCMC] type [sp7s] 73703738 len [ 2] idx [ 34]: S2 Camera Power (Watts) (PCMC)
 [PSDC] type [sp7s] 73703738 len [ 2] idx [ 35]: SSD Fixed 3.3V Power (Watts) (PSDC)
 [PBLC] type [sp7s] 73703738 len [ 2] idx [ 36]: Backlight Input Power   (Watts) (PBLC)
 [PLDC] type [sp7s] 73703738 len [ 2] idx [ 37]: LCD Panel Power (Watts) (PLDC)
 [PR3C] type [sp7s] 73703738 len [ 2] idx [ 38]: 3.3V in S0 Power(Watts) (PR3C)
 [PR5C] type [sp7s] 73703738 len [ 2] idx [ 39]: 5VV in S0 Power(Watts) (PR5C)
 [PC1C] type [sp7s] 73703738 len [ 2] idx [ 40]: 1.05V PCH Power (Watts) (PC1C)
 [PM1C] type [sp7s] 73703738 len [ 2] idx [ 41]: DDR Power 1.2V CPU (Watts) (PM1C)
 [PHSC] type [sp7s] 73703738 len [ 2] idx [ 42]: Thunderbolt Power (Watts) (PHSC)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [ 43]: HP Power (Watts) (PHPC)
 [    ] type [ui8u] 75693820 len [ 1] idx [200]: DCIN Spike Mitigation 
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 42 keys:
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  1]: CPU proximity temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  2]: Dimm Proximity temp(DegC) (TM0P)
 [Th1H] type [sp7s] 73703738 len [ 2] idx [  3]: Fin Stack Proximity temp (DegC) (Th1H)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [  4]: Airflow temp (DegC) (TA0P)
 [TMLB] type [sp7s] 73703738 len [ 2] idx [  5]: MLB Proximity temp(DegC) (TMLB)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  6]: Palm Rest Temp (DegC) (Ts0P)
 [THSP] type [sp7s] 73703738 len [ 2] idx [  7]: Thunderbolt Die temp (DegC) (THSP)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [  8]: Airport Temp (DegC) (TW0P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [  9]: PCH Die Temp Digital (DegC) (TPCD)
 [TC0C] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU Core 0 temp (PECI) (DegC) (TC0C)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Core 1 temp (PECI) (DegC) (TC1C)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU PECI die temp  (DegC) (TCXC)
 [PCPT] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Package Total Power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Package Core Power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU Package Gfx Power (PECI) (Watts) (PCPG)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 18]: Drive 0 OOBv3 raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 19]: Drive 0 OOBv3 raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 20]: Drive 0 OOBv3 raw temp C (DegC) (TH0c)
 [TH0x] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive 0 OOBv3 temp Max  (DegC) (TH0x)
 [TB0T] type [sp7s] 73703738 len [ 2] idx [ 22]: Battery temp (SBS! force bit 0) (DegC) (TB0T)
 [IBAC] type [sp7s] 73703738 len [ 2] idx [ 23]: Battery Current (Amps) (IBAC)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU die Virtual temp (DegC) (TC0E)
 [TCTD] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU PECI die temp Trend (DegC) (TCTD)
 [TCFC] type [ui1u] 75693136 len [ 2] idx [ 26]: CPU PECI die temp filter coeff (TCFC)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 27]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 28]: Drive 0 OOBv3 cooked temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 29]: Drive 0 OOBv3 cooked temp B (DegC) (TH0B)
 [TH0C] type [sp7s] 73703738 len [ 2] idx [ 30]: Drive 0 OOBv3 cooked temp C (DegC) (TH0C)
 [TH0V] type [sp7s] 73703738 len [ 2] idx [ 31]: Drive 0 backup virtual DRAM temp (DegC) (TH0V)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 32]: Drive 0 OOBv3 relative filtered temp Max (DegC) (TH0F)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 33]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 34]: Synthetic bottom skin (DegC) (Ts0S)
 [Ts1S] type [sp7s] 73703738 len [ 2] idx [ 35]: Synthetic top skin (DegC) (Ts1S)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [si1s] 73693136 len [ 2] idx [243]: Battery Actual current. (A) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (V) (B0AV)
Dumping keys for J90...
 Set 0 has 58 keys:
 [IC0C] type [sp8s] 73703837 len [ 2] idx [  1]: CPU Core low side current (Amps) (IC0C)
 [IC0S] type [sp5s] 73703561 len [ 2] idx [  2]: CPU VSA low side current (Amps) (IC0S)
 [ICTR] type [sp5s] 73703561 len [ 2] idx [  3]: CPU Riser 12V high side current (Amps) (ICTR)
 [IG0C] type [sp8s] 73703837 len [ 2] idx [  4]: GPU A Core low side current (Amps) (IG0C)
 [IG0R] type [sp5s] 73703561 len [ 2] idx [  5]: GFX A Riser 12V high side current (Amps) (IG0R)
 [IG0S] type [sp5s] 73703561 len [ 2] idx [  6]: GPU A VDDCI low side current (Amps) (IG0S)
 [IG1C] type [sp8s] 73703837 len [ 2] idx [  7]: GPU B Core low side current (Amps) (IG1C)
 [IG1R] type [sp5s] 73703561 len [ 2] idx [  8]: GFX B Riser 12V high side current (Amps) (IG1R)
 [IG1S] type [sp5s] 73703561 len [ 2] idx [  9]: GPU B VDDCI low side current (Amps) (IG1S)
 [IH0R] type [sp2s] 73703264 len [ 2] idx [ 10]: SSD 3V3 low side current (Amps) (IH0R)
 [II0R] type [sp5s] 73703561 len [ 2] idx [ 11]: I/O Board 12V high side current (Amps) (II0R)
 [IMTR] type [sp3s] 73703363 len [ 2] idx [ 12]: Memory 1V5 high side current (Amps) (IMTR)
 [PC0C] type [spas] 73706135 len [ 2] idx [ 13]: CPU Core low side power (Watts) (PC0C)
 [PC0S] type [spas] 73706135 len [ 2] idx [ 14]: CPU VSA low side power (Watts) (PC0S)
 [PCTR] type [spas] 73706135 len [ 2] idx [ 15]: CPU Riser total power (Watts) (PCTR)
 [PD2R] type [spas] 73706135 len [ 2] idx [ 16]: Power Supply 12V power (Watts) (PD2R)
 [PG0C] type [spas] 73706135 len [ 2] idx [ 17]: GPU A Core low side power (Watts) (PG0C)
 [PG0R] type [spas] 73706135 len [ 2] idx [ 18]: GFX A total power (Watts) (PG0R)
 [PG0S] type [spas] 73706135 len [ 2] idx [ 19]: GPU A VDDCI low side power (Watts) (PG0S)
 [PG1C] type [spas] 73706135 len [ 2] idx [ 20]: GPU B Core low side power (Watts) (PG1C)
 [PG1R] type [spas] 73706135 len [ 2] idx [ 21]: GFX B total power (Watts) (PG1R)
 [PG1S] type [spas] 73706135 len [ 2] idx [ 22]: GPU B VDDCI low side power (Watts) (PG1S)
 [PGTR] type [spas] 73706135 len [ 2] idx [ 23]: GPU total high-side power (PG0R + PG1R) (Watts) (PGTR)
 [PH0R] type [spas] 73706135 len [ 2] idx [ 24]: SSD 3V3 low side power (Watts) (PH0R)
 [PI0R] type [spas] 73706135 len [ 2] idx [ 25]: I/O Board total power (Watts) (PI0R)
 [PMTR] type [spas] 73706135 len [ 2] idx [ 26]: Memory total power (Watts) (PMTR)
 [PZ0G] type [spas] 73706135 len [ 2] idx [ 27]: Zone 0 average power (Watts) (PZ0G)
 [VC0C] type [sp1s] 73703165 len [ 2] idx [ 28]: CPU Core low side voltage (Volts) (VC0C)
 [VC0S] type [sp1s] 73703165 len [ 2] idx [ 29]: CPU VSA low side voltage (Volts) (VC0S)
 [VD2R] type [sp4s] 73703462 len [ 2] idx [ 30]: Power Supply 12V voltage (Volts) (VD2R)
 [VG0C] type [sp1s] 73703165 len [ 2] idx [ 31]: GPU A Core low side voltage (Volts) (VG0C)
 [VG0S] type [sp1s] 73703165 len [ 2] idx [ 32]: GPU A VDDCI low side voltage (Volts) (VG0S)
 [VG1C] type [sp1s] 73703165 len [ 2] idx [ 33]: GPU B Core low side voltage (Volts) (VG1C)
 [VG1S] type [sp1s] 73703165 len [ 2] idx [ 34]: GPU B VDDCI low side voltage (Volts) (VG1S)
 [VH0R] type [sp2s] 73703264 len [ 2] idx [ 35]: SSD 3V3 low side voltage (Volts) (VH0R)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [ui1u] 75693136 len [ 2] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [ui1u] 75693136 len [ 2] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [fltf] 666C7420 len [ 4] idx [226]: Zone 2 Filtered Power (PZ2F)
 [PZ2E] type [fltf] 666C7420 len [ 4] idx [227]: Zone 2 Target Power (PZ2E)
 [PZ2T] type [ui1u] 75693136 len [ 2] idx [228]: Zone 2 Abstract Throttle (PZ2T)
 [PZ3F] type [fltf] 666C7420 len [ 4] idx [229]: Zone 3 Filtered Power (PZ3F)
 [PZ3E] type [fltf] 666C7420 len [ 4] idx [230]: Zone 3 Target Power (PZ3E)
 [PZ3T] type [ui1u] 75693136 len [ 2] idx [231]: Zone 3 Abstract Throttle (PZ3T)
 [PZ4F] type [fltf] 666C7420 len [ 4] idx [232]: Zone 4 Filtered Power (PZ4F)
 [PZ4E] type [fltf] 666C7420 len [ 4] idx [233]: Zone 4 Target Power (PZ4E)
 [PZ4T] type [ui1u] 75693136 len [ 2] idx [234]: Zone 4 Abstract Throttle (PZ4T)
 [PZ5F] type [fltf] 666C7420 len [ 4] idx [235]: Zone 5 Filtered Power (PZ5F)
 [PZ5E] type [fltf] 666C7420 len [ 4] idx [236]: Zone 5 Target Power (PZ5E)
 [PZ5T] type [ui1u] 75693136 len [ 2] idx [237]: Zone 5 Abstract Throttle (PZ5T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 46 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [PCPC] type [spas] 73706135 len [ 2] idx [  2]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPT] type [spas] 73706135 len [ 2] idx [  3]: CPU package total power (PECI) (Watts) (PCPT)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [  4]: Ambient cooked temp 0 (DegC) (TA0P)
 [TA1P] type [sp7s] 73703738 len [ 2] idx [  5]: Ambient cooked temp 1 (DegC) (TA1P)
 [TA2P] type [sp7s] 73703738 len [ 2] idx [  6]: Ambient cooked temp 2 (DegC) (TA2P)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [  7]: CPU PECI Die filtered temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [  8]: CPU PECI Die filtered and adjusted temp for fan/power control (DegC) (TC0F)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [  9]: CPU PECI Die temp max error used in TC0F=TC0E+ (DegC) (TC0J)
 [TC0L] type [ui1u] 75693136 len [ 2] idx [ 10]: CPU PECI Die dynamic filter coeff (Seconds) (TC0L)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Proximity cooked temp (DegC) (TC0P)
 [TC0T] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU PECI Die temp Trend (DegC) (TC0T)
 [TC1P] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU VR Proximity cooked temp (DegC) (TC1P)
 [TCXR] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Max Package Core relative cooked temp (PECI) (DegC) (TCXR)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 15]: GPU A Die cooked temp (DegC) (TG0D)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 16]: GPU A Proximity cooked temp (DegC) (TG0P)
 [TG1D] type [sp7s] 73703738 len [ 2] idx [ 17]: GPU B Die cooked temp (DegC) (TG1D)
 [TG1P] type [sp7s] 73703738 len [ 2] idx [ 18]: GPU A VRAM Proximity cooked temp (DegC) (TG1P)
 [TG2P] type [sp7s] 73703738 len [ 2] idx [ 19]: GPU A VR Proximity cooked temp (DegC) (TG2P)
 [TG3P] type [sp7s] 73703738 len [ 2] idx [ 20]: GPU B Proximity cooked temp (DegC) (TG3P)
 [TG4P] type [sp7s] 73703738 len [ 2] idx [ 21]: GPU B VRAM Proximity cooked temp (DegC) (TG4P)
 [TG5P] type [sp7s] 73703738 len [ 2] idx [ 22]: GPU B VR Proximity cooked temp (DegC) (TG5P)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 23]: Drive OOBv3 absolute cooked temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 24]: Drive OOBv3 absolute cooked temp B (DegC) (TH0B)
 [TH0C] type [sp7s] 73703738 len [ 2] idx [ 25]: Drive OOBv3 absolute cooked temp C (DegC) (TH0C)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 26]: Drive OOBv3 relative filtered temp Max (DegC) (TH0F)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 27]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TI0P] type [sp7s] 73703738 len [ 2] idx [ 28]: I/O Board Proximity cooked temp (DegC) (TI0P)
 [TI0T] type [sp7s] 73703738 len [ 2] idx [ 29]: Thunderbolt Proximity cooked temp (DegC) (TI0T)
 [TI1P] type [sp7s] 73703738 len [ 2] idx [ 30]: 5V/3V3 VR Proximity cooked temp (DegC) (TI1P)
 [TM0D] type [sp7s] 73703738 len [ 2] idx [ 31]: DIMM 0 PECI cooked temp (DegC) (TM0D)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 32]: DIMM 0/1 Top Proximity cooked temp (DegC) (TM0P)
 [TM1D] type [sp7s] 73703738 len [ 2] idx [ 33]: DIMM 1 PECI cooked temp (DegC) (TM1D)
 [TM1P] type [sp7s] 73703738 len [ 2] idx [ 34]: DIMM 2/3 Top Proximity cooked temp (DegC) (TM1P)
 [TM2D] type [sp7s] 73703738 len [ 2] idx [ 35]: DIMM 2 PECI cooked temp (DegC) (TM2D)
 [TM2P] type [sp7s] 73703738 len [ 2] idx [ 36]: DIMM 0/1 VR Proximity cooked temp (DegC) (TM2P)
 [TM3D] type [sp7s] 73703738 len [ 2] idx [ 37]: DIMM 3 PECI cooked temp (DegC) (TM3D)
 [TM3P] type [sp7s] 73703738 len [ 2] idx [ 38]: DIMM 2/3 VR Proximity cooked temp (DegC) (TM3P)
 [TMXD] type [sp7s] 73703738 len [ 2] idx [ 39]: DIMM max cooked temp (DegC) (TMXD)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 40]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 41]: PCH Die cooked temp (DegC) (TPCD)
 [Te0T] type [sp7s] 73703738 len [ 2] idx [ 42]: PCIe Switch Diode cooked temp (DegC) (Te0T)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [ 43]: MLB Proximity 0 cooked temp (DegC) (Tm0P)
 [Tp0T] type [sp7s] 73703738 len [ 2] idx [ 44]: PSU Secondary H/S Diode cooked temp (DegC) (Tp0T)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [spas] 73706135 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J16...
 Set 0 has 35 keys:
 [IC0C] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Core load-side current (Amps) (IC0C)
 [IC0M] type [sp5s] 73703561 len [ 2] idx [  2]: CPU Mem  load-side current (Amps) (IC0M)
 [ID2R] type [sp6s] 73703639 len [ 2] idx [  3]: Power Supply 12V current (Amps) (ID2R)
 [IH05] type [sp2s] 73703264 len [ 2] idx [  4]: Drive 0 5V   load-side current (Amps) (IH05)
 [IH1R] type [sp3s] 73703363 len [ 2] idx [  5]: Drive 1 3.3V load-side current (Amps) (IH1R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [  6]: DIMM load-side current (Amps) (IM0R)
 [IW0R] type [sp3s] 73703363 len [ 2] idx [  7]: Wifi load-side current (Amps) (IW0R)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [  8]: CPU Core load-side power (Watts) (PC0C)
 [PC0M] type [sp9s] 73703936 len [ 2] idx [  9]: CPU Mem  load-side power (Watts) (PC0M)
 [PCPR] type [sp9s] 73703936 len [ 2] idx [ 10]: CPU package total power (SMC) (PCPR)
 [PCTR] type [sp9s] 73703936 len [ 2] idx [ 11]: CPU total equivalent input-side power (PCTR)
 [PD2R] type [sp9s] 73703936 len [ 2] idx [ 12]: Power Supply 12V power (Watts) (PD2R)
 [PH0R] type [sp9s] 73703936 len [ 2] idx [ 13]: Drive 0 total (5V) load-side power (Watts) (PH0R)
 [PH1R] type [sp9s] 73703936 len [ 2] idx [ 14]: Drive 1 load-side power (Watts) (PH1R)
 [PM0R] type [sp9s] 73703936 len [ 2] idx [ 15]: DIMM load-side power (Watts) (PM0R)
 [PW0R] type [sp9s] 73703936 len [ 2] idx [ 16]: Wifi load-side power (Watts) (PW0R)
 [PZ0G] type [sp9s] 73703936 len [ 2] idx [ 17]: Zone 0 average power (Watts) (PZ0G)
 [PZ4G] type [sp9s] 73703936 len [ 2] idx [ 18]: Zone 4 average power (Watts) (PZ4G)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 19]: CPU Core load-side voltage (Volts) (VC0C)
 [VC0M] type [sp2s] 73703264 len [ 2] idx [ 20]: CPU Mem  load-side voltage (Volts) (VC0M)
 [VD2R] type [sp4s] 73703462 len [ 2] idx [ 21]: Power Supply 12V voltage (Volts) (VD2R)
 [VH05] type [sp3s] 73703363 len [ 2] idx [ 22]: Drive 0 5V load-side voltage (Volts) (VH05)
 [VM0R] type [sp2s] 73703264 len [ 2] idx [ 23]: DIMM load-side voltage (Volts) (VM0R)
 [VR1R] type [sp2s] 73703264 len [ 2] idx [ 24]: PCH/GPU/TBT load-side voltage (Volts) (VR1R)
 [VR3R] type [sp3s] 73703363 len [ 2] idx [ 25]: 3.3V S5 load-side voltage (Volts) (VR3R)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ5F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 5 Filtered Power (PZ5F)
 [PZ5E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 5 Target Power (PZ5E)
 [PZ5T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 5 Abstract Throttle (PZ5T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 50 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [Tb0p] type [sp7s] 73703738 len [ 2] idx [  2]: Backlight Controller proximity raw temp (DegC) (Tb0p)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Proximity raw temp (DegC) (TC0p)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [  6]: Drive 0 OOBv3 absolute raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [  7]: Drive 0 OOBv3 absolute raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [  8]: Drive 0 OOBv3 absolute raw temp C (DegC) (TH0c)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [  9]: Drive 0 OOBv1 raw bit-mapped temp (TH0o)
 [TH1a] type [sp7s] 73703738 len [ 2] idx [ 10]: Drive 1 OOBv3 absolute raw temp A (DegC) (TH1a)
 [TH1b] type [sp7s] 73703738 len [ 2] idx [ 11]: Drive 1 OOBv3 absolute raw temp B (DegC) (TH1b)
 [TH1c] type [sp7s] 73703738 len [ 2] idx [ 12]: Drive 1 OOBv3 absolute raw temp C (DegC) (TH1c)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [ 13]: Drive 1 OOBv1 raw bit-mapped temp (TH1o)
 [TL0p] type [sp7s] 73703738 len [ 2] idx [ 14]: LCD unfiltered front-of-screen raw temp (DegC) (TL0p)
 [TL1p] type [sp7s] 73703738 len [ 2] idx [ 15]: LCD TCON Proximity raw temp (DegC) (TL1p)
 [TL2p] type [sp8s] 73703837 len [ 2] idx [ 16]: LCD IR target hotspot calculated temp (DegC) (TL2p)
 [TL3p] type [spas] 73706135 len [ 2] idx [ 17]: LCD IR temp sensor die raw temp (DegC) (TL3p)
 [TM0p] type [sp7s] 73703738 len [ 2] idx [ 18]: DIMM 0 Proximity raw temp (DegC) (TM0p)
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [ 19]: MLB Proximity 0 raw    temp (Tm0p)
 [Tm1p] type [sp7s] 73703738 len [ 2] idx [ 20]: MLB Proximity 1 raw    temp (Tm1p)
 [Tm2p] type [sp7s] 73703738 len [ 2] idx [ 21]: MLB Proximity 2 raw    temp (Tm2p)
 [Tp2h] type [sp7s] 73703738 len [ 2] idx [ 22]: Power Supply T2 Secondary Heatsink raw temp (DegC) (Tp2h)
 [VL3t] type [si1s] 73693136 len [ 2] idx [ 23]: LCD IR temp sensor voltage (Raw Register) (VL3t)
 [PCPC] type [sp9s] 73703936 len [ 2] idx [ 24]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp9s] 73703936 len [ 2] idx [ 25]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [PCPT] type [sp9s] 73703936 len [ 2] idx [ 26]: CPU package total power (PECI) (Watts) (PCPT)
 [PH0F] type [sp7s] 73703738 len [ 2] idx [ 27]: Drive 0 total (5V) filtered load-side power * 2 (Watts) (PH0F)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 28]: Drive 1 filtered load-side power * 3 (Watts) (PH1F)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 29]: Ambient cooked temp (DegC) (TA0P)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 30]: Ambient virtual temp (DegC) (TA0V)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 31]: CPU PECI Die filtered temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 32]: CPU PECI Die filtered and adjusted temp for fan/power control (DegC) (TC0F)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 33]: Drive 0 OOBv3 relative filtered temp Max (DegC) (TH0F)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 34]: Drive 0 OOBv1 mapped temp (DegC) (TH0O)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 35]: Drive 0 OOBv1 filtered temp (DegC) (TH0P)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 36]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [ 37]: Drive 1 OOBv3 relative filtered temp Max (DegC) (TH1F)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 38]: Drive 1 OOBv1 mapped temp (DegC) (TH1O)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 39]: Drive 1 OOBv1 filtered temp (DegC) (TH1P)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 40]: Drive 1 OOBv3 relative cooked temp Max (DegC) (TH1R)
 [TL1V] type [sp7s] 73703738 len [ 2] idx [ 41]: LCD TL1v-filtered center front-of-screen temp for color compensation (DegC) (TL1V)
 [TL1v] type [sp7s] 73703738 len [ 2] idx [ 42]: LCD filtered center front-of-screen temp that feeds TL1V (DegC) (TL1v)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 43]: DIMM virtual temp (DegC) (TM0V)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 44]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 45]: PCH Die cooked temp (DegC) (TPCD)
 [Tp2F] type [sp7s] 73703738 len [ 2] idx [ 46]: Power Supply T2 Secondary Heatsink filtered temp (DegC) (Tp2F)
 [Tp2H] type [sp7s] 73703738 len [ 2] idx [ 47]: Power Supply T2 Secondary Heatsink cooked temp (DegC) (Tp2H)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [ 48]: Skin 0 virtual temp (DegC) (TS0V)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp9s] 73703936 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J17...
 Set 0 has 65 keys:
 [IC0C] type [sp7s] 73703738 len [ 2] idx [  1]: CPU Core load-side current (Amps) (IC0C)
 [IC0M] type [sp5s] 73703561 len [ 2] idx [  2]: CPU Mem  load-side current (Amps) (IC0M)
 [ID2R] type [sp6s] 73703639 len [ 2] idx [  3]: Power Supply 12V current (Amps) (ID2R)
 [IG0C] type [sp8s] 73703837 len [ 2] idx [  4]: GPU Core  load-side current (Amps) (IG0C)
 [IG0F] type [sp3s] 73703363 len [ 2] idx [  5]: GPU FB   input-side current (Amps) (IG0F)
 [IG1C] type [sp4s] 73703462 len [ 2] idx [  6]: GPU Core input-side current (Amps) (IG1C)
 [IH05] type [sp2s] 73703264 len [ 2] idx [  7]: Drive 0 5V   load-side current (Amps) (IH05)
 [IH02] type [sp3s] 73703363 len [ 2] idx [  8]: Drive 0 12V load-side current (Amps) (IH02)
 [IH1R] type [sp3s] 73703363 len [ 2] idx [  9]: Drive 1 3.3V load-side current (Amps) (IH1R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [ 10]: DIMM load-side current (Amps) (IM0R)
 [IW0R] type [sp3s] 73703363 len [ 2] idx [ 11]: Wifi load-side current (Amps) (IW0R)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [ 12]: CPU Core load-side power (Watts) (PC0C)
 [PC0M] type [sp9s] 73703936 len [ 2] idx [ 13]: CPU Mem  load-side power (Watts) (PC0M)
 [PCPR] type [sp9s] 73703936 len [ 2] idx [ 14]: CPU package total power (SMC) (PCPR)
 [PCTR] type [sp9s] 73703936 len [ 2] idx [ 15]: CPU total equivalent input-side power (PCTR)
 [PD2R] type [sp9s] 73703936 len [ 2] idx [ 16]: Power Supply 12V power (Watts) (PD2R)
 [PG0C] type [sp9s] 73703936 len [ 2] idx [ 17]: GPU Core       load-side power (Watts) (PG0C)
 [PG0F] type [sp9s] 73703936 len [ 2] idx [ 18]: GPU Frame Buf input-side power (Watts) (PG0F)
 [PG1C] type [sp9s] 73703936 len [ 2] idx [ 19]: GPU Core      input-side power (Watts) (PG1C)
 [PGPR] type [sp9s] 73703936 len [ 2] idx [ 20]: GPU package total power (SMC) (PGPR)
 [PGTR] type [sp9s] 73703936 len [ 2] idx [ 21]: GPU total equivalent high-side power (PGTR)
 [PH05] type [sp9s] 73703936 len [ 2] idx [ 22]: Drive 0 5V load-side power (Watts) (PH05)
 [PH02] type [sp9s] 73703936 len [ 2] idx [ 23]: Drive 0 12V load-side power (Watts) (PH02)
 [PH0R] type [sp9s] 73703936 len [ 2] idx [ 24]: Drive 0 total load-side power (PH02 + PH05) (Watts) (PH0R)
 [PH1R] type [sp9s] 73703936 len [ 2] idx [ 25]: Drive 1 load-side power (Watts) (PH1R)
 [PM0R] type [sp9s] 73703936 len [ 2] idx [ 26]: DIMM load-side power (Watts) (PM0R)
 [PW0R] type [sp9s] 73703936 len [ 2] idx [ 27]: Wifi load-side power (Watts) (PW0R)
 [PZ0G] type [sp9s] 73703936 len [ 2] idx [ 28]: Zone 0 average power (Watts) (PZ0G)
 [PZ1G] type [sp9s] 73703936 len [ 2] idx [ 29]: Zone 1 average power (Watts) (PZ1G)
 [PZ2G] type [sp9s] 73703936 len [ 2] idx [ 30]: Zone 2 average power (Watts) (PZ2G)
 [PZ3G] type [sp9s] 73703936 len [ 2] idx [ 31]: Zone 3 average power (Watts) (PZ3G)
 [PZ4G] type [sp9s] 73703936 len [ 2] idx [ 32]: Zone 4 average power (Watts) (PZ4G)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 33]: CPU Core load-side voltage (Volts) (VC0C)
 [VC0M] type [sp2s] 73703264 len [ 2] idx [ 34]: CPU Mem  load-side voltage (Volts) (VC0M)
 [VD2R] type [sp4s] 73703462 len [ 2] idx [ 35]: Power Supply 12V voltage (Volts) (VD2R)
 [VG0C] type [sp2s] 73703264 len [ 2] idx [ 36]: GPU Core  load-side voltage (Volts) (VG0C)
 [VG0F] type [sp4s] 73703462 len [ 2] idx [ 37]: GPU Frame Buffer input-side voltage (Volts) (VG0F)
 [VG1C] type [sp4s] 73703462 len [ 2] idx [ 38]: GPU Core input-side voltage (Volts) (VG1C)
 [VH05] type [sp3s] 73703363 len [ 2] idx [ 39]: Drive 0 5V load-side voltage (Volts) (VH05)
 [VM0R] type [sp2s] 73703264 len [ 2] idx [ 40]: DIMM load-side voltage (Volts) (VM0R)
 [VR1R] type [sp2s] 73703264 len [ 2] idx [ 41]: PCH/GPU/TBT load-side voltage (Volts) (VR1R)
 [VR3R] type [sp3s] 73703363 len [ 2] idx [ 42]: 3.3V S5 load-side voltage (Volts) (VR3R)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [fltf] 666C7420 len [ 4] idx [226]: Zone 2 Filtered Power (PZ2F)
 [PZ2E] type [fltf] 666C7420 len [ 4] idx [227]: Zone 2 Target Power (PZ2E)
 [PZ2T] type [fltf] 666C7420 len [ 4] idx [228]: Zone 2 Abstract Throttle (PZ2T)
 [PZ3F] type [fltf] 666C7420 len [ 4] idx [229]: Zone 3 Filtered Power (PZ3F)
 [PZ3E] type [fltf] 666C7420 len [ 4] idx [230]: Zone 3 Target Power (PZ3E)
 [PZ3T] type [fltf] 666C7420 len [ 4] idx [231]: Zone 3 Abstract Throttle (PZ3T)
 [PZ4F] type [fltf] 666C7420 len [ 4] idx [232]: Zone 4 Filtered Power (PZ4F)
 [PZ4E] type [fltf] 666C7420 len [ 4] idx [233]: Zone 4 Target Power (PZ4E)
 [PZ4T] type [fltf] 666C7420 len [ 4] idx [234]: Zone 4 Abstract Throttle (PZ4T)
 [PZ5F] type [fltf] 666C7420 len [ 4] idx [235]: Zone 5 Filtered Power (PZ5F)
 [PZ5E] type [fltf] 666C7420 len [ 4] idx [236]: Zone 5 Target Power (PZ5E)
 [PZ5T] type [fltf] 666C7420 len [ 4] idx [237]: Zone 5 Abstract Throttle (PZ5T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTm] type [ui8u] 75693820 len [ 1] idx [242]: MEM Plimit (MSTm)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 58 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [Tb0p] type [sp7s] 73703738 len [ 2] idx [  2]: Backlight Controller proximity raw temp (DegC) (Tb0p)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Proximity raw temp (DegC) (TC0p)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [  4]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [  5]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [TG0p] type [sp7s] 73703738 len [ 2] idx [  6]: GPU 0 Proximity raw temp (DegC) (TG0p)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [  7]: Drive 0 OOBv3 absolute raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [  8]: Drive 0 OOBv3 absolute raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [  9]: Drive 0 OOBv3 absolute raw temp C (DegC) (TH0c)
 [TH0e] type [sp7s] 73703738 len [ 2] idx [ 10]: Drive 0 temp sensor existence used for TM0V (0) = present (TH0e)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [ 11]: Drive 0 OOBv1 raw bit-mapped temp (TH0o)
 [TH1a] type [sp7s] 73703738 len [ 2] idx [ 12]: Drive 1 OOBv3 absolute raw temp A (DegC) (TH1a)
 [TH1b] type [sp7s] 73703738 len [ 2] idx [ 13]: Drive 1 OOBv3 absolute raw temp B (DegC) (TH1b)
 [TH1c] type [sp7s] 73703738 len [ 2] idx [ 14]: Drive 1 OOBv3 absolute raw temp C (DegC) (TH1c)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [ 15]: Drive 1 OOBv1 raw bit-mapped temp (TH1o)
 [TL0p] type [sp7s] 73703738 len [ 2] idx [ 16]: LCD unfiltered front-of-screen raw temp (DegC) (TL0p)
 [TL1p] type [sp7s] 73703738 len [ 2] idx [ 17]: LCD TCON Proximity raw temp (DegC) (TL1p)
 [TL2p] type [sp8s] 73703837 len [ 2] idx [ 18]: LCD IR target hotspot calculated temp (DegC) (TL2p)
 [TL3p] type [spas] 73706135 len [ 2] idx [ 19]: LCD IR temp sensor die raw temp (DegC) (TL3p)
 [TM0p] type [sp7s] 73703738 len [ 2] idx [ 20]: DIMM 0 Proximity raw temp (DegC) (TM0p)
 [TM1p] type [sp7s] 73703738 len [ 2] idx [ 21]: DIMM 1 Proximity raw temp (DegC) (TM1p)
 [TM2p] type [sp7s] 73703738 len [ 2] idx [ 22]: DIMM 2 Proximity raw temp (DegC) (TM2p)
 [TM3p] type [sp7s] 73703738 len [ 2] idx [ 23]: DIMM 3 Proximity raw temp (DegC) (TM3p)
 [TS0p] type [sp7s] 73703738 len [ 2] idx [ 24]: Skin 0 raw temp (DegC) (TS0p)
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [ 25]: MLB Proximity 0 raw temp (DegC) (Tm0p)
 [Tm1p] type [sp7s] 73703738 len [ 2] idx [ 26]: MLB Proximity 1 raw temp (DegC) (Tm1p)
 [Tp2h] type [sp7s] 73703738 len [ 2] idx [ 27]: Power Supply T2 Secondary Heatsink raw temp (DegC) (Tp2h)
 [VL3t] type [si1s] 73693136 len [ 2] idx [ 28]: LCD IR temp sensor voltage (Raw Register) (VL3t)
 [PCPC] type [sp9s] 73703936 len [ 2] idx [ 29]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp9s] 73703936 len [ 2] idx [ 30]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [PCPT] type [sp9s] 73703936 len [ 2] idx [ 31]: CPU package total power (PECI) (Watts) (PCPT)
 [PH0F] type [sp7s] 73703738 len [ 2] idx [ 32]: Drive 0 filtered total load-side power (PH02 + PH05) * 2 (Watts) (PH0F)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 33]: Drive 1 filtered load-side power * 3 (Watts) (PH1F)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 34]: Ambient cooked temp (DegC) (TA0P)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 35]: Ambient virtual temp (DegC) (TA0V)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 36]: CPU PECI Die filtered temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 37]: CPU PECI Die filtered and adjusted temp for fan/power control (DegC) (TC0F)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 38]: GPU 0 Die cooked temp (DegC) (TG0D)
 [TG0E] type [sp7s] 73703738 len [ 2] idx [ 39]: GPU 0 Die filtered temp (DegC) (TG0E)
 [TG0F] type [sp7s] 73703738 len [ 2] idx [ 40]: GPU 0 Die filtered and adjusted temp for fan/power control (DegC) (TG0F)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 41]: Drive 0 OOBv3 relative filtered temp Max (DegC) (TH0F)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 42]: Drive 0 OOBv1 mapped temp (DegC) (TH0O)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 43]: Drive 0 OOBv1 filtered temp (DegC) (TH0P)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 44]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [ 45]: Drive 1 OOBv3 relative filtered temp Max (DegC) (TH1F)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 46]: Drive 1 OOBv1 filtered temp (DegC) (TH1P)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 47]: Drive 1 OOBv3 relative cooked temp Max (DegC) (TH1R)
 [TL0V] type [sp7s] 73703738 len [ 2] idx [ 48]: LCD filtered front-of-screen hotspot virtual temp (DegC) (TL0V)
 [TL1V] type [sp7s] 73703738 len [ 2] idx [ 49]: LCD TL1v-filtered center front-of-screen temp for color compensation (DegC) (TL1V)
 [TL1v] type [sp7s] 73703738 len [ 2] idx [ 50]: LCD filtered center front-of-screen temp that feeds TL1V (DegC) (TL1v)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 51]: DIMM virtual temp (DegC) (TM0V)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 52]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 53]: PCH Die cooked temp (DegC) (TPCD)
 [Tp2F] type [sp7s] 73703738 len [ 2] idx [ 54]: Power Supply T2 Secondary Heatsink filtered temp (DegC) (Tp2F)
 [Tp2H] type [sp7s] 73703738 len [ 2] idx [ 55]: Power Supply T2 Secondary Heatsink cooked temp (DegC) (Tp2H)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [ 56]: Skin 0 virtual temp (DegC) (TS0V)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp9s] 73703936 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J16G...
 Set 0 has 67 keys:
 [VD2R] type [sp4s] 73703462 len [ 2] idx [  1]: Power Supply 12V voltage (Volts) (VD2R)
 [ID2R] type [sp6s] 73703639 len [ 2] idx [  2]: Power Supply 12V current (Amps) (ID2R)
 [VG1C] type [sp4s] 73703462 len [ 2] idx [  3]: GPU Core input-side voltage (Volts) (VG1C)
 [IG1C] type [sp4s] 73703462 len [ 2] idx [  4]: GPU Core input-side current (Amps) (IG1C)
 [VC0M] type [sp2s] 73703264 len [ 2] idx [  5]: CPU Mem  load-side voltage (Volts) (VC0M)
 [IC0M] type [sp5s] 73703561 len [ 2] idx [  6]: CPU Mem  load-side current (Amps) (IC0M)
 [VM0R] type [sp2s] 73703264 len [ 2] idx [  7]: DIMM load-side voltage (Volts) (VM0R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [  8]: DIMM load-side current (Amps) (IM0R)
 [VG0F] type [sp4s] 73703462 len [ 2] idx [  9]: GPU Frame Buffer input-side voltage (Volts) (VG0F)
 [IG0F] type [sp3s] 73703363 len [ 2] idx [ 10]: GPU FB   input-side current (Amps) (IG0F)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 11]: CPU Core load-side voltage (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core load-side current (Amps) (IC0C)
 [VG0C] type [sp2s] 73703264 len [ 2] idx [ 13]: GPU Core  load-side voltage (Volts) (VG0C)
 [IG0C] type [sp8s] 73703837 len [ 2] idx [ 14]: GPU Core  load-side current (Amps) (IG0C)
 [VH05] type [sp3s] 73703363 len [ 2] idx [ 15]: Drive 0 5V load-side voltage (Volts) (VH05)
 [IH05] type [sp2s] 73703264 len [ 2] idx [ 16]: Drive 0 5V   load-side current (Amps) (IH05)
 [VR1R] type [sp2s] 73703264 len [ 2] idx [ 17]: PCH/GPU/TBT load-side voltage (Volts) (VR1R)
 [IH1R] type [sp3s] 73703363 len [ 2] idx [ 18]: Drive 1 3.3V load-side current (Amps) (IH1R)
 [VR3R] type [sp3s] 73703363 len [ 2] idx [ 19]: 3.3V S5 load-side voltage (Volts) (VR3R)
 [PD2R] type [sp9s] 73703936 len [ 2] idx [ 20]: Power Supply 12V power (Watts) (PD2R)
 [PG1C] type [sp9s] 73703936 len [ 2] idx [ 21]: GPU Core      input-side power (Watts) (PG1C)
 [PC0M] type [sp9s] 73703936 len [ 2] idx [ 22]: CPU Mem  load-side power (Watts) (PC0M)
 [PM0R] type [sp9s] 73703936 len [ 2] idx [ 23]: DIMM load-side power (Watts) (PM0R)
 [PG0F] type [sp9s] 73703936 len [ 2] idx [ 24]: GPU Frame Buf input-side power (Watts) (PG0F)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [ 25]: CPU Core load-side power (Watts) (PC0C)
 [PG0C] type [sp9s] 73703936 len [ 2] idx [ 26]: GPU Core       load-side power (Watts) (PG0C)
 [PH05] type [sp9s] 73703936 len [ 2] idx [ 27]: Drive 0 5V load-side power (Watts) (PH05)
 [PH1R] type [sp9s] 73703936 len [ 2] idx [ 28]: Drive 1 load-side power (Watts) (PH1R)
 [PH0R] type [sp9s] 73703936 len [ 2] idx [ 29]: Drive 0 total (5V) load-side power (Watts) (PH0R)
 [PGPR] type [sp9s] 73703936 len [ 2] idx [ 30]: GPU package total power (SMC) (PGPR)
 [PGTR] type [sp9s] 73703936 len [ 2] idx [ 31]: GPU total equivalent high-side power (PGTR)
 [PCPR] type [sp9s] 73703936 len [ 2] idx [ 32]: CPU package total power (SMC) (PCPR)
 [PCTR] type [sp9s] 73703936 len [ 2] idx [ 33]: CPU total equivalent input-side power (PCTR)
 [PZ0G] type [sp9s] 73703936 len [ 2] idx [ 34]: Zone 0 average power (Watts) (PZ0G)
 [PZ1G] type [sp9s] 73703936 len [ 2] idx [ 35]: Zone 1 average power (Watts) (PZ1G)
 [PZ2G] type [sp9s] 73703936 len [ 2] idx [ 36]: Zone 2 average power (Watts) (PZ2G)
 [PZ3G] type [sp9s] 73703936 len [ 2] idx [ 37]: Zone 3 average power (Watts) (PZ3G)
 [PZ4G] type [sp9s] 73703936 len [ 2] idx [ 38]: Zone 4 average power (Watts) (PZ4G)
 [PZ5G] type [sp9s] 73703936 len [ 2] idx [ 39]: Zone 5 average power (Watts) (PZ5G)
 [ID2E] type [sp7s] 73703738 len [ 2] idx [ 40]: Power Supply 12V current filtered (Amps) (ID2E)
 [ID2F] type [sp7s] 73703738 len [ 2] idx [ 41]: Power Supply 12V current filtered and adjusted (ID2F)
 [ID2I] type [sp7s] 73703738 len [ 2] idx [ 42]: Power Supply 12V current filter input S7.8 (Amps) (ID2I)
 [ID2J] type [sp7s] 73703738 len [ 2] idx [ 43]: Power Supply 12V current max error (Amps) (ID2J)
 [ID2L] type [ui1u] 75693136 len [ 2] idx [ 44]: Power Supply 12V current dynamic filter coeff (Seconds) (ID2L)
 [ID2T] type [sp7s] 73703738 len [ 2] idx [ 45]: Power Supply 12V current trend (Amps) (ID2T)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [fltf] 666C7420 len [ 4] idx [226]: Zone 2 Filtered Power (PZ2F)
 [PZ2E] type [fltf] 666C7420 len [ 4] idx [227]: Zone 2 Target Power (PZ2E)
 [PZ2T] type [fltf] 666C7420 len [ 4] idx [228]: Zone 2 Abstract Throttle (PZ2T)
 [PZ3F] type [fltf] 666C7420 len [ 4] idx [229]: Zone 3 Filtered Power (PZ3F)
 [PZ3E] type [fltf] 666C7420 len [ 4] idx [230]: Zone 3 Target Power (PZ3E)
 [PZ3T] type [fltf] 666C7420 len [ 4] idx [231]: Zone 3 Abstract Throttle (PZ3T)
 [PZ4F] type [fltf] 666C7420 len [ 4] idx [232]: Zone 4 Filtered Power (PZ4F)
 [PZ4E] type [fltf] 666C7420 len [ 4] idx [233]: Zone 4 Target Power (PZ4E)
 [PZ4T] type [fltf] 666C7420 len [ 4] idx [234]: Zone 4 Abstract Throttle (PZ4T)
 [PZ5F] type [fltf] 666C7420 len [ 4] idx [235]: Zone 5 Filtered Power (PZ5F)
 [PZ5E] type [fltf] 666C7420 len [ 4] idx [236]: Zone 5 Target Power (PZ5E)
 [PZ5T] type [fltf] 666C7420 len [ 4] idx [237]: Zone 5 Abstract Throttle (PZ5T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 84 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [Tb0p] type [sp7s] 73703738 len [ 2] idx [  2]: Backlight Controller proximity raw temp (DegC) (Tb0p)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Proximity raw temp (DegC) (TC0p)
 [TM0p] type [sp7s] 73703738 len [ 2] idx [  4]: DIMM 0 Proximity raw temp (DegC) (TM0p)
 [TG0d] type [sp7s] 73703738 len [ 2] idx [  5]: GPU 0 Die raw temp (DegC) (TG0d)
 [TG0p] type [sp7s] 73703738 len [ 2] idx [  6]: GPU 0 Proximity raw temp (DegC) (TG0p)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [  7]: Drive 0 OOBv1 raw bit-mapped temp (TH0o)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [  8]: Drive 1 OOBv1 raw bit-mapped temp (TH1o)
 [TL0p] type [sp7s] 73703738 len [ 2] idx [  9]: LCD unfiltered front-of-screen raw temp (DegC) (TL0p)
 [TL1p] type [sp7s] 73703738 len [ 2] idx [ 10]: LCD TCON Proximity raw temp (DegC) (TL1p)
 [TL2p] type [sp8s] 73703837 len [ 2] idx [ 11]: LCD IR target hotspot calculated temp (DegC) (TL2p)
 [TL3p] type [spas] 73706135 len [ 2] idx [ 12]: LCD IR temp sensor die raw temp (DegC) (TL3p)
 [VL3t] type [si1s] 73693136 len [ 2] idx [ 13]: LCD IR temp sensor voltage (Raw Register) (VL3t)
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [ 14]: MLB Proximity 0 raw    temp: MLB bottom near memory (DegC) (Tm0p)
 [Tm1p] type [sp7s] 73703738 len [ 2] idx [ 15]: MLB Proximity 1 raw    temp: MLB top near GPU (DegC) (Tm1p)
 [Tm2p] type [sp7s] 73703738 len [ 2] idx [ 16]: MLB Proximity 2 raw    temp: MLB bottom near memory VR (DegC) (Tm2p)
 [TC0c] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU Core 0 absolute raw temp (PECI) (DegC) (TC0c)
 [TC1c] type [sp7s] 73703738 len [ 2] idx [ 18]: CPU Core 1 absolute raw temp (PECI) (DegC) (TC1c)
 [TC2c] type [sp7s] 73703738 len [ 2] idx [ 19]: CPU Core 2 absolute raw temp (PECI) (DegC) (TC2c)
 [TC3c] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU Core 3 absolute raw temp (PECI) (DegC) (TC3c)
 [TCGc] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU Gfx absolute raw temp (PECI) (DegC) (TCGc)
 [TCSc] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU System Agent Core absolute raw temp (PECI) (DegC) (TCSc)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [ 23]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [Tp2h] type [sp7s] 73703738 len [ 2] idx [ 25]: Power Supply T2 Secondary Heatsink raw temp (DegC) (Tp2h)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 26]: Drive 0 OOBv3 absolute raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 27]: Drive 0 OOBv3 absolute raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 28]: Drive 0 OOBv3 absolute raw temp C (DegC) (TH0c)
 [TH1a] type [sp7s] 73703738 len [ 2] idx [ 29]: Drive 1 OOBv3 absolute raw temp A (DegC) (TH1a)
 [TH1b] type [sp7s] 73703738 len [ 2] idx [ 30]: Drive 1 OOBv3 absolute raw temp B (DegC) (TH1b)
 [TH1c] type [sp7s] 73703738 len [ 2] idx [ 31]: Drive 1 OOBv3 absolute raw temp C (DegC) (TH1c)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 32]: Ambient cooked temp (DegC) (TA0P)
 [Tb0P] type [sp7s] 73703738 len [ 2] idx [ 33]: Backlight Controller proximity cooked temp (DegC) (Tb0P)
 [TC0L] type [ui1u] 75693136 len [ 2] idx [ 34]: CPU PECI Die dynamic filter coeff (Seconds) (TC0L)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 35]: CPU Proximity cooked temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 36]: DIMM 0 Proximity cooked temp (DegC) (TM0P)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 37]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 38]: Drive 0 OOBv1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 39]: Drive 1 OOBv1 mapped temp (DegC) (TH1O)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 40]: GPU 0 Die cooked temp (DegC) (TG0D)
 [TG0L] type [ui1u] 75693136 len [ 2] idx [ 41]: GPU 0 Die dynamic filter coeff (Seconds) (TG0L)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 42]: GPU 0 Proximity cooked temp (DegC) (TG0P)
 [TL0P] type [sp7s] 73703738 len [ 2] idx [ 43]: LCD unfiltered front-of-screen cooked temp (DegC) (TL0P)
 [TL1P] type [sp7s] 73703738 len [ 2] idx [ 44]: LCD TCON Proximity cooked temp (DegC) (TL1P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [ 45]: MLB Proximity 0 cooked temp: MLB bottom near memory (DegC) (Tm0P)
 [Tm1P] type [sp7s] 73703738 len [ 2] idx [ 46]: MLB Proximity 1 cooked temp: MLB top near GPU (DegC) (Tm1P)
 [Tm2P] type [sp7s] 73703738 len [ 2] idx [ 47]: MLB Proximity 2 cooked temp: MLB bottom near memory VR (DegC) (Tm2P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 48]: PCH Die cooked temp (DegC) (TPCD)
 [TCXR] type [sp7s] 73703738 len [ 2] idx [ 49]: CPU Max Package Core relative cooked temp (PECI) (DegC) (TCXR)
 [PCPC] type [sp9s] 73703936 len [ 2] idx [ 50]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp9s] 73703936 len [ 2] idx [ 51]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [PCPT] type [sp9s] 73703936 len [ 2] idx [ 52]: CPU package total power (PECI) (Watts) (PCPT)
 [Tp2H] type [sp7s] 73703738 len [ 2] idx [ 53]: Power Supply T2 Secondary Heatsink cooked temp (DegC) (Tp2H)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 54]: Drive 0 OOBv3 absolute cooked temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 55]: Drive 0 OOBv3 absolute cooked temp B (DegC) (TH0B)
 [TH0C] type [sp7s] 73703738 len [ 2] idx [ 56]: Drive 0 OOBv3 absolute cooked temp C (DegC) (TH0C)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 57]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH1A] type [sp7s] 73703738 len [ 2] idx [ 58]: Drive 1 OOBv3 absolute cooked temp A (DegC) (TH1A)
 [TH1B] type [sp7s] 73703738 len [ 2] idx [ 59]: Drive 1 OOBv3 absolute cooked temp B (DegC) (TH1B)
 [TH1C] type [sp7s] 73703738 len [ 2] idx [ 60]: Drive 1 OOBv3 absolute cooked temp C (DegC) (TH1C)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 61]: Drive 1 OOBv3 relative cooked temp Max (DegC) (TH1R)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 62]: Ambient virtual temp (DegC) (TA0V)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 63]: DIMM virtual temp (DegC) (TM0V)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 64]: Drive 0 OOBv1 filtered temp (DegC) (TH0P)
 [PH0F] type [sp7s] 73703738 len [ 2] idx [ 65]: Drive 0 total (5V) filtered load-side power * 2 (Watts) (PH0F)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 66]: Drive 1 OOBv1 filtered temp (DegC) (TH1P)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 67]: Drive 1 filtered load-side power * 3 (Watts) (PH1F)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 68]: CPU PECI Die filtered temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 69]: CPU PECI Die filtered and adjusted temp for fan/power control (DegC) (TC0F)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 70]: CPU PECI Die temp max error used in TC0F=TC0E+ (DegC) (TC0J)
 [TC0T] type [sp7s] 73703738 len [ 2] idx [ 71]: CPU PECI Die temp Trend (DegC) (TC0T)
 [TG0E] type [sp7s] 73703738 len [ 2] idx [ 72]: GPU 0 Die filtered temp (DegC) (TG0E)
 [TG0F] type [sp7s] 73703738 len [ 2] idx [ 73]: GPU 0 Die filtered and adjusted temp for fan/power control (DegC) (TG0F)
 [TG0J] type [sp7s] 73703738 len [ 2] idx [ 74]: GPU 0 Die temp max error used in TG0F=TG0E+ (DegC) (TG0J)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [ 75]: GPU 0 Die temp Trend (DegC) (TG0T)
 [TL1v] type [sp7s] 73703738 len [ 2] idx [ 76]: LCD filtered center front-of-screen temp that feeds TL1V (DegC) (TL1v)
 [TL1V] type [sp7s] 73703738 len [ 2] idx [ 77]: LCD TL1v-filtered center front-of-screen temp for color compensation (DegC) (TL1V)
 [Tp2F] type [sp7s] 73703738 len [ 2] idx [ 78]: Power Supply T2 Secondary Heatsink filtered temp (DegC) (Tp2F)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [ 79]: Skin 0 virtual temp (DegC) (TS0V)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 80]: Drive 0 OOBv3 relative filtered temp Max (DegC) (TH0F)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [ 81]: Drive 1 OOBv3 relative filtered temp Max (DegC) (TH1F)
 [PM0f] type [sp2s] 73703264 len [ 2] idx [ 82]: DIMM load-side power / SQR(Fan RPM) (PM0f)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp9s] 73703936 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J70...
 Set 0 has 38 keys:
 [VD2R] type [sp4s] 73703462 len [ 2] idx [  1]: Power Supply 12V voltage (Volts) (VD2R)
 [ID2R] type [sp6s] 73703639 len [ 2] idx [  2]: Power Supply 12V current (Amps) (ID2R)
 [VM0R] type [sp2s] 73703264 len [ 2] idx [  3]: DIMM load-side voltage (Volts) (VM0R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [  4]: DIMM load-side current (Amps) (IM0R)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [  5]: CPU Core load-side voltage (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [  6]: CPU Core load-side current (Amps) (IC0C)
 [VR3R] type [sp3s] 73703363 len [ 2] idx [  7]: 3.3V load-side voltage (Volts) (VR3R)
 [IH1R] type [sp3s] 73703363 len [ 2] idx [  8]: Drive 1 3.3V load-side current (Amps) (IH1R)
 [PD2R] type [sp9s] 73703936 len [ 2] idx [  9]: Power Supply 12V power (Watts) (PD2R)
 [PM0R] type [sp9s] 73703936 len [ 2] idx [ 10]: DIMM load-side power (Watts) (PM0R)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [ 11]: CPU Core load-side power (Watts) (PC0C)
 [PH1R] type [sp9s] 73703936 len [ 2] idx [ 12]: Drive 1 load-side power (Watts) (PH1R)
 [PCPR] type [sp9s] 73703936 len [ 2] idx [ 13]: CPU package total power (SMC) (PCPR)
 [PCTR] type [sp9s] 73703936 len [ 2] idx [ 14]: CPU total equivalent input-side power (PCTR)
 [PZ0G] type [sp9s] 73703936 len [ 2] idx [ 15]: Zone 0 average power (Watts) (PZ0G)
 [PZ5G] type [sp9s] 73703936 len [ 2] idx [ 16]: Zone 5 average power (Watts) (PZ5G)
 [ID2I] type [sp7s] 73703738 len [ 2] idx [ 17]: Power Supply 12V current filter input S7.8 (Amps) (ID2I)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [fltf] 666C7420 len [ 4] idx [226]: Zone 2 Filtered Power (PZ2F)
 [PZ2E] type [fltf] 666C7420 len [ 4] idx [227]: Zone 2 Target Power (PZ2E)
 [PZ2T] type [fltf] 666C7420 len [ 4] idx [228]: Zone 2 Abstract Throttle (PZ2T)
 [PZ3F] type [fltf] 666C7420 len [ 4] idx [229]: Zone 3 Filtered Power (PZ3F)
 [PZ3E] type [fltf] 666C7420 len [ 4] idx [230]: Zone 3 Target Power (PZ3E)
 [PZ3T] type [fltf] 666C7420 len [ 4] idx [231]: Zone 3 Abstract Throttle (PZ3T)
 [PZ4F] type [fltf] 666C7420 len [ 4] idx [232]: Zone 4 Filtered Power (PZ4F)
 [PZ4E] type [fltf] 666C7420 len [ 4] idx [233]: Zone 4 Target Power (PZ4E)
 [PZ4T] type [fltf] 666C7420 len [ 4] idx [234]: Zone 4 Abstract Throttle (PZ4T)
 [PZ5F] type [fltf] 666C7420 len [ 4] idx [235]: Zone 5 Filtered Power (PZ5F)
 [PZ5E] type [fltf] 666C7420 len [ 4] idx [236]: Zone 5 Target Power (PZ5E)
 [PZ5T] type [fltf] 666C7420 len [ 4] idx [237]: Zone 5 Abstract Throttle (PZ5T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 67 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [Tb0p] type [sp7s] 73703738 len [ 2] idx [  2]: Backlight Controller proximity raw temp (DegC) (Tb0p)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Proximity raw temp (DegC) (TC0p)
 [TM0p] type [sp7s] 73703738 len [ 2] idx [  4]: DIMM 0 Proximity raw temp (DegC) (TM0p)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [  5]: Drive 0 OOBv1 raw bit-mapped temp (TH0o)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [  6]: Drive 1 OOBv1 raw bit-mapped temp (TH1o)
 [TL0p] type [sp7s] 73703738 len [ 2] idx [  7]: LCD unfiltered front-of-screen raw temp (DegC) (TL0p)
 [TL1p] type [sp7s] 73703738 len [ 2] idx [  8]: LCD TCON Proximity raw temp (DegC) (TL1p)
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [  9]: MLB Proximity 0 raw    temp: MLB top near CPU (DegC) (Tm0p)
 [Tm2p] type [sp7s] 73703738 len [ 2] idx [ 10]: MLB Proximity 2 raw    temp: MLB bottom near CPU VR (DegC) (Tm2p)
 [TC0c] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU Core 0 absolute raw temp (PECI) (DegC) (TC0c)
 [TC1c] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core 1 absolute raw temp (PECI) (DegC) (TC1c)
 [TC2c] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU Core 2 absolute raw temp (PECI) (DegC) (TC2c)
 [TC3c] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Core 3 absolute raw temp (PECI) (DegC) (TC3c)
 [TCGc] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU Gfx absolute raw temp (PECI) (DegC) (TCGc)
 [TCSc] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU System Agent Core absolute raw temp (PECI) (DegC) (TCSc)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [ 18]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [Tp2h] type [sp7s] 73703738 len [ 2] idx [ 19]: Power Supply T2 Secondary Heatsink raw temp (DegC) (Tp2h)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 20]: Drive 0 OOBv3 absolute raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 21]: Drive 0 OOBv3 absolute raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 22]: Drive 0 OOBv3 absolute raw temp C (DegC) (TH0c)
 [TH1a] type [sp7s] 73703738 len [ 2] idx [ 23]: Drive 1 OOBv3 absolute raw temp A (DegC) (TH1a)
 [TH1b] type [sp7s] 73703738 len [ 2] idx [ 24]: Drive 1 OOBv3 absolute raw temp B (DegC) (TH1b)
 [TH1c] type [sp7s] 73703738 len [ 2] idx [ 25]: Drive 1 OOBv3 absolute raw temp C (DegC) (TH1c)
 [TI0p] type [sp7s] 73703738 len [ 2] idx [ 26]: TBT Proximity raw temp (DegC) (TI0p)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 27]: Ambient cooked temp (DegC) (TA0P)
 [TC0L] type [ui1u] 75693136 len [ 2] idx [ 28]: CPU PECI Die dynamic filter coeff (Seconds) (TC0L)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 29]: CPU Proximity cooked temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 30]: DIMM 0 Proximity cooked temp (DegC) (TM0P)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 31]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 32]: Drive 0 OOBv1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 33]: Drive 1 OOBv1 mapped temp (DegC) (TH1O)
 [TL0P] type [sp7s] 73703738 len [ 2] idx [ 34]: LCD unfiltered front-of-screen cooked temp (DegC) (TL0P)
 [TL1P] type [sp7s] 73703738 len [ 2] idx [ 35]: LCD TCON Proximity cooked temp (DegC) (TL1P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 36]: PCH Die cooked temp (DegC) (TPCD)
 [TCXR] type [sp7s] 73703738 len [ 2] idx [ 37]: CPU Max Package Core relative cooked temp (PECI) (DegC) (TCXR)
 [PCPC] type [sp9s] 73703936 len [ 2] idx [ 38]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp9s] 73703936 len [ 2] idx [ 39]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [PCPT] type [sp9s] 73703936 len [ 2] idx [ 40]: CPU package total power (PECI) (Watts) (PCPT)
 [Tp2H] type [sp7s] 73703738 len [ 2] idx [ 41]: Power Supply T2 Secondary Heatsink cooked temp (DegC) (Tp2H)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 42]: Drive 0 OOBv3 absolute cooked temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 43]: Drive 0 OOBv3 absolute cooked temp B (DegC) (TH0B)
 [TH0C] type [sp7s] 73703738 len [ 2] idx [ 44]: Drive 0 OOBv3 absolute cooked temp C (DegC) (TH0C)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 45]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH1A] type [sp7s] 73703738 len [ 2] idx [ 46]: Drive 1 OOBv3 absolute cooked temp A (DegC) (TH1A)
 [TH1B] type [sp7s] 73703738 len [ 2] idx [ 47]: Drive 1 OOBv3 absolute cooked temp B (DegC) (TH1B)
 [TH1C] type [sp7s] 73703738 len [ 2] idx [ 48]: Drive 1 OOBv3 absolute cooked temp C (DegC) (TH1C)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 49]: Drive 1 OOBv3 relative cooked temp Max (DegC) (TH1R)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 50]: Ambient virtual temp (DegC) (TA0V)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 51]: DIMM virtual temp (DegC) (TM0V)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 52]: Drive 0 OOBv1 filtered temp (DegC) (TH0P)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 53]: Drive 1 OOBv1 filtered temp (DegC) (TH1P)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 54]: Drive 1 filtered load-side power * 3 (Watts) (PH1F)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 55]: CPU PECI Die filtered temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 56]: CPU PECI Die filtered and adjusted temp for fan/power control (DegC) (TC0F)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 57]: CPU PECI Die temp max error used in TC0F=TC0E+ (DegC) (TC0J)
 [TC0T] type [sp7s] 73703738 len [ 2] idx [ 58]: CPU PECI Die temp Trend (DegC) (TC0T)
 [TL1v] type [sp7s] 73703738 len [ 2] idx [ 59]: LCD filtered center front-of-screen temp that feeds TL1V (DegC) (TL1v)
 [TL1V] type [sp7s] 73703738 len [ 2] idx [ 60]: LCD TL1v-filtered center front-of-screen temp for color compensation (DegC) (TL1V)
 [Tp2F] type [sp7s] 73703738 len [ 2] idx [ 61]: Power Supply T2 Secondary Heatsink filtered temp (DegC) (Tp2F)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [ 62]: Skin 0 virtual temp (DegC) (TS0V)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 63]: Drive 0 OOBv3 relative filtered temp Max (DegC) (TH0F)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [ 64]: Drive 1 OOBv3 relative filtered temp Max (DegC) (TH1F)
 [PM0f] type [sp2s] 73703264 len [ 2] idx [ 65]: DIMM load-side power / SQR(Fan RPM) (PM0f)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp9s] 73703936 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J78...
 Set 0 has 74 keys:
 [VD2R] type [sp4s] 73703462 len [ 2] idx [  1]: Power Supply 12V voltage (Volts) (VD2R)
 [ID2R] type [sp6s] 73703639 len [ 2] idx [  2]: Power Supply 12V current (Amps) (ID2R)
 [VG1C] type [sp4s] 73703462 len [ 2] idx [  3]: GPU Core input-side voltage (Volts) (VG1C)
 [IG1C] type [sp6s] 73703639 len [ 2] idx [  4]: GPU Core input-side current (Amps) (IG1C)
 [VC0M] type [sp2s] 73703264 len [ 2] idx [  5]: CPU Mem  load-side voltage (Volts) (VC0M)
 [IC0M] type [sp5s] 73703561 len [ 2] idx [  6]: CPU Mem  load-side current (Amps) (IC0M)
 [VM0R] type [sp2s] 73703264 len [ 2] idx [  7]: DIMM load-side voltage (Volts) (VM0R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [  8]: DIMM load-side current (Amps) (IM0R)
 [VG1F] type [sp4s] 73703462 len [ 2] idx [  9]: GPU Frame Buffer input-side voltage (Volts) (VG1F)
 [IG1F] type [sp3s] 73703363 len [ 2] idx [ 10]: GPU FB   input-side current (Amps) (IG1F)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 11]: CPU Core load-side voltage (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core load-side current (Amps) (IC0C)
 [VG0C] type [sp2s] 73703264 len [ 2] idx [ 13]: GPU Core  load-side voltage (Volts) (VG0C)
 [IG0C] type [sp8s] 73703837 len [ 2] idx [ 14]: GPU Core  load-side current (Amps) (IG0C)
 [VH05] type [sp3s] 73703363 len [ 2] idx [ 15]: Drive 0 5V load-side voltage (Volts) (VH05)
 [IH05] type [sp2s] 73703264 len [ 2] idx [ 16]: Drive 0 5V   load-side current (Amps) (IH05)
 [IW0R] type [sp3s] 73703363 len [ 2] idx [ 17]: Wifi load-side current (Amps) (IW0R)
 [IH02] type [sp3s] 73703363 len [ 2] idx [ 18]: Drive 0 12V load-side current (Amps) (IH02)
 [VR1R] type [sp2s] 73703264 len [ 2] idx [ 19]: PCH/GPU/TBT load-side voltage (Volts) (VR1R)
 [IG1A] type [sp3s] 73703363 len [ 2] idx [ 20]: GPU Aux  input-side current (Amps) (IG1A)
 [VR3R] type [sp3s] 73703363 len [ 2] idx [ 21]: 3.3V load-side voltage (Volts) (VR3R)
 [IH1R] type [sp3s] 73703363 len [ 2] idx [ 22]: Drive 1 3.3V load-side current (Amps) (IH1R)
 [VG0I] type [sp2s] 73703264 len [ 2] idx [ 23]: GPU VDDCI load-side voltage (Volts) (VG0I)
 [IG0I] type [sp5s] 73703561 len [ 2] idx [ 24]: GPU VDDCI load-side current (Amps) (IG0I)
 [PD2R] type [sp9s] 73703936 len [ 2] idx [ 25]: Power Supply 12V power (Watts) (PD2R)
 [PG1C] type [sp9s] 73703936 len [ 2] idx [ 26]: GPU Core+VDDCI input-side power (Watts) (PG1C)
 [PC0M] type [sp9s] 73703936 len [ 2] idx [ 27]: CPU Mem  load-side power (Watts) (PC0M)
 [PM0R] type [sp9s] 73703936 len [ 2] idx [ 28]: DIMM load-side power (Watts) (PM0R)
 [PG1F] type [sp9s] 73703936 len [ 2] idx [ 29]: GPU Frame Buf  input-side power (Watts) (PG1F)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [ 30]: CPU Core load-side power (Watts) (PC0C)
 [PG0C] type [sp9s] 73703936 len [ 2] idx [ 31]: GPU Core    load-side power (Watts) (PG0C)
 [PG1A] type [sp9s] 73703936 len [ 2] idx [ 32]: GPU Aux    input-side power (Watts) (PG1A)
 [PG0A] type [sp9s] 73703936 len [ 2] idx [ 33]: GPU Aux     load-side power (= x% of PG1A) (Watts) (PG0A)
 [PG0I] type [sp9s] 73703936 len [ 2] idx [ 34]: GPU VDDCI   load-side power (Watts) (PG0I)
 [PG0M] type [sp9s] 73703936 len [ 2] idx [ 35]: GPU Mem Ctl load-side power (= 30% of PG1F * efficiency) (Watts) (PG0M)
 [PG0V] type [sp9s] 73703936 len [ 2] idx [ 36]: GPU VRAM    load-side power (= 70% of PG1F * efficiency) (Watts) (PG0V)
 [PH05] type [sp9s] 73703936 len [ 2] idx [ 37]: Drive 0 5V load-side power (Watts) (PH05)
 [PH02] type [sp9s] 73703936 len [ 2] idx [ 38]: Drive 0 12V load-side power (Watts) (PH02)
 [PW0R] type [sp9s] 73703936 len [ 2] idx [ 39]: Wifi load-side power (Watts) (PW0R)
 [PH1R] type [sp9s] 73703936 len [ 2] idx [ 40]: Drive 1 load-side power (Watts) (PH1R)
 [PH0R] type [sp9s] 73703936 len [ 2] idx [ 41]: Drive 0 total load-side power (PH02 + PH05) (Watts) (PH0R)
 [PGPR] type [sp9s] 73703936 len [ 2] idx [ 42]: GPU package total load-side power (SMC) (PGPR)
 [PGTR] type [sp9s] 73703936 len [ 2] idx [ 43]: GPU total input-side power (PGTR)
 [PCPR] type [sp9s] 73703936 len [ 2] idx [ 44]: CPU package total power (SMC) (PCPR)
 [PCTR] type [sp9s] 73703936 len [ 2] idx [ 45]: CPU total equivalent input-side power (PCTR)
 [PZ0G] type [sp9s] 73703936 len [ 2] idx [ 46]: Zone 0 average power (Watts) (PZ0G)
 [PZ1G] type [sp9s] 73703936 len [ 2] idx [ 47]: Zone 1 average power (Watts) (PZ1G)
 [PZ2G] type [sp9s] 73703936 len [ 2] idx [ 48]: Zone 2 average power (Watts) (PZ2G)
 [PZ3G] type [sp9s] 73703936 len [ 2] idx [ 49]: Zone 3 average power (Watts) (PZ3G)
 [PZ4G] type [sp9s] 73703936 len [ 2] idx [ 50]: Zone 4 average power (Watts) (PZ4G)
 [PZ5G] type [sp9s] 73703936 len [ 2] idx [ 51]: Zone 5 average power (Watts) (PZ5G)
 [ID2I] type [sp7s] 73703738 len [ 2] idx [ 52]: Power Supply 12V current filter input S7.8 (Amps) (ID2I)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [fltf] 666C7420 len [ 4] idx [226]: Zone 2 Filtered Power (PZ2F)
 [PZ2E] type [fltf] 666C7420 len [ 4] idx [227]: Zone 2 Target Power (PZ2E)
 [PZ2T] type [fltf] 666C7420 len [ 4] idx [228]: Zone 2 Abstract Throttle (PZ2T)
 [PZ3F] type [fltf] 666C7420 len [ 4] idx [229]: Zone 3 Filtered Power (PZ3F)
 [PZ3E] type [fltf] 666C7420 len [ 4] idx [230]: Zone 3 Target Power (PZ3E)
 [PZ3T] type [fltf] 666C7420 len [ 4] idx [231]: Zone 3 Abstract Throttle (PZ3T)
 [PZ4F] type [fltf] 666C7420 len [ 4] idx [232]: Zone 4 Filtered Power (PZ4F)
 [PZ4E] type [fltf] 666C7420 len [ 4] idx [233]: Zone 4 Target Power (PZ4E)
 [PZ4T] type [fltf] 666C7420 len [ 4] idx [234]: Zone 4 Abstract Throttle (PZ4T)
 [PZ5F] type [fltf] 666C7420 len [ 4] idx [235]: Zone 5 Filtered Power (PZ5F)
 [PZ5E] type [fltf] 666C7420 len [ 4] idx [236]: Zone 5 Target Power (PZ5E)
 [PZ5T] type [fltf] 666C7420 len [ 4] idx [237]: Zone 5 Abstract Throttle (PZ5T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 105 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [Tb0p] type [sp7s] 73703738 len [ 2] idx [  2]: Backlight Controller proximity raw temp (DegC) (Tb0p)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Proximity raw temp (DegC) (TC0p)
 [TM0p] type [sp7s] 73703738 len [ 2] idx [  4]: DIMM 0 Proximity raw temp (DegC) (TM0p)
 [TM1p] type [sp7s] 73703738 len [ 2] idx [  5]: DIMM 1 Proximity raw temp (DegC) (TM1p)
 [TM2p] type [sp7s] 73703738 len [ 2] idx [  6]: DIMM 2 Proximity raw temp (DegC) (TM2p)
 [TM3p] type [sp7s] 73703738 len [ 2] idx [  7]: DIMM 3 Proximity raw temp (DegC) (TM3p)
 [TG0d] type [sp7s] 73703738 len [ 2] idx [  8]: GPU Die raw temp (DegC) (TG0d)
 [TG0p] type [sp7s] 73703738 len [ 2] idx [  9]: GPU Proximity 0 (internal EMC1414) raw temp (DegC) (TG0p)
 [TG1p] type [sp7s] 73703738 len [ 2] idx [ 10]: GPU GDDR5 Proximity 1 raw temp (DegC) (TG1p)
 [TG2p] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU VR Proximity 2 raw temp (DegC) (TG2p)
 [TG3p] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU FB VR Proximity 3 (via diode connected to EMC1428) raw temp (DegC) (TG3p)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [ 13]: Drive 0 OOBv1 raw bit-mapped temp (TH0o)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [ 14]: Drive 1 OOBv1 raw bit-mapped temp (TH1o)
 [TL0p] type [sp7s] 73703738 len [ 2] idx [ 15]: LCD unfiltered front-of-screen raw temp (DegC) (TL0p)
 [TL1p] type [sp7s] 73703738 len [ 2] idx [ 16]: LCD TCON Proximity raw temp (DegC) (TL1p)
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [ 17]: MLB Proximity 0 raw    temp: MLB top near power connector (DegC) (Tm0p)
 [Tm1p] type [sp7s] 73703738 len [ 2] idx [ 18]: MLB Proximity 1 raw    temp: MLB top near GPU (DegC) (Tm1p)
 [Tm2p] type [sp7s] 73703738 len [ 2] idx [ 19]: MLB Proximity 2 raw    temp: MLB bottom near CPU (DegC) (Tm2p)
 [TC0c] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU Core 0 absolute raw temp (PECI) (DegC) (TC0c)
 [TC1c] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU Core 1 absolute raw temp (PECI) (DegC) (TC1c)
 [TC2c] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU Core 2 absolute raw temp (PECI) (DegC) (TC2c)
 [TC3c] type [sp7s] 73703738 len [ 2] idx [ 23]: CPU Core 3 absolute raw temp (PECI) (DegC) (TC3c)
 [TCGc] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU Gfx absolute raw temp (PECI) (DegC) (TCGc)
 [TCSc] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU System Agent Core absolute raw temp (PECI) (DegC) (TCSc)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [ 26]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [ 27]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [Tp2h] type [sp7s] 73703738 len [ 2] idx [ 28]: Power Supply T2 Secondary Heatsink raw temp (DegC) (Tp2h)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 29]: Drive 0 OOBv3 absolute raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 30]: Drive 0 OOBv3 absolute raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 31]: Drive 0 OOBv3 absolute raw temp C (DegC) (TH0c)
 [TH0e] type [sp7s] 73703738 len [ 2] idx [ 32]: Drive 0 temp sensor existence used for TM0V (0) = present (TH0e)
 [TH1a] type [sp7s] 73703738 len [ 2] idx [ 33]: Drive 1 OOBv3 absolute raw temp A (DegC) (TH1a)
 [TH1b] type [sp7s] 73703738 len [ 2] idx [ 34]: Drive 1 OOBv3 absolute raw temp B (DegC) (TH1b)
 [TH1c] type [sp7s] 73703738 len [ 2] idx [ 35]: Drive 1 OOBv3 absolute raw temp C (DegC) (TH1c)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 36]: Ambient cooked temp (DegC) (TA0P)
 [Tb0P] type [sp7s] 73703738 len [ 2] idx [ 37]: Backlight Controller proximity cooked temp (DegC) (Tb0P)
 [TC0L] type [ui1u] 75693136 len [ 2] idx [ 38]: CPU PECI Die dynamic filter coeff (Seconds) (TC0L)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 39]: CPU Proximity cooked temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 40]: DIMM 0 Proximity cooked temp (DegC) (TM0P)
 [TM1P] type [sp7s] 73703738 len [ 2] idx [ 41]: DIMM 1 Proximity cooked temp (DegC) (TM1P)
 [TM2P] type [sp7s] 73703738 len [ 2] idx [ 42]: DIMM 2 Proximity cooked temp (DegC) (TM2P)
 [TM3P] type [sp7s] 73703738 len [ 2] idx [ 43]: DIMM 3 Proximity cooked temp (DegC) (TM3P)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 44]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 45]: Drive 0 OOBv1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 46]: Drive 1 OOBv1 mapped temp (DegC) (TH1O)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 47]: GPU Die cooked temp (DegC) (TG0D)
 [TG0L] type [ui1u] 75693136 len [ 2] idx [ 48]: GPU Die dynamic filter coeff (Seconds) (TG0L)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 49]: GPU Proximity 0 (internal EMC1414) cooked temp (DegC) (TG0P)
 [TG1P] type [sp7s] 73703738 len [ 2] idx [ 50]: GPU GDDR5 Proximity 1 cooked temp (DegC) (TG1P)
 [TG2P] type [sp7s] 73703738 len [ 2] idx [ 51]: GPU VR Proximity 2 cooked temp (DegC) (TG2P)
 [TG3P] type [sp7s] 73703738 len [ 2] idx [ 52]: GPU FB VR Proximity 3 (via diode connected to EMC1428) cooked temp (DegC) (TG3P)
 [TL0P] type [sp7s] 73703738 len [ 2] idx [ 53]: LCD unfiltered front-of-screen cooked temp (DegC) (TL0P)
 [TL1P] type [sp7s] 73703738 len [ 2] idx [ 54]: LCD TCON Proximity cooked temp (DegC) (TL1P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [ 55]: MLB Proximity 0 cooked temp: MLB top near power connector (DegC) (Tm0P)
 [Tm1P] type [sp7s] 73703738 len [ 2] idx [ 56]: MLB Proximity 1 cooked temp: MLB top near GPU (DegC) (Tm1P)
 [Tm2P] type [sp7s] 73703738 len [ 2] idx [ 57]: MLB Proximity 2 cooked temp: MLB bottom near CPU (DegC) (Tm2P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 58]: PCH Die cooked temp (DegC) (TPCD)
 [TCXR] type [sp7s] 73703738 len [ 2] idx [ 59]: CPU Max Package Core relative cooked temp (PECI) (DegC) (TCXR)
 [PCPC] type [sp9s] 73703936 len [ 2] idx [ 60]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp9s] 73703936 len [ 2] idx [ 61]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [PCPT] type [sp9s] 73703936 len [ 2] idx [ 62]: CPU package total power (PECI) (Watts) (PCPT)
 [Tp2H] type [sp7s] 73703738 len [ 2] idx [ 63]: Power Supply T2 Secondary Heatsink cooked temp (DegC) (Tp2H)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 64]: Drive 0 OOBv3 absolute cooked temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 65]: Drive 0 OOBv3 absolute cooked temp B (DegC) (TH0B)
 [TH0C] type [sp7s] 73703738 len [ 2] idx [ 66]: Drive 0 OOBv3 absolute cooked temp C (DegC) (TH0C)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 67]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH1A] type [sp7s] 73703738 len [ 2] idx [ 68]: Drive 1 OOBv3 absolute cooked temp A (DegC) (TH1A)
 [TH1B] type [sp7s] 73703738 len [ 2] idx [ 69]: Drive 1 OOBv3 absolute cooked temp B (DegC) (TH1B)
 [TH1C] type [sp7s] 73703738 len [ 2] idx [ 70]: Drive 1 OOBv3 absolute cooked temp C (DegC) (TH1C)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 71]: Drive 1 OOBv3 relative cooked temp Max (DegC) (TH1R)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 72]: Ambient virtual temp (DegC) (TA0V)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 73]: DIMM virtual temp (DegC) (TM0V)
 [TM1a] type [sp7s] 73703738 len [ 2] idx [ 74]: DIMM virtual temp for 2x DIMM Slot1+2+3+4 config (DegC) (TM1a)
 [TM2a] type [sp7s] 73703738 len [ 2] idx [ 75]: DIMM virtual temp for 2x DIMM Slot1+3 config (DegC) (TM2a)
 [TM2b] type [sp7s] 73703738 len [ 2] idx [ 76]: DIMM virtual temp for 2x DIMM Slot1+2 or Slot2+3 config (DegC) (TM2b)
 [TM2c] type [sp7s] 73703738 len [ 2] idx [ 77]: DIMM virtual temp for 2x DIMM Slot1+4 or Slot2+4 config (DegC) (TM2c)
 [TM2d] type [sp7s] 73703738 len [ 2] idx [ 78]: DIMM virtual temp for 2x DIMM Slot3+4 config (DegC) (TM2d)
 [TM3a] type [sp7s] 73703738 len [ 2] idx [ 79]: DIMM virtual temp for 3x DIMM Slot2+3+4 config (DegC) (TM3a)
 [TM3b] type [sp7s] 73703738 len [ 2] idx [ 80]: DIMM virtual temp for 3x DIMM Slot1+3+4 config (DegC) (TM3b)
 [TM3c] type [sp7s] 73703738 len [ 2] idx [ 81]: DIMM virtual temp for 3x DIMM Slot1+2+4 config (DegC) (TM3c)
 [TM3d] type [sp7s] 73703738 len [ 2] idx [ 82]: DIMM virtual temp for 3x DIMM Slot1+2+3 config (DegC) (TM3d)
 [TM4a] type [sp7s] 73703738 len [ 2] idx [ 83]: DIMM virtual temp for 4x DIMM Slot1+2+3+4 config (DegC) (TM4a)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 84]: Drive 0 OOBv1 filtered temp (DegC) (TH0P)
 [PH0F] type [sp7s] 73703738 len [ 2] idx [ 85]: Drive 0 filtered total load-side power (PH02 + PH05) * 2 (Watts) (PH0F)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 86]: Drive 1 OOBv1 filtered temp (DegC) (TH1P)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 87]: Drive 1 filtered load-side power * 3 (Watts) (PH1F)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 88]: CPU PECI Die filtered temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 89]: CPU PECI Die filtered and adjusted temp for fan/power control (DegC) (TC0F)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 90]: CPU PECI Die temp max error used in TC0F=TC0E+ (DegC) (TC0J)
 [TC0T] type [sp7s] 73703738 len [ 2] idx [ 91]: CPU PECI Die temp Trend (DegC) (TC0T)
 [TG0E] type [sp7s] 73703738 len [ 2] idx [ 92]: GPU Die filtered temp (DegC) (TG0E)
 [TG0F] type [sp7s] 73703738 len [ 2] idx [ 93]: GPU Die filtered and adjusted temp for fan/power control (DegC) (TG0F)
 [TG0J] type [sp7s] 73703738 len [ 2] idx [ 94]: GPU Die temp max error used in TG0F=TG0E+ (DegC) (TG0J)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [ 95]: GPU Die temp Trend (DegC) (TG0T)
 [TL0V] type [sp7s] 73703738 len [ 2] idx [ 96]: LCD filtered front-of-screen hotspot virtual temp (DegC) (TL0V)
 [TL1v] type [sp7s] 73703738 len [ 2] idx [ 97]: LCD filtered center front-of-screen temp that feeds TL1V (DegC) (TL1v)
 [TL1V] type [sp7s] 73703738 len [ 2] idx [ 98]: LCD TL1v-filtered center front-of-screen temp for color compensation (DegC) (TL1V)
 [Tp2F] type [sp7s] 73703738 len [ 2] idx [ 99]: Power Supply T2 Secondary Heatsink filtered temp (DegC) (Tp2F)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [100]: Skin 0 virtual temp (DegC) (TS0V)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [101]: Drive 0 OOBv3 relative filtered temp Max (DegC) (TH0F)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [102]: Drive 1 OOBv3 relative filtered temp Max (DegC) (TH1F)
 [PM0f] type [sp2s] 73703264 len [ 2] idx [103]: DIMM load-side power / SQR(Fan RPM) (PM0f)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp9s] 73703936 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J78a...
 Set 0 has 74 keys:
 [VD2R] type [sp4s] 73703462 len [ 2] idx [  1]: Power Supply 12V voltage (Volts) (VD2R)
 [ID2R] type [sp6s] 73703639 len [ 2] idx [  2]: Power Supply 12V current (Amps) (ID2R)
 [VG1C] type [sp4s] 73703462 len [ 2] idx [  3]: GPU Core input-side voltage (Volts) (VG1C)
 [IG1C] type [sp6s] 73703639 len [ 2] idx [  4]: GPU Core input-side current (Amps) (IG1C)
 [VC0M] type [sp2s] 73703264 len [ 2] idx [  5]: CPU Mem  load-side voltage (Volts) (VC0M)
 [IC0M] type [sp5s] 73703561 len [ 2] idx [  6]: CPU Mem  load-side current (Amps) (IC0M)
 [VM0R] type [sp2s] 73703264 len [ 2] idx [  7]: DIMM load-side voltage (Volts) (VM0R)
 [IM0R] type [sp5s] 73703561 len [ 2] idx [  8]: DIMM load-side current (Amps) (IM0R)
 [VG1F] type [sp4s] 73703462 len [ 2] idx [  9]: GPU Frame Buffer input-side voltage (Volts) (VG1F)
 [IG1F] type [sp3s] 73703363 len [ 2] idx [ 10]: GPU FB   input-side current (Amps) (IG1F)
 [VC0C] type [sp2s] 73703264 len [ 2] idx [ 11]: CPU Core load-side voltage (Volts) (VC0C)
 [IC0C] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU Core load-side current (Amps) (IC0C)
 [VG0C] type [sp2s] 73703264 len [ 2] idx [ 13]: GPU Core  load-side voltage (Volts) (VG0C)
 [IG0C] type [sp8s] 73703837 len [ 2] idx [ 14]: GPU Core  load-side current (Amps) (IG0C)
 [VH05] type [sp3s] 73703363 len [ 2] idx [ 15]: Drive 0 5V load-side voltage (Volts) (VH05)
 [IH05] type [sp2s] 73703264 len [ 2] idx [ 16]: Drive 0 5V   load-side current (Amps) (IH05)
 [IW0R] type [sp3s] 73703363 len [ 2] idx [ 17]: Wifi load-side current (Amps) (IW0R)
 [IH02] type [sp3s] 73703363 len [ 2] idx [ 18]: Drive 0 12V load-side current (Amps) (IH02)
 [VR1R] type [sp2s] 73703264 len [ 2] idx [ 19]: PCH/GPU/TBT load-side voltage (Volts) (VR1R)
 [IG1A] type [sp3s] 73703363 len [ 2] idx [ 20]: GPU Aux  input-side current (Amps) (IG1A)
 [VR3R] type [sp3s] 73703363 len [ 2] idx [ 21]: 3.3V load-side voltage (Volts) (VR3R)
 [IH1R] type [sp3s] 73703363 len [ 2] idx [ 22]: Drive 1 3.3V load-side current (Amps) (IH1R)
 [VG0I] type [sp2s] 73703264 len [ 2] idx [ 23]: GPU VDDCI load-side voltage (Volts) (VG0I)
 [IG0I] type [sp5s] 73703561 len [ 2] idx [ 24]: GPU VDDCI load-side current (Amps) (IG0I)
 [PD2R] type [sp9s] 73703936 len [ 2] idx [ 25]: Power Supply 12V power (Watts) (PD2R)
 [PG1C] type [sp9s] 73703936 len [ 2] idx [ 26]: GPU Core+VDDCI input-side power (Watts) (PG1C)
 [PC0M] type [sp9s] 73703936 len [ 2] idx [ 27]: CPU Mem  load-side power (Watts) (PC0M)
 [PM0R] type [sp9s] 73703936 len [ 2] idx [ 28]: DIMM load-side power (Watts) (PM0R)
 [PG1F] type [sp9s] 73703936 len [ 2] idx [ 29]: GPU Frame Buf  input-side power (Watts) (PG1F)
 [PC0C] type [sp9s] 73703936 len [ 2] idx [ 30]: CPU Core load-side power (Watts) (PC0C)
 [PG0C] type [sp9s] 73703936 len [ 2] idx [ 31]: GPU Core    load-side power (Watts) (PG0C)
 [PG1A] type [sp9s] 73703936 len [ 2] idx [ 32]: GPU Aux    input-side power (Watts) (PG1A)
 [PG0A] type [sp9s] 73703936 len [ 2] idx [ 33]: GPU Aux     load-side power (= x% of PG1A) (Watts) (PG0A)
 [PG0I] type [sp9s] 73703936 len [ 2] idx [ 34]: GPU VDDCI   load-side power (Watts) (PG0I)
 [PG0M] type [sp9s] 73703936 len [ 2] idx [ 35]: GPU Mem Ctl load-side power (= 30% of PG1F * efficiency) (Watts) (PG0M)
 [PG0V] type [sp9s] 73703936 len [ 2] idx [ 36]: GPU VRAM    load-side power (= 70% of PG1F * efficiency) (Watts) (PG0V)
 [PH05] type [sp9s] 73703936 len [ 2] idx [ 37]: Drive 0 5V load-side power (Watts) (PH05)
 [PH02] type [sp9s] 73703936 len [ 2] idx [ 38]: Drive 0 12V load-side power (Watts) (PH02)
 [PW0R] type [sp9s] 73703936 len [ 2] idx [ 39]: Wifi load-side power (Watts) (PW0R)
 [PH1R] type [sp9s] 73703936 len [ 2] idx [ 40]: Drive 1 load-side power (Watts) (PH1R)
 [PH0R] type [sp9s] 73703936 len [ 2] idx [ 41]: Drive 0 total load-side power (PH02 + PH05) (Watts) (PH0R)
 [PGPR] type [sp9s] 73703936 len [ 2] idx [ 42]: GPU package total load-side power (SMC) (PGPR)
 [PGTR] type [sp9s] 73703936 len [ 2] idx [ 43]: GPU total input-side power (PGTR)
 [PCPR] type [sp9s] 73703936 len [ 2] idx [ 44]: CPU package total power (SMC) (PCPR)
 [PCTR] type [sp9s] 73703936 len [ 2] idx [ 45]: CPU total equivalent input-side power (PCTR)
 [PZ0G] type [sp9s] 73703936 len [ 2] idx [ 46]: Zone 0 average power (Watts) (PZ0G)
 [PZ1G] type [sp9s] 73703936 len [ 2] idx [ 47]: Zone 1 average power (Watts) (PZ1G)
 [PZ2G] type [sp9s] 73703936 len [ 2] idx [ 48]: Zone 2 average power (Watts) (PZ2G)
 [PZ3G] type [sp9s] 73703936 len [ 2] idx [ 49]: Zone 3 average power (Watts) (PZ3G)
 [PZ4G] type [sp9s] 73703936 len [ 2] idx [ 50]: Zone 4 average power (Watts) (PZ4G)
 [PZ5G] type [sp9s] 73703936 len [ 2] idx [ 51]: Zone 5 average power (Watts) (PZ5G)
 [ID2I] type [sp7s] 73703738 len [ 2] idx [ 52]: Power Supply 12V current filter input S7.8 (Amps) (ID2I)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [fltf] 666C7420 len [ 4] idx [226]: Zone 2 Filtered Power (PZ2F)
 [PZ2E] type [fltf] 666C7420 len [ 4] idx [227]: Zone 2 Target Power (PZ2E)
 [PZ2T] type [fltf] 666C7420 len [ 4] idx [228]: Zone 2 Abstract Throttle (PZ2T)
 [PZ3F] type [fltf] 666C7420 len [ 4] idx [229]: Zone 3 Filtered Power (PZ3F)
 [PZ3E] type [fltf] 666C7420 len [ 4] idx [230]: Zone 3 Target Power (PZ3E)
 [PZ3T] type [fltf] 666C7420 len [ 4] idx [231]: Zone 3 Abstract Throttle (PZ3T)
 [PZ4F] type [fltf] 666C7420 len [ 4] idx [232]: Zone 4 Filtered Power (PZ4F)
 [PZ4E] type [fltf] 666C7420 len [ 4] idx [233]: Zone 4 Target Power (PZ4E)
 [PZ4T] type [fltf] 666C7420 len [ 4] idx [234]: Zone 4 Abstract Throttle (PZ4T)
 [PZ5F] type [fltf] 666C7420 len [ 4] idx [235]: Zone 5 Filtered Power (PZ5F)
 [PZ5E] type [fltf] 666C7420 len [ 4] idx [236]: Zone 5 Target Power (PZ5E)
 [PZ5T] type [fltf] 666C7420 len [ 4] idx [237]: Zone 5 Abstract Throttle (PZ5T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTi] type [ui8u] 75693820 len [ 1] idx [243]: 2nd GPU Plimit (MSTi)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 105 keys:
 [TA0p] type [sp7s] 73703738 len [ 2] idx [  1]: Ambient raw temp (DegC) (TA0p)
 [Tb0p] type [sp7s] 73703738 len [ 2] idx [  2]: Backlight Controller proximity raw temp (DegC) (Tb0p)
 [TC0p] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Proximity raw temp (DegC) (TC0p)
 [TM0p] type [sp7s] 73703738 len [ 2] idx [  4]: DIMM 0 Proximity raw temp (DegC) (TM0p)
 [TM1p] type [sp7s] 73703738 len [ 2] idx [  5]: DIMM 1 Proximity raw temp (DegC) (TM1p)
 [TM2p] type [sp7s] 73703738 len [ 2] idx [  6]: DIMM 2 Proximity raw temp (DegC) (TM2p)
 [TM3p] type [sp7s] 73703738 len [ 2] idx [  7]: DIMM 3 Proximity raw temp (DegC) (TM3p)
 [TG0d] type [sp7s] 73703738 len [ 2] idx [  8]: GPU Die raw temp (DegC) (TG0d)
 [TG0p] type [sp7s] 73703738 len [ 2] idx [  9]: GPU Proximity 0 (internal EMC1414) raw temp (DegC) (TG0p)
 [TG1p] type [sp7s] 73703738 len [ 2] idx [ 10]: GPU GDDR5 Proximity 1 raw temp (DegC) (TG1p)
 [TG2p] type [sp7s] 73703738 len [ 2] idx [ 11]: GPU VR Proximity 2 raw temp (DegC) (TG2p)
 [TG3p] type [sp7s] 73703738 len [ 2] idx [ 12]: GPU FB VR Proximity 3 (via diode connected to EMC1428) raw temp (DegC) (TG3p)
 [TH0o] type [ui1u] 75693136 len [ 2] idx [ 13]: Drive 0 OOBv1 raw bit-mapped temp (TH0o)
 [TH1o] type [ui1u] 75693136 len [ 2] idx [ 14]: Drive 1 OOBv1 raw bit-mapped temp (TH1o)
 [TL0p] type [sp7s] 73703738 len [ 2] idx [ 15]: LCD unfiltered front-of-screen raw temp (DegC) (TL0p)
 [TL1p] type [sp7s] 73703738 len [ 2] idx [ 16]: LCD TCON Proximity raw temp (DegC) (TL1p)
 [Tm0p] type [sp7s] 73703738 len [ 2] idx [ 17]: MLB Proximity 0 raw    temp: MLB top near power connector (DegC) (Tm0p)
 [Tm1p] type [sp7s] 73703738 len [ 2] idx [ 18]: MLB Proximity 1 raw    temp: MLB top near GPU (DegC) (Tm1p)
 [Tm2p] type [sp7s] 73703738 len [ 2] idx [ 19]: MLB Proximity 2 raw    temp: MLB bottom near CPU (DegC) (Tm2p)
 [TC0c] type [sp7s] 73703738 len [ 2] idx [ 20]: CPU Core 0 absolute raw temp (PECI) (DegC) (TC0c)
 [TC1c] type [sp7s] 73703738 len [ 2] idx [ 21]: CPU Core 1 absolute raw temp (PECI) (DegC) (TC1c)
 [TC2c] type [sp7s] 73703738 len [ 2] idx [ 22]: CPU Core 2 absolute raw temp (PECI) (DegC) (TC2c)
 [TC3c] type [sp7s] 73703738 len [ 2] idx [ 23]: CPU Core 3 absolute raw temp (PECI) (DegC) (TC3c)
 [TCGc] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU Gfx absolute raw temp (PECI) (DegC) (TCGc)
 [TCSc] type [sp7s] 73703738 len [ 2] idx [ 25]: CPU System Agent Core absolute raw temp (PECI) (DegC) (TCSc)
 [TCXc] type [sp7s] 73703738 len [ 2] idx [ 26]: CPU Max Package Core absolute raw temp (PECI) (DegC) (TCXc)
 [TCXr] type [sp7s] 73703738 len [ 2] idx [ 27]: CPU Max Package Core relative raw temp (PECI) (DegC) (TCXr)
 [Tp2h] type [sp7s] 73703738 len [ 2] idx [ 28]: Power Supply T2 Secondary Heatsink raw temp (DegC) (Tp2h)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 29]: Drive 0 OOBv3 absolute raw temp A (DegC) (TH0a)
 [TH0b] type [sp7s] 73703738 len [ 2] idx [ 30]: Drive 0 OOBv3 absolute raw temp B (DegC) (TH0b)
 [TH0c] type [sp7s] 73703738 len [ 2] idx [ 31]: Drive 0 OOBv3 absolute raw temp C (DegC) (TH0c)
 [TH0e] type [sp7s] 73703738 len [ 2] idx [ 32]: Drive 0 temp sensor existence used for TM0V (0) = present (TH0e)
 [TH1a] type [sp7s] 73703738 len [ 2] idx [ 33]: Drive 1 OOBv3 absolute raw temp A (DegC) (TH1a)
 [TH1b] type [sp7s] 73703738 len [ 2] idx [ 34]: Drive 1 OOBv3 absolute raw temp B (DegC) (TH1b)
 [TH1c] type [sp7s] 73703738 len [ 2] idx [ 35]: Drive 1 OOBv3 absolute raw temp C (DegC) (TH1c)
 [TA0P] type [sp7s] 73703738 len [ 2] idx [ 36]: Ambient cooked temp (DegC) (TA0P)
 [Tb0P] type [sp7s] 73703738 len [ 2] idx [ 37]: Backlight Controller proximity cooked temp (DegC) (Tb0P)
 [TC0L] type [ui1u] 75693136 len [ 2] idx [ 38]: CPU PECI Die dynamic filter coeff (Seconds) (TC0L)
 [TC0P] type [sp7s] 73703738 len [ 2] idx [ 39]: CPU Proximity cooked temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [ 40]: DIMM 0 Proximity cooked temp (DegC) (TM0P)
 [TM1P] type [sp7s] 73703738 len [ 2] idx [ 41]: DIMM 1 Proximity cooked temp (DegC) (TM1P)
 [TM2P] type [sp7s] 73703738 len [ 2] idx [ 42]: DIMM 2 Proximity cooked temp (DegC) (TM2P)
 [TM3P] type [sp7s] 73703738 len [ 2] idx [ 43]: DIMM 3 Proximity cooked temp (DegC) (TM3P)
 [TMXP] type [sp7s] 73703738 len [ 2] idx [ 44]: DIMM Proximity max cooked temp (DegC) (TMXP)
 [TH0O] type [sp7s] 73703738 len [ 2] idx [ 45]: Drive 0 OOBv1 mapped temp (DegC) (TH0O)
 [TH1O] type [sp7s] 73703738 len [ 2] idx [ 46]: Drive 1 OOBv1 mapped temp (DegC) (TH1O)
 [TG0D] type [sp7s] 73703738 len [ 2] idx [ 47]: GPU Die cooked temp (DegC) (TG0D)
 [TG0L] type [ui1u] 75693136 len [ 2] idx [ 48]: GPU Die dynamic filter coeff (Seconds) (TG0L)
 [TG0P] type [sp7s] 73703738 len [ 2] idx [ 49]: GPU Proximity 0 (internal EMC1414) cooked temp (DegC) (TG0P)
 [TG1P] type [sp7s] 73703738 len [ 2] idx [ 50]: GPU GDDR5 Proximity 1 cooked temp (DegC) (TG1P)
 [TG2P] type [sp7s] 73703738 len [ 2] idx [ 51]: GPU VR Proximity 2 cooked temp (DegC) (TG2P)
 [TG3P] type [sp7s] 73703738 len [ 2] idx [ 52]: GPU FB VR Proximity 3 (via diode connected to EMC1428) cooked temp (DegC) (TG3P)
 [TL0P] type [sp7s] 73703738 len [ 2] idx [ 53]: LCD unfiltered front-of-screen cooked temp (DegC) (TL0P)
 [TL1P] type [sp7s] 73703738 len [ 2] idx [ 54]: LCD TCON Proximity cooked temp (DegC) (TL1P)
 [Tm0P] type [sp7s] 73703738 len [ 2] idx [ 55]: MLB Proximity 0 cooked temp: MLB top near power connector (DegC) (Tm0P)
 [Tm1P] type [sp7s] 73703738 len [ 2] idx [ 56]: MLB Proximity 1 cooked temp: MLB top near GPU (DegC) (Tm1P)
 [Tm2P] type [sp7s] 73703738 len [ 2] idx [ 57]: MLB Proximity 2 cooked temp: MLB bottom near CPU (DegC) (Tm2P)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [ 58]: PCH Die cooked temp (DegC) (TPCD)
 [TCXR] type [sp7s] 73703738 len [ 2] idx [ 59]: CPU Max Package Core relative cooked temp (PECI) (DegC) (TCXR)
 [PCPC] type [sp9s] 73703936 len [ 2] idx [ 60]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp9s] 73703936 len [ 2] idx [ 61]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [PCPT] type [sp9s] 73703936 len [ 2] idx [ 62]: CPU package total power (PECI) (Watts) (PCPT)
 [Tp2H] type [sp7s] 73703738 len [ 2] idx [ 63]: Power Supply T2 Secondary Heatsink cooked temp (DegC) (Tp2H)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 64]: Drive 0 OOBv3 absolute cooked temp A (DegC) (TH0A)
 [TH0B] type [sp7s] 73703738 len [ 2] idx [ 65]: Drive 0 OOBv3 absolute cooked temp B (DegC) (TH0B)
 [TH0C] type [sp7s] 73703738 len [ 2] idx [ 66]: Drive 0 OOBv3 absolute cooked temp C (DegC) (TH0C)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 67]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH1A] type [sp7s] 73703738 len [ 2] idx [ 68]: Drive 1 OOBv3 absolute cooked temp A (DegC) (TH1A)
 [TH1B] type [sp7s] 73703738 len [ 2] idx [ 69]: Drive 1 OOBv3 absolute cooked temp B (DegC) (TH1B)
 [TH1C] type [sp7s] 73703738 len [ 2] idx [ 70]: Drive 1 OOBv3 absolute cooked temp C (DegC) (TH1C)
 [TH1R] type [sp7s] 73703738 len [ 2] idx [ 71]: Drive 1 OOBv3 relative cooked temp Max (DegC) (TH1R)
 [TA0V] type [sp7s] 73703738 len [ 2] idx [ 72]: Ambient virtual temp (DegC) (TA0V)
 [TM0V] type [sp7s] 73703738 len [ 2] idx [ 73]: DIMM virtual temp (DegC) (TM0V)
 [TM1a] type [sp7s] 73703738 len [ 2] idx [ 74]: DIMM virtual temp for 2x DIMM Slot1+2+3+4 config (DegC) (TM1a)
 [TM2a] type [sp7s] 73703738 len [ 2] idx [ 75]: DIMM virtual temp for 2x DIMM Slot1+3 config (DegC) (TM2a)
 [TM2b] type [sp7s] 73703738 len [ 2] idx [ 76]: DIMM virtual temp for 2x DIMM Slot1+2 or Slot2+3 config (DegC) (TM2b)
 [TM2c] type [sp7s] 73703738 len [ 2] idx [ 77]: DIMM virtual temp for 2x DIMM Slot1+4 or Slot2+4 config (DegC) (TM2c)
 [TM2d] type [sp7s] 73703738 len [ 2] idx [ 78]: DIMM virtual temp for 2x DIMM Slot3+4 config (DegC) (TM2d)
 [TM3a] type [sp7s] 73703738 len [ 2] idx [ 79]: DIMM virtual temp for 3x DIMM Slot2+3+4 config (DegC) (TM3a)
 [TM3b] type [sp7s] 73703738 len [ 2] idx [ 80]: DIMM virtual temp for 3x DIMM Slot1+3+4 config (DegC) (TM3b)
 [TM3c] type [sp7s] 73703738 len [ 2] idx [ 81]: DIMM virtual temp for 3x DIMM Slot1+2+4 config (DegC) (TM3c)
 [TM3d] type [sp7s] 73703738 len [ 2] idx [ 82]: DIMM virtual temp for 3x DIMM Slot1+2+3 config (DegC) (TM3d)
 [TM4a] type [sp7s] 73703738 len [ 2] idx [ 83]: DIMM virtual temp for 4x DIMM Slot1+2+3+4 config (DegC) (TM4a)
 [TH0P] type [sp7s] 73703738 len [ 2] idx [ 84]: Drive 0 OOBv1 filtered temp (DegC) (TH0P)
 [PH0F] type [sp7s] 73703738 len [ 2] idx [ 85]: Drive 0 filtered total load-side power (PH02 + PH05) * 2 (Watts) (PH0F)
 [TH1P] type [sp7s] 73703738 len [ 2] idx [ 86]: Drive 1 OOBv1 filtered temp (DegC) (TH1P)
 [PH1F] type [sp7s] 73703738 len [ 2] idx [ 87]: Drive 1 filtered load-side power * 3 (Watts) (PH1F)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 88]: CPU PECI Die filtered temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 89]: CPU PECI Die filtered and adjusted temp for fan/power control (DegC) (TC0F)
 [TC0J] type [sp7s] 73703738 len [ 2] idx [ 90]: CPU PECI Die temp max error used in TC0F=TC0E+ (DegC) (TC0J)
 [TC0T] type [sp7s] 73703738 len [ 2] idx [ 91]: CPU PECI Die temp Trend (DegC) (TC0T)
 [TG0E] type [sp7s] 73703738 len [ 2] idx [ 92]: GPU Die filtered temp (DegC) (TG0E)
 [TG0F] type [sp7s] 73703738 len [ 2] idx [ 93]: GPU Die filtered and adjusted temp for fan/power control (DegC) (TG0F)
 [TG0J] type [sp7s] 73703738 len [ 2] idx [ 94]: GPU Die temp max error used in TG0F=TG0E+ (DegC) (TG0J)
 [TG0T] type [sp7s] 73703738 len [ 2] idx [ 95]: GPU Die temp Trend (DegC) (TG0T)
 [TL0V] type [sp7s] 73703738 len [ 2] idx [ 96]: LCD filtered front-of-screen hotspot virtual temp (DegC) (TL0V)
 [TL1v] type [sp7s] 73703738 len [ 2] idx [ 97]: LCD filtered center front-of-screen temp that feeds TL1V (DegC) (TL1v)
 [TL1V] type [sp7s] 73703738 len [ 2] idx [ 98]: LCD TL1v-filtered center front-of-screen temp for color compensation (DegC) (TL1V)
 [Tp2F] type [sp7s] 73703738 len [ 2] idx [ 99]: Power Supply T2 Secondary Heatsink filtered temp (DegC) (Tp2F)
 [TS0V] type [sp7s] 73703738 len [ 2] idx [100]: Skin 0 virtual temp (DegC) (TS0V)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [101]: Drive 0 OOBv3 relative filtered temp Max (DegC) (TH0F)
 [TH1F] type [sp7s] 73703738 len [ 2] idx [102]: Drive 1 OOBv3 relative filtered temp Max (DegC) (TH1F)
 [PM0f] type [sp2s] 73703264 len [ 2] idx [103]: DIMM load-side power / SQR(Fan RPM) (PM0f)
 [F0Ac] type [fpef] 66706532 len [ 2] idx [220]: Fan0 Actual RPM(F0Ac)
 [PSTR] type [sp9s] 73703936 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
Dumping keys for J92...
 Set 0 has 23 keys:
 [PPBR] type [sp7s] 73703738 len [ 2] idx [  1]: PBus on battery power (Watts) (PPBR)
 [PDTR] type [sp7s] 73703738 len [ 2] idx [  2]: DC-In total power  (Watts) (PDTR)
 [PC0R] type [sp7s] 73703738 len [ 2] idx [  3]: CPU Computing High Side Power (Watts) (PC0R)
 [PHPC] type [sp7s] 73703738 len [ 2] idx [  4]: Thermal control Power (Watts) (PHPC)
 [VP0R] type [sp5s] 73703561 len [ 2] idx [  5]: PBus rail voltage. (Volts) (VP0R)
 [VD0R] type [sp5s] 73703561 len [ 2] idx [  6]: DC In voltage. (Volts) (VD0R)
 [IPBR] type [sp5s] 73703561 len [ 2] idx [  7]: PBus on battery current. (Amps) (IPBR)
 [ID0R] type [sp5s] 73703561 len [ 2] idx [  8]: DC In rail current. (Amps) (ID0R)
 [IC0R] type [sp5s] 73703561 len [ 2] idx [  9]: CPU Computing High Side current. (Amps) (IC0R)
 [VCFR] type [sp5s] 73703561 len [ 2] idx [ 10]: FIVR CPU supply voltage. (Volts) (VCFR)
 [VACC] type [sp5s] 73703561 len [ 2] idx [ 11]: ACC voltage. (Volts) (VACC)
 [PZ0F] type [fltf] 666C7420 len [ 4] idx [220]: Zone 0 Filtered Power (PZ0F)
 [PZ0E] type [fltf] 666C7420 len [ 4] idx [221]: Zone 0 Target Power (PZ0E)
 [PZ0T] type [fltf] 666C7420 len [ 4] idx [222]: Zone 0 Abstract Throttle (PZ0T)
 [PZ1F] type [fltf] 666C7420 len [ 4] idx [223]: Zone 1 Filtered Power (PZ1F)
 [PZ1E] type [fltf] 666C7420 len [ 4] idx [224]: Zone 1 Target Power (PZ1E)
 [PZ1T] type [fltf] 666C7420 len [ 4] idx [225]: Zone 1 Abstract Throttle (PZ1T)
 [PZ2F] type [fltf] 666C7420 len [ 4] idx [226]: Zone 2 Filtered Power (PZ2F)
 [PZ2E] type [fltf] 666C7420 len [ 4] idx [227]: Zone 2 Target Power (PZ2E)
 [PZ2T] type [fltf] 666C7420 len [ 4] idx [228]: Zone 2 Abstract Throttle (PZ2T)
 [MSTc] type [ui8u] 75693820 len [ 1] idx [240]: CPU Plimit (MSTc)
 [MSTg] type [ui8u] 75693820 len [ 1] idx [241]: GPU Plimit (MSTg)
 [MSTf] type [ui8u] 75693820 len [ 1] idx [244]: Forced Idle Limit (MSTf)
 Set 1 has 34 keys:
 [TC0P] type [sp7s] 73703738 len [ 2] idx [  1]: CPU proximity temp (DegC) (TC0P)
 [TM0P] type [sp7s] 73703738 len [ 2] idx [  2]: Memory proximity (DegC) (TM0P)
 [TCHP] type [sp7s] 73703738 len [ 2] idx [  3]: Charger proximity temp  (DegC) (TCHP)
 [TW0P] type [sp7s] 73703738 len [ 2] idx [  4]: Wireless proximity (DegC) (TW0P)
 [Ts0P] type [sp7s] 73703738 len [ 2] idx [  5]: Trackpad Temp (DegC) (Ts0P)
 [Ts1P] type [sp7s] 73703738 len [ 2] idx [  6]: Actuator Temp (DegC) (Ts1P)
 [Th0N] type [sp7s] 73703738 len [ 2] idx [  7]: Nand temp  (DegC) (Th0N)
 [TPCD] type [sp7s] 73703738 len [ 2] idx [  8]: PCH Die temp (DegC) (TPCD)
 [Th0R] type [sp7s] 73703738 len [ 2] idx [  9]: RIO temp  (DegC) (Th0R)
 [TCXC] type [sp7s] 73703738 len [ 2] idx [ 10]: CPU Core PECI temp (DegC) (SIS! force bit 7) (TCXC)
 [PCPT] type [sp7s] 73703738 len [ 2] idx [ 11]: CPU package total power (PECI) (Watts) (PCPT)
 [PCPC] type [sp7s] 73703738 len [ 2] idx [ 12]: CPU package core power (PECI) (Watts) (PCPC)
 [PCPG] type [sp7s] 73703738 len [ 2] idx [ 13]: CPU package Gfx power (PECI) (Watts) (PCPG)
 [TC1C] type [sp7s] 73703738 len [ 2] idx [ 14]: CPU Core 0 temp (PECI) (DegC) (TC1C)
 [TC2C] type [sp7s] 73703738 len [ 2] idx [ 15]: CPU Core 1 temp (PECI) (DegC) (TC2C)
 [TCGC] type [sp7s] 73703738 len [ 2] idx [ 16]: CPU Gfx Core temp (PECI) (DegC) (TCGC)
 [TCSA] type [sp7s] 73703738 len [ 2] idx [ 17]: CPU System Agent Core temp (PECI) (DegC) (TCSA)
 [TH0a] type [sp7s] 73703738 len [ 2] idx [ 18]: Drive 0 OOBv3 raw temp A (DegC) (TH0a)
 [TBXT] type [sp7s] 73703738 len [ 2] idx [ 21]: Battery temp (Same as TB0T) (DegC) (TBXT)
 [Ts0S] type [sp7s] 73703738 len [ 2] idx [ 22]: Synthetic bottom skin (DegC) (Ts0S)
 [TCMX] type [sp7s] 73703738 len [ 2] idx [ 23]: Max PECI reported temp  (DegC) (TCMX)
 [TC0E] type [sp7s] 73703738 len [ 2] idx [ 24]: CPU die Virtual temp (DegC) (TC0E)
 [TC0F] type [sp7s] 73703738 len [ 2] idx [ 26]: CPU PECI die temp filtered then adjusted (DegC) (TC0F)
 [IBAC] type [sp7s] 73703738 len [ 2] idx [ 27]: Battery Current (IBAC)
 [TH0A] type [sp7s] 73703738 len [ 2] idx [ 28]: Drive 0 OOBv3 cooked temp A (DegC) (TH0A)
 [TH0R] type [sp7s] 73703738 len [ 2] idx [ 31]: Drive 0 OOBv3 relative cooked temp Max (DegC) (TH0R)
 [TH0V] type [sp7s] 73703738 len [ 2] idx [ 32]: Drive 0 backup virtual DRAM temp (DegC) (TH0V)
 [TH0F] type [sp7s] 73703738 len [ 2] idx [ 33]: Drive 0 OOBv3 relative filtered temp Max (DegC) (TH0F)
 [PSTR] type [sp7s] 73703738 len [ 2] idx [239]: System Total Power Consumed (Delayed 1 Second) (Watts) (PSTR)
 [B0FC] type [ui1u] 75693136 len [ 2] idx [240]: Battery full charge capacity. (mAh) (B0FC)
 [B0RM] type [ui1u] 75693136 len [ 2] idx [241]: Battery remain capacity. (mAh) (B0RM)
 [CHBI] type [ui1u] 75693136 len [ 2] idx [242]: Battery charge current. (mAh) (CHBI)
 [B0AC] type [si1s] 73693136 len [ 2] idx [243]: Battery Actual current. (A) (B0AC)
 [B0AV] type [ui1u] 75693136 len [ 2] idx [244]: Battery Actual Voltage. (V) (B0AV)
