/*
 * Intel ACPI Component Architecture
 * AML/ASL+ Disassembler version 20180427 (64-bit version)(RM)
 * Copyright (c) 2000 - 2018 Intel Corporation
 * 
 * Disassembling to symbolic ASL+ operators
 *
 * Disassembly of /Volumes/EFI/EFI/OC/ACPI/SSDT-MEM2.aml, Sat Nov 14 15:43:02 2020
 *
 * Original Table Header:
 *     Signature        "SSDT"
 *     Length           0x00000088 (136)
 *     Revision         0x02
 *     Checksum         0x6A
 *     OEM ID           "OCLT"
 *     OEM Table ID     "MEM2"
 *     OEM Revision     0x00000000 (0)
 *     Compiler ID      "INTL"
 *     Compiler Version 0x20200110 (538968336)
 */
DefinitionBlock ("", "SSDT", 2, "OCLT", "MEM2", 0x00000000)
{
    Device (MEM2)
    {
        Name (_HID, EisaId ("PNP0C01"))  // _HID: Hardware ID
        Name (_UID, 0x02)  // _UID: Unique ID
        Name (CRS, ResourceTemplate ()
        {
            Memory32Fixed (ReadWrite,
                0x20000000,         // Address Base
                0x00200000,         // Address Length
                )
            Memory32Fixed (ReadWrite,
                0x40000000,         // Address Base
                0x00200000,         // Address Length
                )
        })
        Method (_CRS, 0, NotSerialized)  // _CRS: Current Resource Settings
        {
            Return (CRS)
        }

        Method (_STA, 0, NotSerialized)  // _STA: Status
        {
            If (_OSI ("Darwin"))
            {
                Return (0x0F)
            }
            Else
            {
                Return (Zero)
            }
        }
    }
}

