[
{"data":{"title":"IOReportLegend"},"attr":{"id":"8651","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8652","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"8654","ColType":"String","ColValue":"PWRB 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"8656","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8657","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8658","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"8659","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8660","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"8661","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8662","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"8663","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8664","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"8665","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8666","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"8667","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8668","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"8669","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8670","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"8671","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8672","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"8673","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8674","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"8675","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8676","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"8678","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"8680","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"8682","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"8684","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8685","ColType":"Data","ColValue":"&lt;0200000000000000&gt;"}}]},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"8687","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"8689","ColType":"Data","ColValue":"&lt;\"PNP0C0C\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"8691","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"8693","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8694","ColType":"String","ColValue":"ACPIEventController"}}]},
{"data":{"title":"_STA"},"attr":{"id":"8696","ColType":"Number","ColValue":"15"}}
]
