[
{"data":{"title":"built-in"},"attr":{"id":"9272","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"9274","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9275","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9276","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"9278","ColType":"Number","ColValue":"3978297344"}},{"data":{"title":"length"},"attr":{"id":"9280","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"9282","ColType":"Data","ColValue":"&lt;04a80000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"9284","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"9286","ColType":"Data","ColValue":"&lt;\"pci144d,a804\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"9288","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP09@1d0000/PXSX@0"}},
{"data":{"title":"IOName"},"attr":{"id":"9290","ColType":"String","ColValue":"pci144d,a804"}},
{"data":{"title":"vendor-id"},"attr":{"id":"9292","ColType":"Data","ColValue":"&lt;4d140000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"9294","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"9296","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"9298","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"9300","ColType":"Data","ColValue":"&lt;4d140000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"9302","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9303","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"9304","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"9306","ColType":"Number","ColValue":"4683843"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"9308","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9309","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"9311","ColType":"String","ColValue":"PXSX 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"9313","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9314","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9315","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"9316","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9317","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"9318","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9319","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"9320","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9321","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"9322","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9323","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"9324","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9325","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"9326","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9327","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"9328","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9329","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"9330","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9331","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"9332","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9333","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"9335","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"9337","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"9339","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"9341","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"9343","ColType":"String","ColValue":"65:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"9345","ColType":"Number","ColValue":"4131"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"9347","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"9349","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"9351","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"9353","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"9355","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"9357","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"9359","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"9361","ColType":"Data","ColValue":"&lt;02080100&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"9363","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"9365","ColType":"Data","ColValue":"&lt;\"pci144d,a801\",\"pci144d,a804\",\"pciclass,010802\",\"PXSX\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"9367","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"9369","ColType":"Data","ColValue":"&lt;01a80000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"9371","ColType":"Data","ColValue":"&lt;1000418200000000000020ed0000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"9373","ColType":"Data","ColValue":"&lt;00004100000000000000000000000000000000001000410200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"9375","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9376","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"9377","ColType":"Data","ColValue":"&lt;0a00000000000100&gt;"}}]}
]
