[
{"data":{"title":"PinConfigurations"},"attr":{"id":"3850","ColType":"Data","ColValue":"&lt;&gt;"}},
{"data":{"title":"@3,connector-type"},"attr":{"id":"3852","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"3854","ColType":"Data","ColValue":"&lt;1001018200000000000008ed0000000000400000&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"3856","ColType":"String","ColValue":"1:0:1"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"3858","ColType":"Number","ColValue":"3"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"3860","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3861","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"3862","ColType":"Data","ColValue":"&lt;0200000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"3864","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/PEG0@10000/HDAU@1"}},
{"data":{"title":"DigitalAudioCapabilities"},"attr":{"id":"3866","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"HDMI"},"attr":{"id":"3868","ColType":"Number","ColValue":"1"}},{"data":{"title":"DisplayPort"},"attr":{"id":"3870","ColType":"Number","ColValue":"1"}}]},
{"data":{"title":"layout-id"},"attr":{"id":"3872","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"3874","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3875","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"3876","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"3878","ColType":"Number","ColValue":"2"}},
{"data":{"title":"@0,connector-type"},"attr":{"id":"3880","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"3882","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"3884","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"3886","ColType":"Data","ColValue":"&lt;42380000&gt;"}},
{"data":{"title":"@2,connector-type"},"attr":{"id":"3888","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"3890","ColType":"Data","ColValue":"&lt;de100000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"3892","ColType":"Data","ColValue":"&lt;\"pci10de,10f1\"&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"3894","ColType":"Data","ColValue":"&lt;\"pci3842,6262\",\"pci10de,10f1\",\"pciclass,040300\",\"HDAU\",\"HDAU\",\"HDAU\",\"HDAU\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"3896","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"3898","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"3900","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"3902","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"3904","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"3906","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"3908","ColType":"Data","ColValue":"&lt;a1000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"3910","ColType":"Number","ColValue":"4537603"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"3912","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"built-in"},"attr":{"id":"3914","ColType":"Data","ColValue":"&lt;01&gt;"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"3916","ColType":"Number","ColValue":"4353"}},
{"data":{"title":"hda-gfx"},"attr":{"id":"3918","ColType":"Data","ColValue":"&lt;\"onboard-2\"&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"3920","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3921","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3922","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"3924","ColType":"Number","ColValue":"3976724480"}},{"data":{"title":"length"},"attr":{"id":"3926","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"IOName"},"attr":{"id":"3928","ColType":"String","ColValue":"pci10de,10f1"}},
{"data":{"title":"acpi-device"},"attr":{"id":"3930","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"3932","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"3934","ColType":"Data","ColValue":"&lt;62620000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"3936","ColType":"Data","ColValue":"&lt;00010100000000000000000000000000000000001001010200000000000000000000000000400000&gt;"}},
{"data":{"title":"@1,connector-type"},"attr":{"id":"3938","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"3940","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3941","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"3943","ColType":"String","ColValue":"HDAU 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"3945","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3946","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3947","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"3948","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3949","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"3950","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3951","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"3952","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3953","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"3954","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3955","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"3956","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3957","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"3958","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3959","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"3960","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3961","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"3962","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"3963","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"3964","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"3965","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"3967","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"3969","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"3971","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"3973","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"3975","ColType":"Data","ColValue":"&lt;f1100000&gt;"}}
]
