[
{"data":{"title":"built-in"},"attr":{"id":"85596","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"85598","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85599","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85600","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"85602","ColType":"Number","ColValue":"3978297344"}},{"data":{"title":"length"},"attr":{"id":"85604","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"85606","ColType":"Data","ColValue":"&lt;04a80000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"85608","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"85610","ColType":"Data","ColValue":"&lt;\"pci144d,a804\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"85612","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP09@1d0000/PXSX@0"}},
{"data":{"title":"IOName"},"attr":{"id":"85614","ColType":"String","ColValue":"pci144d,a804"}},
{"data":{"title":"vendor-id"},"attr":{"id":"85616","ColType":"Data","ColValue":"&lt;4d140000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"85618","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"85620","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"85622","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"85624","ColType":"Data","ColValue":"&lt;4d140000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"85626","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85627","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"85628","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"85630","ColType":"Number","ColValue":"4683843"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"85632","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85633","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"85635","ColType":"String","ColValue":"PXSX 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"85637","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85638","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85639","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"85640","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"85641","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"85642","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85643","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"85644","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"85645","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"85646","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85647","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"85648","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"85649","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"85650","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85651","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"85652","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"85653","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"85654","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85655","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"85656","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"85657","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"85659","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"85661","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"85663","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"85665","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"85667","ColType":"String","ColValue":"65:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"85669","ColType":"Number","ColValue":"4131"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"85671","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"85673","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"85675","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"85677","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"85679","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"85681","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"85683","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"85685","ColType":"Data","ColValue":"&lt;02080100&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"85687","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"85689","ColType":"Data","ColValue":"&lt;\"pci144d,a801\",\"pci144d,a804\",\"pciclass,010802\",\"PXSX\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"85691","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"85693","ColType":"Data","ColValue":"&lt;01a80000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"85695","ColType":"Data","ColValue":"&lt;1000418200000000000020ed0000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"85697","ColType":"Data","ColValue":"&lt;00004100000000000000000000000000000000001000410200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"85699","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"85700","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"85701","ColType":"Data","ColValue":"&lt;0a00000000000100&gt;"}}]}
]
