00:00.0 Host bridge: Intel Corporation Device 591f (rev 05)
00:01.0 PCI bridge: Intel Corporation Skylake PCIe Controller (x16) (rev 05)
## 00.01:0 is a bridge from 00 to 01-01
00:08.0 System peripheral: Intel Corporation Skylake Gaussian Mixture Model
00:14.0 USB controller: Intel Corporation Device a2af
00:16.0 Communication controller: Intel Corporation Device a2ba
00:17.0 SATA controller: Intel Corporation Device a282
00:1b.0 PCI bridge: Intel Corporation Device a2e7 (rev f0)
## 00.1b:0 is a bridge from 00 to 02-02
00:1b.2 PCI bridge: Intel Corporation Device a2e9 (rev f0)
## 00.1b:2 is a bridge from 00 to 03-03
00:1b.4 PCI bridge: Intel Corporation Device a2eb (rev f0)
## 00.1b:4 is a bridge from 00 to 04-04
00:1c.0 PCI bridge: Intel Corporation Device a290 (rev f0)
## 00.1c:0 is a bridge from 00 to 05-05
00:1c.1 PCI bridge: Intel Corporation Device a291 (rev f0)
## 00.1c:1 is a bridge from 00 to 06-06
00:1c.2 PCI bridge: Intel Corporation Device a292 (rev f0)
## 00.1c:2 is a bridge from 00 to 07-07
00:1c.4 PCI bridge: Intel Corporation Device a294 (rev f0)
## 00.1c:4 is a bridge from 00 to 08-0d
00:1d.0 PCI bridge: Intel Corporation Device a298 (rev f0)
## 00.1d:0 is a bridge from 00 to 41-41
00:1d.2 PCI bridge: Intel Corporation Device a29a (rev f0)
## 00.1d:2 is a bridge from 00 to 42-42
00:1d.5 PCI bridge: Intel Corporation Device a29d (rev f0)
## 00.1d:5 is a bridge from 00 to 43-43
00:1f.0 ISA bridge: Intel Corporation Device a2c5
00:1f.2 Memory controller: Intel Corporation Device a2a1
00:1f.3 Audio device: Intel Corporation Device a2f0
00:1f.4 SMBus: Intel Corporation Device a2a3
00:1f.6 Ethernet controller: Intel Corporation Ethernet Connection (2) I219-V
01:00.0 VGA compatible controller: NVIDIA Corporation GP106 [GeForce GTX 1060 6GB] (rev a1)
01:00.1 Audio device: NVIDIA Corporation Device 10f1 (rev a1)
05:00.0 FireWire (IEEE 1394): LSI Corporation FW643 [TrueFire] PCIe 1394b Controller (rev 08)
07:00.0 Ethernet controller: Qualcomm Atheros Device e0b1 (rev 10)
08:00.0 PCI bridge: Intel Corporation JHL6540 Thunderbolt 3 Bridge (C step) [Alpine Ridge 4C 2016] (rev 02)
## 08.00:0 is a bridge from 08 to 09-0d
09:00.0 PCI bridge: Intel Corporation JHL6540 Thunderbolt 3 Bridge (C step) [Alpine Ridge 4C 2016] (rev 02)
## 09.00:0 is a bridge from 09 to 0d-0d
09:01.0 PCI bridge: Intel Corporation JHL6540 Thunderbolt 3 Bridge (C step) [Alpine Ridge 4C 2016] (rev 02)
## 09.01:0 is a bridge from 09 to 0c-0c
09:02.0 PCI bridge: Intel Corporation JHL6540 Thunderbolt 3 Bridge (C step) [Alpine Ridge 4C 2016] (rev 02)
## 09.02:0 is a bridge from 09 to 0b-0b
09:04.0 PCI bridge: Intel Corporation JHL6540 Thunderbolt 3 Bridge (C step) [Alpine Ridge 4C 2016] (rev 02)
## 09.04:0 is a bridge from 09 to 0a-0a
0b:00.0 USB controller: Intel Corporation Device 15d4 (rev 02)
41:00.0 Non-Volatile memory controller: Samsung Electronics Co Ltd Device a804
43:00.0 Network controller: Qualcomm Atheros AR93xx Wireless Network Adapter (rev 01)
82:0e.0 Unassigned class [ffff]: Illegal Vendor ID Device ffff (rev ff)
f3:19.0 Unassigned class [ffff]: Illegal Vendor ID Device ffff (rev ff)

Summary of buses:

00: Primary host bus
	1d.5 Bridge to 43-43
	1d.2 Bridge to 42-42
	1d.0 Bridge to 41-41
	1c.4 Bridge to 08-0d
	1c.2 Bridge to 07-07
	1c.1 Bridge to 06-06
	1c.0 Bridge to 05-05
	1b.4 Bridge to 04-04
	1b.2 Bridge to 03-03
	1b.0 Bridge to 02-02
	01.0 Bridge to 01-01
01: Entered via 00:01.0
05: Entered via 00:1c.0
07: Entered via 00:1c.2
08: Entered via 00:1c.4
	00.0 Bridge to 09-0d
09: Entered via 08:00.0
	04.0 Bridge to 0a-0a
	02.0 Bridge to 0b-0b
	01.0 Bridge to 0c-0c
	00.0 Bridge to 0d-0d
0b: Entered via 09:02.0
41: Entered via 00:1d.0
43: Entered via 00:1d.5
82: Secondary host bus (?)
f3: Secondary host bus (?)
