[
{"data":{"title":"built-in"},"attr":{"id":"8488","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"8490","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8491","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8492","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"8494","ColType":"Number","ColValue":"3981443072"}},{"data":{"title":"length"},"attr":{"id":"8496","ColType":"Number","ColValue":"131072"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"8498","ColType":"Number","ColValue":"200"}},
{"data":{"title":"device-id"},"attr":{"id":"8500","ColType":"Data","ColValue":"&lt;b8150000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"8502","ColType":"Data","ColValue":"&lt;\"ethernet\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"8504","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/GLAN@1f0006"}},
{"data":{"title":"IOName"},"attr":{"id":"8506","ColType":"String","ColValue":"ethernet"}},
{"data":{"title":"vendor-id"},"attr":{"id":"8508","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"8510","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"8512","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"8514","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"acpi-device"},"attr":{"id":"8516","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"8518","ColType":"Data","ColValue":"&lt;58140000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"8520","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8521","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"8522","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOReportLegend"},"attr":{"id":"8524","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8525","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"8527","ColType":"String","ColValue":"GLAN 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"8529","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8530","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8531","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"8532","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8533","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"8534","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8535","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"8536","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8537","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"8538","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8539","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"8540","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8541","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"8542","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8543","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"8544","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8545","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"8546","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8547","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"8548","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8549","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"8551","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"8553","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"8555","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pcidebug"},"attr":{"id":"8557","ColType":"String","ColValue":"0:31:6"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"8559","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"8561","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"8563","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"8565","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"8567","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"8569","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"8571","ColType":"Data","ColValue":"&lt;00000200&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"8573","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"8575","ColType":"Data","ColValue":"&lt;\"pci1458,e000\",\"pci8086,15b8\",\"pciclass,020000\",\"GLAN\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"8577","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"8579","ColType":"Data","ColValue":"&lt;00e00000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"8581","ColType":"Data","ColValue":"&lt;10fe008200000000000050ed0000000000000200&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"8583","ColType":"Data","ColValue":"&lt;00fe00000000000000000000000000000000000010fe000200000000000000000000000000000200&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"8585","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8586","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"8587","ColType":"Data","ColValue":"&lt;0700000000000100&gt;"}}]}
]
