[
{"data":{"title":"PinConfigurations"},"attr":{"id":"4083","ColType":"Data","ColValue":"&lt;&gt;"}},
{"data":{"title":"@3,connector-type"},"attr":{"id":"4085","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"4087","ColType":"Data","ColValue":"&lt;1001018200000000000008ed0000000000400000&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"4089","ColType":"String","ColValue":"1:0:1"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"4091","ColType":"Number","ColValue":"3"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"4093","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4094","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"4095","ColType":"Data","ColValue":"&lt;0200000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"4097","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/PEG0@10000/HDAU@1"}},
{"data":{"title":"DigitalAudioCapabilities"},"attr":{"id":"4099","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"HDMI"},"attr":{"id":"4101","ColType":"Number","ColValue":"1"}},{"data":{"title":"DisplayPort"},"attr":{"id":"4103","ColType":"Number","ColValue":"1"}}]},
{"data":{"title":"layout-id"},"attr":{"id":"4105","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"4107","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4108","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"4109","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"4111","ColType":"Number","ColValue":"2"}},
{"data":{"title":"@0,connector-type"},"attr":{"id":"4113","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"4115","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"4117","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"4119","ColType":"Data","ColValue":"&lt;42380000&gt;"}},
{"data":{"title":"@2,connector-type"},"attr":{"id":"4121","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"4123","ColType":"Data","ColValue":"&lt;de100000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"4125","ColType":"Data","ColValue":"&lt;\"pci10de,10f1\"&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"4127","ColType":"Data","ColValue":"&lt;\"pci3842,6262\",\"pci10de,10f1\",\"pciclass,040300\",\"HDAU\",\"HDAU\",\"HDAU\",\"HDAU\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"4129","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"4131","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"4133","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"4135","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"4137","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"4139","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"4141","ColType":"Data","ColValue":"&lt;a1000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"4143","ColType":"Number","ColValue":"4537603"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"4145","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"built-in"},"attr":{"id":"4147","ColType":"Data","ColValue":"&lt;01&gt;"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"4149","ColType":"Number","ColValue":"4353"}},
{"data":{"title":"hda-gfx"},"attr":{"id":"4151","ColType":"Data","ColValue":"&lt;\"onboard-2\"&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"4153","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4154","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4155","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"4157","ColType":"Number","ColValue":"3976724480"}},{"data":{"title":"length"},"attr":{"id":"4159","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"IOName"},"attr":{"id":"4161","ColType":"String","ColValue":"pci10de,10f1"}},
{"data":{"title":"acpi-device"},"attr":{"id":"4163","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"4165","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"4167","ColType":"Data","ColValue":"&lt;62620000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"4169","ColType":"Data","ColValue":"&lt;00010100000000000000000000000000000000001001010200000000000000000000000000400000&gt;"}},
{"data":{"title":"@1,connector-type"},"attr":{"id":"4171","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"4173","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4174","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"4176","ColType":"String","ColValue":"HDAU 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"4178","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4179","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4180","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"4181","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4182","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"4183","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4184","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"4185","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4186","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"4187","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4188","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"4189","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4190","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"4191","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4192","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"4193","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4194","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"4195","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4196","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"4197","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4198","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"4200","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"4202","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"4204","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"4206","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"4208","ColType":"Data","ColValue":"&lt;f1100000&gt;"}}
]
