[
{"data":{"title":"IOReportLegend"},"attr":{"id":"101232","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"101233","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"101235","ColType":"String","ColValue":"PWRB 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"101237","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"101238","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"101239","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"101240","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"101241","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"101242","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"101243","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"101244","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"101245","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"101246","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"101247","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"101248","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"101249","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"101250","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"101251","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"101252","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"101253","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"101254","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"101255","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"101256","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"101257","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"101259","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"101261","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"101263","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"101265","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"101266","ColType":"Data","ColValue":"&lt;0200000000000000&gt;"}}]},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"101268","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"101270","ColType":"Data","ColValue":"&lt;\"PNP0C0C\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"101272","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"101274","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"101275","ColType":"String","ColValue":"ACPIEventController"}}]},
{"data":{"title":"_STA"},"attr":{"id":"101277","ColType":"Number","ColValue":"15"}}
]
