+-o Root  <class IORegistryEntry, id 0x100000100, retain 13>
  | {
  |   "IOKitBuildVersion" = "Darwin Kernel Version 16.7.0: Thu Jun 15 17:36:27 PDT 2017; root:xnu-3789.70.16~2/RELEASE_X86_64"
  |   "OS Build Version" = "16G29"
  |   "IONDRVFramebufferGeneration" = <0600000006000000>
  |   "OSKernelCPUSubtype" = 3
  |   "OSKernelCPUType" = 16777223
  |   "OSPrelinkKextCount" = 275
  |   "IOConsoleLocked" = No
  |   "IORegistryPlanes" = {"IOPower"="IOPower","IOService"="IOService","IOFireWire"="IOFireWire","IO80211Plane"="IO80211Plane","CoreCapture"="CoreCapture","IOUSB"="IOUSB","IOACPIPlane"="IOACPIPlane","IODeviceTree"="IODeviceTree"}
  |   "IOConsoleUsers" = ({"kCGSSessionOnConsoleKey"=Yes,"kCGSSessionLoginwindowSafeLogin"=No,"kSCSecuritySessionID"=100007,"kCGSessionLongUserNameKey"="admin","kCGSSessionUserIDKey"=501,"kCGSSessionSystemSafeBoot"=No,"kCGSSessionUserNameKey"="admin","kCGSSessionIDKey"=257,"kCGSessionLoginDoneKey"=Yes,"kCGSSessionGroupIDKey"=20,"kCGSSessionAuditIDKey"=100007})
  |   "IOKitDiagnostics" = {"Container allocation"=5521822,"Instance allocation"=6803968,"Pageable allocation"=861177168,"Classes"={"IONDRVFramebuffer"=1,"IOKitDiagnosticsClient"=0,"IONaturalMemoryCursor"=1,"IOAudioClientBufferSet"=0,"AppleUSBDiagnostics"=0,"com_Logitech_USBInterfaceDriver"=1,"IOUSBHostHIDDevice"=2,"FakeSMCKeyHandler"=1,"IOAccelDisplayPipe2"=1,"AppleHDAMikeyInternalCS4208"=0,"AppleFWOHCI_PM_PPC"=0,"AppleUSBXHCIIsochronousRequestPool"=2,"DspFuncBuzzKill"=0,"IOFireWireDevice"=0,"AppleHDATDM_Codec"=0,"nvVirtualAddress"=732,"NVDAStartup"=0,"AppleAHCIWorkLoop"=5,"IOHDACodecDevice"=2,"CoreStorageLogical"=2,"FakeSMCDevice"=1,"IORegistryEntry"=104,"AppleAHCIPort"=5,"AppleHDAWorkLoop"=2,"IOHIDevice"=2,"IOFWUserWriteCommand"=0,"IOPCIEventSource"=0,"IO80211DriverCommandDescriptor"=0,"AppleHDAHardwareConfigDriverLoader"=0,"DspFuncUserClient"=0,"IOMemoryCursor"=2,"AppleHDATDM_CS42L81"=0,"com_Logitech_USBLogitechInterfaceDriverStd"=1,"IOBreaker"=0,"AppleHDAFunctionGroup_80862807"=0,"IOUSBLowLatencyCommandLegacy"=0,"FakeSMCKeyStore"=1,"EFIData"=124,"AppleUSBXHCIPort"=2,"IOAccelCommandQueue"=1,"DspFunc4ChOutput"=0,"nvHAL"=1,"IOBluetoothHostControllerUserClient"=0,"CoreStorageShadowDescriptor"=0,"AppleHDAFunctionGroupWM8800"=1,"AppleKeyStoreUserClient"=9,"IOSMBusRequest"=0,"IOFWUserAsyncStreamCommand"=0,"DspFuncBeamFormer"=0,"CoreStorageMemoryDescriptor"=1152,"AppleACPILid"=0,"IOPMServiceInterestNotifier"=95,"AppleUpstreamUserClientDriver"=6,"IOHIDResourceQueue"=0,"IOStorage"=5,"IOFWAddressSpaceAux"=2,"IOAccelSegmentResourceList"=0,"CoreStorageFamily"=2,"IOSerialStreamSync"=1,"IOHIDConsumer"=0,"IO80211AWDLMulticastPeer"=0,"AppleUSBHostCompositeDevice"=3,"IOAHCIBlockStorageDevice"=4,"IOSharedInterruptController"=4,"IOHIDClientData"=11,"IOBluetoothMemoryDescriptorRetainer"=0,"IOGraphicsWorkLoop"=2,"hv_vmx_vm_t"=0,"AppleHDATDMBusManagerCS4208"=0,"OSSerializer"=78,"nvDevice"=22,"IOPCIMessagedInterruptController"=1,"IOUserEthernetResourceUserClient"=0,"AppleAHCIWatchdogTimer"=4,"OSCollection"=5,"IOUSBDeviceUserClientV2"=1,"IOFWPhysicalAddressSpaceAux"=0,"AppleHDAEngineOutput"=4,"AppleFWOHCI_DCLPool"=0,"nvMemory"=1,"_IOServiceNullNotifier"=1,"ACPIProbeProfile"=0,"AppleFWOHCI_CallbackContainer"=1,"IntelGraphicsFixup"=1,"IOBluetoothHCIUserClient"=0,"com_apple_driver_pm_cpu_reporter"=0,"IONetworkStackUserClient"=1,"AppleDisplay"=1,"IOBluetoothHostController"=0,"IOInterleavedMemoryDescriptor"=0,"_IOServiceNotifier"=361,"AppleHDAFunctionGroupGT216"=0,"AppleGraphicsDevicePolicy"=1,"IOFireWireController"=1,"AppleHDAFunctionGroupCS4208"=0,"DspFuncVolume_4ch"=0,"AppleUSBXHCILPTCommandRing"=0,"IOUSBHostDevice"=5,"IOSubMemoryDescriptor"=13,"IOBluetoothL2CAPSignalChannel"=0,"nvTextureBuffer"=528,"IOAHCIPortInterface"=1,"IOServiceUserNotification"=286,"AppleFDEKeyStoreUserClient"=0,"IO80211PacketDescriptor"=0,"DspFuncPreGain"=0,"IOAccelDevice2"=1,"AtherosNewma40WorkLoop"=0,"DigitizerTransducer"=0,"IOAccelCLContext2"=1,"IOBluetoothL2CAPInformationFrameMemoryBlock"=0,"IOMbufMemoryCursor"=1,"AppleHDAController"=2,"IOSKMemoryArray"=0,"IOCPU"=1,"AppleBusPowerControllerSMC"=0,"IOAccelEventMachineFast2"=1,"IOFWUserPseudoAddressSpace"=0,"AppleACPIEventPoller"=1,"FakeSMCKey"=70,"IO80211ActionFrameDescriptor"=0,"IONetworkStack"=1,"nvDisplayPipe"=6,"CCDataPipeBlob"=0,"ApplePlatformEnabler"=1,"AppleFWOHCI_SendDCL"=0,"DspFuncBiquad"=0,"CSRBluetoothHostController"=0,"AppleHDAFunctionGroupATI_RS710"=0,"IO80211Interface"=1,"IOSimpleReporter"=69,"AppleUSBXHCILPTHB"=0,"IOModemSerialStreamSync"=0,"AppleHDATDM_CS42L83"=0,"IOHDIXControllerUserClient"=0,"AppleALC"=1,"com_apple_AppleFSCompression_AppleFSCompressionTypeZlib"=1,"AppleHDATDMAmpMAX98706"=0,"DspFunc2Dot2Crossover"=0,"IOFireWireNubAux"=1,"AppleAHCIEventSource"=5,"org_rehabman_USBInjectAll"=0,"IOUSBInterface"=1,"IOAccelChannel2"=1,"AppleUSBLegacyRoot"=1,"IOFireWireBusAux"=1,"CCFaultReporter"=0,"AppleUSBHostRequestPool"=2,"AppleCSRBluetoothHostController"=0,"IOConfigEntry"=13,"AppleHDAPathControl"=10,"IOFWReadCommand"=0,"AGPMClient"=0,"AppleHDATDMAmpTAS5764L"=0,"IOBluetoothRFCOMMChannelUserClient"=0,"IOSCSIPrimaryCommandsDevice"=1,"AppleNVMeWorkLoop"=1,"IOAHCIPollerInterface"=1,"AppleSMBusControllerMCP"=0,"IOHIDProviderPropertyMerger"=0,"IOUSBDevice"=1,"AppleFWOHCI_DCLProgram"=0,"IOAccelVidMemory"=1,"AppleHDAEngineInput"=1,"IOAccelDisplayPipeTransaction2"=0,"com_Logitech_USBMouseHPP"=0,"IOHIDKeyboard"=0,"com_Logitech_TCommand"=0,"AppleSATAExpress"=0,"IOACPIPlatformDevice"=183,"_IOServiceInterestNotifier"=158,"AppleUSBHostRequestCompleter"=7,"IOBluetoothLocalUtilityEventSource"=0,"IOFramebufferI2CInterface"=6,"IOPowerConnection"=131,"IOBluetoothSerialClientModemStreamSync"=0,"SCSITaskUserClient"=1,"nvGpFifoChannelInterface"=28,"IOWatchDogTimer"=2,"IOEventSource"=18,"IODMACommand"=237,"IOFWAsyncStreamReceiver"=0,"IOMachPort"=901,"IOPMinformeeList"=144,"AppleCredentialManager"=1,"AppleUSB30XHCITypeCPort"=0,"AppleACPIPowerResource"=0,"CCLogStream"=1,"nvSemaphoreManager"=12,"AppleUSBHostControllerIsochEndpoint"=0,"nvMaxwellHAL"=1,"IOHIDEvent"=0,"IOAccelTask"=1,"DspFuncNoiseCanceller"=0,"OSDictionary"=13883,"IOAccelGLContext2"=1,"nvHandleManager"=3,"IOAGPDevice"=0,"IOHDACodecDeviceUserClient"=0,"AppleUSBXHCIParkingCommandRing"=0,"AppleFDEKeyStore"=1,"IODisplayWrangler"=1,"nvAccelerator"=1,"AppleUSBIORequest"=40,"LPCSensors"=1,"CoreStorage"=1,"IOUSBPipeV2"=1,"AppleUSBHostLegacyClient"=5,"DspFuncFIRdirect"=0,"IOFWSyncer"=0,"AppleHDATDMSinkDevice"=0,"Dont_Steal_Mac_OS_X"=1,"IOAudioTimeIntervalFilterIIR"=0,"IOHIDEventSource"=9,"AppleHVClient"=0,"OSSet"=1623,"AppleFWOHCI_MultiIsochReceiver"=1,"F718xxSensors"=0,"AppleNVMeRequestPool"=1,"IOFWUserCompareSwapCommand"=0,"IOAccelBlockFence"=0,"DspFuncCalibrationEQ"=0,"AppleUSB30XHCICardReaderPort"=0,"IOAudioEngineUserClient"=58,"AGPMHeuristic4"=0,"AppleUSBHostPacketFilterService"=1,"nvGpFifoBuffer"=28,"IORegistryDescriptorC1"=3,"AppleHDAWidget_80862805"=0,"DspFuncChOutput"=0,"IOFWDCLPool"=0,"AppleAHCIDiskDriver"=4,"IOFireWireDeviceAux"=0,"nvStatistics"=1,"IOCommand"=138,"AppleHDAWidgetAD1984"=0,"IOAudioTimerEvent"=0,"CCDataPipe"=1,"DspPatchPoint"=0,"IOSCSIProtocolInterface"=2,"AppleUSBXHCIAR"=1,"com_Logitech_HIPointing"=4,"IOBluetoothGamepadHIDDriver"=0,"AppleHDAFunctionGroupALC885"=0,"AppleHDAFunctionGroup"=2,"AppleHDAFunctionGroupExternalControl"=1,"IOGUIDPartitionScheme"=5,"AppleHDANode"=2,"OSCollectionIterator"=33,"AppleEFIRuntime"=1,"IOFWUserPHYPacketListener"=0,"nv2DContext"=6,"IOFilterScheme"=0,"AppleMCCSIOController"=12,"AppleUSBHostResources"=1,"IONVMeController"=1,"AppleAHCIRequestTimer"=4,"IOFireWireDuplicateGUIDList"=1,"IOApplePartitionScheme"=0,"IOSurfaceRootUserClient"=15,"IO80211PeerExtendedStats"=0,"IODisplay"=1,"IOFWUserPhysicalAddressSpace"=0,"IOFWRingBufferQ"=0,"AppleFWOHCI_ReceiveDCL"=0,"TDMConfig"=0,"IOHIDAsyncReportQueue"=0,"IOUserEthernetResource"=1,"IOBasicOutputQueue"=3,"NCT677xSensors"=0,"AppleHDACodec"=1,"AppleS3ELabController"=0,"AppleUSBHostControllerListElement"=0,"IOAccelSharedUserClient2"=1,"IOFramebufferSharedUserClient"=1,"IOPacketQueue"=0,"IOUSBControllerIsochListElement"=0,"IOUserClient"=29,"IOHITabletPointer"=0,"nvMemoryManagerDevice"=0,"AppleBusPowerControllerUSB"=0,"AppleUSBHostControllerIsochListElement"=0,"com_Logitech_HIDeviceUserClient"=1,"IOHIDEventSystemUserClient"=1,"AppleHDAWidgetFactory"=0,"IOHDIXHDDrive"=0,"AGPM"=1,"nvPushBuffer"=1,"IO80211AWDLPeer"=0,"IOAccelEventMachine2"=1,"IOSlaveRelayCommandPool"=0,"IOAccelBufferMemoryDescriptorPool2"=0,"DspFunc3ChOutput"=0,"AppleMCCSControlModule"=6,"IOUSBHostPipe"=1,"IOFWUserVectorCommand"=0,"IOPolledFilePollers"=0,"PTIDSensors"=1,"IOAccelDisplayMachine2"=1,"IOHDIXHDDriveOutKernelUserClient"=0,"IOUSBNotification"=0,"AppleHDAWidgetSTAC9220"=0,"AppleHDAMikeyInternal"=0,"IOUSBInterfaceUserClient"=0,"IOAccelGPURestartReport2"=0,"IOFramebufferParameterHandler"=6,"IOSurface"=61,"IOGatedOutputQueue"=12,"AppleUSBRootHubDevice"=1,"AppleHDAFunctionGroupMCP89"=0,"IOReportLegend"=2,"AppleUSBHostDescriptor"=21,"AppleUSBXHCIEndpoint"=8,"IOHIDEventQueue"=0,"IOAccelShared2"=1,"IOSurfaceSendRight"=0,"AppleAPICInterruptController"=1,"AppleSMC"=1,"IOCommandPool"=9,"IOFWLocalIsochPort"=0,"IOBlockStorageDevice"=3,"IORegistryDescriptorC4"=1,"AGPMHeuristic"=0,"com_Logitech_USBMouse"=1,"IOPMrootDomain"=1,"IOAccelFenceMachine"=1,"IODVDServices"=1,"AppleUSBNetworkingCommandPool"=0,"IO80211VirtualInterfaceNamer"=1,"IOFWSimpleContiguousPhysicalAddressSpace"=0,"IOUSBDeviceUserClient"=1,"IOI2CInterfaceUserClient"=0,"AppleHDAFunctionGroupAD1984"=0,"DspFuncControlFreak"=0,"IOHDIXCommandQueue"=0,"_IOOpenServiceIterator"=0,"IOFWUserObjectExporter"=1,"IOCommandGate"=384,"EventElementCollection"=0,"IOFWReceiveDCL"=0,"DspParameter"=0,"AppleUSBNetworkingHostCommandPool"=0,"IOPMRequestQueue"=2,"IOBDMedia"=0,"W836xxSensors"=0,"IOBlockStorageDriver"=6,"nvMemoryManagerWorkingSet"=0,"AppleHDAWidgetALC262"=0,"DspFuncThermalSpeakerProtection"=0,"IOHIDWorkLoop"=1,"nvDisplayPipeTransaction"=0,"AppleACPIACAdapter"=0,"IOUSBInterfaceIterator"=0,"IOConfigDirectoryIterator"=0,"IODTPlatformExpert"=1,"IOAppleLabelScheme"=0,"AppleHDAControllerUserClient"=0,"IOHIDEventSystemQueue"=0,"IOMbufBigMemoryCursor"=0,"AppleUSBXHCICommandRing"=2,"AppleUSBXHCIIsochronousEndpoint"=0,"AppleUSBXHCIPCI"=2,"IOFWSendDCL"=0,"AppleUSBXHCIInterrupter"=6,"IOBluetoothMemoryBlock"=0,"nvMemoryMap"=732,"IO80211Peer"=0,"RootDomainUserClient"=70,"DspFuncSplineLimiter"=0,"IOFWPseudoAddressSpace"=2,"DspFuncMozartCompressorDualBand"=0,"IONDRV"=0,"AppleSATAExpressPort"=0,"IOPCIDevice"=33,"AppleUSB20XHCIPort"=15,"IOBluetoothInactivityTimerEventSource"=0,"OSNumber"=13107,"IOAccelMemoryAllocator2"=0,"CCFaultReport"=0,"IOAHCIDiskQueueManager"=1,"Lock"=0,"AppleHDAFunctionGroupExternalControl_VirtualGPO"=2,"AtherosNewma40Interface"=1,"AppleUSBXHCI"=1,"nvTraceStream"=1,"AppleBroadcomBluetoothHostController"=0,"AppleHDAFunctionGroup_1002AAA0"=0,"IOUserNotification"=2,"AppleIntelPchSeriesAHCIPort"=0,"IOHIDKeyboardDevice"=0,"IOFWAsyncCommand"=1,"com_Logitech_HIDEventService"=0,"IOHDAStream"=5,"IOBluetoothRFCOMMMemoryBlock"=0,"AppleUSBXHCILPT"=0,"com_apple_AppleFSCompression_AppleFSCompressionTypeDataless"=1,"AGPMHeuristic3"=0,"IOFireWireIRM"=1,"nvCudaContext"=0,"AppleUSBXHCITransferRing"=8,"AppleHDAFunctionGroupATI_Broadway"=0,"IOFireWireUserClient"=0,"org_rehabman_USBInjectAll_config"=1,"IOUSBHubDevice"=0,"AppleUSBHostDeviceIdler"=5,"IORemoteConfigDirectory"=0,"IOPMWorkQueue"=1,"com_Logitech_USBLogitechInterfaceDriver"=1,"AppleUSB30XHCIPort"=7,"AppleSMBusControllerUserClient"=0,"IOSlaveProcessorUSBHostRelay"=0,"IODeblocker"=0,"AppleRTC"=1,"AppleUSBXHCISPT"=1,"IOAccelDeviceShmem"=65,"nvDisplayManager"=1,"com_Logitech_HIDEventServiceUserClient"=0,"X86PlatformShim"=1,"IOSharedDataQueue"=7,"nvSPIService"=1,"IOSyncer"=0,"CoreStorageDaemon"=0,"nvShared"=22,"nvPageTableMapping"=226,"IORangeAllocator"=2,"IOMediaBSDClient"=24,"OSBoolean"=2,"IOFWWorkLoop"=1,"AppleUSBXHCIRequest"=12,"CoreStorageGroup"=2,"IOAccelSubmitter2"=2,"nvVideoContext"=0,"IOWorkQueue"=3,"ApplePlatformEnablerUserClient"=0,"DspFuncAutoGainControl"=0,"IOMapper"=0,"nvVidMemory"=276,"LogManagerDevice"=3,"IOPCI2PCIBridge"=16,"IOAppleBluetoothHIDDriver"=0,"IOSurfaceRoot"=1,"IOHIDSystem"=1,"AppleACPIInterruptLink"=0,"IOUSBInterfaceUserClientV3"=0,"IOHIDInterface"=9,"com_apple_BootCache"=1,"nvKeplerSharedPixels"=1,"IOUSBHostStream"=0,"IOAccelRangeAllocator"=0,"IOFWAddressSpace"=2,"IOUSBController"=1,"IOAccelFIFOChannel2"=0,"AppleFWOHCI_AsyncReceive"=2,"AppleHDAWidgetATI_Park"=0,"AppleHDAFunctionGroupATI_RS730"=0,"AppleACPICPU"=8,"AppleMCCSControlFamily"=1,"com_Logitech_HIKeyboard"=1,"IONetworkInterface"=2,"KernelRelay"=0,"IOBluetoothACLMemoryDescriptor"=0,"IONetworkUserClient"=0,"IOReportUserClient"=2,"DspFunc2To4Splitter"=0,"AppleUSBXHCIPipe"=8,"DspFuncDRC"=0,"IOHDACodecFunction"=2,"IOCharacterDevice"=3,"IOUSBNub"=2,"nvEventManager"=1,"_IOConfigThread"=0,"AppleFWOHCI_PM"=1,"AppleHDAEngine"=2,"AppleUSBXHCIARRequest"=5,"IOFireWireIRMAllocation"=0,"IO80211FlowQueueDatabase"=2,"AppleHDAWidgetGK10X"=10,"AppleUSBHostController"=1,"IODiskImageBlockStorageDeviceOutKernel"=0,"IODVDBlockStorageDriver"=1,"nvGLContext"=1,"nvSharedPixels"=1,"AppleFWOHCI"=1,"IOCPUInterruptController"=1,"IOFireWireLocalNode"=1,"AppleHDAFunctionGroupFactory"=0,"CoreStorageLogicalBSDClient"=2,"IO80211P2PInterface"=1,"CCLogPipeUserClient"=0,"AppleHDAFunctionGroupALC262"=0,"nvGeneralDisplayLayerBaseInternal"=1,"PMHaltWorker"=0,"IOCDPartitionScheme"=0,"AppleHDATDMDevice"=0,"com_Logitech_HIDEventDriver"=1,"AppleMCCSUserClient"=0,"SCSITaskUserClientIniter"=1,"nvDisplayManagerInternal"=1,"AppleUSBXHCIFL1100"=0,"AppleUpstreamUserClient"=0,"IOAudioTimeIntervalFilter"=0,"AppleAHCIDiskQueueManager"=4,"IOFWDelayCommand"=2,"IOBootFramebuffer"=0,"IOHIDResourceDeviceUserClient"=0,"IOInterruptController"=5,"DspFunc"=0,"SMCPolledInterface"=1,"AppleUSBHostResourcesClient"=1,"IOEthernetInterface"=3,"IOSerialATARequestFIS"=274,"AppleHDAFunctionGroup_80862805"=0,"AppleUSBXHCIARIsochronousRequest"=5,"AGDCPlugin"=0,"IOMbufLittleMemoryCursor"=0,"AppleHDATDMBusManager"=0,"AppleUSBHubPolicyMaker"=1,"IOConfigDirectory"=1,"IOConditionLock"=0,"IO80211WorkLoop"=1,"IOFireWirePowerManager"=1,"NVDCUserClient"=0,"IOFireWireLink"=1,"AppleHDAFunctionGroupGK10X"=1,"AppleUSBHostIORequestPool"=8,"IOUSBUserClientLegacy"=1,"IOFWWriteQuadCommand"=0,"IOFWReadQuadCommand"=0,"IOFireWireROMCache"=0,"IOAccel2DContext2"=1,"com_apple_driver_pm_pch_reporter"=1,"DspFuncMultiBandDRC"=0,"IOAccelerator"=1,"AppleNVMeBuffer"=5,"com_Logitech_BTHIDDriver_K760"=0,"PMTraceWorker"=1,"IOAudioControl"=3,"IO80211QueueCall"=1,"AppleSMBusControllerICH"=0,"IOI2CInterface"=1,"AppleHDAWidgetCS4206"=0,"IOAHCISerialATAPI"=1,"IOAccelStatistics2"=1,"IO80211QueueDescriptor"=0,"IONVMeBlockStorageDevice"=1,"AppleHDAFunctionGroupSTAC9220"=0,"IOUSBHostIOSource"=1,"IONetworkController"=2,"OSString"=8283,"IOFWAsyncPHYCommand"=0,"AppleFWOHCI_AsyncTransmitRequest"=1,"CCIOReporterHub"=4,"AppleFWOHCI_DCLProgram_U"=0,"IOUserIterator"=12,"AppleMCCSParameterHandler"=6,"DspFunc2To6Splitter"=0,"IOSortableConfigurationDescriptor"=0,"PMSettingHandle"=3,"AppleMobileFileIntegrityUserClient"=0,"AppleAHCI"=1,"AppleUSBXHCIIsochronousRequest"=6,"OSOrderedSet"=237,"IOFWSkipCycleDCL"=0,"IOFWUserLocalIsochPort"=0,"IOLocalConfigDirectory"=3,"IOCDBlockStorageDevice"=1,"IOHIDEventDriver"=9,"DspFuncClientGainAdjust"=0,"AppleFWOHCI_CycleTimeRequest"=0,"nvTimerManager"=1,"AppleUSBXHCIStream"=0,"IOAudioStream"=1,"IOStateReporter"=13,"IOAccelContext2"=3,"AppleUSBXHCIPPT"=0,"IOSerialBSDClient"=1,"AppleIntelPchSeriesAHCI"=0,"com_apple_driver_pm_flex_reporter"=0,"CPUSensors"=1,"IONotifier"=4,"AppleHPET"=1,"AGPMHeuristic2"=0,"IOBluetoothL2CAPMemoryBlock"=0,"AppleUSBPipe"=1,"IOFilterInterruptEventSource"=19,"IOLittleMemoryCursor"=0,"DspFuncGain"=0,"IOFWIsochChannel"=0,"IOFWDCL"=0,"IOHIDPointingDevice"=0,"AppleUSBXHCIWPT"=0,"_IOFramebufferNotifier"=27,"nvSPIUserClient"=1,"IOBluetoothDataQueue"=0,"IOHDAController"=1,"nvTimerAction"=8,"AppleIntelSlowAdaptiveClockingManager"=1,"AppleUSBHostRequest"=2,"IOMedia"=24,"IO80211VirtualInterface"=1,"IOHistogramReporter"=3,"IOPlatformPluginFamilyPriv"=1,"IONVMeControllerPolledAdapter"=1,"AppleHDAFunctionGroupExternalControlFactory"=0,"IO80211AWDLPeerManager"=0,"AppleSMBusDevice"=0,"IOBluetoothMemoryBlockQueue"=0,"OSSymbol"=7241,"IOAccelSurface2"=1,"IOSMBusController"=0,"IOAHCIDevice"=5,"AppleACPIPlatformExpert"=1,"IORegistryPlane"=8,"nvFermiSharedPixels"=1,"AppleFWOHCI_AsyncTransmitResponse"=1,"NVDAUser"=0,"IOHIDLibUserClient"=5,"IOFireWireMultiIsochReceivePacket"=0,"AppleUSBInterfaceIterator"=0,"IOBDBlockStorageDevice"=0,"AppleHDAFunctionGroupExternalControl_GPIO"=0,"AppleFWOHCI_IsocXmitHelperPort"=0,"AppleSMBusController"=0,"IOInterruptEventSource"=82,"AudioAUUCDriver"=4,"AppleMCP89AHCI"=0,"IO80211ServiceRequestDescriptor"=0,"OSObject"=134,"IOBluetoothSerialManager"=1,"IOFireWireBus"=1,"AppleHDAMikeyInternalCS8409"=0,"AppleFWOHCI_AsyncReceiveResponse"=1,"IOHDIXController"=1,"AppleMCP79AHCIPort"=0,"nvRingBuffer"=28,"IOMbufNaturalMemoryCursor"=7,"AppleHDAPathSet"=6,"IOKDP"=0,"CCIOReporterDataStream"=1,"IOSlaveRelayEndpoint"=0,"IORegistryDescriptorC2"=2,"IOBluetoothHIDDriver"=0,"IO80211AssociationJoinSnapshot"=1,"IOFence"=0,"AppleUSBNetworkingCommand"=0,"IOGraphicsDevice"=1,"IOUSBControllerListElement"=0,"AppleNVMeRequest"=256,"IOResources"=1,"IOAccelNamespace"=24,"AppleHDAWidgetAD1988"=0,"IOFireWireUnit"=0,"com_Logitech_HILLEventQueue"=1,"DspFuncMultiBandCompressor"=0,"com_Logitech_HIDevice"=1,"IOSCSIPeripheralDeviceNub"=1,"AirPort_AtherosNewma40"=1,"RSNSupplicant"=1,"AppleUSBXHCIARRequestPool"=1,"IOSurfaceDeviceCache"=12,"com_Logitech_USBKeyboardHPP"=0,"AGPMController"=1,"AppleUSBXHCIRequestPool"=3,"nvGeneralDisplayLayerBase"=1,"AppleGraphicsDeviceControlClient"=5,"IOUSBBus"=1,"nvSurface"=11,"IOServicePM"=144,"IOBigMemoryCursor"=0,"AppleBusControllerCS8409"=0,"IOFireWireMagicMatchingNub"=0,"AtherosNewma40P2PInterface"=1,"AppleUSBHostBusCurrentPool"=0,"AppleHDAWidgetMCP89"=0,"IOMemoryDescriptor"=3,"AppleFWOHCI_PM_x86"=1,"IOCDMediaBSDClient"=0,"AppleHDAFunctionGroupATI_RS780"=0,"IOUSBInterfaceUserClientV2"=0,"IODMAController"=0,"AppleUSBInterface"=5,"AppleMCP89AHCIPort"=0,"IOUSBControllerV3"=1,"AppleGraphicsControl"=0,"AppleS3XController"=0,"IOFWQEventSource"=1,"ACPISensors"=2,"NVDAStartupWeb"=0,"nvDisplayLayer"=1,"EventQueue"=1,"IOBluetoothSCOMemoryDescriptorRetainer"=0,"AppleAHCISerialATAPITimer"=1,"AppleHDATDMBusManagerCS8409"=0,"AGPMEventSource"=1,"DspFuncEQ"=0,"IOCatalogue"=1,"IOWorkLoop"=63,"FakeSMCPlugin"=4,"nvCommandQueue"=9,"IODataQueue"=2,"AppleFWOHCI_IRMSpace"=1,"CCIOReporterLogStream"=3,"AppleFWOHCI_KDP"=0,"IOHIDDevice"=3,"IOHDACodecDriver"=2,"AppleHDAWidgetATI_RS730"=0,"IOBluetoothL2CAPChannel"=0,"com_Logitech_HIDataQueue"=1,"nvFermiCLContext"=0,"CCStream"=2,"AppleHDAWidgetATI_RS780"=0,"IOFWAsyncStreamReceivePort"=0,"IOHIDElement"=1,"IOReportHub"=1,"DspFunc6ChOutput"=0,"nvFermiHAL"=1,"IO80211ScanManager"=1,"nvFermiGLContext"=2,"IOEthernetController"=3,"DspFuncStereoEnhancer"=0,"IOSlowAdaptiveClockingDomain"=0,"IOTimerEventSource"=168,"AppleHDAFunctionGroupCS8409"=0,"IOSerialDriverSync"=1,"IOPCIConfigurator"=1,"com_apple_filesystems_hfs_encodings"=1,"Stopwatch"=5,"IO80211NetBootNub"=0,"IOSlaveRelayCommand"=0,"DspFunc2WayCrossover"=0,"CCLogPipe"=2,"AppleSMCClient"=2,"AppleHDAWidgetGT216"=0,"IOServiceMessageUserNotification"=204,"DspFuncVolume_3ch"=0,"IOReporter"=3,"nvGpFifoChannel"=28,"AppleUSBHostBusCurrentClient"=2,"IOMultiMemoryDescriptor"=0,"IOAccelDrawable2"=0,"IOPlatformPluginFamily"=1,"IOSCSILogicalUnitNub"=0,"NVDA"=6,"IOFWPseudoAddressSpaceAux"=2,"IORegistryDescriptorC5"=4,"AppleHDAWidget_80862807"=0,"IOSCSIHierarchicalLogicalUnit"=0,"com_Logitech_USBMultimediaKeys"=0,"IOFWIsochPort"=0,"AppleHDATDMDeviceFactory"=0,"IOAccelAllocationInfo"=0,"NVDC"=1,"KDIURL"=0,"CoreStorageAdmin"=0,"IOFWCommand"=2,"AGPMHeuristic1"=0,"IOPanicPlatform"=0,"IODMAEventSource"=0,"IOSCSIMultipathedLogicalUnit"=0,"IOPlatformDevice"=4,"AppleNVMeSMARTUserClient"=0,"AppleHDAWidgetCS4208"=0,"AppleAHCIWorkLoopLock"=4,"DspFuncSum"=0,"AppleUSBHostDARTDMACommand"=0,"DspFuncStereoToMono"=0,"AppleHDATDMAmpSSM3515"=0,"AtherosNewma40Timer"=1,"IOFWUserReadCommand"=0,"AppleHDAAudioSelectorControlDP"=0,"CCCapture"=0,"IOFWUserCommand"=0,"IO80211RangingManager"=1,"nvMaxwellSharedPixels"=1,"IOBluetoothRFCOMMConnectionUserClient"=0,"IOAudioControlUserClient"=12,"DspBuffer"=10,"AppleFWOHCI_CycleTimeManager"=1,"OSSerialize"=1,"IOAudioEngine"=1,"IOAudioDevice"=1,"OSKext"=130,"IOAccelCommandBufferPool2"=0,"IOBluetoothSerialClientSerialStreamSync"=1,"AppleSMBIOS"=1,"com_apple_driver_pm_msr_reporter"=1,"IODCLProgram"=0,"AppleFWOHCI_DescriptorPool"=1,"HDMIDisplay"=0,"SMCWatchDogTimer"=1,"__GLNVEvoBasePushBuf"=1,"AppleHDAFunctionGroupAD1988"=0,"AGDPClientControl"=1,"IO80211InterfaceMonitor"=2,"_IOServiceJob"=0,"IOPMPowerStateQueue"=1,"IOBluetoothRFCOMMConnection"=0,"OSIterator"=2,"hv_vcpu_t"=0,"IOAccelerationUserClient"=1,"com_Logitech_USBMultimediaKeysHPP"=0,"IOBluetoothTimerEventSource"=0,"IOFWUserPHYCommand"=0,"AppleUSBHostBusCurrentAllocator"=22,"IOMemoryMap"=1472,"CCDataStream"=1,"DspFuncDelay"=0,"AppleAHCIDiskPolledInterface"=4,"IOAudioToggleControl"=5,"com_apple_driver_pmtelemetry"=1,"IOBluetoothHCIRequest"=0,"SCSITask"=0,"IOBluetoothL2CAPSupervisoryFrameMemoryBlock"=0,"IOHDIXHDDriveOutKernel"=0,"AppleUSBHostSynchronousRequestCompleter"=5,"AppleUSBXHCIDevice"=5,"AppleNVMeController"=0,"AppleFWOHCI_SkipCycleDCL"=0,"IO80211Controller"=1,"AppleMobileFileIntegrity"=1,"AppleHDAEngineUserClient"=0,"IOBDMediaBSDClient"=0,"AppleICH8AHCI"=0,"X86PlatformPlugin"=1,"AppleHDAFunctionGroupMCP79"=0,"IOFWPhysicalAddressSpace"=0,"IOPCIDiagnosticsClient"=0,"IOHIDParamUserClient"=1,"IOPCIBridge"=2,"AppleFWOHCI_IOMemoryBlock32"=5,"nvEvoChannel"=1,"nvKeplerHAL"=1,"IOSlaveRelayMemoryBuffer"=0,"IORegistryIterator"=0,"OSData"=3853,"nvVirtualAddressSpace"=13,"IOGraphicsAccelerator2"=1,"AppleMCP79AHCI"=0,"IOSCSIPeripheralDeviceType05"=1,"PMAssertionsTracker"=1,"IOOutputQueue"=1,"NVDAGP100HAL"=1,"AppleUSBHostDMACommand"=0,"AppleEmbeddedKeyboard"=0,"IOSlaveRelayMemory"=0,"DspFuncCrossover"=0,"IO80211PeerManager"=0,"IOHDIXHDDriveNub"=0,"AppleKeyStoreCommand"=1,"AppleNVMeRequestTimer"=1,"AppleACPIPlatformUserClient"=0,"IOHIDKeyboardEventDevice"=2,"IOBluetoothL2CAPChannelUserClient"=0,"IOSCSITargetDevice"=0,"AppleBacklightDisplay"=0,"IOSlaveProcessorRelay"=0,"AppleFWOHCI_AsyncReceiveRequest"=1,"nvShareGroupContext"=2,"IORootParent"=1,"DspFuncMozartCompressor"=0,"FakeSMCSensor"=35,"com_apple_driver_pm_cstate_reporter"=0,"IO80211PeerMonitor"=0,"IOFWCompareAndSwapCommand"=1,"IOFWSimplePhysicalAddressSpace"=0,"PMSettingObject"=3,"AppleACPIPCI"=1,"AppleKeyStore"=1,"IOFWController"=1,"IOFWUserIsochChannel"=0,"IOPMinformee"=115,"IOSlowAdaptiveClockingManager"=1,"IOUSBCommand"=0,"AppleAHCISerialATAPIWorkLoopLock"=1,"IOPMPowerSource"=0,"hv_vmx_space_t"=0,"IOCDMedia"=0,"AppleUSBHostDMABufferMemoryDescriptor"=29,"IOUSBLog"=1,"DspFuncLimiter"=0,"CCPipeUserClient"=0,"AHCISMARTUserClient"=0,"AppleHDAMikeyInternalFactory"=0,"IOFireWireUserClientIniter"=2,"IOBluetoothDevice"=0,"AppleBusPowerController"=0,"DspFuncWithSharedMemory"=0,"IODisplayParameterHandler"=2,"SuperIODevice"=1,"IOAccelSharedNamespace2"=22,"IOBufferMemoryDescriptor"=889,"AppleUSBXHCILPTH"=0,"AppleACPIButton"=2,"AppleHDADriverUserClient"=0,"CCPipe"=2,"IOHIDEventServiceUserClient"=11,"AppleHDAWidgetALC885"=0,"nvEventLog"=1,"AppleHDAWidgetCS8409"=0,"DspFuncBeam2"=0,"DspFunc2Dot1Crossover"=0,"IOPolledInterface"=6,"IONDRVDevice"=6,"CoreStoragePhysical"=2,"IOAccelMemory"=2,"AppleUSBDevice"=6,"IOPlatformExpertDevice"=1,"IOUSBHubPolicyMaker"=1,"IOHIPointing"=1,"IOBluetoothHCIController"=1,"IOFireWireMultiIsochReceiveListener"=0,"IOFireWireControllerAux"=1,"AudioAUUC"=0,"nvEvoChannelInterface"=1,"IOFireWireUnitInfo"=0,"IODVDMediaBSDClient"=0,"nvGeneralDisplayLayer"=1,"IONetworkData"=22,"AppleFWOHCI_KPF"=0,"IOAudioLevelControl"=2,"AppleUSBXHCISPTLP"=0,"IOBluetoothRFCOMMChannel"=0,"IOUSBCommandPool"=0,"IOBluetoothHCIPacketLogUserClient"=0,"AppleS1XController"=0,"IOFWInterface"=1,"IOFireWireUnitAux"=0,"ACPIProbe"=0,"IO80211FlowQueue"=0,"AppleHDADriver"=2,"nvVidmemPushBuffer"=0,"ACPIProbeUserClient"=0,"IOFireWireNub"=1,"IOPlatformPluginDevice"=2,"IOKernelDebugger"=0,"IOBacklightDisplay"=0,"IONetworkMedium"=26,"IODisplayConnect"=1,"CoreStorageIORequest"=144,"AppleAHCIPortPolledAdapter"=4,"AppleHDAWidgetATI_RS710"=0,"IOHIDResource"=1,"IOFWPHYPacketListener"=0,"AGPMHeuristic0"=0,"AppleHDAWidgetWM8800"=24,"IOUSBRootHubDevice"=0,"IOSlaveRelayActionCommand"=0,"IOHIDPointingEventDevice"=4,"IOHIDDeviceShim"=2,"AppleSCSISubsystemGlobals"=1,"AppleHDAWidget_1002AAA0"=0,"IOAHCIPort"=1,"IOUSBHIDDriver"=1,"IOBluetoothObject"=0,"nvChannelInterface"=2,"OSMetaClass"=0,"AppleUSBXHCIARIsochronousRequestPool"=1,"KernelRelayEndpoint"=0,"DspFuncVolume"=0,"AppleGraphicsDeviceControl"=2,"IOAccelDisplayPipeGammaTable2"=0,"IOUSBControllerV2"=1,"IOHIDPointing"=0,"AppleUSBHostDescriptorCache"=5,"IOSCSIMultimediaCommandsDevice"=1,"IOAudioSelectorControl"=5,"DspFuncAudioMeter"=0,"CCDataSession"=0,"IOBluetoothDeviceUserClient"=0,"IOSCSIProtocolServices"=2,"nvAcceleratorParent"=1,"AppleEFINVRAM"=1,"IOKitDiagnostics"=1,"HDMIAudio"=0,"IODTNVRAM"=1,"IOHIDEventServiceQueue"=12,"com_apple_driver_pm_reporter"=3,"AppleUSBXHCITDPool"=2,"IOAccelDisplayPipeUserClient2"=0,"AppleRTCUserClient"=0,"DspFuncXTC"=0,"AppleHDAWidgetMCP79"=0,"hv_vm_t"=0,"IOHDIXCommand"=0,"AppleSSE"=1,"IOPMRequest"=0,"IOSlaveRelayRemoteMemoryBuffer"=0,"IOAccelMemoryMap"=1,"IOHIKeyboard"=2,"IOHIDUserDevice"=0,"AppleHDATDMAmpTAS5758L"=0,"AppleMCCSControlCello"=0,"AppleHDAFunctionGroupATI_Park"=0,"IOService"=155,"IORS232SerialStreamSync"=1,"CoreStorageUserClient"=0,"AppleHDAWidget_10DE0014"=0,"IOBluetoothWorkLoop"=0,"IOHIDEventRepairDriver"=0,"AppleHDAFunctionGroup_10DE0014"=0,"IOCDBlockStorageDriver"=1,"IOAccelBlockFencePort2"=9,"IOSKMemoryBuffer"=0,"IOFireWireIP"=1,"nvCLContext"=0,"IOFireWireLocalNodeAux"=1,"AppleSMCFamily"=1,"IOAccelSysMemory"=1,"IOFramebuffer"=1,"IntelMausi"=1,"AppleUSBXHCIIsochronousTransferRing"=0,"IOPMCompletionQueue"=1,"DspFuncVirtualization"=0,"AppleOSXWatchdog"=1,"FakeSMC"=1,"AppleHV"=1,"IOCompactDiscServices"=0,"AppleCredentialManagerUserClient"=1,"BroadcomBluetoothHostController"=0,"AppleUSBHostPort"=1,"CCDataPipeUserClient"=0,"AppleHDAWidget"=2,"IOAccelMemoryInfoUserClient"=0,"IOFDiskPartitionScheme"=0,"com_apple_filesystems_hfs"=1,"IOBDServices"=0,"at_obdev_LSNKE"=1,"AppleHDAFunctionGroupCS4206"=0,"CoreStorageShadowPool"=0,"AppleUSBXHCIStreamingEndpoint"=0,"IODVDMedia"=0,"AppleHDACodecGeneric"=2,"AppleSSEUserClient"=0,"IOBluetoothSerialClient"=1,"KernelRelayHost"=0,"nvChannelManager"=1,"IOAccelResource2"=1,"AppleFWOHCI_DMAManager"=1,"com_Logitech_USBReceiverHPP"=0,"IOFireWireIPDiagnostics"=1,"IOPMPowerSourceList"=0,"IOBDBlockStorageDriver"=0,"AppleHDAEngineOutputDP"=0,"IOFWAsyncStreamCommand"=0,"nvSysmemPushBuffer"=29,"AppleVTDDeviceMapper"=0,"IOAccelTraceStream2"=1,"AtherosE2200"=1,"AppleHDAStream"=9,"IOUSBPipe"=1,"AppleACPICPUInterruptController"=1,"AppleVTD"=0,"AppleFWOHCI_CallbackEventSource"=3,"nvSysMemory"=628,"IOAHCIBlockStorageDriver"=1,"IORegistryDescriptorC3"=1,"EupDSP"=0,"Lilu"=1,"AppleBusControllerFactory"=0,"IOPlatformExpert"=1,"nvSegmentResourceList"=0,"IOUserEthernetController"=0,"IOAccelDisplayPipePostCSCGammaVID"=0,"AppleFWOHCI_IsocXmitHelper"=0,"FakeSMCKeyStoreUserClient"=0,"AppleUSBController"=1,"IOPartitionScheme"=1,"IOFWBusCommand"=1,"AppleAHCIPolledAdapter"=1,"com_Logitech_USBLogitechInterfaceDriverHPP"=0,"AppleFWOHCI_AsyncTransmit"=2,"com_Logitech_HISpecialKeys"=1,"IOHIDUserClient"=1,"LogManager"=1,"IOACPIPlatformExpert"=1,"AppleOSXWatchdogClient"=1,"IOAccelVideoContext2"=0,"com_apple_driver_pm_cpu_mbox"=0,"IOUSBControllerIsochEndpoint"=0,"IOUSBPortInterruptEventSource"=22,"AppleFWOHCI_ReceiveDCL_U"=0,"DspFuncLoudness"=0,"com_mologie_NVWebDriverLibValFix"=1,"IOHIDEventService"=2,"IOAudioTimeIntervalFilterFIR"=0,"nvSharedUserClient"=22,"IOAccelDisplayPipePreCSCLinearizationVID"=0,"IOUserEthernetInterface"=0,"IOAudioPort"=0,"IODVDBlockStorageDevice"=1,"IT87xxSensors"=1,"IOHIKeyboardMapper"=2,"AppleUSBBusPowerClient"=0,"KRActionCommandPool"=0,"IOUSBHostInterface"=5,"com_apple_driver_pm_msr_limits_reporter"=0,"hv_vmx_vcpu_t"=0,"IOAHCIPortMultiplier"=0,"OSArray"=7207,"IOGeneralMemoryDescriptor"=593,"IOUSBIsocCommand"=0,"STUCWorkLoopLock"=1,"IO80211FlowQueueLegacy"=0,"IO80211ControllerMonitor"=1,"IOFWAsyncStreamListener"=0,"IOUSBWorkLoop"=1,"IOSurfaceClient"=73,"IOAudioEngineEntry"=0,"com_Logitech_USBKeyboard"=0,"IOConfigurationDescriptorOrderedSet"=0,"com_apple_driver_pm_ltr_reporter"=1,"AppleBusController"=0,"AHCIRequest"=134,"AppleGraphicsDeviceControlPlugin"=1,"IO80211CommandQueue"=0,"DspFuncManager"=5,"AppleUSB20XHCITypeCPort"=0,"DspFuncSplitBand"=0,"IOBootNDRV"=0,"IOHIDElementPrivate"=1981,"AppleHDAPath"=6,"AppleSSEInterface"=1,"IOFWUserAsyncStreamListener"=0,"IOHITablet"=0,"__GLNVEvoOverlayPushBuf"=0,"AppleACPIEventController"=1,"IOFWWriteCommand"=0,"IOFramebufferUserClient"=6},"IOMalloc allocation"=98450527}
  | }
  | 
  +-o /  <class IOPlatformExpertDevice, id 0x100000114, registered, matched, active, busy 0 (2835 ms), retain 49>
    | {
    |   "IOInterruptSpecifiers" = (<0900000005000000>)
    |   "IOPolledInterface" = "SMCPolledInterface is not serializable"
    |   "system-type" = <01>
    |   "serial-number" = <4a31474a00000000000000000043303256313248314a31474a000000000000000000000000000000000000>
    |   "platform-feature" = <0000000000000000>
    |   "IOPlatformSystemSleepPolicy" = < >
    |   "IOBusyInterest" = "IOCommand is not serializable"
    |   "target-type" = <"Mac">
    |   "IOInterruptControllers" = ("io-apic-0")
    |   "version" = <"1.0">
    |   "name" = <"/">
    |   "manufacturer" = <"Apple Inc.">
    |   "compatible" = <"iMac18,3">
    |   "product-name" = <"iMac18,3">
    |   "IOConsoleSecurityInterest" = "IOCommand is not serializable"
    |   "IOPlatformSerialNumber" = "C02V12H1J1GJ"
    |   "clock-frequency" = <00e1f505>
    |   "board-id" = <"Mac-BE088AF8C5EB4FA2">
    |   "model" = <"iMac18,3">
    |   "IOPlatformUUID" = "6AD18952-1521-5655-B394-893A8D0EC705"
    | }
    | 
    +-o chosen  <class IOService, id 0x100000101, !registered, !matched, active, busy 0, retain 7>
    | | {
    | |   "boot-args" = <"kext-dev-mode=1 ">
    | |   "boot-uuid" = <"952B9E39-1015-344B-9C53-18B242901757">
    | |   "IOScreenLockState" = <01000000>
    | |   "boot-file-path" = <040450005c00530079007300740065006d005c004c006900620072006100720079005c0043006f0072006500530065007200760069006300650073005c0062006f006f0074002e0065006600690000007fff0400>
    | |   "booter-name" = <"boot.efi">
    | |   "random-seed" = <00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000>
    | |   "boot-file" = <"System\Library\PrelinkedKernels\prelinkedkernel">
    | |   "booter-version" = <"version:324.50.13">
    | |   "machine-signature" = <00000000>
    | |   "IOProgressBackbuffer" = < >
    | |   "IOProgressColorTheme" = 1
    | |   "boot-kernelcache-adler32" = <1dbec3d0>
    | |   "boot-device-path" = <02010c00d041030a0000000001010600001d01010600000003171000010000000025385671b09d1504012a00020000002840060000000000b02fda4500000000427a8eba8f41c44c96a4e0e7b5ef878f02027fff0400>
    | |   "name" = <"chosen">
    | | }
    | | 
    | +-o memory-map  <class IOService, id 0x100000102, !registered, !matched, active, busy 0, retain 4>
    |     {
    |       "name" = <"memory-map">
    |       "FailedCLUT" = <0090150e00100000>
    |       "FailedImage" = <00a0150e20190000>
    |     }
    |     
    +-o efi  <class IOService, id 0x100000103, !registered, !matched, active, busy 0, retain 8>
    | | {
    | |   "firmware-revision" = <0c000500>
    | |   "device-properties" = < >
    | |   "firmware-abi" = <"EFI64">
    | |   "name" = <"efi">
    | |   "firmware-vendor" = <41006d00650072006900630061006e0020004d006500670061007400720065006e00640073000000>
    | | }
    | | 
    | +-o kernel-compatibility  <class IOService, id 0x100000104, !registered, !matched, active, busy 0, retain 4>
    | |   {
    | |     "name" = <"kernel-compatibility">
    | |     "x86_64" = <b75ee2ad>
    | |   }
    | |   
    | +-o runtime-services  <class IOService, id 0x100000105, !registered, !matched, active, busy 0, retain 4>
    | |   {
    | |     "name" = <"runtime-services">
    | |     "table" = <988e789f00000000>
    | |   }
    | |   
    | +-o configuration-table  <class IOService, id 0x100000106, !registered, !matched, active, busy 0, retain 16>
    | | | {
    | | |   "name" = <"configuration-table">
    | | | }
    | | | 
    | | +-o B122A263-3661-4F68-9929-78F8B0D62180  <class IOService, id 0x100000107, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"B122A263-3661-4F68-9929-78F8B0D62180">
    | | |     "guid" = <63a222b16136684f992978f8b0d62180>
    | | |     "table" = <98e0e79c00000000>
    | | |   }
    | | |   
    | | +-o EB9D2D2F-2D88-11D3-9A16-0090273FC14D  <class IOService, id 0x100000108, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"EB9D2D2F-2D88-11D3-9A16-0090273FC14D">
    | | |     "guid" = <2f2d9deb882dd3119a160090273fc14d>
    | | |     "table" = <30ca0f0000000000>
    | | |   }
    | | |   
    | | +-o F2FD1544-9794-4A2C-992E-E5BBCF20E394  <class IOService, id 0x100000109, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"F2FD1544-9794-4A2C-992E-E5BBCF20E394">
    | | |     "guid" = <4415fdf294972c4a992ee5bbcf20e394>
    | | |     "table" = <00306b9f00000000>
    | | |   }
    | | |   
    | | +-o EB9D2D31-2D88-11D3-9A16-0090273FC14D  <class IOService, id 0x10000010a, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"EB9D2D31-2D88-11D3-9A16-0090273FC14D">
    | | |     "guid" = <312d9deb882dd3119a160090273fc14d>
    | | |     "table" = <0040069f00000000>
    | | |   }
    | | |   
    | | +-o EB9D2D30-2D88-11D3-9A16-0090273FC14D  <class IOService, id 0x10000010b, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "alias" = <"ACPI">
    | | |     "name" = <"EB9D2D30-2D88-11D3-9A16-0090273FC14D">
    | | |     "table" = <0020cc9e00000000>
    | | |     "guid" = <302d9deb882dd3119a160090273fc14d>
    | | |   }
    | | |   
    | | +-o 8868E871-E4F1-11D3-BC22-0080C73C8881  <class IOService, id 0x10000010c, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "alias" = <"ACPI_20">
    | | |     "name" = <"8868E871-E4F1-11D3-BC22-0080C73C8881">
    | | |     "table" = <0020cc9e00000000>
    | | |     "guid" = <71e86888f1e4d311bc220080c73c8881>
    | | |   }
    | | |   
    | | +-o 00781CA1-5DE3-405F-ABB8-379C3C076984  <class IOService, id 0x10000010d, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"00781CA1-5DE3-405F-ABB8-379C3C076984">
    | | |     "guid" = <a11c7800e35d5f40abb8379c3c076984>
    | | |     "table" = <5873789f00000000>
    | | |   }
    | | |   
    | | +-o 49152E77-1ADA-4764-B7A2-7AFEFED95E8B  <class IOService, id 0x10000010e, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"49152E77-1ADA-4764-B7A2-7AFEFED95E8B">
    | | |     "guid" = <772e1549da1a6447b7a27afefed95e8b>
    | | |     "table" = <c860149300000000>
    | | |   }
    | | |   
    | | +-o 4C19049F-4137-4DD3-9C10-8B97A83FFDFA  <class IOService, id 0x10000010f, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"4C19049F-4137-4DD3-9C10-8B97A83FFDFA">
    | | |     "guid" = <9f04194c3741d34d9c108b97a83ffdfa>
    | | |     "table" = <40c5129300000000>
    | | |   }
    | | |   
    | | +-o 7739F24C-93D7-11D4-9A3A-0090273FC14D  <class IOService, id 0x100000110, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"7739F24C-93D7-11D4-9A3A-0090273FC14D">
    | | |     "guid" = <4cf23977d793d4119a3a0090273fc14d>
    | | |     "table" = <18b0ce9d00000000>
    | | |   }
    | | |   
    | | +-o 05AD34BA-6F02-4214-952E-4DA0398E2BB9  <class IOService, id 0x100000111, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"05AD34BA-6F02-4214-952E-4DA0398E2BB9">
    | | |     "guid" = <ba34ad05026f1442952e4da0398e2bb9>
    | | |     "table" = <f0cb129300000000>
    | | |   }
    | | |   
    | | +-o EE4E5898-3914-4259-9D6E-DC7BD79403CF  <class IOService, id 0x100000112, !registered, !matched, active, busy 0, retain 4>
    | |     {
    | |       "name" = <"EE4E5898-3914-4259-9D6E-DC7BD79403CF">
    | |       "guid" = <98584eee143959429d6edc7bd79403cf>
    | |       "table" = <d86fd29d00000000>
    | |     }
    | |     
    | +-o platform  <class IOService, id 0x100000113, !registered, !matched, active, busy 0, retain 10>
    |     {
    |       "name" = <"platform">
    |       "BEMB" = <00>
    |       "Model" = <69004d0061006300310038002c0033000000>
    |       "CPUFrequency" = <402c66fa00000000>
    |       "REV" = <02410f000001>
    |       "FSBFrequency" = <7216f60500000000>
    |       "OEMVendor" = <"Gigabyte Technology Co., Ltd.">
    |       "Settings" = < >
    |       "OEMBoard" = <"Z270X-Gaming 7">
    |       "clovergui-revision" = <ac100000>
    |       "system-id" = <1c021b030d049a05e006540700080009>
    |       "RPlt" = <6a31333500000000>
    |       "InitialTSC" = <c4ae5ffa00000000>
    |       "RBr" = <"j133_4_">
    |       "EPCI" = <0970f000>
    |       "boot-log" = < >
    |       "DevicePathsSupported" = <01000000>
    |       "OEMProduct" = <"Z270X-Gaming 7">
    |       "SystemSerialNumber" = <430030003200560031003200480031004a00310047004a000000>
    |     }
    |     
    +-o cpus  <class IOPlatformDevice, id 0x10000011b, registered, matched, active, busy 0 (46 ms), retain 14>
    | | {
    | |   "name" = <"cpus">
    | | }
    | | 
    | +-o CPU0@0  <class IOACPIPlatformDevice, id 0x10000011c, registered, matched, active, busy 0 (230 ms), retain 9>
    | |   {
    | |     "processor-lapic" = 0
    | |     "clock-frequency" = <402c66fa>
    | |     "processor-number" = 0
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 1
    | |     "bus-frequency" = <00e1f505>
    | |     "plugin-type" = 1
    | |     "cpu-type" = <0507>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 0
    | |     "name" = <"CPU0">
    | |   }
    | |   
    | +-o CPU1@2  <class IOACPIPlatformDevice, id 0x10000011d, registered, matched, active, busy 0 (64 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 2
    | |     "clock-frequency" = <402c66fa>
    | |     "processor-number" = 2
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 2
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <0507>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 1
    | |     "name" = <"CPU1">
    | |   }
    | |   
    | +-o CPU2@4  <class IOACPIPlatformDevice, id 0x10000011e, registered, matched, active, busy 0 (64 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 4
    | |     "clock-frequency" = <402c66fa>
    | |     "processor-number" = 4
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 3
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <0507>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 2
    | |     "name" = <"CPU2">
    | |   }
    | |   
    | +-o CPU3@6  <class IOACPIPlatformDevice, id 0x10000011f, registered, matched, active, busy 0 (65 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 6
    | |     "clock-frequency" = <402c66fa>
    | |     "processor-number" = 6
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 4
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <0507>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 3
    | |     "name" = <"CPU3">
    | |   }
    | |   
    | +-o CPU4@1  <class IOACPIPlatformDevice, id 0x100000120, registered, matched, active, busy 0 (65 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 1
    | |     "clock-frequency" = <402c66fa>
    | |     "processor-number" = 1
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 5
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <0507>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 4
    | |     "name" = <"CPU4">
    | |   }
    | |   
    | +-o CPU5@3  <class IOACPIPlatformDevice, id 0x100000121, registered, matched, active, busy 0 (66 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 3
    | |     "clock-frequency" = <402c66fa>
    | |     "processor-number" = 3
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 6
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <0507>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 5
    | |     "name" = <"CPU5">
    | |   }
    | |   
    | +-o CPU6@5  <class IOACPIPlatformDevice, id 0x100000122, registered, matched, active, busy 0 (67 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 5
    | |     "clock-frequency" = <402c66fa>
    | |     "processor-number" = 5
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 7
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <0507>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 6
    | |     "name" = <"CPU6">
    | |   }
    | |   
    | +-o CPU7@7  <class IOACPIPlatformDevice, id 0x100000123, registered, matched, active, busy 0 (68 ms), retain 8>
    |     {
    |       "processor-lapic" = 7
    |       "clock-frequency" = <402c66fa>
    |       "processor-number" = 7
    |       "timebase-frequency" = <00ca9a3b>
    |       "processor-id" = 8
    |       "bus-frequency" = <00e1f505>
    |       "cpu-type" = <0507>
    |       "device_type" = <"processor">
    |       "processor-index" = 7
    |       "name" = <"CPU7">
    |     }
    |     
    +-o memory  <class IOService, id 0x10000013f, !registered, !matched, active, busy 0, retain 4>
    |   {
    |     "dimm-part-number" = <"F4-4133C19-8GTZA","F4-4133C19-8GTZA","F4-4133C19-8GTZA","F4-4133C19-8GTZA">
    |     "dimm-types" = <"DDR4","DDR4","DDR4","DDR4">
    |     "slot-names" = <"   ","BANK 0/DIMM0","BANK 1/DIMM0","BANK 0/DIMM1","BANK 1/DIMM1">
    |     "dimm-speeds" = <"4140 MHz","4140 MHz","4140 MHz","4140 MHz">
    |     "dimm-manufacturer" = <"G Skill Intl","G Skill Intl","G Skill Intl","G Skill Intl">
    |     "ecc-enabled" = No
    |     "reg" = <0200000000000000020000000000000002000000000000000200000000000000>
    |     "dimm-info" = < >
    |     "dimm-serial-number" = <"0000000000000000","0000000000000000","0000000000000000","0000000000000000">
    |   }
    |   
    +-o rom@0  <class IOService, id 0x100000140, !registered, !matched, active, busy 0, retain 4>
    |   {
    |     "rom-size" = 16777216
    |     "vendor" = <"Apple Inc.">
    |     "fv-main-address" = 18446744073707454464
    |     "fv-main-size" = 1048576
    |     "release-date" = <"08/08/2017">
    |     "version" = <"IM183.88Z.0151.B00.1708080034">
    |   }
    |   
    +-o PCI0@0  <class IOACPIPlatformDevice, id 0x100000142, registered, matched, active, busy 0 (2078 ms), retain 105>
    | | {
    | |   "compatible" = <"PNP0A03">
    | |   "IODTPersist" = <>
    | |   "_STA" = 18446744073709551615
    | |   "IOPCIConfigured" = Yes
    | |   "acpi-address-spaces" = < >
    | |   "IODeviceMemory" = (({"address"=3320,"length"=8}))
    | |   "#size-cells" = <02000000>
    | |   "_UID" = "0"
    | |   "acpi-pci-routing-table" = < >
    | |   "_ADR" = 0
    | |   "device-properties" = {"acpi-device"="IOACPIPlatformDevice is not serializable","acpi-path"="IOACPIPlane:/_SB/PCI0@0"}
    | |   "#address-cells" = <03000000>
    | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0"
    | |   "name" = <"PNP0A08">
    | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | }
    | | 
    | +-o GFX0@20000  <class IORegistryEntry, id 0x1000001ec, retain 20>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000"
    | | | }
    | | | 
    | | +-o DD01@100  <class IORegistryEntry, id 0x1000001ed, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD01@100"
    | | |   }
    | | |   
    | | +-o DD02@2  <class IORegistryEntry, id 0x1000001ee, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD02@2"
    | | |   }
    | | |   
    | | +-o DD03@300  <class IORegistryEntry, id 0x1000001ef, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD03@300"
    | | |   }
    | | |   
    | | +-o DD04@301  <class IORegistryEntry, id 0x1000001f0, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD04@301"
    | | |   }
    | | |   
    | | +-o DD05@302  <class IORegistryEntry, id 0x1000001f1, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD05@302"
    | | |   }
    | | |   
    | | +-o DD06@303  <class IORegistryEntry, id 0x1000001f2, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD06@303"
    | | |   }
    | | |   
    | | +-o DD07@304  <class IORegistryEntry, id 0x1000001f3, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD07@304"
    | | |   }
    | | |   
    | | +-o DD08@305  <class IORegistryEntry, id 0x1000001f4, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD08@305"
    | | |   }
    | | |   
    | | +-o DD09@9  <class IORegistryEntry, id 0x1000001f5, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD09@9"
    | | |   }
    | | |   
    | | +-o DD0A@a  <class IORegistryEntry, id 0x1000001f6, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD0A@a"
    | | |   }
    | | |   
    | | +-o DD0B@b  <class IORegistryEntry, id 0x1000001f7, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD0B@b"
    | | |   }
    | | |   
    | | +-o DD0C@c  <class IORegistryEntry, id 0x1000001f8, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD0C@c"
    | | |   }
    | | |   
    | | +-o DD0D@d  <class IORegistryEntry, id 0x1000001f9, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD0D@d"
    | | |   }
    | | |   
    | | +-o DD0E@e  <class IORegistryEntry, id 0x1000001fa, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD0E@e"
    | | |   }
    | | |   
    | | +-o DD0F@f  <class IORegistryEntry, id 0x1000001fb, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD0F@f"
    | | |   }
    | | |   
    | | +-o DD1F@400  <class IORegistryEntry, id 0x1000001fc, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GFX0@20000/DD1F@400"
    | |     }
    | |     
    | +-o B0D4@40000  <class IORegistryEntry, id 0x1000001fd, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/B0D4@40000"
    | |   }
    | |   
    | +-o PEG1@10001  <class IORegistryEntry, id 0x100000203, retain 6>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG1@10001"
    | | | }
    | | | 
    | | +-o PEGP@0  <class IORegistryEntry, id 0x100000204, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG1@10001/PEGP@0"
    | | |   }
    | | |   
    | | +-o D05D@0  <class IORegistryEntry, id 0x100000205, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG1@10001/D05D@0"
    | |     }
    | |     
    | +-o PEG2@10002  <class IORegistryEntry, id 0x100000206, retain 6>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG2@10002"
    | | | }
    | | | 
    | | +-o PEGP@0  <class IORegistryEntry, id 0x100000207, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG2@10002/PEGP@0"
    | | |   }
    | | |   
    | | +-o D05E@0  <class IORegistryEntry, id 0x100000208, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG2@10002/D05E@0"
    | |     }
    | |     
    | +-o RP10@1d0001  <class IORegistryEntry, id 0x10000020c, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP10@1d0001"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x10000020d, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP10@1d0001/PXSX@0"
    | |     }
    | |     
    | +-o RP12@1d0003  <class IORegistryEntry, id 0x100000210, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP12@1d0003"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000211, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP12@1d0003/PXSX@0"
    | |     }
    | |     
    | +-o RP13@1d0004  <class IORegistryEntry, id 0x100000212, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP13@1d0004"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000213, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP13@1d0004/PXSX@0"
    | |     }
    | |     
    | +-o RP04@1c0003  <class IORegistryEntry, id 0x10000021b, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP04@1c0003"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x10000021c, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP04@1c0003/PXSX@0"
    | |     }
    | |     
    | +-o RP06@1c0005  <class IORegistryEntry, id 0x10000021f, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP06@1c0005"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000220, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP06@1c0005/PXSX@0"
    | |     }
    | |     
    | +-o RP07@1c0006  <class IORegistryEntry, id 0x100000221, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP07@1c0006"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000222, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP07@1c0006/PXSX@0"
    | |     }
    | |     
    | +-o RP08@1c0007  <class IORegistryEntry, id 0x100000223, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP08@1c0007"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000224, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP08@1c0007/PXSX@0"
    | |     }
    | |     
    | +-o RP18@1b0001  <class IORegistryEntry, id 0x100000227, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP18@1b0001"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000228, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP18@1b0001/PXSX@0"
    | |     }
    | |     
    | +-o RP20@1b0003  <class IORegistryEntry, id 0x10000022b, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP20@1b0003"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x10000022c, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP20@1b0003/PXSX@0"
    | |     }
    | |     
    | +-o RP22@1b0005  <class IORegistryEntry, id 0x10000022f, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP22@1b0005"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000230, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP22@1b0005/PXSX@0"
    | |     }
    | |     
    | +-o RP23@1b0006  <class IORegistryEntry, id 0x100000231, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP23@1b0006"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000232, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP23@1b0006/PXSX@0"
    | |     }
    | |     
    | +-o RP24@1b0007  <class IORegistryEntry, id 0x100000233, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP24@1b0007"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000234, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP24@1b0007/PXSX@0"
    | |     }
    | |     
    | +-o RP15@1d0006  <class IORegistryEntry, id 0x100000237, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP15@1d0006"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000238, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP15@1d0006/PXSX@0"
    | |     }
    | |     
    | +-o RP16@1d0007  <class IORegistryEntry, id 0x100000239, retain 5>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP16@1d0007"
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x10000023a, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP16@1d0007/PXSX@0"
    | |     }
    | |     
    | +-o PDRC  <class IOACPIPlatformDevice, id 0x10000019e, registered, matched, active, busy 0 (0 ms), retain 7>
    | |   {
    | |     "_STA" = 18446744073709551615
    | |     "_UID" = "1"
    | |     "IODeviceMemory" = (({"address"=4275109888,"length"=32768}),({"address"=4275142656,"length"=4096}),({"address"=4275146752,"length"=4096}),({"address"=4026531840,"length"=134217728}),({"address"=4275175424,"length"=131072}),({"address"=4275634176,"length"=16384}),({"address"=4275326976,"length"=307200}),({"address"=4278190080,"length"=16777216}),({"address"=4276092928,"length"=1048576}),({"address"=4026400768,"length"=131072}))
    | |     "name" = <"PNP0C02">
    | |   }
    | |   
    | +-o PRRE  <class IOACPIPlatformDevice, id 0x10000019f, registered, matched, active, busy 0 (0 ms), retain 7>
    | |   {
    | |     "_STA" = 3
    | |     "_UID" = "PCHRESV"
    | |     "IODeviceMemory" = (({"address"=4244635648,"length"=11272192}),({"address"=4255973376,"length"=65536}),({"address"=4256169984,"length"=5242880}),({"address"=4261412864,"length"=131072}),({"address"=4261634048,"length"=24576}),({"address"=4261662720,"length"=3944448}),({"address"=4265672704,"length"=4128768}))
    | |     "name" = <"PNP0C02">
    | |   }
    | |   
    | +-o IOTR  <class IOACPIPlatformDevice, id 0x1000001a0, registered, matched, active, busy 0 (1 ms), retain 7>
    | |   {
    | |     "_STA" = 18446744073709551615
    | |     "_UID" = "IoTraps"
    | |     "IODeviceMemory" = (({"address"=65280,"length"=255}))
    | |     "name" = <"PNP0C02">
    | |   }
    | |   
    | +-o XDCI@140001  <class IORegistryEntry, id 0x100000262, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XDCI@140001"
    | |   }
    | |   
    | +-o SIRC  <class IOACPIPlatformDevice, id 0x1000001d4, registered, matched, active, busy 0 (1 ms), retain 7>
    | |   {
    | |     "_STA" = 3
    | |     "IODeviceMemory" = (({"address"=4256104448,"length"=65536}),({"address"=4256038912,"length"=65536}),({"address"=4255907840,"length"=65536}))
    | |     "_UID" = "5"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "IOInterruptSpecifiers" = (<0e00000007000000>)
    | |     "name" = <"PNP0C02">
    | |   }
    | |   
    | +-o GEXP@1  <class IORegistryEntry, id 0x10000026e, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GEXP@1"
    | |   }
    | |   
    | +-o ISHD@130000  <class IORegistryEntry, id 0x10000026f, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/ISHD@130000"
    | |   }
    | |   
    | +-o WMI1  <class IOACPIPlatformDevice, id 0x1000001d8, registered, matched, active, busy 0 (1 ms), retain 7>
    | |   {
    | |     "_UID" = "MXM2"
    | |     "_STA" = 18446744073709551615
    | |     "name" = <"PNP0C14">
    | |   }
    | |   
    | +-o GWMI  <class IOACPIPlatformDevice, id 0x1000001d9, registered, matched, active, busy 0 (0 ms), retain 7>
    | |   {
    | |     "_UID" = "GAIF"
    | |     "_STA" = 18446744073709551615
    | |     "name" = <"PNP0C14">
    | |   }
    | |   
    | +-o pci8086,591f@0  <class IOPCIDevice, id 0x100000283, registered, matched, active, busy 0 (0 ms), retain 8>
    | |   {
    | |     "compatible" = <"pci1458,5000","pci8086,591f","pciclass,060000">
    | |     "subsystem-vendor-id" = <58140000>
    | |     "IOName" = "pci8086,591f"
    | |     "reg" = <0000000000000000000000000000000000000000>
    | |     "device-id" = <1f590000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <05000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:0:0"
    | |     "class-code" = <00000600>
    | |     "name" = <"pci8086,591f">
    | |     "subsystem-id" = <00500000>
    | |   }
    | |   
    | +-o PEG0@1  <class IOPCIDevice, id 0x1000001fe, registered, matched, active, busy 0 (714 ms), retain 14>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 72
    | | |   "subsystem-vendor-id" = <7f000000>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "built-in" = <00>
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "name" = <"pci-bridge">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <01190000>
    | | |   "acpi-pmcap-offset" = 128
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci7f,0","pci8086,1901","pciclass,060400","PEG0">
    | | |   "ranges" = <0000008200000000000000ec0000008200000000000000ec0000000000001001000000c27f00000000000080000000c27f000000000000800000000000000012000000810000000000e00000000000810000000000e000000000000000100000>
    | | |   "IOPCIExpressLinkCapabilities" = 39955715
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG0@10000"
    | | |   "subsystem-id" = <00000000>
    | | |   "revision-id" = <05000000>
    | | |   "IOPCIExpressLinkStatus" = 53505
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:1:0(1:1)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <0008000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 796032
    | | | }
    | | | 
    | | +-o PEGP@f  <class IORegistryEntry, id 0x1000001ff, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG0@10000/PEGP@f"
    | | |   }
    | | |   
    | | +-o GFX0@0  <class IORegistryEntry, id 0x100000201, retain 4>
    | | |   {
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG0@10000/GFX0@0"
    | | |     "@5,connector-type" = <00080000>
    | | |     "hda-gfx" = <"onboard-2">
    | | |     "@4,connector-type" = <00080000>
    | | |     "@3,connector-type" = <00080000>
    | | |     "@1,connector-type" = <00080000>
    | | |     "@2,connector-type" = <00080000>
    | | |     "@0,connector-type" = <00080000>
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   }
    | | |   
    | | +-o D05C@0  <class IOPCIDevice, id 0x100000200, registered, matched, active, busy 0 (697 ms), retain 32>
    | | | | {
    | | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | | |   "built-in" = <00>
    | | | |   "saved-config" = < >
    | | | |   "NVDA,Features" = <00080000>
    | | | |   "NVDAType" = "Web"
    | | | |   "rom-revision" = <"VBIOS 86.06.39.00.62">
    | | | |   "IODeviceMemory" = (({"address"=3959422976,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=3976200192,"length"=524288}))
    | | | |   "NVArch" = "GP100"
    | | | |   "VRAM,totalMB" = <ff170000>
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG0@10000/D05C@0"
    | | | |   "pci-aspm-default" = 0
    | | | |   "reg" = <0000010000000000000000000000000000000000100001020000000000000000000000000000000114000142000000000000000000000000000000101c0001420000000000000000000000000000000224000101000000000000000000000000800000003000010200000000000000000000000000000800>
    | | | |   "NVDA,noEFI" = <"true">
    | | | |   "NVCLASS" = "NVDA"
    | | | |   "hda-gfx" = <"onboard-2">
    | | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="D05C 1"})
    | | | |   "@2,connector-type" = <00080000>
    | | | |   "IOName" = "display"
    | | | |   "IOPCIExpressLinkCapabilities" = 4537603
    | | | |   "IOChildIndex" = 1
    | | | |   "attached-gpu-control-path" = "IOService:/AppleACPIPlatformExpert/PCI0@0/AppleACPIPCI/PEG0@1/IOPP/D05C@0/NVDA,Display-A@0/NVDA/AGPM"
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "AAPL,iokit-ndrv" = <01000000>
    | | | |   "@0,connector-type" = <00080000>
    | | | |   "vbios-revision" = <6200390686>
    | | | |   "rm_board_number" = <00000000>
    | | | |   "class-code" = <00000300>
    | | | |   "IOPCIResourced" = Yes
    | | | |   "name" = <"display">
    | | | |   "NVCAP" = <050000000000ffffffff00000000000e00000000>
    | | | |   "IOReportLegendPublic" = Yes
    | | | |   "IOInterruptSpecifiers" = (<1000000007000000>,<0300000000000100>)
    | | | |   "compatible" = <"pci3842,6262","pci10de,1c03","pciclass,030000","D05C">
    | | | |   "revision-id" = <a1000000>
    | | | |   "IOPCIMSIMode" = Yes
    | | | |   "subsystem-vendor-id" = <42380000>
    | | | |   "VRAM,totalsize" = <00000010>
    | | | |   "assigned-addresses" = <1000018200000000000000ec0000000000000001140001c27f0000000000008000000000000000101c0001c27f000000000000900000000000000002240001810000000000e0000000000000800000003000018200000000000000ed0000000000000800>
    | | | |   "device-id" = <031c0000>
    | | | |   "AAPL,ndrv-dev" = Yes
    | | | |   "IOPCIExpressLinkStatus" = 4353
    | | | |   "@3,connector-type" = <00080000>
    | | | |   "pcidebug" = "1:0:0"
    | | | |   "IOPCIExpressCapabilities" = 18
    | | | |   "@1,connector-type" = <00080000>
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | | |   "IONVRAMProperty" = Yes
    | | | |   "IOHibernateState" = <00000000>
    | | | |   "subsystem-id" = <10000000>
    | | | |   "device_type" = <"NVDA,Parent">
    | | | |   "vendor-id" = <de100000>
    | | | |   "NVDA,accel-loaded" = <01000000>
    | | | |   "model" = <"NVIDIA GeForce GTX 1060 6GB">
    | | | |   "IOPMIsPowerManaged" = Yes
    | | | |   "NVDAinitgl_created" = "yes"
    | | | | }
    | | | | 
    | | | +-o NVDA,Display-A@0  <class IONDRVDevice, id 0x100000452, registered, matched, active, busy 0 (8 ms), retain 8>
    | | | |   {
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "connector-type" = <00080000>
    | | | |     "IOFBDependentIndex" = 0
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "AAPL,RegEntryID" = <60f82700000000009f07d8ffffffffff656d6953000000007a6c755200000000>
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "IODeviceMemory" = (({"address"=3959422976,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=3976200192,"length"=524288}))
    | | | |     "IOFBDependentID" = 4294967808
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "device_type" = <"display">
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "av-signal-type" = <00000000>
    | | | |     "display-cfg" = <ffffffff>
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "name" = <"NVDA,Display-A">
    | | | |     "port-number" = <00000000>
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-B@1  <class IONDRVDevice, id 0x100000453, registered, matched, active, busy 0 (0 ms), retain 8>
    | | | |   {
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "connector-type" = <00080000>
    | | | |     "IOFBDependentIndex" = 1
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "AAPL,RegEntryID" = <409b190000000000bf64e6ffffffffff656d6953000000007a6c755200000000>
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "IODeviceMemory" = (({"address"=3959422976,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=3976200192,"length"=524288}))
    | | | |     "IOFBDependentID" = 4294967808
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "device_type" = <"display">
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "av-signal-type" = <00000000>
    | | | |     "display-cfg" = <ffffffff>
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "name" = <"NVDA,Display-B">
    | | | |     "port-number" = <01000000>
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-C@2  <class IONDRVDevice, id 0x100000454, registered, matched, active, busy 0 (0 ms), retain 8>
    | | | |   {
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "connector-type" = <00080000>
    | | | |     "IOFBDependentIndex" = 2
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "AAPL,RegEntryID" = <e0a51900000000001f5ae6ffffffffff656d6953000000007a6c755200000000>
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "IODeviceMemory" = (({"address"=3959422976,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=3976200192,"length"=524288}))
    | | | |     "IOFBDependentID" = 4294967808
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "device_type" = <"display">
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "av-signal-type" = <00000000>
    | | | |     "display-cfg" = <ffffffff>
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "name" = <"NVDA,Display-C">
    | | | |     "port-number" = <02000000>
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-D@3  <class IONDRVDevice, id 0x100000455, registered, matched, active, busy 0 (0 ms), retain 8>
    | | | |   {
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "connector-type" = <00080000>
    | | | |     "IOFBDependentIndex" = 3
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "AAPL,RegEntryID" = <e0a01900000000001f5fe6ffffffffff656d6953000000007a6c755200000000>
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "IODeviceMemory" = (({"address"=3959422976,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=3976200192,"length"=524288}))
    | | | |     "IOFBDependentID" = 4294967808
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "device_type" = <"display">
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "av-signal-type" = <00000000>
    | | | |     "display-cfg" = <ffffffff>
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "name" = <"NVDA,Display-D">
    | | | |     "port-number" = <03000000>
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-E@4  <class IONDRVDevice, id 0x100000456, registered, matched, active, busy 0 (1 ms), retain 8>
    | | | |   {
    | | | |     "audio-codec-info" = <00010500>
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "IODeviceMemory" = (({"address"=3959422976,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=3976200192,"length"=524288}))
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "IOFBDependentID" = 4294967808
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "display-cfg" = <ffffffff>
    | | | |     "name" = <"NVDA,Display-E">
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "av-signal-type" = <08000000>
    | | | |     "IOFBDependentIndex" = 4
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "display-type" = <"LCD">
    | | | |     "port-number" = <04000000>
    | | | |     "AAPL,RegEntryID" = <20b6190000000000df49e6ffffffffff656d6953000000007a6c755200000000>
    | | | |     "device_type" = <"display">
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-F@5  <class IONDRVDevice, id 0x100000457, registered, matched, active, busy 0 (0 ms), retain 8>
    | | |     {
    | | |       "compatible" = <"NVDA,NVMac">
    | | |       "IOFBDependentIndex" = 5
    | | |       "nativeNDRV" = <"advn">
    | | |       "AAPL,RegEntryID" = <60b71900000000009f48e6ffffffffff656d6953000000007a6c755200000000>
    | | |       "AAPL,ndrv-dev" = Yes
    | | |       "IODeviceMemory" = (({"address"=3959422976,"length"=16777216}),({"address"=547608330240,"length"=268435456}),({"address"=547876765696,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=3976200192,"length"=524288}))
    | | |       "IOFBDependentID" = 4294967808
    | | |       "AAPL,gray-page" = <01000000>
    | | |       "device_type" = <"display">
    | | |       "NVDA,DeviceClass" = <80000000>
    | | |       "NVDA,SubDeviceClass" = <80200000>
    | | |       "av-signal-type" = <00000000>
    | | |       "display-cfg" = <ffffffff>
    | | |       "AAPL,gray-value" = <00000000>
    | | |       "noNVRAM" = <01000000>
    | | |       "name" = <"NVDA,Display-F">
    | | |       "display-connect-flags" = <00000000>
    | | |     }
    | | |     
    | | +-o HDAU@0,1  <class IOPCIDevice, id 0x100000202, registered, matched, active, busy 0 (50 ms), retain 10>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "@0,connector-type" = <00080000>
    | |       "assigned-addresses" = <1001018200000000000008ed0000000000400000>
    | |       "class-code" = <00030400>
    | |       "subsystem-vendor-id" = <42380000>
    | |       "vendor-id" = <de100000>
    | |       "hda-gfx" = <"onboard-2">
    | |       "IOPCIExpressLinkCapabilities" = 4537603
    | |       "IOName" = "pci10de,10f1"
    | |       "IOPCIMSIMode" = Yes
    | |       "DigitalAudioCapabilities" = {"DisplayPort"=1,"HDMI"=1}
    | |       "IOChildIndex" = 2
    | |       "pcidebug" = "1:0:1"
    | |       "layout-id" = <01000000>
    | |       "IOPCIExpressLinkStatus" = 4353
    | |       "pci-aspm-default" = 3
    | |       "IOPCIExpressCapabilities" = 2
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "@3,connector-type" = <00080000>
    | |       "built-in" = <01>
    | |       "IOPCIResourced" = Yes
    | |       "IODeviceMemory" = (({"address"=3976724480,"length"=16384}))
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "PinConfigurations" = <>
    | |       "name" = <"pci10de,10f1">
    | |       "subsystem-id" = <62620000>
    | |       "@2,connector-type" = <00080000>
    | |       "compatible" = <"pci3842,6262","pci10de,10f1","pciclass,040300","HDAU","HDAU","HDAU","HDAU">
    | |       "@1,connector-type" = <00080000>
    | |       "IOReportLegendPublic" = Yes
    | |       "reg" = <00010100000000000000000000000000000000001001010200000000000000000000000000400000>
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="HDAU 1"})
    | |       "device-id" = <f1100000>
    | |       "revision-id" = <a1000000>
    | |       "IOInterruptSpecifiers" = (<1100000007000000>,<0200000000000100>)
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PEG0@10000/HDAU@1"
    | |     }
    | |     
    | +-o pci8086,1911@8  <class IOPCIDevice, id 0x100000284, registered, matched, active, busy 0 (0 ms), retain 8>
    | |   {
    | |     "compatible" = <"pci1458,5000","pci8086,1911","pciclass,088000">
    | |     "subsystem-vendor-id" = <58140000>
    | |     "IOName" = "pci8086,1911"
    | |     "reg" = <00400000000000000000000000000000000000001040000200000000000000000000000000100000>
    | |     "device-id" = <11190000>
    | |     "assigned-addresses" = <104000827f000000005002920000000000100000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IODeviceMemory" = (({"address"=547910471680,"length"=4096}))
    | |     "revision-id" = <00000000>
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:8:0"
    | |     "class-code" = <00800800>
    | |     "IOInterruptSpecifiers" = (<1000000007000000>,<0000000000000100>)
    | |     "subsystem-id" = <00500000>
    | |     "name" = <"pci8086,1911">
    | |   }
    | |   
    | +-o XHC@14  <class IOPCIDevice, id 0x10000023e, registered, matched, active, busy 0 (564 ms), retain 12>
    | | | {
    | | |   "assigned-addresses" = <10a000827f000000000001920000000000000100>
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>,<0100000000000100>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="XHC 1"})
    | | |   "class-code" = <30030c00>
    | | |   "IODeviceMemory" = (({"address"=547910385664,"length"=65536}))
    | | |   "IOReportLegendPublic" = Yes
    | | |   "built-in" = <00>
    | | |   "subsystem-vendor-id" = <58140000>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "AAPL,current-extra" = <bc02>
    | | |   "IOPCIMSIMode" = Yes
    | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci8086,a2af">
    | | |   "device-id" = <afa20000>
    | | |   "acpi-pmcap-offset" = 112
    | | |   "IOPCIResourced" = Yes
    | | |   "AAPL,current-available" = <b004>
    | | |   "compatible" = <"pci1458,5007","pci8086,a2af","pciclass,0c0330","XHC">
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000"
    | | |   "AAPL,current-in-sleep" = <e803>
    | | |   "subsystem-id" = <07500000>
    | | |   "revision-id" = <00000000>
    | | |   "pcidebug" = "0:20:0"
    | | |   "device_type" = <"XHCI">
    | | |   "IOName" = "pci8086,a2af"
    | | |   "reg" = <00a000000000000000000000000000000000000010a0000200000000000000000000000000000100>
    | | |   "AAPL,clock-id" = <00>
    | | | }
    | | | 
    | | +-o RHUB@0  <class IORegistryEntry, id 0x10000023f, retain 30>
    | |   | {
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0"
    | |   | }
    | |   | 
    | |   +-o HS01@1  <class IORegistryEntry, id 0x100000240, retain 8>
    | |   | | {
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS01@1"
    | |   | | }
    | |   | | 
    | |   | +-o DP01@1  <class IORegistryEntry, id 0x100000241, retain 4>
    | |   | |   {
    | |   | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS01@1/DP01@1"
    | |   | |   }
    | |   | |   
    | |   | +-o DP02@2  <class IORegistryEntry, id 0x100000242, retain 4>
    | |   | |   {
    | |   | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS01@1/DP02@2"
    | |   | |   }
    | |   | |   
    | |   | +-o DP03@3  <class IORegistryEntry, id 0x100000243, retain 4>
    | |   | |   {
    | |   | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS01@1/DP03@3"
    | |   | |   }
    | |   | |   
    | |   | +-o DP04@4  <class IORegistryEntry, id 0x100000244, retain 4>
    | |   |     {
    | |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS01@1/DP04@4"
    | |   |     }
    | |   |     
    | |   +-o HS02@2  <class IORegistryEntry, id 0x100000245, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS02@2"
    | |   |   }
    | |   |   
    | |   +-o HS03@3  <class IORegistryEntry, id 0x100000246, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS03@3"
    | |   |   }
    | |   |   
    | |   +-o HS04@4  <class IORegistryEntry, id 0x100000247, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS04@4"
    | |   |   }
    | |   |   
    | |   +-o HS05@5  <class IORegistryEntry, id 0x100000248, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS05@5"
    | |   |   }
    | |   |   
    | |   +-o HS06@6  <class IORegistryEntry, id 0x100000249, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS06@6"
    | |   |   }
    | |   |   
    | |   +-o HS07@7  <class IORegistryEntry, id 0x10000024a, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS07@7"
    | |   |   }
    | |   |   
    | |   +-o HS08@8  <class IORegistryEntry, id 0x10000024b, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS08@8"
    | |   |   }
    | |   |   
    | |   +-o HS09@9  <class IORegistryEntry, id 0x10000024c, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS09@9"
    | |   |   }
    | |   |   
    | |   +-o HS10@a  <class IORegistryEntry, id 0x10000024d, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS10@a"
    | |   |   }
    | |   |   
    | |   +-o USR1@f  <class IORegistryEntry, id 0x10000024e, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/USR1@f"
    | |   |   }
    | |   |   
    | |   +-o USR2@10  <class IORegistryEntry, id 0x10000024f, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/USR2@10"
    | |   |   }
    | |   |   
    | |   +-o SS01@11  <class IORegistryEntry, id 0x100000250, retain 8>
    | |   | | {
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS01@11"
    | |   | | }
    | |   | | 
    | |   | +-o DP01@1  <class IORegistryEntry, id 0x100000251, retain 4>
    | |   | |   {
    | |   | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS01@11/DP01@1"
    | |   | |   }
    | |   | |   
    | |   | +-o DP02@2  <class IORegistryEntry, id 0x100000252, retain 4>
    | |   | |   {
    | |   | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS01@11/DP02@2"
    | |   | |   }
    | |   | |   
    | |   | +-o DP03@3  <class IORegistryEntry, id 0x100000253, retain 4>
    | |   | |   {
    | |   | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS01@11/DP03@3"
    | |   | |   }
    | |   | |   
    | |   | +-o DP04@4  <class IORegistryEntry, id 0x100000254, retain 4>
    | |   |     {
    | |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS01@11/DP04@4"
    | |   |     }
    | |   |     
    | |   +-o SS02@12  <class IORegistryEntry, id 0x100000255, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS02@12"
    | |   |   }
    | |   |   
    | |   +-o SS03@13  <class IORegistryEntry, id 0x100000256, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS03@13"
    | |   |   }
    | |   |   
    | |   +-o SS04@14  <class IORegistryEntry, id 0x100000257, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS04@14"
    | |   |   }
    | |   |   
    | |   +-o SS05@15  <class IORegistryEntry, id 0x100000258, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS05@15"
    | |   |   }
    | |   |   
    | |   +-o SS06@16  <class IORegistryEntry, id 0x100000259, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS06@16"
    | |   |   }
    | |   |   
    | |   +-o HS11@b  <class IORegistryEntry, id 0x10000025a, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS11@b"
    | |   |   }
    | |   |   
    | |   +-o HS12@c  <class IORegistryEntry, id 0x10000025b, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS12@c"
    | |   |   }
    | |   |   
    | |   +-o HS13@d  <class IORegistryEntry, id 0x10000025c, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS13@d"
    | |   |   }
    | |   |   
    | |   +-o HS14@e  <class IORegistryEntry, id 0x10000025d, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/HS14@e"
    | |   |   }
    | |   |   
    | |   +-o SS07@17  <class IORegistryEntry, id 0x10000025e, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS07@17"
    | |   |   }
    | |   |   
    | |   +-o SS08@18  <class IORegistryEntry, id 0x10000025f, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS08@18"
    | |   |   }
    | |   |   
    | |   +-o SS09@19  <class IORegistryEntry, id 0x100000260, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS09@19"
    | |   |   }
    | |   |   
    | |   +-o SS10@1a  <class IORegistryEntry, id 0x100000261, retain 4>
    | |       {
    | |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC@140000/RHUB@0/SS10@1a"
    | |       }
    | |       
    | +-o HECI@16  <class IOPCIDevice, id 0x100000270, registered, matched, active, busy 0 (3 ms), retain 8>
    | |   {
    | |     "assigned-addresses" = <10b000827f000000004002920000000000100000>
    | |     "IOInterruptSpecifiers" = (<1000000007000000>,<0400000000000100>)
    | |     "IODeviceMemory" = (({"address"=547910467584,"length"=4096}))
    | |     "class-code" = <00800700>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <58140000>
    | |     "built-in" = <00>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,a2ba">
    | |     "vendor-id" = <86800000>
    | |     "acpi-pmcap-offset" = 80
    | |     "device-id" = <baa20000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci1458,1c3a","pci8086,a2ba","pciclass,078000","HECI">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/HECI@160000"
    | |     "subsystem-id" = <3a1c0000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:22:0"
    | |     "IOName" = "pci8086,a2ba"
    | |     "reg" = <00b000000000000000000000000000000000000010b0000200000000000000000000000000100000>
    | |   }
    | |   
    | +-o SAT0@17  <class IOPCIDevice, id 0x100000264, registered, matched, active, busy 0 (735 ms), retain 20>
    | | | {
    | | |   "assigned-addresses" = <10b8008200000000008054ed000000000020000014b800820000000000c054ed000000000001000018b800810000000050f0000000000000080000001cb800810000000040f00000000000000400000020b800810000000020f00000000000002000000024b800820000000000b054ed0000000000080000>
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>,<0500000000000100>)
    | | |   "IODeviceMemory" = (({"address"=3981737984,"length"=8192}),({"address"=3981754368,"length"=256}),"IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable",({"address"=3981750272,"length"=2048}))
    | | |   "class-code" = <01060100>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <58140000>
    | | |   "built-in" = <00>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | |   "name" = <"pci8086,a282">
    | | |   "vendor-id" = <86800000>
    | | |   "acpi-pmcap-offset" = 112
    | | |   "device-id" = <82a20000>
    | | |   "IOPCIResourced" = Yes
    | | |   "compatible" = <"pci1458,b005","pci8086,a282","pciclass,010601","SAT0">
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000"
    | | |   "subsystem-id" = <05b00000>
    | | |   "revision-id" = <00000000>
    | | |   "pcidebug" = "0:23:0"
    | | |   "IOName" = "pci8086,a282"
    | | |   "reg" = <00b800000000000000000000000000000000000010b800020000000000000000000000000020000014b800020000000000000000000000000001000018b80001000000000000000000000000080000001cb800010000000000000000000000000400000020b800010000000000000000000000002000000024b8000200000000000000000000000000080000>
    | | | }
    | | | 
    | | +-o PRT1@1ffff  <class IORegistryEntry, id 0x100000266, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000/PRT1@1ffff"
    | | |   }
    | | |   
    | | +-o NVM1@c1ffff  <class IORegistryEntry, id 0x10000026b, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000/NVM1@c1ffff"
    | | |   }
    | | |   
    | | +-o NVM2@c2ffff  <class IORegistryEntry, id 0x10000026c, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000/NVM2@c2ffff"
    | | |   }
    | | |   
    | | +-o NVM3@c3ffff  <class IORegistryEntry, id 0x10000026d, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000/NVM3@c3ffff"
    | | |   }
    | | |   
    | | +-o PRT0@0  <class AppleAHCIPort, id 0x100000265, registered, matched, active, busy 0 (512 ms), retain 12>
    | | | | {
    | | | |   "AHCI Port ALPM" = Yes
    | | | |   "IOPolledInterface" = "AppleAHCIPortPolledAdapter is not serializable"
    | | | |   "AHCI Port Hot Plug" = No
    | | | |   "IOMaximumSegmentByteCountRead" = 4194304
    | | | |   "64-bit" = Yes
    | | | |   "Trace ID" = 1507328
    | | | |   "IOMaximumSegmentByteCountWrite" = 4194304
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | | | |   "AHCI-Built-In" = Yes
    | | | |   "Physical Interconnect Location" = "Internal"
    | | | |   "AHCI Port Optimized Device Number" = 0
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "IOMaximumSegmentCountRead" = 256
    | | | |   "AHCI Port SNotification" = Yes
    | | | |   "AHCI Port ESATA" = No
    | | | |   "IOMaximumSegmentCountWrite" = 256
    | | | |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.31 Supported","Product Name"="AHCI Controller","Vendor Name"="Generic","Port Speed"="6 Gigabit"}
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000/PRT0@ffff"
    | | | |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="Internal"}
    | | | |   "AHCI-Ejectable" = No
    | | | | }
    | | | | 
    | | | +-o PMP@0  <class IOAHCIDevice, id 0x1000002cf, registered, matched, active, busy 0 (512 ms), retain 15>
    | | |   | {
    | | |   |   "IOUnit" = 0
    | | |   |   "Trace ID" = 1507328
    | | |   |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="6 Gigabit","Physical Interconnect Location"="Internal"}
    | | |   | }
    | | |   | 
    | | |   +-o @0:0  <class IOMedia, id 0x100000324, registered, matched, active, busy 0 (482 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "GUID_partition_scheme"
    | | |   |     "Whole" = Yes
    | | |   |     "Leaf" = No
    | | |   |     "BSD Name" = "disk1"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "IOMediaIcon" = {"IOBundleResourceFile"="Internal.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | | |   |     "BSD Minor" = 1
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 120034123776
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = ""
    | | |   |     "BSD Unit" = 1
    | | |   |   }
    | | |   |   
    | | |   +-o @0:1  <class IOMedia, id 0x100000353, registered, matched, active, busy 0 (3 ms), retain 9>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "DE94BBA4-06D1-4D40-A16A-BFD50179D6AC"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk1s1"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 1048576
    | | |   |     "BSD Minor" = 6
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "5BC9244B-75AB-486B-AB96-1B971290A3B8"
    | | |   |     "Partition ID" = 1
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 471859200
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = No
    | | |   |     "Content Hint" = "DE94BBA4-06D1-4D40-A16A-BFD50179D6AC"
    | | |   |     "BSD Unit" = 1
    | | |   |   }
    | | |   |   
    | | |   +-o @0:2  <class IOMedia, id 0x100000356, registered, matched, active, busy 0 (2 ms), retain 9>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk1s2"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 472907776
    | | |   |     "BSD Minor" = 7
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "4C78402F-F8F3-4A49-BE35-502BC1EBED18"
    | | |   |     "Partition ID" = 2
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 104857600
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = No
    | | |   |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "BSD Unit" = 1
    | | |   |   }
    | | |   |   
    | | |   +-o @0:3  <class IOMedia, id 0x100000358, registered, matched, active, busy 0 (3 ms), retain 9>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "E3C9E316-0B5C-4DB8-817D-F92DF00215AE"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk1s3"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 577765376
    | | |   |     "BSD Minor" = 14
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "2AA08AC5-5F04-4A62-89B5-33F8825D7B45"
    | | |   |     "Partition ID" = 3
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 16777216
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = No
    | | |   |     "Content Hint" = "E3C9E316-0B5C-4DB8-817D-F92DF00215AE"
    | | |   |     "BSD Unit" = 1
    | | |   |   }
    | | |   |   
    | | |   +-o @0:4  <class IOMedia, id 0x10000035c, registered, matched, active, busy 0 (3 ms), retain 10>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "EBD0A0A2-B9E5-4433-87C0-68B6B72699C7"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk1s4"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 594542592
    | | |   |     "BSD Minor" = 15
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "424A4603-53F1-471D-9C2F-B365B36AB258"
    | | |   |     "Partition ID" = 4
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 118535976448
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = "EBD0A0A2-B9E5-4433-87C0-68B6B72699C7"
    | | |   |     "BSD Unit" = 1
    | | |   |   }
    | | |   |   
    | | |   +-o @0:5  <class IOMedia, id 0x10000035e, registered, matched, active, busy 0 (3 ms), retain 9>
    | | |       {
    | | |         "Removable" = No
    | | |         "Content" = "DE94BBA4-06D1-4D40-A16A-BFD50179D6AC"
    | | |         "Whole" = No
    | | |         "Leaf" = Yes
    | | |         "BSD Name" = "disk1s5"
    | | |         "Ejectable" = No
    | | |         "Preferred Block Size" = 512
    | | |         "Base" = 119130816512
    | | |         "BSD Minor" = 19
    | | |         "IOGeneralInterest" = "IOCommand is not serializable"
    | | |         "Writable" = Yes
    | | |         "UUID" = "8E4CC719-FD51-4865-BAC5-9B409991E667"
    | | |         "Partition ID" = 5
    | | |         "BSD Major" = 1
    | | |         "Size" = 901775360
    | | |         "IOBusyInterest" = "IOCommand is not serializable"
    | | |         "Open" = No
    | | |         "Content Hint" = "DE94BBA4-06D1-4D40-A16A-BFD50179D6AC"
    | | |         "BSD Unit" = 1
    | | |       }
    | | |       
    | | +-o PRT2@2  <class AppleAHCIPort, id 0x100000267, registered, matched, active, busy 0 (690 ms), retain 12>
    | | | | {
    | | | |   "AHCI Port ALPM" = Yes
    | | | |   "IOPolledInterface" = "AppleAHCIPortPolledAdapter is not serializable"
    | | | |   "AHCI Port Hot Plug" = No
    | | | |   "IOMaximumSegmentByteCountRead" = 4194304
    | | | |   "64-bit" = Yes
    | | | |   "Trace ID" = 1507360
    | | | |   "IOMaximumSegmentByteCountWrite" = 4194304
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | | | |   "AHCI-Built-In" = Yes
    | | | |   "Physical Interconnect Location" = "Internal"
    | | | |   "AHCI Port Optimized Device Number" = 0
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "IOMaximumSegmentCountRead" = 256
    | | | |   "AHCI Port SNotification" = Yes
    | | | |   "AHCI Port ESATA" = No
    | | | |   "IOMaximumSegmentCountWrite" = 256
    | | | |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.31 Supported","Product Name"="AHCI Controller","Vendor Name"="Generic","Port Speed"="6 Gigabit"}
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000/PRT2@2ffff"
    | | | |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="Internal"}
    | | | |   "AHCI-Ejectable" = No
    | | | | }
    | | | | 
    | | | +-o PMP@0  <class IOAHCIDevice, id 0x1000002d2, registered, matched, active, busy 0 (690 ms), retain 13>
    | | |   | {
    | | |   |   "IOUnit" = 0
    | | |   |   "Trace ID" = 1507360
    | | |   |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="6 Gigabit","Physical Interconnect Location"="Internal"}
    | | |   | }
    | | |   | 
    | | |   +-o @0:0  <class IOMedia, id 0x100000309, registered, matched, active, busy 0 (677 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "GUID_partition_scheme"
    | | |   |     "Whole" = Yes
    | | |   |     "Leaf" = No
    | | |   |     "BSD Name" = "disk3"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "IOMediaIcon" = {"IOBundleResourceFile"="Internal.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | | |   |     "BSD Minor" = 3
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 4000787030016
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = ""
    | | |   |     "BSD Unit" = 3
    | | |   |   }
    | | |   |   
    | | |   +-o @0:1  <class IOMedia, id 0x10000035a, registered, matched, active, busy 0 (3 ms), retain 9>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk3s1"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 20480
    | | |   |     "BSD Minor" = 13
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "ED33E0FA-FF70-4DB6-9063-C8E37028D9E3"
    | | |   |     "Partition ID" = 1
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 209715200
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = No
    | | |   |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "BSD Unit" = 3
    | | |   |   }
    | | |   |   
    | | |   +-o @0:2  <class IOMedia, id 0x10000035d, registered, matched, active, busy 0 (191 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "53746F72-6167-11AA-AA11-00306543ECAC"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = No
    | | |   |     "BSD Name" = "disk3s2"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 209735680
    | | |   |     "BSD Minor" = 22
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "888FCF3F-E2EF-4DA9-AB58-3030DA7E94A6"
    | | |   |     "Partition ID" = 2
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 4000443056128
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = "53746F72-6167-11AA-AA11-00306543ECAC"
    | | |   |     "BSD Unit" = 3
    | | |   |   }
    | | |   |   
    | | |   +-o @0:3  <class IOMedia, id 0x100000361, registered, matched, active, busy 0 (24 ms), retain 9>
    | | |       {
    | | |         "Removable" = No
    | | |         "Content" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | | |         "Whole" = No
    | | |         "Leaf" = Yes
    | | |         "BSD Name" = "disk3s3"
    | | |         "Ejectable" = No
    | | |         "Preferred Block Size" = 512
    | | |         "Base" = 4000652791808
    | | |         "BSD Minor" = 18
    | | |         "IOGeneralInterest" = "IOCommand is not serializable"
    | | |         "Writable" = Yes
    | | |         "UUID" = "50584750-0049-4D1D-8098-7AB1B64ED373"
    | | |         "Partition ID" = 3
    | | |         "BSD Major" = 1
    | | |         "Size" = 134217728
    | | |         "IOBusyInterest" = "IOCommand is not serializable"
    | | |         "Open" = No
    | | |         "Content Hint" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | | |         "BSD Unit" = 3
    | | |       }
    | | |       
    | | +-o PRT3@3  <class AppleAHCIPort, id 0x100000268, registered, matched, active, busy 0 (504 ms), retain 12>
    | | | | {
    | | | |   "AHCI Port ALPM" = Yes
    | | | |   "IOPolledInterface" = "AppleAHCIPortPolledAdapter is not serializable"
    | | | |   "AHCI Port Hot Plug" = No
    | | | |   "IOMaximumSegmentByteCountRead" = 4194304
    | | | |   "64-bit" = Yes
    | | | |   "Trace ID" = 1507376
    | | | |   "IOMaximumSegmentByteCountWrite" = 4194304
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | | | |   "AHCI-Built-In" = Yes
    | | | |   "Physical Interconnect Location" = "Internal"
    | | | |   "AHCI Port Optimized Device Number" = 0
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "IOMaximumSegmentCountRead" = 256
    | | | |   "AHCI Port SNotification" = Yes
    | | | |   "AHCI Port ESATA" = No
    | | | |   "IOMaximumSegmentCountWrite" = 256
    | | | |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.31 Supported","Product Name"="AHCI Controller","Vendor Name"="Generic","Port Speed"="6 Gigabit"}
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000/PRT3@3ffff"
    | | | |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="Internal"}
    | | | |   "AHCI-Ejectable" = No
    | | | | }
    | | | | 
    | | | +-o PMP@0  <class IOAHCIDevice, id 0x1000002d5, registered, matched, active, busy 0 (504 ms), retain 13>
    | | |   | {
    | | |   |   "IOUnit" = 0
    | | |   |   "Trace ID" = 1507376
    | | |   |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="6 Gigabit","Physical Interconnect Location"="Internal"}
    | | |   | }
    | | |   | 
    | | |   +-o @0:0  <class IOMedia, id 0x100000313, registered, matched, active, busy 0 (490 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "GUID_partition_scheme"
    | | |   |     "Whole" = Yes
    | | |   |     "Leaf" = No
    | | |   |     "BSD Name" = "disk0"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "IOMediaIcon" = {"IOBundleResourceFile"="Internal.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | | |   |     "BSD Minor" = 0
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 500107862016
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = ""
    | | |   |     "BSD Unit" = 0
    | | |   |   }
    | | |   |   
    | | |   +-o @0:1  <class IOMedia, id 0x100000350, registered, matched, active, busy 0 (3 ms), retain 9>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk0s1"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 20480
    | | |   |     "BSD Minor" = 10
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "9206A9A1-AFF2-4849-9329-B9B904B628FE"
    | | |   |     "Partition ID" = 1
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 209715200
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = No
    | | |   |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "BSD Unit" = 0
    | | |   |   }
    | | |   |   
    | | |   +-o @0:2  <class IOMedia, id 0x100000352, registered, matched, active, busy 0 (5 ms), retain 10>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk0s2"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 209735680
    | | |   |     "BSD Minor" = 11
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "2283B836-B4FC-4ACD-8C6F-945F1B27465D"
    | | |   |     "Partition ID" = 2
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 498598100992
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |   |     "BSD Unit" = 0
    | | |   |   }
    | | |   |   
    | | |   +-o @0:3  <class IOMedia, id 0x100000354, registered, matched, active, busy 0 (5 ms), retain 9>
    | | |       {
    | | |         "Removable" = No
    | | |         "Content" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | | |         "Whole" = No
    | | |         "Leaf" = Yes
    | | |         "BSD Name" = "disk0s3"
    | | |         "Ejectable" = No
    | | |         "Preferred Block Size" = 512
    | | |         "Base" = 498807836672
    | | |         "BSD Minor" = 12
    | | |         "IOGeneralInterest" = "IOCommand is not serializable"
    | | |         "Writable" = Yes
    | | |         "UUID" = "CCC29F1E-6DD5-4493-8556-E21DFE2B7CAD"
    | | |         "Partition ID" = 3
    | | |         "BSD Major" = 1
    | | |         "Size" = 1300004864
    | | |         "IOBusyInterest" = "IOCommand is not serializable"
    | | |         "Open" = No
    | | |         "Content Hint" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | | |         "BSD Unit" = 0
    | | |       }
    | | |       
    | | +-o PRT4@4  <class AppleAHCIPort, id 0x100000269, registered, matched, active, busy 0 (705 ms), retain 12>
    | | | | {
    | | | |   "AHCI Port ALPM" = Yes
    | | | |   "IOPolledInterface" = "AppleAHCIPortPolledAdapter is not serializable"
    | | | |   "AHCI Port Hot Plug" = No
    | | | |   "IOMaximumSegmentByteCountRead" = 4194304
    | | | |   "64-bit" = Yes
    | | | |   "Trace ID" = 1507392
    | | | |   "IOMaximumSegmentByteCountWrite" = 4194304
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | | | |   "AHCI-Built-In" = Yes
    | | | |   "Physical Interconnect Location" = "Internal"
    | | | |   "AHCI Port Optimized Device Number" = 0
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "IOMaximumSegmentCountRead" = 256
    | | | |   "AHCI Port SNotification" = Yes
    | | | |   "AHCI Port ESATA" = No
    | | | |   "IOMaximumSegmentCountWrite" = 256
    | | | |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.31 Supported","Product Name"="AHCI Controller","Vendor Name"="Generic","Port Speed"="6 Gigabit"}
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000/PRT4@4ffff"
    | | | |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="Internal"}
    | | | |   "AHCI-Ejectable" = No
    | | | | }
    | | | | 
    | | | +-o PMP@0  <class IOAHCIDevice, id 0x1000002d7, registered, matched, active, busy 0 (705 ms), retain 13>
    | | |   | {
    | | |   |   "IOUnit" = 0
    | | |   |   "Trace ID" = 1507392
    | | |   |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="6 Gigabit","Physical Interconnect Location"="Internal"}
    | | |   | }
    | | |   | 
    | | |   +-o @0:0  <class IOMedia, id 0x10000030a, registered, matched, active, busy 0 (692 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "GUID_partition_scheme"
    | | |   |     "Whole" = Yes
    | | |   |     "Leaf" = No
    | | |   |     "BSD Name" = "disk4"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "IOMediaIcon" = {"IOBundleResourceFile"="Internal.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | | |   |     "BSD Minor" = 4
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 4000787030016
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = ""
    | | |   |     "BSD Unit" = 4
    | | |   |   }
    | | |   |   
    | | |   +-o @0:1  <class IOMedia, id 0x10000035f, registered, matched, active, busy 0 (3 ms), retain 9>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk4s1"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 20480
    | | |   |     "BSD Minor" = 20
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "16AEBFF4-BF81-4B13-8393-68B94459F8E2"
    | | |   |     "Partition ID" = 1
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 209715200
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = No
    | | |   |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "BSD Unit" = 4
    | | |   |   }
    | | |   |   
    | | |   +-o @0:2  <class IOMedia, id 0x100000362, registered, matched, active, busy 0 (207 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "53746F72-6167-11AA-AA11-00306543ECAC"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = No
    | | |   |     "BSD Name" = "disk4s2"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 209735680
    | | |   |     "BSD Minor" = 21
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "2D69FE73-69AB-4219-9891-DBFE67AF2532"
    | | |   |     "Partition ID" = 2
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 4000443056128
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = "53746F72-6167-11AA-AA11-00306543ECAC"
    | | |   |     "BSD Unit" = 4
    | | |   |   }
    | | |   |   
    | | |   +-o @0:3  <class IOMedia, id 0x100000363, registered, matched, active, busy 0 (46 ms), retain 9>
    | | |       {
    | | |         "Removable" = No
    | | |         "Content" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | | |         "Whole" = No
    | | |         "Leaf" = Yes
    | | |         "BSD Name" = "disk4s3"
    | | |         "Ejectable" = No
    | | |         "Preferred Block Size" = 512
    | | |         "Base" = 4000652791808
    | | |         "BSD Minor" = 16
    | | |         "IOGeneralInterest" = "IOCommand is not serializable"
    | | |         "Writable" = Yes
    | | |         "UUID" = "5948BF7B-805E-4B56-95B6-7BD12F4053A3"
    | | |         "Partition ID" = 3
    | | |         "BSD Major" = 1
    | | |         "Size" = 134217728
    | | |         "IOBusyInterest" = "IOCommand is not serializable"
    | | |         "Open" = No
    | | |         "Content Hint" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | | |         "BSD Unit" = 4
    | | |       }
    | | |       
    | | +-o PRT5@5  <class AppleAHCIPort, id 0x10000026a, registered, matched, active, busy 0 (133 ms), retain 12>
    | |   | {
    | |   |   "AHCI Port Optimized Device Number" = 0
    | |   |   "AHCI Port Hot Plug" = No
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.31 Supported","Product Name"="AHCI Controller","Vendor Name"="Generic","Port Speed"="6 Gigabit"}
    | |   |   "IOMaximumSegmentCountWrite" = 256
    | |   |   "IOPowerManagement" = {"ChildrenPowerState"=2,"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | |   |   "IOMaximumSegmentByteCountWrite" = 4194304
    | |   |   "IOMaximumSegmentByteCountRead" = 4194304
    | |   |   "Trace ID" = 1507408
    | |   |   "AHCI-Ejectable" = No
    | |   |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="Internal"}
    | |   |   "64-bit" = Yes
    | |   |   "AHCI-Built-In" = Yes
    | |   |   "IOMaximumSegmentCountRead" = 256
    | |   |   "Physical Interconnect Location" = "Internal"
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT0@170000/PRT5@5ffff"
    | |   |   "AHCI Port ALPM" = Yes
    | |   |   "AHCI Port SNotification" = Yes
    | |   |   "AHCI Port ESATA" = No
    | |   | }
    | |   | 
    | |   +-o PMP@0  <class IOAHCIDevice, id 0x1000002d9, registered, matched, active, busy 0 (133 ms), retain 9>
    | |       {
    | |         "IOUnit" = 0
    | |         "Trace ID" = 1507408
    | |         "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="1.5 Gigabit","Physical Interconnect Location"="Internal","ATAPI"=Yes}
    | |       }
    | |       
    | +-o RP17@1B  <class IOPCIDevice, id 0x100000225, registered, matched, active, busy 0 (6 ms), retain 11>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "IOPCIHPType" = 33
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <e7a20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "compatible" = <"pci8086,a2e7","pciclass,060400","RP17">
    | | |   "IOPCIHotPlug" = Yes
    | | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 292650017
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP17@1b0000"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 2049
    | | |   "IOPCIExpressCapabilities" = 66
    | | |   "pcidebug" = "0:27:0(2:2)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00d8000000000000000000000000000000000000>
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP17 0"})
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000226, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP17@1b0000/PXSX@0"
    | |     }
    | |     
    | +-o RP19@1B,2  <class IOPCIDevice, id 0x100000229, registered, matched, active, busy 0 (5 ms), retain 11>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1200000007000000>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP19 0"})
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPCIExpressSlotStatus" = 0
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <e9a20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,a2e9","pciclass,060400","RP19">
    | | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 326266915
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP19@1b0002"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 4097
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:27:2(3:3)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00da000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 11861248
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x10000022a, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP19@1b0002/PXSX@0"
    | |     }
    | |     
    | +-o RP21@1B,4  <class IOPCIDevice, id 0x10000022d, registered, matched, active, busy 0 (5 ms), retain 11>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP21 0"})
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPCIExpressSlotStatus" = 0
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <eba20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,a2eb","pciclass,060400","RP21">
    | | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 359821379
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP21@1b0004"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 4097
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:27:4(4:4)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00dc000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 12909824
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x10000022e, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP21@1b0004/PXSX@0"
    | |     }
    | |     
    | +-o RP01@1C  <class IOPCIDevice, id 0x100000214, registered, matched, active, busy 0 (49 ms), retain 11>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP01 0"})
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPCIExpressSlotStatus" = 320
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <90a20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,a290","pciclass,060400","RP01">
    | | |   "ranges" = <0000008200000000000040ed0000008200000000000040ed0000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 24264723
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 28689
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:28:0(5:5)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e0000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 2404864
    | | | }
    | | | 
    | | +-o PXSX@0  <class IOPCIDevice, id 0x100000215, registered, matched, active, busy 0 (43 ms), retain 10>
    | |     {
    | |       "assigned-addresses" = <1000058200000000000040ed0000000000100000>
    | |       "IOInterruptSpecifiers" = (<1000000007000000>,<0800000000000100>)
    | |       "class-code" = <10000c00>
    | |       "IODeviceMemory" = (({"address"=3980394496,"length"=4096}))
    | |       "pci-aspm-supported" = Yes
    | |       "IOReportLegendPublic" = Yes
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "subsystem-vendor-id" = <01590000>
    | |       "built-in" = <00>
    | |       "pci-aspm-default" = 0
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "IOPCIMSIMode" = Yes
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "name" = <"pci11c1,5901">
    | |       "IOChildIndex" = 1
    | |       "device-id" = <01590000>
    | |       "vendor-id" = <c1110000>
    | |       "acpi-pmcap-offset" = 68
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci5901,1101","pci11c1,5901","pciclass,0c0010","PXSX">
    | |       "IOPCIExpressLinkCapabilities" = 474129
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/PXSX@0"
    | |       "subsystem-id" = <01110000>
    | |       "revision-id" = <08000000>
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "IOPCIExpressCapabilities" = 1
    | |       "pcidebug" = "5:0:0"
    | |       "IOName" = "pci11c1,5901"
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="PXSX 1"})
    | |       "reg" = <00000500000000000000000000000000000000001000050200000000000000000000000000100000>
    | |     }
    | |     
    | +-o RP02@1C,1  <class IOPCIDevice, id 0x100000216, registered, matched, active, busy 0 (5 ms), retain 11>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1100000007000000>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP02 0"})
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPCIExpressSlotStatus" = 0
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <91a20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,a291","pciclass,060400","RP02">
    | | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 41054227
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP02@1c0001"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 4097
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:28:1(6:6)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e1000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 2929152
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x100000217, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP02@1c0001/PXSX@0"
    | |     }
    | |     
    | +-o RP03@1C,2  <class IOPCIDevice, id 0x100000218, registered, matched, active, busy 0 (544 ms), retain 12>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1200000007000000>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP03 0"})
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPCIExpressSlotStatus" = 320
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <92a20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,a292","pciclass,060400","RP03">
    | | |   "ranges" = <0000008200000000000030ed0000008200000000000030ed0000000000001000000000c20000000000000000000000c200000000000000000000000000000000000000810000000000d00000000000810000000000d000000000000000100000>
    | | |   "IOPCIExpressLinkCapabilities" = 57819155
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP03@1c0002"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 28689
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:28:2(7:7)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e2000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 3453440
    | | | }
    | | | 
    | | +-o D061@0  <class IORegistryEntry, id 0x10000021a, retain 4>
    | | |   {
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "built-in" = <01>
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP03@1c0002/D061@0"
    | | |   }
    | | |   
    | | +-o PXSX@0  <class IOPCIDevice, id 0x100000219, registered, matched, active, busy 0 (538 ms), retain 11>
    | |     {
    | |       "assigned-addresses" = <1000078200000000000030ed0000000000000400180007810000000000d000000000000080000000>
    | |       "IOInterruptSpecifiers" = (<1200000007000000>,<0b00000000000100>)
    | |       "class-code" = <00000200>
    | |       "IODeviceMemory" = (({"address"=3979345920,"length"=262144}),"IOSubMemoryDescriptor is not serializable")
    | |       "IOReportLegendPublic" = Yes
    | |       "built-in" = <00>
    | |       "subsystem-vendor-id" = <58140000>
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "pci-aspm-default" = 0
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "IOPCIMSIMode" = Yes
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "name" = <"ethernet">
    | |       "IOChildIndex" = 1
    | |       "device-id" = <b1e00000>
    | |       "vendor-id" = <69190000>
    | |       "acpi-pmcap-offset" = 64
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci1458,e000","pci1969,e0b1","pciclass,020000","PXSX">
    | |       "IOPCIExpressLinkCapabilities" = 523281
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP03@1c0002/PXSX@0"
    | |       "subsystem-id" = <00e00000>
    | |       "revision-id" = <10000000>
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "IOPCIExpressCapabilities" = 1
    | |       "pcidebug" = "7:0:0"
    | |       "IOName" = "ethernet"
    | |       "acpi-wake-type" = 2
    | |       "reg" = <000007000000000000000000000000000000000010000702000000000000000000000000000004001800070100000000000000000000000080000000>
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="PXSX 1"})
    | |     }
    | |     
    | +-o RP05@1C,4  <class IOPCIDevice, id 0x10000021d, registered, matched, active, busy 0 (498 ms), retain 11>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP05 0"})
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPCIExpressSlotStatus" = 320
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <94a20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,a294","pciclass,060400","RP05">
    | | |   "ranges" = <0000008200000000000000dc0000008200000000000000dc0000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 91373635
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 28739
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:28:4(8:13)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e4000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 4521216
    | | | }
    | | | 
    | | +-o PXSX@0  <class IOPCIDevice, id 0x10000021e, registered, matched, active, busy 0 (493 ms), retain 14>
    | |   | {
    | |   |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | |   |   "#address-cells" = <03000000>
    | |   |   "class-code" = <00040600>
    | |   |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |   "built-in" = <00>
    | |   |   "pci-aspm-default" = 0
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "IOInterruptControllers" = ("io-apic-0")
    | |   |   "vendor-id" = <86800000>
    | |   |   "IOChildIndex" = 1
    | |   |   "device-id" = <d3150000>
    | |   |   "name" = <"pci-bridge">
    | |   |   "acpi-pmcap-offset" = 128
    | |   |   "IOPCIResourced" = Yes
    | |   |   "compatible" = <"pci8086,15d3","pciclass,060400","PXSX">
    | |   |   "ranges" = <0000008200000000000000dc0000008200000000000000dc0000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   |   "IOPCIExpressLinkCapabilities" = 4545603
    | |   |   "IODTPersist" = <>
    | |   |   "IOPCIConfigured" = Yes
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP05@1c0004/PXSX@0"
    | |   |   "revision-id" = <02000000>
    | |   |   "IOPCIExpressLinkStatus" = 4163
    | |   |   "IOPCIExpressCapabilities" = 82
    | |   |   "pcidebug" = "8:0:0(9:13)"
    | |   |   "IOName" = "pci-bridge"
    | |   |   "#size-cells" = <02000000>
    | |   |   "reg" = <0000080000000000000000000000000000000000>
    | |   | }
    | |   | 
    | |   +-o pci-bridge@0  <class IOPCIDevice, id 0x100000285, registered, matched, active, busy 0 (0 ms), retain 10>
    | |   |   {
    | |   |     "IOInterruptSpecifiers" = (<1000000007000000>)
    | |   |     "#address-cells" = <03000000>
    | |   |     "class-code" = <00040600>
    | |   |     "IOPCIExpressSlotStatus" = 72
    | |   |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |     "pci-aspm-default" = 0
    | |   |     "IOInterruptControllers" = ("io-apic-0")
    | |   |     "vendor-id" = <86800000>
    | |   |     "IOChildIndex" = 1
    | |   |     "device-id" = <d3150000>
    | |   |     "name" = <"pci-bridge">
    | |   |     "acpi-pmcap-offset" = 128
    | |   |     "IOPCIResourced" = Yes
    | |   |     "compatible" = <"pci8086,15d3","pciclass,060400">
    | |   |     "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   |     "IOPCIExpressLinkCapabilities" = 6380609
    | |   |     "IODTPersist" = <>
    | |   |     "IOPCIConfigured" = Yes
    | |   |     "revision-id" = <02000000>
    | |   |     "IOPCIExpressLinkStatus" = 4161
    | |   |     "IOPCIExpressCapabilities" = 354
    | |   |     "pcidebug" = "9:0:0(13:13)"
    | |   |     "IOName" = "pci-bridge"
    | |   |     "#size-cells" = <02000000>
    | |   |     "reg" = <0000090000000000000000000000000000000000>
    | |   |     "IOPCIExpressSlotCapabilities" = 262144
    | |   |   }
    | |   |   
    | |   +-o pci-bridge@1  <class IOPCIDevice, id 0x100000286, registered, matched, active, busy 0 (1 ms), retain 10>
    | |   |   {
    | |   |     "IOInterruptSpecifiers" = (<1100000007000000>)
    | |   |     "#address-cells" = <03000000>
    | |   |     "class-code" = <00040600>
    | |   |     "IOPCIExpressSlotStatus" = 0
    | |   |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |     "pci-aspm-default" = 0
    | |   |     "IOInterruptControllers" = ("io-apic-0")
    | |   |     "vendor-id" = <86800000>
    | |   |     "IOChildIndex" = 2
    | |   |     "device-id" = <d3150000>
    | |   |     "name" = <"pci-bridge">
    | |   |     "acpi-pmcap-offset" = 128
    | |   |     "IOPCIResourced" = Yes
    | |   |     "compatible" = <"pci8086,15d3","pciclass,060400">
    | |   |     "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   |     "IOPCIExpressLinkCapabilities" = 24206401
    | |   |     "IODTPersist" = <>
    | |   |     "IOPCIConfigured" = Yes
    | |   |     "revision-id" = <02000000>
    | |   |     "IOPCIExpressLinkStatus" = 4161
    | |   |     "IOPCIExpressCapabilities" = 354
    | |   |     "pcidebug" = "9:1:0(12:12)"
    | |   |     "IOName" = "pci-bridge"
    | |   |     "#size-cells" = <02000000>
    | |   |     "reg" = <0008090000000000000000000000000000000000>
    | |   |     "IOPCIExpressSlotCapabilities" = 786528
    | |   |   }
    | |   |   
    | |   +-o pci-bridge@2  <class IOPCIDevice, id 0x100000287, registered, matched, active, busy 0 (460 ms), retain 11>
    | |   | | {
    | |   | |   "IOInterruptSpecifiers" = (<1200000007000000>)
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "class-code" = <00040600>
    | |   | |   "IOPCIExpressSlotStatus" = 72
    | |   | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "IOInterruptControllers" = ("io-apic-0")
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOChildIndex" = 3
    | |   | |   "device-id" = <d3150000>
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "compatible" = <"pci8086,15d3","pciclass,060400">
    | |   | |   "ranges" = <0000008200000000000000dc0000008200000000000000dc0000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "IOPCIExpressLinkCapabilities" = 39935041
    | |   | |   "IODTPersist" = <>
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "revision-id" = <02000000>
    | |   | |   "IOPCIExpressLinkStatus" = 4161
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "pcidebug" = "9:2:0(11:11)"
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "reg" = <0010090000000000000000000000000000000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 262144
    | |   | | }
    | |   | | 
    | |   | +-o pci8086,15d4@0  <class IOPCIDevice, id 0x100000289, registered, matched, active, busy 0 (459 ms), retain 11>
    | |   |     {
    | |   |       "assigned-addresses" = <10000b8200000000000000dc0000000000000100>
    | |   |       "IOInterruptSpecifiers" = (<1200000007000000>,<0c00000000000100>)
    | |   |       "class-code" = <30030c00>
    | |   |       "IODeviceMemory" = (({"address"=3690987520,"length"=65536}))
    | |   |       "IOReportLegendPublic" = Yes
    | |   |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |       "subsystem-vendor-id" = <22220000>
    | |   |       "pci-aspm-default" = 0
    | |   |       "IOPCIMSIMode" = Yes
    | |   |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   |       "vendor-id" = <86800000>
    | |   |       "IOChildIndex" = 1
    | |   |       "acpi-pmcap-offset" = 128
    | |   |       "device-id" = <d4150000>
    | |   |       "name" = <"pci8086,15d4">
    | |   |       "IOPCIResourced" = Yes
    | |   |       "compatible" = <"pci2222,1111","pci8086,15d4","pciclass,0c0330">
    | |   |       "IOPCIExpressLinkCapabilities" = 4545601
    | |   |       "subsystem-id" = <11110000>
    | |   |       "revision-id" = <02000000>
    | |   |       "IOPCIExpressLinkStatus" = 4161
    | |   |       "IOPCIExpressCapabilities" = 2
    | |   |       "pcidebug" = "11:0:0"
    | |   |       "IOName" = "pci8086,15d4"
    | |   |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="pci8086,15d4 1"})
    | |   |       "reg" = <00000b000000000000000000000000000000000010000b0200000000000000000000000000000100>
    | |   |     }
    | |   |     
    | |   +-o pci-bridge@4  <class IOPCIDevice, id 0x100000288, registered, matched, active, busy 0 (0 ms), retain 10>
    | |       {
    | |         "IOInterruptSpecifiers" = (<1000000007000000>)
    | |         "#address-cells" = <03000000>
    | |         "class-code" = <00040600>
    | |         "IOPCIExpressSlotStatus" = 0
    | |         "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |         "pci-aspm-default" = 0
    | |         "IOInterruptControllers" = ("io-apic-0")
    | |         "vendor-id" = <86800000>
    | |         "IOChildIndex" = 4
    | |         "device-id" = <d3150000>
    | |         "name" = <"pci-bridge">
    | |         "acpi-pmcap-offset" = 128
    | |         "IOPCIResourced" = Yes
    | |         "compatible" = <"pci8086,15d3","pciclass,060400">
    | |         "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |         "IOPCIExpressLinkCapabilities" = 74538049
    | |         "IODTPersist" = <>
    | |         "IOPCIConfigured" = Yes
    | |         "revision-id" = <02000000>
    | |         "IOPCIExpressLinkStatus" = 4161
    | |         "IOPCIExpressCapabilities" = 354
    | |         "pcidebug" = "9:4:0(10:10)"
    | |         "IOName" = "pci-bridge"
    | |         "#size-cells" = <02000000>
    | |         "reg" = <0020090000000000000000000000000000000000>
    | |         "IOPCIExpressSlotCapabilities" = 2359392
    | |       }
    | |       
    | +-o RP09@1D  <class IOPCIDevice, id 0x10000020a, registered, matched, active, busy 0 (571 ms), retain 11>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP09 0"})
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPCIExpressSlotStatus" = 320
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <98a20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,a298","pciclass,060400","RP09">
    | | |   "ranges" = <0000008200000000000020ed0000008200000000000020ed0000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 158482467
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP09@1d0000"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 28707
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:29:0(65:65)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e8000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 6618368
    | | | }
    | | | 
    | | +-o PXSX@0  <class IOPCIDevice, id 0x10000020b, registered, matched, active, busy 0 (567 ms), retain 12>
    | |   | {
    | |   |   "assigned-addresses" = <1000418200000000000020ed0000000000400000>
    | |   |   "IOInterruptSpecifiers" = (<1000000007000000>,<0a00000000000100>)
    | |   |   "class-code" = <02080100>
    | |   |   "IODeviceMemory" = (({"address"=3978297344,"length"=16384}))
    | |   |   "IOReportLegendPublic" = Yes
    | |   |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |   "subsystem-vendor-id" = <4d140000>
    | |   |   "built-in" = <00>
    | |   |   "pci-aspm-default" = 0
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "IOPCIMSIMode" = Yes
    | |   |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   |   "name" = <"pci144d,a804">
    | |   |   "IOChildIndex" = 1
    | |   |   "device-id" = <04a80000>
    | |   |   "vendor-id" = <4d140000>
    | |   |   "IOPCIResourced" = Yes
    | |   |   "compatible" = <"pci144d,a801","pci144d,a804","pciclass,010802","PXSX">
    | |   |   "IOPCIExpressLinkCapabilities" = 4683843
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP09@1d0000/PXSX@0"
    | |   |   "subsystem-id" = <01a80000>
    | |   |   "revision-id" = <00000000>
    | |   |   "IOPCIExpressLinkStatus" = 4131
    | |   |   "IOPCIExpressCapabilities" = 2
    | |   |   "pcidebug" = "65:0:0"
    | |   |   "IOName" = "pci144d,a804"
    | |   |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="PXSX 1"})
    | |   |   "reg" = <00004100000000000000000000000000000000001000410200000000000000000000000000400000>
    | |   | }
    | |   | 
    | |   +-o IONVMeController  <class IONVMeController, id 0x1000002db, registered, matched, active, busy 0 (527 ms), retain 10>
    | |     | {
    | |     |   "IOClass" = "IONVMeController"
    | |     |   "IOPolledInterface" = "IONVMeControllerPolledAdapter is not serializable"
    | |     |   "IOMaximumSegmentByteCountRead" = 4096
    | |     |   "IOReportLegendPublic" = Yes
    | |     |   "IOCommandPoolSize" = 256
    | |     |   "IOProviderClass" = "IOPCIDevice"
    | |     |   "Physical Interconnect Location" = "Internal"
    | |     |   "IOMaximumSegmentByteCountWrite" = 4096
    | |     |   "IOMaximumSegmentCountRead" = 256
    | |     |   "Model Number" = "Samsung SSD 960 EVO 1TB"
    | |     |   "IOProbeScore" = 0
    | |     |   "IOPowerManagement" = {"DevicePowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"MaxPowerState"=2,"DriverPowerState"=2}
    | |     |   "IOMaximumSegmentCountWrite" = 256
    | |     |   "Serial Number" = "S3ETNX0J609310V"
    | |     |   "NVMe Revision Supported" = "1.20"
    | |     |   "IOPCIPauseCompatible" = Yes
    | |     |   "Physical Interconnect" = "PCI-Express"
    | |     |   "Chipset Name" = "SSD Controller"
    | |     |   "Controller Characteristics" = {"Preferred IO Size"=131072}
    | |     |   "IOMatchCategory" = "IODefaultMatchCategory"
    | |     |   "CFBundleIdentifier" = "com.apple.iokit.IONVMeFamily"
    | |     |   "Vendor Name" = "Apple"
    | |     |   "IOMinimumSegmentAlignmentByteCount" = 4
    | |     |   "Firmware Revision" = "2B7QCXE7"
    | |     |   "IOPCITunnelCompatible" = Yes
    | |     |   "IOReportLegend" = ({"IOReportChannels"=((5644784279684675442,12885032962,"NVMe Power States")),"IOReportGroupName"="NVMe","IOReportChannelInfo"={"IOReportChannelUnit"=72058100844068865}})
    | |     |   "IOUnitName" = "disk"
    | |     |   "IOPCIClassMatch" = "0x01080200&0xffffff00"
    | |     | }
    | |     | 
    | |     +-o IONVMeBlockStorageDevice@1  <class IONVMeBlockStorageDevice, id 0x10000031a, registered, matched, active, busy 0 (527 ms), retain 13>
    | |       | {
    | |       |   "IOCFPlugInTypes" = {"AA0FA6F9-C2D6-457F-B10B-59A13253292F"="NVMeSMARTLib.plugin"}
    | |       |   "NamespaceUUID" = 1557595046964372736
    | |       |   "NamespaceID" = 1
    | |       |   "IOUnit" = 1
    | |       |   "ThermalThrottlingSupported" = No
    | |       |   "IOReportLegend" = ({"IOReportGroupName"="NVMe","IOReportChannels"=((6082504312848663127,6442450945,"Tier0 BW Scale Factor"),(6082504312865440343,6442450945,"Tier1 BW Scale Factor"),(6082504312882217559,6442450945,"Tier2 BW Scale Factor"),(6082504312898994775,6442450945,"Tier3 BW Scale Factor")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="BW Limits"},{"IOReportGroupName"="NVMe","IOReportChannels"=((6084209303804800357,6442450945,"Total time elapsed"),(6082504312848654368,6442450945,"Tier0 Throttle Time"),(6082504312865431584,6442450945,"Tier1 Throttle Time"),(6082504312882208800,6442450945,"Tier2 Throttle Time"),(6082504312898986016,6442450945,"Tier3 Throttle Time")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="Time weighted throttle statistics"})
    | |       |   "device-type" = "Generic"
    | |       |   "IOReportLegendPublic" = Yes
    | |       |   "Protocol Characteristics" = {"Physical Interconnect"="PCI-Express","Physical Interconnect Location"="Internal"}
    | |       |   "Device Characteristics" = {"Serial Number"="S3ETNX0J609310V","Medium Type"="Solid State","Product Name"="Samsung SSD 960 EVO 1TB","Vendor Name"="","Product Revision Level"="2B7QCXE7"}
    | |       |   "IOStorageFeatures" = {"Unmap"=Yes,"Priority"=No,"Barrier"=No}
    | |       |   "NVMe SMART Capable" = Yes
    | |       | }
    | |       | 
    | |       +-o @1:0  <class IOMedia, id 0x10000031c, registered, matched, active, busy 0 (527 ms), retain 11>
    | |       |   {
    | |       |     "Removable" = No
    | |       |     "Content" = "GUID_partition_scheme"
    | |       |     "Whole" = Yes
    | |       |     "Leaf" = No
    | |       |     "BSD Name" = "disk2"
    | |       |     "Ejectable" = No
    | |       |     "Preferred Block Size" = 512
    | |       |     "IOMediaIcon" = {"IOBundleResourceFile"="Internal.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | |       |     "BSD Minor" = 2
    | |       |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |       |     "Writable" = Yes
    | |       |     "BSD Major" = 1
    | |       |     "Size" = 1000204886016
    | |       |     "IOBusyInterest" = "IOCommand is not serializable"
    | |       |     "Open" = Yes
    | |       |     "Content Hint" = ""
    | |       |     "BSD Unit" = 2
    | |       |   }
    | |       |   
    | |       +-o @1:1  <class IOMedia, id 0x100000355, registered, matched, active, busy 0 (3 ms), retain 9>
    | |       |   {
    | |       |     "Removable" = No
    | |       |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | |       |     "Whole" = No
    | |       |     "Leaf" = Yes
    | |       |     "BSD Name" = "disk2s1"
    | |       |     "Ejectable" = No
    | |       |     "Preferred Block Size" = 512
    | |       |     "Base" = 20480
    | |       |     "BSD Minor" = 5
    | |       |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |       |     "Writable" = Yes
    | |       |     "UUID" = "FC8D3FA3-0924-427E-B973-A85AA1DCDE86"
    | |       |     "Partition ID" = 1
    | |       |     "BSD Major" = 1
    | |       |     "Size" = 209715200
    | |       |     "IOBusyInterest" = "IOCommand is not serializable"
    | |       |     "Open" = No
    | |       |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | |       |     "BSD Unit" = 2
    | |       |   }
    | |       |   
    | |       +-o @1:2  <class IOMedia, id 0x100000357, registered, matched, active, busy 0 (46 ms), retain 11>
    | |       |   {
    | |       |     "Removable" = No
    | |       |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | |       |     "Whole" = No
    | |       |     "Leaf" = Yes
    | |       |     "BSD Name" = "disk2s2"
    | |       |     "Ejectable" = No
    | |       |     "Preferred Block Size" = 512
    | |       |     "Base" = 209735680
    | |       |     "BSD Minor" = 8
    | |       |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |       |     "Writable" = Yes
    | |       |     "UUID" = "BA8E7A42-418F-4CC4-96A4-E0E7B5EF878F"
    | |       |     "Partition ID" = 2
    | |       |     "BSD Major" = 1
    | |       |     "Size" = 600026603520
    | |       |     "IOBusyInterest" = "IOCommand is not serializable"
    | |       |     "Open" = Yes
    | |       |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | |       |     "BSD Unit" = 2
    | |       |   }
    | |       |   
    | |       +-o @1:3  <class IOMedia, id 0x100000359, registered, matched, active, busy 0 (3 ms), retain 9>
    | |       |   {
    | |       |     "Removable" = No
    | |       |     "Content" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | |       |     "Whole" = No
    | |       |     "Leaf" = Yes
    | |       |     "BSD Name" = "disk2s3"
    | |       |     "Ejectable" = No
    | |       |     "Preferred Block Size" = 512
    | |       |     "Base" = 600236339200
    | |       |     "BSD Minor" = 17
    | |       |     "IOGeneralInterest" = "IOCommand is not serializable"
    | |       |     "Writable" = Yes
    | |       |     "UUID" = "ECC1A294-536D-4CAE-AF3A-A790B73F828B"
    | |       |     "Partition ID" = 3
    | |       |     "BSD Major" = 1
    | |       |     "Size" = 650002432
    | |       |     "IOBusyInterest" = "IOCommand is not serializable"
    | |       |     "Open" = No
    | |       |     "Content Hint" = "426F6F74-0000-11AA-AA11-00306543ECAC"
    | |       |     "BSD Unit" = 2
    | |       |   }
    | |       |   
    | |       +-o @1:4  <class IOMedia, id 0x10000035b, registered, matched, active, busy 0 (3 ms), retain 10>
    | |           {
    | |             "Removable" = No
    | |             "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | |             "Whole" = No
    | |             "Leaf" = Yes
    | |             "BSD Name" = "disk2s4"
    | |             "Ejectable" = No
    | |             "Preferred Block Size" = 512
    | |             "Base" = 600886341632
    | |             "BSD Minor" = 9
    | |             "IOGeneralInterest" = "IOCommand is not serializable"
    | |             "Writable" = Yes
    | |             "UUID" = "83730A2D-A2A0-406C-83B6-EB55763BD038"
    | |             "Partition ID" = 4
    | |             "BSD Major" = 1
    | |             "Size" = 399184306176
    | |             "IOBusyInterest" = "IOCommand is not serializable"
    | |             "Open" = Yes
    | |             "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | |             "BSD Unit" = 2
    | |           }
    | |           
    | +-o RP11@1D,2  <class IOPCIDevice, id 0x10000020e, registered, matched, active, busy 0 (3 ms), retain 11>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1200000007000000>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP11 0"})
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPCIExpressSlotStatus" = 264
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <9aa20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,a29a","pciclass,060400","RP11">
    | | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 192036899
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP11@1d0002"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 20513
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:29:2(66:66)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00ea000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 7666944
    | | | }
    | | | 
    | | +-o PXSX@0  <class IORegistryEntry, id 0x10000020f, retain 4>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP11@1d0002/PXSX@0"
    | |     }
    | |     
    | +-o RP14@1D,5  <class IOPCIDevice, id 0x100000235, registered, matched, active, busy 0 (1190 ms), retain 11>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1100000007000000>)
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="RP14 0"})
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPCIExpressSlotStatus" = 320
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <9da20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = <>
    | | |   "compatible" = <"pci8086,a29d","pciclass,060400","RP14">
    | | |   "ranges" = <0000008200000000000010ed0000008200000000000010ed0000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 242380819
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP14@1d0005"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 24593
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:29:5(67:67)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00ed000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 9220608
    | | | }
    | | | 
    | | +-o PXSX@0  <class IOPCIDevice, id 0x100000236, registered, matched, active, busy 0 (1186 ms), retain 12>
    | |     {
    | |       "assigned-addresses" = <1000438200000000000010ed0000000000000200>
    | |       "IOInterruptSpecifiers" = (<1100000007000000>,<0900000000000100>)
    | |       "class-code" = <00800200>
    | |       "IODeviceMemory" = (({"address"=3977248768,"length"=131072}))
    | |       "IOReportLegendPublic" = Yes
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "subsystem-vendor-id" = <8c160000>
    | |       "built-in" = <00>
    | |       "pci-aspm-default" = 0
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "name" = <"pci168c,30">
    | |       "IOChildIndex" = 1
    | |       "device-id" = <30000000>
    | |       "vendor-id" = <8c160000>
    | |       "acpi-pmcap-offset" = 64
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci168c,3112","pci168c,30","pciclass,028000","PXSX">
    | |       "IOPCIExpressLinkCapabilities" = 220177
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP14@1d0005/PXSX@0"
    | |       "subsystem-id" = <12310000>
    | |       "revision-id" = <01000000>
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "IOPCIExpressCapabilities" = 2
    | |       "pcidebug" = "67:0:0"
    | |       "IOName" = "pci168c,30"
    | |       "acpi-wake-type" = 2
    | |       "reg" = <00004300000000000000000000000000000000001000430200000000000000000000000000000200>
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="PXSX 0"})
    | |     }
    | |     
    | +-o LPCB@1F  <class IOPCIDevice, id 0x100000209, registered, matched, active, busy 0 (58 ms), retain 22>
    | | | {
    | | |   "name" = <"pci8086,a2c5">
    | | |   "compatible" = <"pci1458,5001","pci8086,a2c5","pciclass,060100","LPCB">
    | | |   "subsystem-vendor-id" = <58140000>
    | | |   "IOName" = "pci8086,a2c5"
    | | |   "reg" = <00f8000000000000000000000000000000000000>
    | | |   "device-id" = <c5a20000>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "IOPCIResourced" = Yes
    | | |   "revision-id" = <00000000>
    | | |   "vendor-id" = <86800000>
    | | |   "pcidebug" = "0:31:0"
    | | |   "class-code" = <00010600>
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/LPCB@1f0000"
    | | |   "subsystem-id" = <01500000>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | }
    | | | 
    | | +-o SIO1  <class IOACPIPlatformDevice, id 0x100000161, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "_UID" = "0"
    | | |     "IODeviceMemory" = (({"address"=2560,"length"=48}),({"address"=2608,"length"=16}),({"address"=2624,"length"=16}))
    | | |     "name" = <"PNP0C02">
    | | |   }
    | | |   
    | | +-o PS2K  <class IOACPIPlatformDevice, id 0x100000162, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "IODeviceMemory" = (({"address"=96,"length"=1}),({"address"=100,"length"=1}))
    | | |     "acpi-wake-gpe" = 29
    | | |     "compatible" = <"PNP030B">
    | | |     "_UID" = "0"
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "_STA" = 15
    | | |     "IOInterruptSpecifiers" = (<0100000000000000>)
    | | |     "name" = <"PNP0303">
    | | |   }
    | | |   
    | | +-o PS2M  <class IOACPIPlatformDevice, id 0x100000163, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "IODeviceMemory" = (({"address"=96,"length"=1}),({"address"=100,"length"=1}))
    | | |     "acpi-wake-gpe" = 29
    | | |     "compatible" = <"PNP0F13">
    | | |     "_UID" = "0"
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "_STA" = 15
    | | |     "IOInterruptSpecifiers" = (<0c00000000000000>)
    | | |     "name" = <"PNP0F03">
    | | |   }
    | | |   
    | | +-o FWHD  <class IOACPIPlatformDevice, id 0x100000164, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "name" = <"INT0800">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=4278190080,"length"=16777216}))
    | | |   }
    | | |   
    | | +-o HPET  <class IOACPIPlatformDevice, id 0x100000165, registered, matched, active, busy 0 (1 ms), retain 8>
    | | |   {
    | | |     "_STA" = 15
    | | |     "_UID" = "0"
    | | |     "IODeviceMemory" = (({"address"=4275044352,"length"=1024}))
    | | |     "name" = <"PNP0103">
    | | |     "IOInterruptControllers" = ("io-apic-0","io-apic-0","io-apic-0","io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<1400000000000000>,<1500000000000000>,<0b00000000000000>,<1600000000000000>)
    | | |   }
    | | |   
    | | +-o IPIC  <class IOACPIPlatformDevice, id 0x100000166, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=32,"length"=2}),({"address"=36,"length"=2}),({"address"=40,"length"=2}),({"address"=44,"length"=2}),({"address"=48,"length"=2}),({"address"=52,"length"=2}),({"address"=56,"length"=2}),({"address"=60,"length"=2}),({"address"=160,"length"=2}),({"address"=164,"length"=2}),({"address"=168,"length"=2}),({"address"=172,"length"=2}),({"address"=176,"length"=2}),({"address"=180,"length"=2}),({"address"=184,"length"=2}),({"address"=188,"length"=2}),({"address"=1232,"length"=2}))
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<0200000000000000>)
    | | |     "name" = <"PNP0000">
    | | |   }
    | | |   
    | | +-o MATH  <class IOACPIPlatformDevice, id 0x100000167, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "_STA" = 31
    | | |     "IODeviceMemory" = (({"address"=240,"length"=1}))
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<0d00000000000000>)
    | | |     "name" = <"PNP0C04">
    | | |   }
    | | |   
    | | +-o LDRC  <class IOACPIPlatformDevice, id 0x100000168, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "_UID" = "2"
    | | |     "IODeviceMemory" = (({"address"=46,"length"=2}),({"address"=78,"length"=2}),({"address"=97,"length"=1}),({"address"=99,"length"=1}),({"address"=101,"length"=1}),({"address"=103,"length"=1}),({"address"=112,"length"=1}),({"address"=128,"length"=1}),({"address"=146,"length"=1}),({"address"=178,"length"=2}),({"address"=1664,"length"=32}),({"address"=65535,"length"=1}),({"address"=65535,"length"=1}),({"address"=65535,"length"=1}),({"address"=6144,"length"=255}),({"address"=5710,"length"=2}))
    | | |     "name" = <"PNP0C02">
    | | |   }
    | | |   
    | | +-o LDR2  <class IOACPIPlatformDevice, id 0x100000169, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "_STA" = 15
    | | |     "_UID" = "LPC_DEV"
    | | |     "IODeviceMemory" = (({"address"=2048,"length"=128}))
    | | |     "name" = <"PNP0C02">
    | | |   }
    | | |   
    | | +-o RTC  <class IOACPIPlatformDevice, id 0x10000016a, registered, matched, active, busy 0 (17 ms), retain 9>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=112,"length"=8}))
    | | |     "name" = <"PNP0B00">
    | | |     "IOInterruptControllers" = ("io-apic-0","ACPIEventController")
    | | |     "acpi-wake-type" = 4
    | | |     "IOInterruptSpecifiers" = (<0800000000000000>,<0400000000000000>)
    | | |   }
    | | |   
    | | +-o TIMR  <class IOACPIPlatformDevice, id 0x10000016b, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "name" = <"PNP0100">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=64,"length"=4}),({"address"=80,"length"=4}))
    | | |   }
    | | |   
    | | +-o CWDT  <class IOACPIPlatformDevice, id 0x10000016c, registered, matched, active, busy 0 (0 ms), retain 7>
    | |     {
    | |       "_STA" = 15
    | |       "IODeviceMemory" = (({"address"=6228,"length"=4}))
    | |       "name" = <"INT3F0D">
    | |       "compatible" = <"PNP0C02">
    | |     }
    | |     
    | +-o PPMC@1F,2  <class IOPCIDevice, id 0x10000023b, registered, matched, active, busy 0 (2 ms), retain 8>
    | |   {
    | |     "name" = <"pci8086,a2a1">
    | |     "subsystem-vendor-id" = <58140000>
    | |     "compatible" = <"pci1458,5001","pci8086,a2a1","pciclass,058000","PPMC">
    | |     "IOName" = "pci8086,a2a1"
    | |     "reg" = <00fa00000000000000000000000000000000000010fa000200000000000000000000000000400000>
    | |     "device-id" = <a1a20000>
    | |     "assigned-addresses" = <10fa008200000000004054ed0000000000400000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <00000000>
    | |     "IODeviceMemory" = (({"address"=3981721600,"length"=16384}))
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:31:2"
    | |     "class-code" = <00800500>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PPMC@1f0002"
    | |     "subsystem-id" = <01500000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o HDEF@1F,3  <class IOPCIDevice, id 0x100000263, registered, matched, active, busy 0 (186 ms), retain 10>
    | |   {
    | |     "assigned-addresses" = <10fb00827f00000000000292000000000040000020fb00827f000000000000920000000000000100>
    | |     "IOInterruptSpecifiers" = (<1000000007000000>,<0600000000000100>)
    | |     "class-code" = <00030400>
    | |     "IODeviceMemory" = (({"address"=547910451200,"length"=16384}),({"address"=547910320128,"length"=65536}))
    | |     "IOReportLegendPublic" = Yes
    | |     "PinConfigurations" = <20400101602045012f40210130402101401001011091a190>
    | |     "subsystem-vendor-id" = <58140000>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "built-in" = <00>
    | |     "MaximumBootBeepVolume" = <00>
    | |     "IOPCIMSIMode" = Yes
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,a2f0">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <f0a20000>
    | |     "acpi-pmcap-offset" = 80
    | |     "layout-id" = <0b000000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci1458,a036","pci8086,a2f0","pciclass,040300","HDEF">
    | |     "AFGLowPowerState" = <03000000>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/HDEF@1f0003"
    | |     "subsystem-id" = <36a00000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:31:3"
    | |     "IOName" = "pci8086,a2f0"
    | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="HDEF 1"})
    | |     "reg" = <00fb00000000000000000000000000000000000010fb00020000000000000000000000000040000020fb000200000000000000000000000000000100>
    | |   }
    | |   
    | +-o SBUS@1F,4  <class IOPCIDevice, id 0x10000023c, registered, matched, active, busy 0 (24 ms), retain 8>
    | |   {
    | |     "assigned-addresses" = <10fc00827f00000000600292000000000001000020fc00810000000000f000000000000020000000>
    | |     "IOInterruptSpecifiers" = (<1000000007000000>)
    | |     "IODeviceMemory" = (({"address"=547910475776,"length"=256}),"IOSubMemoryDescriptor is not serializable")
    | |     "class-code" = <00050c00>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <58140000>
    | |     "built-in" = <00>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "name" = <"pci8086,a2a3">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <a3a20000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci1458,5001","pci8086,a2a3","pciclass,0c0500","SBUS">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0004"
    | |     "subsystem-id" = <01500000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:31:4"
    | |     "IOName" = "pci8086,a2a3"
    | |     "reg" = <00fc00000000000000000000000000000000000010fc00020000000000000000000000000001000020fc000100000000000000000000000020000000>
    | |   }
    | |   
    | +-o GLAN@1F,6  <class IOPCIDevice, id 0x10000023d, registered, matched, active, busy 0 (822 ms), retain 11>
    |     {
    |       "assigned-addresses" = <10fe008200000000000050ed0000000000000200>
    |       "IOInterruptSpecifiers" = (<1000000007000000>,<0700000000000100>)
    |       "class-code" = <00000200>
    |       "IODeviceMemory" = (({"address"=3981443072,"length"=131072}))
    |       "IOReportLegendPublic" = Yes
    |       "built-in" = <00>
    |       "subsystem-vendor-id" = <58140000>
    |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |       "IOPCIMSIMode" = Yes
    |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    |       "name" = <"ethernet">
    |       "vendor-id" = <86800000>
    |       "acpi-pmcap-offset" = 200
    |       "device-id" = <b8150000>
    |       "IOPCIResourced" = Yes
    |       "compatible" = <"pci1458,e000","pci8086,15b8","pciclass,020000","GLAN">
    |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GLAN@1f0006"
    |       "subsystem-id" = <00e00000>
    |       "revision-id" = <00000000>
    |       "pcidebug" = "0:31:6"
    |       "IOName" = "ethernet"
    |       "acpi-wake-type" = 2
    |       "reg" = <00fe00000000000000000000000000000000000010fe000200000000000000000000000000000200>
    |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="GLAN 1"})
    |     }
    |     
    +-o PAGD  <class IOACPIPlatformDevice, id 0x1000001da, registered, matched, active, busy 0 (1 ms), retain 7>
    |   {
    |     "name" = <"ACPI000C">
    |     "_STA" = 18446744073709551615
    |   }
    |   
    +-o LNKA  <class IOACPIPlatformDevice, id 0x1000001db, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "1"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKB  <class IOACPIPlatformDevice, id 0x1000001dc, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "2"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKC  <class IOACPIPlatformDevice, id 0x1000001dd, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "3"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKD  <class IOACPIPlatformDevice, id 0x1000001de, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "4"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKE  <class IOACPIPlatformDevice, id 0x1000001df, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "5"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKF  <class IOACPIPlatformDevice, id 0x1000001e0, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "6"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKG  <class IOACPIPlatformDevice, id 0x1000001e1, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "7"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKH  <class IOACPIPlatformDevice, id 0x1000001e2, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "8"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o SLPB  <class IOACPIPlatformDevice, id 0x1000001e3, registered, matched, active, busy 0 (13 ms), retain 8>
    |   {
    |     "name" = <"PNP0C0E">
    |     "_STA" = 11
    |   }
    |   
    +-o WTBT  <class IOACPIPlatformDevice, id 0x1000001e4, registered, matched, active, busy 0 (1 ms), retain 7>
    |   {
    |     "_UID" = "TBFP"
    |     "_STA" = 18446744073709551615
    |     "name" = <"PNP0C14">
    |   }
    |   
    +-o PWRB  <class IOACPIPlatformDevice, id 0x1000001e5, registered, matched, active, busy 0 (13 ms), retain 9>
    |   {
    |     "acpi-wake-type" = 1
    |     "IOReportLegendPublic" = Yes
    |     "IOInterruptControllers" = ("ACPIEventController")
    |     "_STA" = 15
    |     "IOInterruptSpecifiers" = (<0200000000000000>)
    |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="PWRB 0"})
    |     "name" = <"PNP0C0C">
    |   }
    |   
    +-o PTID  <class IOACPIPlatformDevice, id 0x1000001e6, registered, matched, active, busy 0 (1013 ms), retain 8>
    |   {
    |     "compatible" = <"PNP0C02">
    |     "_STA" = 15
    |     "name" = <"INT340E">
    |   }
    |   
    +-o FAN0  <class IOACPIPlatformDevice, id 0x1000001e7, registered, matched, active, busy 0 (1 ms), retain 7>
    |   {
    |     "_STA" = 18446744073709551615
    |     "_UID" = "0"
    |     "IOPowerManagement" = {"CapabilityFlags"=0,"MaxPowerState"=2,"CurrentPowerState"=0}
    |     "name" = <"PNP0C0B">
    |   }
    |   
    +-o FAN1  <class IOACPIPlatformDevice, id 0x1000001e8, registered, matched, active, busy 0 (1 ms), retain 7>
    |   {
    |     "_STA" = 18446744073709551615
    |     "_UID" = "1"
    |     "IOPowerManagement" = {"CapabilityFlags"=0,"MaxPowerState"=2,"CurrentPowerState"=0}
    |     "name" = <"PNP0C0B">
    |   }
    |   
    +-o FAN2  <class IOACPIPlatformDevice, id 0x1000001e9, registered, matched, active, busy 0 (1 ms), retain 7>
    |   {
    |     "_STA" = 18446744073709551615
    |     "_UID" = "2"
    |     "IOPowerManagement" = {"CapabilityFlags"=0,"MaxPowerState"=2,"CurrentPowerState"=0}
    |     "name" = <"PNP0C0B">
    |   }
    |   
    +-o FAN3  <class IOACPIPlatformDevice, id 0x1000001ea, registered, matched, active, busy 0 (1 ms), retain 7>
    |   {
    |     "_STA" = 18446744073709551615
    |     "_UID" = "3"
    |     "IOPowerManagement" = {"CapabilityFlags"=0,"MaxPowerState"=2,"CurrentPowerState"=0}
    |     "name" = <"PNP0C0B">
    |   }
    |   
    +-o FAN4  <class IOACPIPlatformDevice, id 0x1000001eb, registered, matched, active, busy 0 (1 ms), retain 7>
    |   {
    |     "_STA" = 18446744073709551615
    |     "_UID" = "4"
    |     "IOPowerManagement" = {"CapabilityFlags"=0,"MaxPowerState"=2,"CurrentPowerState"=0}
    |     "name" = <"PNP0C0B">
    |   }
    |   
    +-o options  <class AppleEFINVRAM, id 0x100000282, registered, matched, active, busy 0 (0 ms), retain 679>
        {
          "fakesmc-key-BEMB-flag" = <00>
          "fakesmc-key-RPlt-ch8*" = <6a31333500000000>
          "EFILoginHiDPI" = <00000000>
          "fakesmc-key-RBr -ch8*" = <"j133_4_">
          "Clover.Theme" = <"Clover Bootcamp">
          "fakesmc-key-#KEY-ui32" = <00000011>
          "install-product-url" = <"x-osproduct://44868F21-1594-3202-B10F-164E1A08E369/macOS%20Install%20Data">
          "fakesmc-key-BATP-flag" = <00>
          "EmuVariableUefiPresent" = <"Yes">
          "fakesmc-key-MSTc-ui8" = <00>
          "prev-lang:kbd" = <"de:92">
          "fakesmc-key-BNum-ui8" = <00>
          "security-mode" = "none"
          "csr-active-config" = <67000000>
          "fakesmc-key-$Num-ui8" = <01>
          "fakesmc-key-MSFW-ui8" = <0100>
          "fakesmc-key-MSPS-ui16" = <0003>
          "fakesmc-key-REV -ch8*" = <02410f000001>
          "fmm-computer-name" = <"admins iMac">
          "bootercfg" = <"(">
          "fakesmc-key-$Adr-ui32" = <00000300>
          "fakesmc-key-EPCI-ui32" = <0970f000>
          "nvda_drv" = <"1">
          "fakesmc-key-MSAc-ui16" = <0000>
          "fakesmc-key-MSLD-ui8" = <00>
          "fakesmc-key-RMde-char" = <41>
          "Clover.KeepBackupLimit" = <30>
          "flagstate" = <0000000000000000000000000000000000000000000000000000000000000000>
          "specialbootdevice" = <02010c00d041030a0000000001010600001d01010600000003171000010000000025385671b09d1504012a00020000002840060000000000b02fda4500000000427a8eba8f41c44c96a4e0e7b5ef878f02027fff0400>
          "fakesmc-key-MSWr-ui8" = <00>
        }
        
