[
{"data":{"title":"built-in"},"attr":{"id":"7689","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"7691","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7692","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7693","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"7695","ColType":"Number","ColValue":"3977248768"}},{"data":{"title":"length"},"attr":{"id":"7697","ColType":"Number","ColValue":"131072"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"7699","ColType":"Number","ColValue":"64"}},
{"data":{"title":"device-id"},"attr":{"id":"7701","ColType":"Data","ColValue":"&lt;30000000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"7703","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"7705","ColType":"Data","ColValue":"&lt;\"pci168c,30\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"7707","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP14@1d0005/PXSX@0"}},
{"data":{"title":"IOName"},"attr":{"id":"7709","ColType":"String","ColValue":"pci168c,30"}},
{"data":{"title":"vendor-id"},"attr":{"id":"7711","ColType":"Data","ColValue":"&lt;8c160000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"7713","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"7715","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"7717","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"7719","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"7721","ColType":"Data","ColValue":"&lt;8c160000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"7723","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7724","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"7725","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"7727","ColType":"Number","ColValue":"220177"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"7729","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7730","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"7732","ColType":"String","ColValue":"PXSX 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"7734","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7735","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7736","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"7737","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7738","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"7739","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7740","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"7741","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7742","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"7743","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7744","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"7745","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7746","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"7747","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7748","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"7749","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7750","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"7751","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7752","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"7753","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7754","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"7756","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"7758","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"7760","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"7762","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"7764","ColType":"String","ColValue":"67:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"7766","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"7768","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"7770","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"7772","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"7774","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"7776","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"7778","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"7780","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"7782","ColType":"Data","ColValue":"&lt;00800200&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"7784","ColType":"Data","ColValue":"&lt;\"pci168c,3112\",\"pci168c,30\",\"pciclass,028000\",\"PXSX\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"7786","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"7788","ColType":"Data","ColValue":"&lt;12310000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"7790","ColType":"Data","ColValue":"&lt;1000438200000000000010ed0000000000000200&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"7792","ColType":"Data","ColValue":"&lt;00004300000000000000000000000000000000001000430200000000000000000000000000000200&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"7794","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7795","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"7796","ColType":"Data","ColValue":"&lt;0900000000000100&gt;"}}]}
]
