[
{"data":{"title":"built-in"},"attr":{"id":"8318","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"layout-id"},"attr":{"id":"8320","ColType":"Data","ColValue":"&lt;0b000000&gt;"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"8322","ColType":"Number","ColValue":"80"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"8324","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8325","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8326","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"8328","ColType":"Number","ColValue":"547910451200"}},{"data":{"title":"length"},"attr":{"id":"8330","ColType":"Number","ColValue":"16384"}}]}]},{"data":{"title":"1"},"attr":{"id":"8331","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8332","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"8334","ColType":"Number","ColValue":"547910320128"}},{"data":{"title":"length"},"attr":{"id":"8336","ColType":"Number","ColValue":"65536"}}]}]}]},
{"data":{"title":"PinConfigurations"},"attr":{"id":"8338","ColType":"Data","ColValue":"&lt;20400101602045012f40210130402101401001011091a190&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"8340","ColType":"Data","ColValue":"&lt;f0a20000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"8342","ColType":"Data","ColValue":"&lt;\"pci8086,a2f0\"&gt;"}},
{"data":{"title":"AFGLowPowerState"},"attr":{"id":"8344","ColType":"Data","ColValue":"&lt;03000000&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"8346","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/HDEF@1f0003"}},
{"data":{"title":"IOName"},"attr":{"id":"8348","ColType":"String","ColValue":"pci8086,a2f0"}},
{"data":{"title":"vendor-id"},"attr":{"id":"8350","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"8352","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"8354","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"8356","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"8358","ColType":"Data","ColValue":"&lt;58140000&gt;"}},
{"data":{"title":"MaximumBootBeepVolume"},"attr":{"id":"8360","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"8362","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8363","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"8364","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOReportLegend"},"attr":{"id":"8366","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8367","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"8369","ColType":"String","ColValue":"HDEF 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"8371","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8372","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8373","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"8374","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8375","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"8376","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8377","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"8378","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8379","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"8380","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8381","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"8382","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8383","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"8384","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8385","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"8386","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8387","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"8388","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8389","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"8390","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"8391","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"8393","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"8395","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"8397","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pcidebug"},"attr":{"id":"8399","ColType":"String","ColValue":"0:31:3"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"8401","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"8403","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"8405","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"8407","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"8409","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"8411","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"8413","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"8415","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"8417","ColType":"Data","ColValue":"&lt;\"pci1458,a036\",\"pci8086,a2f0\",\"pciclass,040300\",\"HDEF\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"8419","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"8421","ColType":"Data","ColValue":"&lt;36a00000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"8423","ColType":"Data","ColValue":"&lt;10fb00827f00000000000292000000000040000020fb00827f000000000000920000000000000100&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"8425","ColType":"Data","ColValue":"&lt;00fb00000000000000000000000000000000000010fb00020000000000000000000000000040000020fb000200000000000000000000000000000100&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"8427","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"8428","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"8429","ColType":"Data","ColValue":"&lt;0600000000000100&gt;"}}]}
]
