[
{"data":{"title":"built-in"},"attr":{"id":"9712","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"9714","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9715","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9716","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"9718","ColType":"Number","ColValue":"3977248768"}},{"data":{"title":"length"},"attr":{"id":"9720","ColType":"Number","ColValue":"131072"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"9722","ColType":"Number","ColValue":"64"}},
{"data":{"title":"device-id"},"attr":{"id":"9724","ColType":"Data","ColValue":"&lt;30000000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"9726","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"9728","ColType":"Data","ColValue":"&lt;\"pci168c,30\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"9730","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP14@1d0005/PXSX@0"}},
{"data":{"title":"IOName"},"attr":{"id":"9732","ColType":"String","ColValue":"pci168c,30"}},
{"data":{"title":"vendor-id"},"attr":{"id":"9734","ColType":"Data","ColValue":"&lt;8c160000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"9736","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"9738","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"9740","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"9742","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"9744","ColType":"Data","ColValue":"&lt;8c160000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"9746","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9747","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"9748","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"9750","ColType":"Number","ColValue":"220177"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"9752","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9753","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"9755","ColType":"String","ColValue":"PXSX 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"9757","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9758","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9759","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"9760","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9761","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"9762","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9763","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"9764","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9765","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"9766","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9767","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"9768","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9769","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"9770","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9771","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"9772","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9773","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"9774","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9775","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"9776","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"9777","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"9779","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"9781","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"9783","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"9785","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"9787","ColType":"String","ColValue":"67:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"9789","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"9791","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"9793","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"9795","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"9797","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"9799","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"9801","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"9803","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"9805","ColType":"Data","ColValue":"&lt;00800200&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"9807","ColType":"Data","ColValue":"&lt;\"pci168c,3112\",\"pci168c,30\",\"pciclass,028000\",\"PXSX\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"9809","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"9811","ColType":"Data","ColValue":"&lt;12310000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"9813","ColType":"Data","ColValue":"&lt;1000438200000000000010ed0000000000000200&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"9815","ColType":"Data","ColValue":"&lt;00004300000000000000000000000000000000001000430200000000000000000000000000000200&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"9817","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"9818","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"9819","ColType":"Data","ColValue":"&lt;0900000000000100&gt;"}}]}
]
