[
{"data":{"title":"PinConfigurations"},"attr":{"id":"6681","ColType":"Data","ColValue":"&lt;&gt;"}},
{"data":{"title":"@3,connector-type"},"attr":{"id":"6683","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"6685","ColType":"Data","ColValue":"&lt;1001018200000000000008ed0000000000400000&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"6687","ColType":"String","ColValue":"1:0:1"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"6689","ColType":"Number","ColValue":"3"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"6691","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6692","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"6693","ColType":"Data","ColValue":"&lt;0200000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"6695","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/PEG0@10000/HDAU@1"}},
{"data":{"title":"DigitalAudioCapabilities"},"attr":{"id":"6697","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"HDMI"},"attr":{"id":"6699","ColType":"Number","ColValue":"1"}},{"data":{"title":"DisplayPort"},"attr":{"id":"6701","ColType":"Number","ColValue":"1"}}]},
{"data":{"title":"layout-id"},"attr":{"id":"6703","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"6705","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6706","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"6707","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"6709","ColType":"Number","ColValue":"2"}},
{"data":{"title":"@0,connector-type"},"attr":{"id":"6711","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"6713","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"6715","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"6717","ColType":"Data","ColValue":"&lt;42380000&gt;"}},
{"data":{"title":"@2,connector-type"},"attr":{"id":"6719","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"6721","ColType":"Data","ColValue":"&lt;de100000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"6723","ColType":"Data","ColValue":"&lt;\"pci10de,10f1\"&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"6725","ColType":"Data","ColValue":"&lt;\"pci3842,6262\",\"pci10de,10f1\",\"pciclass,040300\",\"HDAU\",\"HDAU\",\"HDAU\",\"HDAU\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"6727","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"6729","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"6731","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"6733","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"6735","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"6737","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"6739","ColType":"Data","ColValue":"&lt;a1000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"6741","ColType":"Number","ColValue":"4537603"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"6743","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"built-in"},"attr":{"id":"6745","ColType":"Data","ColValue":"&lt;01&gt;"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"6747","ColType":"Number","ColValue":"4353"}},
{"data":{"title":"hda-gfx"},"attr":{"id":"6749","ColType":"Data","ColValue":"&lt;\"onboard-2\"&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"6751","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6752","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6753","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"6755","ColType":"Number","ColValue":"3976724480"}},{"data":{"title":"length"},"attr":{"id":"6757","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"IOName"},"attr":{"id":"6759","ColType":"String","ColValue":"pci10de,10f1"}},
{"data":{"title":"acpi-device"},"attr":{"id":"6761","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"6763","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"6765","ColType":"Data","ColValue":"&lt;62620000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"6767","ColType":"Data","ColValue":"&lt;00010100000000000000000000000000000000001001010200000000000000000000000000400000&gt;"}},
{"data":{"title":"@1,connector-type"},"attr":{"id":"6769","ColType":"Data","ColValue":"&lt;00080000&gt;"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"6771","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6772","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"6774","ColType":"String","ColValue":"HDAU 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"6776","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6777","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6778","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"6779","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6780","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"6781","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6782","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"6783","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6784","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"6785","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6786","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"6787","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6788","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"6789","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6790","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"6791","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6792","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"6793","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6794","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"6795","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"6796","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"6798","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"6800","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"6802","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"6804","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"6806","ColType":"Data","ColValue":"&lt;f1100000&gt;"}}
]
