[
{"data":{"title":"built-in"},"attr":{"id":"7518","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"7520","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7521","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7522","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"7524","ColType":"Number","ColValue":"3980394496"}},{"data":{"title":"length"},"attr":{"id":"7526","ColType":"Number","ColValue":"4096"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"7528","ColType":"Number","ColValue":"68"}},
{"data":{"title":"pci-aspm-supported"},"attr":{"id":"7530","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"device-id"},"attr":{"id":"7532","ColType":"Data","ColValue":"&lt;01590000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"7534","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"7536","ColType":"Data","ColValue":"&lt;\"pci11c1,5901\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"7538","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/PXSX@0"}},
{"data":{"title":"IOName"},"attr":{"id":"7540","ColType":"String","ColValue":"pci11c1,5901"}},
{"data":{"title":"vendor-id"},"attr":{"id":"7542","ColType":"Data","ColValue":"&lt;c1110000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"7544","ColType":"Data","ColValue":"&lt;08000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"7546","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"7548","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"7550","ColType":"Data","ColValue":"&lt;01590000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"7552","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7553","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"7554","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"7556","ColType":"Number","ColValue":"474129"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"7558","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7559","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"7561","ColType":"String","ColValue":"PXSX 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"7563","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7564","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7565","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"7566","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7567","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"7568","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7569","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"7570","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7571","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"7572","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7573","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"7574","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7575","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"7576","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7577","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"7578","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7579","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"7580","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7581","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"7582","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7583","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"7585","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"7587","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"7589","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"7591","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"7593","ColType":"String","ColValue":"5:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"7595","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"7597","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"7599","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"7601","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"7603","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"7605","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"7607","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"7609","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"7611","ColType":"Data","ColValue":"&lt;10000c00&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"7613","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"7615","ColType":"Data","ColValue":"&lt;\"pci5901,1101\",\"pci11c1,5901\",\"pciclass,0c0010\",\"PXSX\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"7617","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"7619","ColType":"Data","ColValue":"&lt;01110000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"7621","ColType":"Data","ColValue":"&lt;1000058200000000000040ed0000000000100000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"7623","ColType":"Data","ColValue":"&lt;00000500000000000000000000000000000000001000050200000000000000000000000000100000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"7625","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7626","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"7627","ColType":"Data","ColValue":"&lt;0800000000000100&gt;"}}]}
]
