[
{"data":{"title":"built-in"},"attr":{"id":"83455","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"83457","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83458","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83459","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"83461","ColType":"Number","ColValue":"3980394496"}},{"data":{"title":"length"},"attr":{"id":"83463","ColType":"Number","ColValue":"4096"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"83465","ColType":"Number","ColValue":"68"}},
{"data":{"title":"pci-aspm-supported"},"attr":{"id":"83467","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"device-id"},"attr":{"id":"83469","ColType":"Data","ColValue":"&lt;01590000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"83471","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"83473","ColType":"Data","ColValue":"&lt;\"pci11c1,5901\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"83475","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/PXSX@0"}},
{"data":{"title":"IOName"},"attr":{"id":"83477","ColType":"String","ColValue":"pci11c1,5901"}},
{"data":{"title":"vendor-id"},"attr":{"id":"83479","ColType":"Data","ColValue":"&lt;c1110000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"83481","ColType":"Data","ColValue":"&lt;08000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"83483","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"83485","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"83487","ColType":"Data","ColValue":"&lt;01590000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"83489","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83490","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"83491","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"83493","ColType":"Number","ColValue":"474129"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"83495","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83496","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"83498","ColType":"String","ColValue":"PXSX 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"83500","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83501","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83502","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"83503","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"83504","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"83505","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83506","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"83507","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"83508","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"83509","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83510","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"83511","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"83512","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"83513","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83514","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"83515","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"83516","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"83517","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83518","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"83519","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"83520","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"83522","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"83524","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"83526","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"83528","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"83530","ColType":"String","ColValue":"5:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"83532","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"83534","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"83536","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"83538","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"83540","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"83542","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"83544","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"83546","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"83548","ColType":"Data","ColValue":"&lt;10000c00&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"83550","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"83552","ColType":"Data","ColValue":"&lt;\"pci5901,1101\",\"pci11c1,5901\",\"pciclass,0c0010\",\"PXSX\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"83554","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"83556","ColType":"Data","ColValue":"&lt;01110000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"83558","ColType":"Data","ColValue":"&lt;1000058200000000000040ed0000000000100000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"83560","ColType":"Data","ColValue":"&lt;00000500000000000000000000000000000000001000050200000000000000000000000000100000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"83562","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"83563","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"83564","ColType":"Data","ColValue":"&lt;0800000000000100&gt;"}}]}
]
