[
{"data":{"title":"built-in"},"attr":{"id":"5927","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"5929","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5930","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5931","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5933","ColType":"Number","ColValue":"3980394496"}},{"data":{"title":"length"},"attr":{"id":"5935","ColType":"Number","ColValue":"4096"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"5937","ColType":"Number","ColValue":"68"}},
{"data":{"title":"pci-aspm-supported"},"attr":{"id":"5939","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"device-id"},"attr":{"id":"5941","ColType":"Data","ColValue":"&lt;01590000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"5943","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"5945","ColType":"Data","ColValue":"&lt;\"pci11c1,5901\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"5947","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/PXSX@0"}},
{"data":{"title":"IOName"},"attr":{"id":"5949","ColType":"String","ColValue":"pci11c1,5901"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5951","ColType":"Data","ColValue":"&lt;c1110000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5953","ColType":"Data","ColValue":"&lt;08000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"5955","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5957","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5959","ColType":"Data","ColValue":"&lt;01590000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5961","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5962","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"5963","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5965","ColType":"Number","ColValue":"474129"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"5967","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5968","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"5970","ColType":"String","ColValue":"PXSX 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"5972","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5973","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5974","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"5975","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5976","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5977","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5978","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"5979","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5980","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5981","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5982","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"5983","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5984","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5985","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5986","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"5987","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5988","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5989","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5990","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"5991","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5992","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"5994","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"5996","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"5998","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"6000","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"6002","ColType":"String","ColValue":"5:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"6004","ColType":"Number","ColValue":"4113"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"6006","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"6008","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"6010","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"6012","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"6014","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"6016","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"6018","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"6020","ColType":"Data","ColValue":"&lt;10000c00&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"6022","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"6024","ColType":"Data","ColValue":"&lt;\"pci5901,1101\",\"pci11c1,5901\",\"pciclass,0c0010\",\"PXSX\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"6026","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"6028","ColType":"Data","ColValue":"&lt;01110000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"6030","ColType":"Data","ColValue":"&lt;1000058200000000000040ed0000000000100000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"6032","ColType":"Data","ColValue":"&lt;00000500000000000000000000000000000000001000050200000000000000000000000000100000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"6034","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6035","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"6036","ColType":"Data","ColValue":"&lt;0800000000000100&gt;"}}]}
]
