[
{"data":{"title":"IOReportLegend"},"attr":{"id":"4874","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4875","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"4877","ColType":"String","ColValue":"PWRB 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"4879","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4880","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4881","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"4882","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4883","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"4884","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4885","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"4886","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4887","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"4888","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4889","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"4890","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4891","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"4892","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4893","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"4894","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4895","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"4896","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4897","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"4898","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4899","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"4901","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"4903","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"4905","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"4907","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4908","ColType":"Data","ColValue":"&lt;0200000000000000&gt;"}}]},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"4910","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"4912","ColType":"Data","ColValue":"&lt;\"PNP0C0C\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"4914","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"4916","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4917","ColType":"String","ColValue":"ACPIEventController"}}]},
{"data":{"title":"_STA"},"attr":{"id":"4919","ColType":"Number","ColValue":"15"}}
]
