[
{"data":{"title":"built-in"},"attr":{"id":"6997","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"6999","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7000","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7001","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"7003","ColType":"Number","ColValue":"3978297344"}},{"data":{"title":"length"},"attr":{"id":"7005","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"7007","ColType":"Data","ColValue":"&lt;04a80000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"7009","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"7011","ColType":"Data","ColValue":"&lt;\"pci144d,a804\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"7013","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP09@1d0000/PXSX@0"}},
{"data":{"title":"IOName"},"attr":{"id":"7015","ColType":"String","ColValue":"pci144d,a804"}},
{"data":{"title":"vendor-id"},"attr":{"id":"7017","ColType":"Data","ColValue":"&lt;4d140000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"7019","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"7021","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"7023","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"7025","ColType":"Data","ColValue":"&lt;4d140000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"7027","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7028","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"7029","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"7031","ColType":"Number","ColValue":"4683843"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"7033","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7034","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"7036","ColType":"String","ColValue":"PXSX 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"7038","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7039","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7040","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"7041","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7042","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"7043","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7044","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"7045","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7046","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"7047","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7048","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"7049","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7050","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"7051","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7052","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"7053","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7054","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"7055","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7056","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"7057","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"7058","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"7060","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"7062","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"7064","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"7066","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"7068","ColType":"String","ColValue":"65:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"7070","ColType":"Number","ColValue":"4131"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"7072","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"7074","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"7076","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"7078","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"7080","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"7082","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"7084","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"7086","ColType":"Data","ColValue":"&lt;02080100&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"7088","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"7090","ColType":"Data","ColValue":"&lt;\"pci144d,a801\",\"pci144d,a804\",\"pciclass,010802\",\"PXSX\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"7092","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"7094","ColType":"Data","ColValue":"&lt;01a80000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"7096","ColType":"Data","ColValue":"&lt;1000418200000000000020ed0000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"7098","ColType":"Data","ColValue":"&lt;00004100000000000000000000000000000000001000410200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"7100","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"7101","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"7102","ColType":"Data","ColValue":"&lt;0a00000000000100&gt;"}}]}
]
