flashrom v0.9.7-unknown on Darwin 16.7.0 (x86_64)
flashrom was built with libpci 3.1.9, GCC 4.2.1 (Apple Inc. build 5666) (dot 3), little endian
Command line (6 args): /private/var/folders/gv/kl89fyqd3x184q_7lr_14jl00000gn/T/AppTranslocation/4F755393-E996-4115-A99D-5460E6AB4CD6/d/DarwinDumper.app/Contents/Resources/public/tools/flashrom -p internal -r /Users/admin/Desktop/DarwinDumper_3.0.2_02.11_13.37.31_iMac18,3_AMI_X64_4268_Sierra_16G29_admin/BIOS/System/biosbackup.rom -o /Users/admin/Desktop/DarwinDumper_3.0.2_02.11_13.37.31_iMac18,3_AMI_X64_4268_Sierra_16G29_admin/BIOS/System/flashrom_log.txt
Calibrating delay loop... OS timer resolution is 1 usecs, 4091M loops per second, 10 myus = 10 us, 100 myus = 97 us, 1000 myus = 984 us, 10000 myus = 10179 us, 4 myus = 4 us, OK.
Initializing internal programmer
No coreboot table found.
Using Internal DMI decoder.
DMI string chassis-type: "Desktop"
DMI string system-manufacturer: "Gigabyte Technology Co., Ltd."
DMI string system-product-name: "Z270X-Gaming 7"
DMI string system-version: "Default string"
DMI string baseboard-manufacturer: "Gigabyte Technology Co., Ltd."
DMI string baseboard-product-name: "Z270X-Gaming 7"
DMI string baseboard-version: "x.x"
Found ITE Super I/O, ID 0x8686 on port 0x2e
Found ITE Super I/O, ID 0x8733 on port 0x4e
WARNING: No chipset found. Flash detection will most likely fail.
Super I/O ID 0x8686 is not on the list of flash-capable controllers.
Super I/O ID 0x8733 is not on the list of flash-capable controllers.
The following protocols are supported: Non-SPI.
Probing for AMD Am29F010A/B, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29F002(N)BB, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29F002(N)BT, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29F016D, 2048 kB: probe_jedec_common: id1 0x82, id2 0x33, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29F040B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29F080B, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV001BB, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV001BT, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV002BB, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV002BT, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV004BB, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV004BT, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV008BB, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV008BT, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV040B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMD Am29LV081B, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for AMIC A29002B, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMIC A29002T, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMIC A29040B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for AMIC A49LF040A, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT29C512, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT29C010A, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT29C020, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT29C040A, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT49BV512, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT49F002(N), 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT49F002(N)T, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT49(H)F010, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT49F020, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT49F040, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT49F080, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT49F080T, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for Atmel AT49LH002, 256 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Catalyst CAT28F512, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Bright BM29F040, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ESMT F49B002UA, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Eon EN29F010, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Eon EN29F002(A)(N)B, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Eon EN29F002(A)(N)T, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Eon EN29LV640B, 8192 kB: probe_en29lv640b: id1 0xffff, id2 0x00ff
Probing for Fujitsu MBM29F004BC, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Fujitsu MBM29F004TC, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Fujitsu MBM29F400BC, 512 kB: probe_m29f400bt: id1 0xff, id2 0xff
Probing for Fujitsu MBM29F400TC, 512 kB: probe_m29f400bt: id1 0xff, id2 0xff
Probing for Fujitsu MBM29LV160BE, 2048 kB: probe_m29f400bt: id1 0x82, id2 0x07
Probing for Fujitsu MBM29LV160TE, 2048 kB: probe_m29f400bt: id1 0x82, id2 0x07
Probing for Hyundai HY29F002T, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Hyundai HY29F002B, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Hyundai HY29F040A, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 28F001BN/BX-B, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 28F001BN/BX-T, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 28F002BC/BL/BV/BX-T, 256 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 28F008S3/S5/SC, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 28F004B5/BE/BV/BX-B, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 28F004B5/BE/BV/BX-T, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 28F400BV/BX/CE/CV-B, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 28F400BV/BX/CE/CV-T, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 82802AB, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Intel 82802AC, 1024 kB: probe_82802ab: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for Macronix MX29F001B, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Macronix MX29F001T, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Macronix MX29F002(N)B, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Macronix MX29F002(N)T, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Macronix MX29F040, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Macronix MX29LV040, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for MoselVitelic V29C51000B, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for MoselVitelic V29C51000T, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for MoselVitelic V29C51400B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for MoselVitelic V29C51400T, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for MoselVitelic V29LC51000, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for MoselVitelic V29LC51001, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for MoselVitelic V29LC51002, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm29F002T, 256 kB: Chip lacks correct probe timing information, using default 10mS/40uS. probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm29F002B, 256 kB: Chip lacks correct probe timing information, using default 10mS/40uS. probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm39LV010, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm39LV020, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm39LV040, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm39LV512, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm49FL002, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for PMC Pm49FL004, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Sharp LH28F008BJT-BTLZ1, 1024 kB: probe_82802ab: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for Sharp LHF00L04, 1024 kB: probe_82802ab: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for SST SST28SF040A, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST29EE010, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST29LE010, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST29EE020A, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST29LE020, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST39SF512, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST39SF010A, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST39SF020A, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST39SF040, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST39VF512, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST39VF010, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST39VF020, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST39VF040, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST39VF080, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF002A/B, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF003A/B, 384 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF004A/B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF004C, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF008A, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF008C, 1024 kB: probe_82802ab: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF016C, 2048 kB: probe_82802ab: id1 0x82, id2 0x33, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF020, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF020A, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF040, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF040B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF080A, 1024 kB: Chip lacks correct probe timing information, using default 10mS/40uS. probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for SST SST49LF160C, 2048 kB: probe_82802ab: id1 0x82, id2 0x33, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M29F002B, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M29F002T/NT, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M29F040B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M29F400BB, 512 kB: probe_m29f400bt: id1 0xff, id2 0xff
Probing for ST M29F400BT, 512 kB: probe_m29f400bt: id1 0xff, id2 0xff
Probing for ST M29W010B, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M29W040B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M29W512B, 64 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW040A, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW040B, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW080A, 1024 kB: probe_82802ab: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FLW080B, 1024 kB: probe_82802ab: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW002, 256 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW016, 2048 kB: probe_82802ab: id1 0x82, id2 0x33, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW040, 512 kB: probe_82802ab: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for ST M50FW080, 1024 kB: probe_82802ab: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for ST M50LPW080, 1024 kB: probe_82802ab: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for ST M50LPW116, 2048 kB: probe_82802ab: id1 0x82, id2 0x33, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SyncMOS/MoselVitelic {F,S,V}29C51001B, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SyncMOS/MoselVitelic {F,S,V}29C51001T, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SyncMOS/MoselVitelic {F,S,V}29C51002B, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SyncMOS/MoselVitelic {F,S,V}29C51002T, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SyncMOS/MoselVitelic {F,S,V}29C51004B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SyncMOS/MoselVitelic {F,S,V}29C51004T, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SyncMOS/MoselVitelic {S,V}29C31004B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for SyncMOS/MoselVitelic {S,V}29C31004T, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for TI TMS29F002RB, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for TI TMS29F002RT, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W29C010(M)/W29C011A/W29EE011/W29EE012-old, 128 kB: Old Winbond W29* probe method disabled because the probing sequence puts the AMIC A49LF040A in a funky state. Use 'flashrom -c W29C010(M)/W29C011A/W29EE011/W29EE012-old' if you have a board with such a chip.
Probing for Winbond W29C010(M)/W29C011A/W29EE011/W29EE012, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W29C020(C)/W29C022, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W29C040/P, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39F010, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39L010, 128 kB: probe_jedec_common: id1 0xeb, id2 0x2e, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39L020, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39L040, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040A, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040B, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040C, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040FA, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040FB, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V040FC, 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V080A, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W49F002U/N, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W49F020, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W49V002A, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W49V002FA, 256 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V080FA, 1024 kB: probe_jedec_common: id1 0xc8, id2 0x73, id1 is normal flash content, id2 is normal flash content
Probing for Winbond W39V080FA (dual mode), 512 kB: probe_jedec_common: id1 0xff, id2 0xff, id1 parity violation, id1 is normal flash content, id2 is normal flash content
No EEPROM/flash device found.
Note: flashrom can never write if the flash chip isn't found automatically.
