[
{"data":{"title":"built-in"},"attr":{"id":"14918","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"14920","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14921","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14922","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"14924","ColType":"Number","ColValue":"549775937536"}},{"data":{"title":"length"},"attr":{"id":"14926","ColType":"Number","ColValue":"4096"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"14928","ColType":"Data","ColValue":"&lt;a7a20000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"14930","ColType":"Data","ColValue":"&lt;\"pci8086,a2a7\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"14932","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/URT0@1e0000"}},
{"data":{"title":"IOName"},"attr":{"id":"14934","ColType":"String","ColValue":"pci8086,a2a7"}},
{"data":{"title":"vendor-id"},"attr":{"id":"14936","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"14938","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"14940","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"acpi-device"},"attr":{"id":"14942","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"14944","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"14946","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14947","ColType":"String","ColValue":"io-apic-0"}}]},
{"data":{"title":"IOReportLegend"},"attr":{"id":"14949","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14950","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"14952","ColType":"String","ColValue":"URT0 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"14954","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14955","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14956","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"14957","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"14958","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"14959","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14960","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"14961","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"14962","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"14963","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14964","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"14965","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"14966","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"14967","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14968","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"14969","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"14970","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"14971","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"14972","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"14973","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"14974","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"14976","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"14978","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"14980","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pcidebug"},"attr":{"id":"14982","ColType":"String","ColValue":"0:30:0"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"14984","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"14986","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"14988","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"14990","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"14992","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"14994","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"14996","ColType":"Data","ColValue":"&lt;00801100&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"14998","ColType":"Data","ColValue":"&lt;\"pci8086,7270\",\"pci8086,a2a7\",\"pciclass,118000\",\"URT0\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"15000","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"uart-channel-number"},"attr":{"id":"15002","ColType":"Data","ColValue":"&lt;0000000000000000&gt;"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"15004","ColType":"Data","ColValue":"&lt;70720000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"15006","ColType":"Data","ColValue":"&lt;10f0008280000000001033010000000000100000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"15008","ColType":"Data","ColValue":"&lt;00f000000000000000000000000000000000000010f0000200000000000000000000000000100000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"15010","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"15011","ColType":"Data","ColValue":"&lt;1400000007000000&gt;"}}]}
]
