[
{"data":{"title":"built-in"},"attr":{"id":"4472","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"4474","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4475","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4476","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"4478","ColType":"Number","ColValue":"549775818752"}},{"data":{"title":"length"},"attr":{"id":"4480","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"4482","ColType":"Data","ColValue":"&lt;21200000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"4484","ColType":"Data","ColValue":"&lt;\"pci8086,2021\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"4486","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/CB0G@40006"}},
{"data":{"title":"IOName"},"attr":{"id":"4488","ColType":"String","ColValue":"pci8086,2021"}},
{"data":{"title":"vendor-id"},"attr":{"id":"4490","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"4492","ColType":"Data","ColValue":"&lt;04000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"4494","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"4496","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"4498","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"4500","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4501","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"4502","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"4504","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"4506","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"4508","ColType":"String","ColValue":"0:4:6"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"4510","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"4512","ColType":"Number","ColValue":"146"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"4514","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"4516","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"4518","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"4520","ColType":"Number","ColValue":"3"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"4522","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"4524","ColType":"Data","ColValue":"&lt;00800800&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"4526","ColType":"Data","ColValue":"&lt;\"pci8086,0\",\"pci8086,2021\",\"pciclass,088000\",\"CB0G\"&gt;"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"4528","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"4530","ColType":"Data","ColValue":"&lt;1026008280000000004031010000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"4532","ColType":"Data","ColValue":"&lt;00260000000000000000000000000000000000001026000200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"4534","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4535","ColType":"Data","ColValue":"&lt;1200000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"4536","ColType":"Data","ColValue":"&lt;0600000000000100&gt;"}}]}
]
