[
{"data":{"title":"IOPCITunnelLinkChange"},"attr":{"id":"35855","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"ranges"},"attr":{"id":"35857","ColType":"Data","ColValue":"&lt;0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"35859","ColType":"String","ColValue":"124:1:0(184:184)"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"35861","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"35863","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35864","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"35865","ColType":"Data","ColValue":"&lt;0c00000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"35867","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000"}},
{"data":{"title":"Thunderbolt Path"},"attr":{"id":"35869","ColType":"String","ColValue":"IOService:/AppleACPIPlatformExpert/PC02@0/AppleACPIPCI/BR2C@2/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType3/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType3/IOThunderboltPort@6"}},
{"data":{"title":"IOPCIExpressSlotCapabilities"},"attr":{"id":"35871","ColType":"Number","ColValue":"786528"}},
{"data":{"title":"IOPCIExpressSlotStatus"},"attr":{"id":"35873","ColType":"Number","ColValue":"0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"35875","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"35877","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35878","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"35879","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"35881","ColType":"Number","ColValue":"354"}},
{"data":{"title":"AAPL,slot-name"},"attr":{"id":"35883","ColType":"Data","ColValue":"&lt;\"PCI Slot 1\"&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"35885","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCITunnelID"},"attr":{"id":"35887","ColType":"Number","ColValue":"4294968415"}},
{"data":{"title":"IOPCIConfigured"},"attr":{"id":"35889","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"35891","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IODTPersist"},"attr":{"id":"35893","ColType":"Number","ColValue":"0"}},
{"data":{"title":"#size-cells"},"attr":{"id":"35895","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"35897","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"35899","ColType":"Data","ColValue":"&lt;\"pci-bridge\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"35901","ColType":"Number","ColValue":"48"}},
{"data":{"title":"compatible"},"attr":{"id":"35903","ColType":"Data","ColValue":"&lt;\"pci8086,15d3\",\"pciclass,060400\",\"DSB1\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"35905","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"DevicePowerState"},"attr":{"id":"35907","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"35909","ColType":"Number","ColValue":"0"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"35911","ColType":"Number","ColValue":"0"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"35913","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"35915","ColType":"Number","ColValue":"2"}},{"data":{"title":"PowerOverrideOn"},"attr":{"id":"35917","ColType":"Boolean","ColValue":"Yes"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"35919","ColType":"Number","ColValue":"2"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"35921","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"35923","ColType":"Number","ColValue":"24206401"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"35925","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"35927","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"#address-cells"},"attr":{"id":"35929","ColType":"Data","ColValue":"&lt;03000000&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"35931","ColType":"String","ColValue":"pci-bridge"}},
{"data":{"title":"acpi-device"},"attr":{"id":"35933","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"35935","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"reg"},"attr":{"id":"35937","ColType":"Data","ColValue":"&lt;00087c0000000000000000000000000000000000&gt;"}},
{"data":{"title":"Thunderbolt Entry ID"},"attr":{"id":"35939","ColType":"Number","ColValue":"4294968471"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"35941","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35942","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"35944","ColType":"String","ColValue":"DSB1 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"35946","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35947","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35948","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"35949","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35950","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"35951","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35952","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"35953","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35954","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"35955","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35956","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"35957","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35958","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"35959","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35960","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"35961","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35962","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"35963","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35964","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"35965","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35966","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"35968","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"35970","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"35972","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"35974","ColType":"Data","ColValue":"&lt;00040600&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"35976","ColType":"Data","ColValue":"&lt;d3150000&gt;"}}
]
