+-o Root  <class IORegistryEntry, id 0x100000100, retain 20>
  | {
  |   "IOKitBuildVersion" = "Darwin Kernel Version 17.3.0: Thu Nov 30 16:32:47 PST 2017; root:xnu-4570.37.11~1/RELEASE_X86_64"
  |   "OS Build Version" = "17C2120"
  |   "IOBluetoothActive" = Yes
  |   "OSKernelCPUSubtype" = 3
  |   "OSKernelCPUType" = 16777223
  |   "OSPrelinkKextCount" = 263
  |   "IOConsoleLocked" = No
  |   "IORegistryPlanes" = {"IOPower"="IOPower","IOService"="IOService","IO80211Plane"="IO80211Plane","IOUSB"="IOUSB","CoreCapture"="CoreCapture","IOACPIPlane"="IOACPIPlane","IODeviceTree"="IODeviceTree"}
  |   "IOConsoleUsers" = ({"kCGSSessionOnConsoleKey"=Yes,"kCGSSessionLoginwindowSafeLogin"=No,"kSCSecuritySessionID"=100008,"kCGSessionLongUserNameKey"="Apple","kCGSSessionUserIDKey"=502,"kCGSSessionSystemSafeBoot"=No,"kCGSSessionUserNameKey"="apple","kCGSSessionIDKey"=257,"kCGSessionLoginDoneKey"=Yes,"kCGSSessionGroupIDKey"=20,"kCGSSessionAuditIDKey"=100008})
  |   "IOKitDiagnostics" = {"Container allocation"=12349739,"Instance allocation"=18552248,"Pageable allocation"=2081636352,"Classes"={"IONDRVFramebuffer"=0,"AppleUSBVHCIPipe"=10,"IOHIDEventServiceFastPathUserClient"=0,"IOKitDiagnosticsClient"=0,"AtiDacEncoderControlInterface_V1"=0,"IOAudioClientBufferSet"=0,"IONaturalMemoryCursor"=0,"AppleUSBVHCIBCETransferQueue"=1,"IOUSBHostHIDDevice"=2,"IOAccelDisplayPipe2"=1,"AppleUSBRequest"=1,"AppleUSBDiagnostics"=0,"AppleUSBXHCIIsochronousRequestPool"=2,"AppleSMCPMC"=1,"AMDRadeonX5000_IAMDSMLVCE"=1,"AMDRadeonX5000_AMDSMLCTT"=0,"IOUSBMassStorageDriverRequestTimer"=0,"CHDCP"=0,"IOThunderboltDeficitCommandQueue"=2,"IORegistryEntry"=133,"OSLiveNumber"=12,"IOUSBMassStorageUASDriver"=0,"IORTC"=1,"IOHIDevice"=0,"IOPCIEventSource"=0,"com_apple_driver_AppleUSBCardReaderInterfaceNub"=0,"IOBufferCopySubmissionQueue"=28,"IOThunderboltAbstractMicro"=1,"IO80211DriverCommandDescriptor"=0,"IOMemoryCursor"=1,"IOThunderboltXDPropertiesDirectory"=4,"AppleGFXHDAAudioSelectorControlDP"=0,"IOBreaker"=0,"AMDRadeonX5000_AMDAccelCLContext"=0,"IOUSBLowLatencyCommandLegacy"=0,"AppleThunderboltNHIReceiveRingManager"=2,"AppleHIDKeyboardEventDriver"=0,"AppleThunderboltIPReceiveCommand"=0,"EFIData"=68,"AMDRadeonX5000_AMDAccelEventMachine"=1,"AppleUSBXHCIPort"=2,"IOAccelCommandQueue"=1,"AMDRadeonX5000_AMDVCE4"=1,"com_apple_driver_AppleUSBCardReaderUMC"=1,"AtiFbStub"=6,"IOBluetoothHostControllerUserClient"=0,"AppleKeyStoreUserClient"=12,"IOThunderboltSwitchType1"=0,"AMDRadeonX5000_AMDHWChannelStatsGroup"=12,"IOSMBusRequest"=0,"IOSkywalkPacket"=0,"AppleUSBVHCIEventQueue"=1,"IOPMServiceInterestNotifier"=123,"AppleACPILid"=0,"AppleUpstreamUserClientDriver"=6,"IOHIDResourceQueue"=0,"IOStorage"=4,"AtiAsicInit_V1_1"=0,"IOAccelSegmentResourceList"=0,"AppleUSBRequestPool"=4,"IOSerialStreamSync"=1,"IOHIDConsumer"=0,"IO80211AWDLMulticastPeer"=1,"AppleUSBHostCompositeDevice"=5,"AppleSMCRTC"=1,"IOThunderboltXDPropertiesEntry"=22,"IOHIDClientData"=4,"IOSharedInterruptController"=3,"IOBluetoothMemoryDescriptorRetainer"=0,"IOGraphicsWorkLoop"=2,"AtiFbInterruptDeferredCallback"=5,"AtiPackingConnectorAssigner"=0,"AtiDac2OutputControl_V1_V1"=0,"hv_vmx_vm_t"=0,"AMDRadeonX5000_IAMDHWVMM"=1,"IOTimeSyncClockManagerUserClient"=0,"OSSerializer"=89,"IOPCIMessagedInterruptController"=1,"IOUserEthernetResourceUserClient"=0,"IOThunderboltConfigMultiReadCommand"=2,"OSCollection"=6,"AtiFirmwareInfoInterface_V1_4"=0,"IOThunderboltSet"=48,"AtiAsicInit_V2_1"=1,"AppleGFXHDAWidgetATI_Park"=1,"IOUSBDeviceUserClientV2"=1,"AppleUSBVHCIBCEMessageQueue"=5,"AtiLinkedList"=123,"AIDReporters"=0,"AppleBCMWLANQueueDescriptor"=0,"_IOServiceNullNotifier"=1,"AIDInterface"=0,"AMDRadeonX5000_AMDUVD7EncLLQChannel"=1,"AtiCompositor"=0,"IOImageDescriptor"=1,"IOSkywalkMemorySegment"=0,"AMDRadeonX5000_AMDAccelTraceStream"=7,"IOBluetoothHCIUserClient"=9,"AppleIntelPCHPMC"=1,"AtiLineBuffer"=1,"com_apple_driver_pm_cpu_reporter"=0,"IONetworkStackUserClient"=1,"AppleMultitouchEventDriverV2Wrapper"=1,"AppleDisplay"=0,"AtiNvramParserInterface"=1,"IOBluetoothHostController"=1,"IOInterleavedMemoryDescriptor"=0,"_IOServiceNotifier"=413,"AppleAPFSUserClient"=0,"AppleBCMWLANItemRing"=2,"IOBufferCopyControllerBase"=1,"Vega10PowerPlayManager"=1,"AppleGraphicsDevicePolicy"=1,"AppleBCMWLANTxCommandBuffer"=0,"IOBufferCopyEngineTestUserClient"=0,"IOSkywalkEthernetInterface"=0,"AppleBCMWLANByteRing"=2,"BridgeAudioPCI"=1,"IOSKArena"=1,"AppleUSBXHCILPTCommandRing"=0,"AppleUSBVHCIHostCommandQueue"=1,"IOSubMemoryDescriptor"=29,"AppleBCMWLANCommandWithXTLV"=0,"AppleUSBRequestCompleter"=1,"IOUSBHostDevice"=5,"IOThunderboltXDPropertiesCache"=1,"AppleHSBluetoothInterface"=5,"IOBluetoothL2CAPSignalChannel"=2,"AtiDiagLedProgrammer"=0,"AtiPackingConnectorAssignerLegacy"=0,"AtiGetEngineClockInterface_V1"=0,"AMDRadeonX5000_AMDGFX9GLContext"=35,"IOThunderboltXDomainLink"=0,"AMDRadeonX5000_AMDGFX9CLContext"=0,"AMDRadeonX5000_AMDHWGart"=1,"AppleGFXHDADriver"=1,"IOServiceUserNotification"=311,"AppleMultitouchTrackpadHIDEventDriver"=0,"AppleFDEKeyStoreUserClient"=0,"IOThunderboltConfigPrepareToSleepCommand"=2,"IO80211PacketDescriptor"=8192,"IOSkywalkNetworkBSDClient"=0,"AMDRadeonX5000_IAMDSMLInterface"=1,"MemoryAllocator"=1,"IOAccelDevice2"=1,"AppleBCMWLANIO80211VirtualInterface"=3,"com_apple_filesystems_apfs"=0,"AppleGFXHDAFunctionGroup_80862805"=0,"IOSKRegionMapper"=5,"DigitizerTransducer"=0,"IOMbufMemoryCursor"=1,"IOBluetoothL2CAPInformationFrameMemoryBlock"=0,"IOSKMemoryArray"=0,"AppleGFXHDAFunctionGroup_80862807"=0,"BridgeAudioControllerPCI"=1,"IOAccelCLContext2"=0,"AppleThunderboltDPAdapterFamily"=1,"AMDRadeonX5000_AMDGFX9PM4Channel"=1,"IOCPU"=1,"AtiFbInterruptManager"=1,"IOAccelEventMachineFast2"=1,"AppleACPIEventPoller"=1,"AppleBCMWLANTestManager"=1,"IO80211ActionFrameDescriptor"=0,"IONetworkStack"=1,"ATIConnection"=2,"CCDataPipeBlob"=0,"IOThunderboltTransmitQueue"=2,"ApplePlatformEnabler"=1,"AtiEnableCrtc_V2_V1"=1,"IOSCSIPeripheralDeviceType07"=0,"IOSlaveMemory"=1,"AMDRadeonX5000_AMDAccelSurface"=10,"CSRBluetoothHostController"=0,"AppleMMIOSerial"=1,"IO80211Interface"=1,"IOSimpleReporter"=188,"AppleUSBXHCILPTHB"=0,"AppleIntelLpssUARTv1"=2,"IOModemSerialStreamSync"=0,"AtiSetPixelClock_V1_7"=1,"IOHDIXControllerUserClient"=0,"IOUSBMassStorageCBIDriverNub"=0,"AppleEffaceableBCE"=1,"com_apple_AppleFSCompression_AppleFSCompressionTypeZlib"=1,"AtiFbInterruptCallbackInterface"=2,"AppleBCMWLANChipManagerPCIe"=1,"AppleThunderboltNHIType2"=0,"AMDRadeonX5000_AMDAccelSharedUserClient"=35,"IOUSBInterface"=1,"AppleUSBLegacyRoot"=1,"CCFaultReporter"=1,"AppleGFXHDAEngine"=0,"AtiFirmwareInfoInterface_V2_1"=0,"IOAccelChannel2"=1,"AppleCSRBluetoothHostController"=0,"AMDRadeonX5000_AMDAccelDisplayMachine"=1,"AGPMClient"=0,"BridgeAudioCommunicationQueue"=2,"AMDRadeonX5000_AMDHWRing"=0,"IOBluetoothRFCOMMChannelUserClient"=0,"IOSCSIPrimaryCommandsDevice"=1,"AppleNVMeWorkLoop"=2,"AtiBlankCrtc_V2_V1"=1,"IOThunderboltConfigWriteCommand"=10,"AppleUSBALSService"=1,"AppleMCCSControlGibraltar"=1,"AppleBCMWLANChipLogger"=1,"IOHIDProviderPropertyMerger"=0,"AppleSMBusControllerMCP"=0,"IOThunderboltCommand"=5,"IOUSBDevice"=1,"AppleSEPControl"=1,"AppleUSBVHCIBringupDriver"=0,"IOAccelVidMemory"=1,"AppleGFXHDAWidget_80862805"=0,"AMDRadeonX5000_AMDCPEvent"=16,"AppleGFXHDAPath"=0,"IOThunderboltCallbackEventSource"=6,"AppleGFXHDAController"=1,"AppleHPMUserClient"=0,"IOAccelDisplayPipeTransaction2"=2,"AMDRadeonX5000_IAMDSMLPSP"=0,"IOImageLoaderRequest"=1,"AppleGFXHDAWorkLoop"=1,"IOHIDKeyboard"=0,"IOSkywalkNetworkInterface"=0,"AtiEnableCrtcInterface_V2"=1,"AIDQueueEventSourceWorkItem"=0,"IOACPIPlatformDevice"=281,"AMDRadeonX5000_AMDGFX9PM4Engine"=1,"_IOServiceInterestNotifier"=315,"AppleUSBHostRequestCompleter"=9,"IOBluetoothLocalUtilityEventSource"=0,"ExpansionEdidBlock"=4,"AppleUSBVHCIHostCxQueue"=4,"IOFramebufferI2CInterface"=6,"IOPowerConnection"=244,"Edid"=24,"IOFBController"=1,"AppleUSBVHCIMessageQueue"=1,"AppleThunderboltIPTransmitCommand"=0,"IOBluetoothSerialClientModemStreamSync"=0,"SCSITaskUserClient"=0,"IOWatchDogTimer"=2,"IOThunderboltConfigPollQuadletCommand"=0,"IOEventSource"=20,"AtiFirmwareInfoInterface_V1"=0,"IODMACommand"=98,"IOMachPort"=1293,"AppleEthernetAquantiaAqtion"=1,"AMDRadeonX5000_AMDSMLVCE"=1,"AtiScalerEnhanced"=1,"AppleGFXHDAStream"=0,"IOPMinformeeList"=272,"IOThunderboltReceiveQueue"=2,"AMDRadeonX5000_AMDAccelShared"=35,"AppleCredentialManager"=1,"AppleGFXHDAFunctionGroupFactory"=0,"AppleUSB30XHCITypeCPort"=4,"AppleACPIPowerResource"=0,"IOThunderboltXDPropertiesImmediateValue"=14,"CCLogStream"=12,"AtiSetDceClockInterface_V2"=1,"AppleUSBHostControllerIsochEndpoint"=0,"IOHIDEvent"=0,"AMDRadeonX5000_IAMDSMLUVD"=1,"IOAccelTask"=1,"OSDictionary"=13197,"IOAccelGLContext2"=1,"IOAGPDevice"=0,"AppleMultitouchMouseHIDEventDriver"=1,"AppleUSBXHCIParkingCommandRing"=0,"AMDRadeonX5000_AMDAtomicBlitManager"=1,"AtiSelectCrtcSourceInterface_V1"=0,"AppleFDEKeyStore"=1,"IODisplayWrangler"=1,"AtiAsicInitInterface_V2"=1,"AppleOnboardSerialBSDClient"=2,"AppleIntelI2CController"=0,"AppleUSBIORequest"=70,"IOThunderboltConfigXDomainROMChangedRequestCommand"=0,"IOUSBMassStorageDriverUFIDevice"=0,"IOUSBPipeV2"=1,"AppleUSBHostLegacyClient"=5,"ATIPanel"=6,"AppleEffaceableNOR"=1,"Vega10BiosAnalogConnection"=0,"AtiObjectInfoTableInterface_V1"=0,"IOAccelKernelMappedMemory"=47,"Dont_Steal_Mac_OS_X"=1,"IOAudioTimeIntervalFilterIIR"=0,"IOHIDEventSource"=10,"AppleGFXHDAFunctionGroupATI_Tahiti"=1,"AppleHVClient"=0,"OSSet"=2016,"AppleNVMeRequestPool"=1,"IOAccelBlockFence"=0,"AppleUSB30XHCICardReaderPort"=1,"IOAudioEngineUserClient"=0,"AMDRadeonX5000_AMDAccel2DContext"=6,"AGPMHeuristic4"=0,"AppleUSBHostPacketFilterService"=1,"AppleBCENORFlashDevice"=1,"AMDRadeonX5000_AMDGFX9SDMAEngine"=2,"AMDRadeonX5000_AMDRadeonHWServicesAbstract"=1,"IOCommand"=143,"AppleBCMWLANBusInterface"=1,"IOAudioTimerEvent"=0,"CCDataPipe"=2,"IOSCSIProtocolInterface"=2,"AppleTDMType00"=0,"AppleUSBXHCIAR"=2,"AppleGFXHDADriverUserClient"=0,"AMDRadeonX5000_AMDHardware"=1,"IOBluetoothGamepadHIDDriver"=0,"com_apple_driver_AppleUSBCardReaderSBC"=1,"ATIController"=1,"AtiEncoderControl_V1_5"=1,"AppleBCMWLANChipImage"=1,"IOGUIDPartitionScheme"=2,"AMDRadeonX5000_IAMDHWInterface"=1,"IOUSBMassStorageUFIDriverNub"=0,"OSCollectionIterator"=63,"AtiPowerPlayTableInterface_V1"=0,"AppleEFIRuntime"=1,"AMDRadeonX5000_AMDGFX9PM4ComputeChannel"=4,"AppleBCMWLANIOReportingPerSlice"=1,"AMDRadeonX5000_AMDDPTChannel"=6,"IOFilterScheme"=0,"IOImageLoaderDatastore"=0,"AppleMCCSIOController"=14,"AppleUSBHostResources"=1,"IONVMeController"=1,"IOApplePartitionScheme"=0,"IOSurfaceRootUserClient"=27,"AppleBCMWLANCommander"=1,"IOSkywalkInterface"=0,"IO80211PeerExtendedStats"=0,"IODisplay"=1,"AtiGetMemoryClockInterface_V1"=0,"AMDRadeonX5000_IAMDHWChannel"=2,"AMDRadeonX5000_AMDGFX9HWGart"=1,"IOHIDAsyncReportQueue"=0,"IOSkywalkPacketQueue"=0,"IOThunderboltSwitch"=1,"IOUserEthernetResource"=1,"AtiDeviceControl"=1,"IOBasicOutputQueue"=1,"AtiDac1EncoderControl_V1_V1"=0,"Vega10RegisterService"=1,"AppleS3ELabController"=0,"AppleUSBHostControllerListElement"=0,"AppleSEPIntelIOP"=1,"IOThunderboltConfigReadCommand"=11,"AMDRadeonX5000_IAMDHWRegisters"=1,"AtiSetPixelClock_V1_V7"=0,"AtiTableConnectorAssigner"=1,"IOUSBControllerIsochListElement"=0,"IOFramebufferSharedUserClient"=1,"IOPacketQueue"=19,"AppleGPUWranglerClient"=2,"AtiEnableCrtc_V1_V1"=0,"IOAccelSharedUserClient2"=1,"IOUserClient"=31,"IOHITabletPointer"=0,"AMDRadeonX5000_AMDAccelVideoContext"=1,"AMDRadeonX5000_AmdUbmInterface"=1,"AppleUSBHostControllerIsochListElement"=0,"AMDRadeonX5000_IAMDHWDisplay"=1,"IOHIDEventSystemUserClient"=1,"AtiEnableCrtcInterface_V1"=0,"IOHDIXHDDrive"=0,"AMDRadeonX5000_AMDPspDPPTestInterface"=1,"AGPM"=1,"AppleSimpleUARTCommand"=32,"AppleBCMWLANCoreDbg"=1,"IO80211AWDLPeer"=0,"AppleBCMWLANPCIeTransmitFlowRing"=5,"IOAccelEventMachine2"=1,"AtiPowerPlayTableInterface_V1_5"=0,"IOSlaveRelayCommandPool"=0,"IOAccelBufferMemoryDescriptorPool2"=0,"AppleMCCSControlModule"=6,"IOUSBHostPipe"=2,"IOPolledFilePollers"=0,"_HACK_RingBuffer"=0,"AtomBiosProxy"=1,"AppleBCMWLANHistogram"=4,"AtiBlankCrtc_V1_V1"=0,"IOBufferCopyCommandQueue"=1,"IO80211String"=0,"IOHDIXHDDriveOutKernelUserClient"=0,"IOUSBNotification"=0,"IOAccelDisplayMachine2"=1,"IOThunderboltSwitchI2CCommandQueue"=2,"AppleGFXHDAEngineInput"=0,"AMDRadeonX5000_AMDAccelUVDContext"=1,"AtiPowerPlayUserClient"=0,"AppleBCMWLANPCIeFlowQueue"=5,"IOSkywalkRxSubmissionQueue"=0,"IOUSBInterfaceUserClient"=1,"AtiDac2EncoderControl_V1_V1"=0,"AtiSpreadSpectrumInfoInterface_V1_1"=0,"IOAccelGPURestartReport2"=0,"IOFramebufferParameterHandler"=6,"AMDRadeonX5000_GmmSharedInfoList"=1,"IOThunderboltLinkController"=4,"IOSurface"=151,"AppleUSBRootHubDevice"=2,"IOGatedOutputQueue"=21,"IOReportLegend"=5,"AppleTDMControlLUN"=0,"IOSkywalkGeneralPacketQueue"=0,"IOThunderboltConfigCompareSwapCommand"=0,"IOBufferCopyDMACommand"=88,"Vega10FbCompressionManager"=0,"AppleUSBXHCIEndpoint"=3,"AppleBCMWLANPortInterfacePCIe"=1,"IOHIDEventQueue"=1,"IOSurfaceSendRight"=0,"IOAccelShared2"=1,"AIDService"=0,"AppleAPICInterruptController"=4,"AppleSMC"=1,"IOSkywalkNetworkController"=0,"IOTimeSyncService"=0,"AtiFbInterrupt"=7,"AtiSetPixelClockInterface_V1"=0,"IOCommandPool"=22,"IOBlockStorageDevice"=2,"AMDRadeonX5000_AMDGFX9Resource"=1634,"AppleXsanDriver"=0,"AppleBCMWLANTimeSyncClockInfo"=0,"AGPMHeuristic"=0,"IOPMrootDomain"=1,"IOAccelFenceMachine"=1,"AppleEffaceableStorage"=1,"IOImageLoaderImageDictionary"=0,"AppleUSBNetworkingCommandPool"=0,"IO80211VirtualInterfaceNamer"=1,"IOUSBDeviceUserClient"=1,"IOI2CInterfaceUserClient"=2,"IOThunderboltDispatchCallback"=2,"AppleThunderboltDPInAdapter"=4,"AppleOnboardSerialSkywalkInterface"=0,"IOHDIXCommandQueue"=0,"_IOOpenServiceIterator"=0,"IOBufferCopyEngineUserClient"=0,"IOCommandGate"=478,"EventElementCollection"=0,"IOUSBMassStorageDriver"=2,"AppleUSBNetworkingHostCommandPool"=0,"HDCPAuxHandler"=0,"AtiDacOutputControlInterface_V1"=0,"IOPMRequestQueue"=2,"AtiDisplayPortEventInterrupt"=6,"IOSkywalkRxCompletionQueue"=0,"AppleECSMBusController"=0,"AquantiaTimeSyncEthernetNICClock"=0,"IOBlockStorageDriver"=3,"AtiBlankCrtcInterface_V1"=0,"AMDRadeonX5000_AMDUVD7DecChannel"=1,"PrimaryEdidBlock"=4,"IOHIDWorkLoop"=1,"IOThunderboltArray"=6,"IOBlockStorageServices"=2,"AppleACPIACAdapter"=0,"IOUSBInterfaceIterator"=0,"AppleThunderboltPCIDownAdapter"=4,"IOImageLoaderUserClient"=0,"IODTPlatformExpert"=1,"IOAppleLabelScheme"=0,"IOHIDEventSystemQueue"=0,"IOMbufBigMemoryCursor"=0,"AppleUSBXHCIInterrupter"=1,"AppleUSBXHCICommandRing"=3,"AppleUSBXHCIIsochronousEndpoint"=0,"AppleUSBXHCIPCI"=2,"IOSlaveMemoryBuffer"=4,"IOBluetoothMemoryBlock"=0,"IOBluetoothHostControllerTransport"=1,"AMDRadeonX5000_AMDGFX9Hardware"=1,"AppleHPMIECS"=2,"AMDRadeonX5000_AMDUVD7EncLLQRing"=1,"IO80211Peer"=6,"AMDRadeonX5000_AMDRadeonHWServicesInterface"=1,"RootDomainUserClient"=93,"AtiNvramParserV1"=0,"R800_CHDCP"=0,"IOBufferCopyEngineUserClientBuffer"=0,"IOThunderboltTimerCommand"=8,"AppleAPFSContainer"=1,"AppleBCMWLANCommandMonitor"=1,"IONDRV"=0,"AppleHSBluetoothNub"=1,"IOThunderboltConfigCommand"=9,"AppleBCMWLANDynamicRingOperationContext"=0,"IOPCIDevice"=125,"AMDRadeonX5000_AMDPM4HWChannel"=2,"AppleUSB20XHCIPort"=7,"AMDRadeonX5000_AMDVCE4Ring"=2,"IOBluetoothInactivityTimerEventSource"=2,"APowerPlayManager"=1,"AppleBCMWLANScanManager"=1,"OSNumber"=12721,"IOAccelMemoryAllocator2"=4,"AppleThunderboltNHIMemoryBlock"=0,"IOThunderboltConfigXDomainPathTeardownRequestCommand"=0,"BridgeAudioTransportIOBCE"=1,"AIDUserClientLogger"=0,"AppleThunderboltNHITransmitRingManager"=2,"IOThunderboltIECSNub"=2,"CCFaultReport"=0,"AppleBCMWLANCommand"=96,"Vega10AuxChannelProxy"=6,"AtiTransmitterControl_V1_V5"=0,"AtiTimingGenerator"=1,"AppleThunderboltNHITransmitRing"=24,"AppleUSBXHCI"=1,"AppleBCMWLANRxItemRing"=1,"AppleBroadcomBluetoothHostController"=1,"IOTimeSyncIntervalFilter"=0,"AtiCommandGate"=0,"AMDRadeonX5000_AMDHWDisplay"=1,"AtiBiosParser2"=1,"AppleBCMWLANLogger"=1,"AppleBCMWLANPlatformFunction"=1,"IOThunderboltConfigErrorCommand"=2,"IOUserNotification"=2,"IOHIDKeyboardDevice"=0,"IOThunderboltEEPROM"=4,"AppleBCMWLANChipUART"=1,"AppleGFXHDAFunctionGroupATI_Broadway"=0,"AppleGFXHDAWidget"=1,"AtiSpreadSpectrumInfoInterface_V2_1"=0,"IOBluetoothRFCOMMMemoryBlock"=0,"AppleHPMCommandGate"=2,"AppleUSBXHCILPT"=0,"AppleGPUWrangler_GPUPostStartWorkItem"=0,"com_apple_AppleFSCompression_AppleFSCompressionTypeDataless"=1,"AGPMHeuristic3"=0,"IOThunderboltControlPathListener"=9,"AppleUSBXHCITransferRing"=3,"AppleThunderboltNHI"=1,"Vega10DiagLedProgrammerV2"=0,"AtiEncoderControlInterface_V1"=0,"IOThunderboltHopSet"=36,"IOThunderboltXDPropertiesLeafData"=0,"IOUSBHubDevice"=0,"AppleUSBHostDeviceIdler"=5,"IOPMWorkQueue"=1,"IOTimeSyncFilteredService"=0,"AMDRadeonX5000_AMDGFX9VMContext"=35,"AMDRadeonX5000_AMDUVD7EncChannel"=2,"AppleSMBusControllerUserClient"=0,"AppleUSB30XHCIPort"=6,"IOThunderboltTimerCommandQueue"=2,"IOSlaveProcessorUSBHostRelay"=0,"IODeblocker"=0,"AMDRadeonX5000_AMDDMAHWChannel"=1,"AppleHPM"=1,"AppleUSBXHCISPT"=1,"AMDRadeonX5000_AMDUVD7EncRing"=2,"AppleThunderboltIPControlCommand"=0,"AMDRadeonX5000_AMDCTT4"=0,"AMDRadeonX5000_AMDSMLGFX9Interface"=1,"IOAccelDeviceShmem"=81,"AtiPowerPlayInfoInterface_V2_V8"=1,"AtiEncoderControl_V1_V5"=0,"AppleBCMWLANProvisioningManager"=1,"AtiSetDceClockInterface_V1"=0,"AppleBCMWLANPCIeSubmissionRing"=4,"AppleBCMWLANChanSpec"=1,"AMDRadeonX5000_IAMDHWSemaphoreMemMgr"=1,"IOBufferCopyEventSource"=19,"IOSharedDataQueue"=6,"IOSyncer"=0,"X86PlatformShim"=1,"AppleGPUWrangler_WorkItem"=0,"AppleDeviceManagementHIDEventService"=2,"AppleThunderboltIPConnection"=0,"IORangeAllocator"=37,"IOMediaBSDClient"=8,"OSBoolean"=2,"AppleSEPCommand"=14,"AMDRadeonX5000_AMDUVDInterruptEventSource"=0,"AppleUSBXHCIRequest"=7,"DisplayPortUtilities"=1,"IOAccelSubmitter2"=2,"AMDRadeonX5000_AMDUVD7HWEngine"=1,"BridgeAudioCommunicationService"=1,"IOWorkQueue"=9,"ApplePlatformEnablerUserClient"=0,"AMDRadeonX5000_AMDVega10GraphicsAccelerator"=1,"IOMapper"=1,"LogManagerDevice"=3,"IOUSBMassStorageUFIDriver"=0,"IOPCI2PCIBridge"=18,"AppleUSBVHCIBCEEventQueue"=5,"IOAppleBluetoothHIDDriver"=1,"IOHIDSystem"=1,"AppleACPIInterruptLink"=0,"IOUSBInterfaceUserClientV3"=2,"IOHIDInterface"=9,"com_apple_BootCache"=1,"IOUSBHostStream"=0,"BridgeAudioControllerDummy"=0,"IOSurfaceRoot"=1,"GammaTable"=6,"IOThunderboltConfigWriteQuadletCommand"=4,"AtiLinkedListItem"=2,"AIDReporter"=0,"AMDRadeonX5000_AMDHWChannel"=4,"AppleBCMWLANCore"=1,"AppleUSBVHCIRequestPool"=1,"IOAccelRangeAllocator"=1,"IOUSBController"=1,"AppleHIDKeyboardEventDriverV2"=1,"IOAccelFIFOChannel2"=1,"AMDRadeonX5000_AMDPPTestInterface"=1,"AppleGFXHDAWidgetATI_RS780"=1,"AppleBCMWLANTaskmaster"=2,"AMDRadeonX5000_AMDSMLSAMU"=0,"AppleACPICPU"=16,"AMDRadeonX5000_AMDHWEngine"=4,"AppleMCCSControlFamily"=2,"IONetworkInterface"=1,"AMDRadeonX5000_AMDTPTManager"=0,"KernelRelay"=0,"IOThunderboltConfigCMOverrideCommand"=2,"AMDRadeonX5000_AMDAccelResource"=1,"IOBluetoothACLMemoryDescriptor"=0,"IONetworkUserClient"=0,"AppleBCMWLANBusInterfacePCIe"=1,"IOThunderboltConfigXDomainResponseCommand"=12,"BridgeAudioCommunicationTransport"=1,"IOReportUserClient"=3,"AppleUSBXHCIPipe"=3,"DpcdInfo"=12,"AtiConstantConnectorAssigner"=0,"IOSkywalkLegacyEthernet"=0,"IOCharacterDevice"=3,"IOUSBNub"=2,"AppleUSBHostMergeProperties"=1,"AMDRadeonX5000_IAMDStatisticsManager"=1,"_IOConfigThread"=0,"IOSkywalkRing"=0,"AppleMultitouchHIDEventDriverV2"=1,"Vega10Soc15Interrupt"=58,"AppleUSBXHCIARRequest"=10,"IOTimeSyncClockManager"=1,"IO80211FlowQueueDatabase"=5,"AtiSpreadSpectrumInfoInterface_V3_1"=0,"AppleGFXHDAFunctionGroupATI_RS730"=0,"AppleUSBHostController"=2,"IODiskImageBlockStorageDeviceOutKernel"=0,"AppleMultitouchHIDService"=0,"IOThunderboltConfigModifyQuadletCommand"=0,"AMD10000Controller"=1,"AtiPowerPlayTableInterface_V1_7"=0,"AtiPllAssigner"=1,"AppleSEPXART"=1,"AtiReGammaGenerator"=1,"IOUSBMassStorageDriverUFIStorageServices"=0,"IOThunderboltPath"=0,"AppleBCMWLANPCIeMMIOHistory"=1,"IOCPUInterruptController"=1,"AppleThunderboltHAL"=2,"AtiTransmitterControl_V1_6"=1,"AMDRadeonX5000_AMDVCEHWChannel"=1,"IO80211P2PInterface"=1,"IOSkywalkKernelPipeBSDClient"=0,"CCLogPipeUserClient"=7,"PMHaltWorker"=0,"AMDRadeonX5000_AMDRTRing"=6,"AppleBCMWLANUserClient"=0,"IOFramebufferDiagnosticUserClient"=0,"AMDRadeonX5000_AMDPM4CommandsUtility"=0,"AtiAsicInit_V1_2"=0,"AppleMCCSUserClient"=0,"AppleHSBluetoothHIDDriver"=5,"SCSITaskUserClientIniter"=0,"AppleUSBXHCIFL1100"=0,"IOSlaveCPU"=1,"AppleUpstreamUserClient"=0,"AtiAnalogPanelInfo"=6,"IOAudioTimeIntervalFilter"=0,"Vega10SharedController"=1,"AppleBCMWLANPCIeCompletionRing"=4,"AppleSimpleUARTSync"=2,"AppleUSBTDMMassStorageClass"=0,"IOBootFramebuffer"=0,"IOHIDResourceDeviceUserClient"=0,"IOInterruptController"=5,"AtiScalerInterface"=1,"SMCPolledInterface"=1,"AppleUSBHostResourcesClient"=1,"IOEthernetInterface"=7,"IOSkywalkPacketPoller"=0,"AtiAsicInitInterface_V1"=0,"IOTimeSyncTimeLineFilter"=0,"Vega10DiagLedProgrammerV1"=0,"AppleANS2Controller"=1,"AtiSmuInfoInterface_V2"=1,"AppleUSBXHCIARIsochronousRequest"=10,"AppleGFXHDAWidgetATI_RS710"=0,"AGDCPlugin"=1,"IOMbufLittleMemoryCursor"=2,"AtiDceInfoInterface_V2"=1,"AMDRadeonX5000_AMDUVD7DecRing"=1,"AppleUSBHubPolicyMaker"=2,"AmdAddress2Services"=1,"IOConditionLock"=0,"AppleBCMWLANKeepAliveOffload"=1,"IO80211WorkLoop"=1,"IOUSBUserClientLegacy"=2,"AppleUSBHostIORequestPool"=13,"IOBufferCopyEngineTestMapper"=0,"IOAccel2DContext2"=1,"com_apple_driver_pm_pch_reporter"=1,"AMDRadeonX5000_AMDHWVMM"=1,"IOAccelerator"=1,"Vega10SharedDigitalConnection"=1,"Vega10HotPlugInterrupt"=6,"AppleAPFSVolume"=4,"AppleNVMeBuffer"=4,"AppleIntelLpssI2CDevice"=0,"IOSkywalkStatisticsReporter"=0,"PMTraceWorker"=1,"AMDRadeonX5000_AMDAccelSegmentResourceList"=0,"IOAudioControl"=0,"IOSCSIBlockCommandsDevice"=1,"IO80211QueueCall"=1,"IOThunderboltUserProtocolListener"=0,"AMDRadeonX5100_AMDRadeonHWLibsSWIP"=1,"AppleSMBusControllerICH"=0,"AMDRadeonX5000_IAMDPM4CommandsUtility"=0,"IONVMeBlockStorageDevice"=1,"AppleGFXHDAControllerUserClient"=0,"IOI2CInterface"=1,"AMDFramebuffer"=6,"IO80211QueueDescriptor"=4,"IOAccelStatistics2"=1,"AtiSetPixelClockInterface_V2"=1,"IOUSBHostIOSource"=1,"AMDRadeonX5100_AMDRadeonHWLibs"=1,"IONetworkController"=1,"OSString"=11395,"AppleIntelLpssDmac"=0,"AtiGetEngineClock_V1_V1"=0,"CCIOReporterHub"=2,"IOThunderboltAbstractPath"=0,"IOUserIterator"=18,"AppleMCCSParameterHandler"=7,"AMDRadeonX5000_AMDVCE4Channel"=2,"IOSortableConfigurationDescriptor"=0,"PMSettingHandle"=5,"AppleBCMWLANChipManager"=0,"AppleMobileFileIntegrityUserClient"=0,"IOThunderboltConfigXDomainROMReadRequestCommand"=0,"AtiBiosParser1"=0,"AppleUSBXHCIIsochronousRequest"=6,"AppleUSBNCMData"=1,"OSOrderedSet"=525,"IOThunderboltString"=57,"AtiGetEngineClockInterface_V2"=1,"AMDRadeonX5000_AMDHWSemaphoreMemMgr"=1,"ARegisterService"=1,"IOHIDEventDriver"=3,"AppleUSBXHCIStream"=0,"AMDRadeonX5000_IAMDHWGart"=1,"AtiGetEngineClock_V2_V1"=1,"IOThunderboltConfigXDomainUUIDRequestCommand"=2,"IOThunderboltIECSCommand"=0,"IOAudioStream"=0,"AppleUSBXHCIPPT"=0,"IOSerialBSDClient"=2,"IOStateReporter"=41,"IOThunderboltSwitchType2"=0,"AppleAPFSMedia"=1,"IOTimeSyncSnapshotService"=0,"AppleOnboardSerialDebugDevice"=0,"APFSCryptoContext"=576,"com_apple_driver_pm_flex_reporter"=0,"HDCPDDCAuxHandler"=0,"IOThunderboltReceiveCommand"=32,"IONotifier"=4,"AGPMHeuristic2"=0,"AIDLoggerUserClient"=0,"IOBluetoothL2CAPMemoryBlock"=0,"AppleIntelLpssUART"=1,"IOAccelContext2"=3,"AMDRadeonX5000_IAMDHWSemaphore"=1,"AppleUSBPipe"=2,"IOTimeSyncTimeLineFilterIIR128"=0,"AppleUSBVHCIBCE"=1,"IOThunderboltPort"=18,"IOFilterInterruptEventSource"=11,"DDCProxy"=1,"IOThunderboltConfigNotifyAckCommand"=0,"IOLittleMemoryCursor"=0,"AtiFbCompressionManager"=0,"AtiDceInfoInterface_V2_V4_1"=1,"AtiSetPixelClock_V1_V5"=0,"IOHIDPointingDevice"=0,"IOSkywalkTxSubmissionQueue"=0,"AppleUSBXHCIWPT"=0,"IOBufferCopyEngineTest"=0,"AppleSEPIntelIOPNub"=1,"IOThunderboltTunnelDriver"=2,"_IOFramebufferNotifier"=33,"AtiDisplayEngineClock"=1,"IOBluetoothDataQueue"=2,"AppleIntelLpssI2CController"=0,"AMDRadeonX5000_AMDAccelVCEContext"=0,"AMDRadeonX5000_AMDInterruptEventSource"=6,"AppleIntelSlowAdaptiveClockingManager"=1,"AppleUSBHostRequest"=3,"AtiPowerPlayCallbackContext"=5,"IOSKRegion"=8,"IOMedia"=8,"IO80211VirtualInterface"=1,"IOHistogramReporter"=20,"IOPlatformPluginFamilyPriv"=1,"AppleBCMWLANPacketQueue"=0,"IONVMeControllerPolledAdapter"=1,"IO80211AWDLPeerManager"=1,"AtiFirmwareInfoInterface_V2_2"=0,"AppleSMBusDevice"=0,"IOBluetoothMemoryBlockQueue"=2,"OSSymbol"=9038,"IOAccelSurface2"=1,"IOSMBusController"=0,"AMDRadeonX5000_AMDGraphicsAccelerator"=1,"AppleACPIPlatformExpert"=1,"AMDRadeonX5000_AMDCommandBufferPool"=51,"IORegistryPlane"=7,"AppleUSBCDCControl"=1,"AtiComponentPanelInfo"=0,"IOHIDLibUserClient"=12,"IOUSBMassStorageDriverNub"=2,"IOThunderboltFrameList"=34,"AppleUSBInterfaceIterator"=0,"IOSlaveEndpoint"=1,"AMDRadeonX5000_AMDPspDPPStatusInterface"=0,"AppleSMBusController"=0,"GTrace"=1,"IOInterruptEventSource"=182,"AppleUSBXHCIInterrupterMSI"=9,"IOSkywalkPacketBufferPool"=0,"ATIAnalogConnection"=0,"AMDRadeonX5000_IAMDSMLSAMU"=0,"BridgeAudioController"=1,"IO80211ServiceRequestDescriptor"=2,"OSObject"=247,"IOBluetoothSerialManager"=1,"AMDRadeonX5000_AMDAccelVidMemory"=2493,"AppleBCMWLANPlatformFunctionEventTimestamp"=0,"AMDRadeonX5000_AMDAccelCPContext"=1,"IOHDIXController"=1,"IOMbufNaturalMemoryCursor"=0,"AMDSupport"=1,"R800SharedHDCP"=0,"Vega10DisplayPortConnection"=1,"IOKDP"=0,"CCIOReporterDataStream"=1,"IOSlaveRelayEndpoint"=0,"IOBluetoothHIDDriver"=1,"IOFence"=0,"IO80211AssociationJoinSnapshot"=1,"IOAccelTraceStreamConnection"=7,"AppleUSBNetworkingCommand"=0,"IOGraphicsDevice"=1,"IOThunderboltNumber"=349,"IOUSBControllerListElement"=0,"AppleNVMeRequest"=128,"IOResources"=1,"AtiDividerRange"=3,"IOBufferCopyEngineTestFirmwareChannel"=0,"IOAccelNamespace"=37,"AtiConnectorAssigner"=1,"IOSCSIPeripheralDeviceNub"=1,"AppleBCMWLANTimeKeeper"=1,"RSNSupplicant"=0,"AppleUSBXHCIARRequestPool"=2,"AmdGfx9AddressServices"=1,"Vega10LineBuffer"=6,"IOSurfaceDeviceCache"=133,"AppleUSBVHCI"=1,"IOThunderboltConfigReadQuadletCommand"=4,"AGPMController"=1,"AppleBCMWLANIO80211P2PInterface"=1,"AppleUSBXHCIRequestPool"=3,"IOThunderboltXDLocalPropertiesCache"=2,"AtiDac1OutputControl_V1_V1"=0,"Vega10HdmiConnection"=4,"AtiUpstreamMessageParserV2"=6,"AppleGraphicsDeviceControlClient"=12,"IOUSBBus"=1,"IOServicePM"=272,"IOBigMemoryCursor"=0,"AppleIntelLpssI2CGate"=0,"AppleThunderboltNHIType3"=2,"AppleUSBVHCIRequest"=16,"AMDRadeonX5000_IAMDAtomicBlitManager"=1,"AppleGFXHDAWidgetATI_RS730"=0,"AppleGFXHDAEngineOutput"=0,"Vega10Scaler"=6,"AppleUSBHostBusCurrentPool"=0,"AEdidBlock"=2,"IOMemoryDescriptor"=2,"AppleTDMAKSServices"=0,"AppleGFXHDAFunctionGroupATI_Park"=1,"AtiTimingsList"=64,"IOUSBInterfaceUserClientV2"=1,"IODMAController"=0,"AppleUSBInterface"=7,"AtiGetSmuClockInfoInterface_V2"=1,"IOThunderboltDictionary"=15,"IOUSBControllerV3"=1,"AppleBCMWLANEnterpriseManager"=1,"AppleGraphicsControl"=0,"AppleS3XController"=0,"IOBluetoothSCOMemoryDescriptorRetainer"=4,"AMDRadeonX5000_AMDGFX9Display"=1,"EventQueue"=1,"AMDRadeonX5000_AMDCPAppInterface"=2,"IOThunderboltI2CCommand"=4,"AGPMEventSource"=1,"AMDRadeonX5000_AMDAccelDisplayPipe"=6,"IOCatalogue"=1,"IOWorkLoop"=85,"AppleBCMWLANNetManager"=1,"IOThunderboltI2CCommandQueue"=1,"AtiPanelInfo"=3,"AppleBCMWLANPCIeSnapshotContext"=0,"IOBufferCopyEngineTestDummy"=1,"AppleBCMWLANBGScanManager"=1,"IODataQueue"=1,"AtiConnectionChangeInterrupt"=6,"CCIOReporterLogStream"=1,"AtiSelectCrtcSource_V1_V3"=0,"AppleBCMWLANJoinManager"=1,"IOHIDDevice"=3,"AppleUSBVHCIEndpoint"=10,"IOSkywalkNetworkPacket"=0,"IOBluetoothL2CAPChannel"=5,"AMDRadeonX5000_AMDVega10Hardware"=1,"CCStream"=2,"IOHIDElement"=1,"AMDRadeonX5000_AMDGFX9CommandRing"=1,"AppleBCMWLANChipMemory"=1,"IOReportHub"=1,"AppleBCMWLANRxByteRing"=1,"AppleIntelI2CCommand"=0,"AMDRadeonX5000_AMDHWSemaphore"=13312,"AppleIntelLpssI2CUserClient"=0,"IO80211ScanManager"=1,"IOEthernetController"=4,"IOThunderboltConfigXDomainRequestCommand"=0,"IOSlowAdaptiveClockingDomain"=0,"AtiGetMemoryClockInterface_V2"=1,"PMKSACache"=1,"IOTimerEventSource"=289,"IOBufferCopyEngineTestSubmissionQueue"=0,"IOThunderboltCommandQueue"=15,"CryptoBufferDescriptor"=576,"AtiHwCursor"=1,"IOSerialDriverSync"=1,"IOPCIConfigurator"=1,"com_apple_filesystems_hfs_encodings"=1,"AppleOnboardSerialBusInterface"=1,"Stopwatch"=13,"AppleGFXHDAPathControl"=0,"AtiHdcpService"=2,"IOSlaveRelayCommand"=0,"CCLogPipe"=7,"AppleSMCClient"=4,"AIDReporterState"=0,"AppleUSBVHCIDevice"=4,"IOServiceMessageUserNotification"=376,"IOTimeSyncUserClient"=0,"AppleXsanScheme"=0,"AppleTDMAKSDriver"=0,"IOReporter"=3,"AtiProcessAuxTransactionInterface_V1"=0,"AtiSmuInfoInterface_V2_V3_1"=1,"AMDRadeonX5000_AmdUbmServices"=1,"AppleUSBHostBusCurrentClient"=9,"IOMultiMemoryDescriptor"=0,"AppleBCMWLANGASManager"=1,"IOPlatformPluginFamily"=1,"AtiEncoderControl_V1_V4"=0,"Vega10HdcpAuthFailInterrupt"=6,"IOAccelDrawable2"=8,"IOSCSILogicalUnitNub"=2,"AtiProcessAuxTransactionInterface_V2"=1,"AppleUSBVHCIPort"=8,"AMDRadeonX5000_AMDHWMemory"=1,"IOSCSIHierarchicalLogicalUnit"=0,"AppleBCMWLANChipConfigSpace"=1,"IOTimeSyncClockMapping"=0,"AIDCircularBuffer"=0,"IOAccelAllocationInfo"=0,"KDIURL"=0,"AGPMHeuristic1"=0,"IOPanicPlatform"=0,"IODMAEventSource"=0,"IOThunderboltConnectionManager"=2,"IOSCSIMultipathedLogicalUnit"=0,"AHwI2cProxy"=1,"IOPlatformDevice"=4,"AppleNVMeSMARTUserClient"=0,"AMDRadeonX5000_AMDSMLCPMsg"=0,"IOThunderboltXDDirectory"=0,"AppleHIDTransportIODataQueue"=0,"AppleUSBHostDARTDMACommand"=0,"AIDLogger"=0,"AppleGFXHDAEngineOutputDP"=0,"CCCapture"=0,"IOSimpleMbufMemoryDescriptor"=0,"IOThunderboltData"=0,"AppleMultitouchHIDEventService"=0,"AppleThunderboltDPPathManager"=4,"IO80211RangingManager"=1,"AppleOnboardSerialSync"=1,"AMDRadeonX5000_AMDHWHandler"=1,"IOUSBMassStorageUASDriverCommand"=0,"IOBluetoothRFCOMMConnectionUserClient"=0,"IOThunderboltCommandGate"=12,"IOSkywalkController"=0,"AtiDigitalPanelInfo"=6,"ATINoConnection"=6,"IOAudioControlUserClient"=0,"AMDRadeonX5000_AMDAccelChannel"=17,"AppleThunderboltNHIType1"=0,"VI_CHDCP"=0,"AppleThunderboltGenericHAL"=1,"OSSerialize"=1,"AppleIntelI2CCommandQueue"=0,"AppleUSBDescriptorCache"=5,"AppleBCMWLANIOReporting"=2,"IOAudioDevice"=1,"IOAudioEngine"=0,"OSKext"=149,"IOAccelCommandBufferPool2"=0,"AppleHSBluetoothDevice"=3,"AppleBCMWLANConfigManager"=1,"ApplePMC"=2,"AppleUSBDescriptor"=35,"Vega10HdcpAuthSuccessInterrupt"=6,"IOBluetoothSerialClientSerialStreamSync"=1,"Vega10DpAudioConnection"=12,"AppleSMBIOS"=1,"AppleGPUWrangler_GPU"=1,"com_apple_driver_pm_msr_reporter"=1,"IOSkywalkTxCompletionQueue"=0,"AppleBCMWLANStopwatch"=16,"SMCWatchDogTimer"=1,"AMDRadeonX5000_IAMDCommandBufferPool"=1,"AtiGetMemoryClock_V1_V1"=0,"AMDRadeonX5000_AMDDMAHWEngine"=1,"AGDPClientControl"=1,"AppleEthernetAquantiaAqtionUserClient"=0,"IO80211InterfaceMonitor"=4,"_IOServiceJob"=0,"IOPMPowerStateQueue"=1,"AMDRadeonX5000_AMDVCEHWEngine"=1,"IOBluetoothRFCOMMConnection"=0,"OSIterator"=3,"AtiNvramParserV2"=1,"hv_vcpu_t"=0,"AtiCommandTableBaseClass"=17,"IOAccelerationUserClient"=2,"IOBluetoothTimerEventSource"=0,"AppleIntelI2CDevice"=0,"AMDRadeonX5000_AMDGFX9SDMARing"=2,"IOThunderboltJTAG"=2,"AppleUSBHostBusCurrentAllocator"=27,"Vega10HdcpRiRequestInterrupt"=6,"IOMemoryMap"=2492,"CCDataStream"=2,"AtiUpstreamDataInterrupt"=6,"AppleHPMLPSS"=0,"IOAudioToggleControl"=0,"AppleSEPTesting"=0,"com_apple_driver_pmtelemetry"=1,"IOThunderboltStatistics"=2,"IOBluetoothHCIRequest"=0,"SCSITask"=1992,"AtiMccsInterrupt"=6,"IOBluetoothL2CAPSupervisoryFrameMemoryBlock"=0,"IOThunderboltLocalNode"=2,"IOHDIXHDDriveOutKernel"=0,"AppleUSBXHCIDevice"=1,"IOUSBMassStorageCBIDriver"=0,"AppleNVMeController"=1,"AtiSelectCrtcSource_V1_V2"=0,"IOImageLoader"=1,"AtiGetMemoryClock_V2_V1"=1,"IO80211Controller"=1,"HDCPDPAuxHandler"=0,"AppleMobileFileIntegrity"=1,"AMDRadeonX5000_AMDGFX9GraphicsAccelerator"=1,"AppleBCMWLANTimeSyncEngine"=0,"IOTimeSyncNotifier"=0,"X86PlatformPlugin"=1,"IOPCIDiagnosticsClient"=0,"IOHIDParamUserClient"=1,"IOPCIBridge"=2,"AMDRadeonX5000_AMDAccelTask"=36,"AMDRadeonX5000_AMDUVDHWChannel"=2,"AppleEffaceableStorageUserClient"=0,"IORegistryIterator"=14,"OSData"=61059,"AppleOnboardSerialPool"=2,"AIDReporterSimple"=0,"AppleBCMWLANHashtable"=12,"AppleBCMWLANParseRing"=1,"IOGraphicsAccelerator2"=1,"AMDRadeonX5000_IAMDHWMemory"=1,"IOThunderboltFindCapabilityCommand"=2,"IOThunderboltPacketLoggerNub"=0,"PMAssertionsTracker"=1,"IOOutputQueue"=1,"AppleSEPUserClient"=0,"AMDRadeonX5000_IAMDHWEngine"=1,"AppleUSBHostDMACommand"=0,"AppleEmbeddedKeyboard"=1,"IOThunderboltTransmitCommand"=6,"Vega10TimingGenerator"=6,"IOThunderboltXDomainPath"=0,"IOSCSIPeripheralDeviceType00"=2,"IO80211PeerManager"=4,"AtiDynamicPllAssigner"=0,"IOHDIXHDDriveNub"=0,"AppleKeyStoreCommand"=2,"AtiSelectCrtcSource_V2_3"=1,"AppleThunderboltIPService"=2,"AppleNVMeRequestTimer"=1,"AppleACPIPlatformUserClient"=0,"IOHIDKeyboardEventDevice"=0,"IOBluetoothL2CAPChannelUserClient"=2,"IOSkywalkLegacyEthernetInterface"=0,"AppleBCMWLANIO80211APSTAInterface"=1,"IOSCSITargetDevice"=0,"AppleBacklightDisplay"=1,"AtiHdcp2Lib"=6,"AtiScaler"=0,"IOSlaveProcessorRelay"=0,"AppleGFXHDAWidget_80862807"=0,"IORootParent"=1,"AppleUSBMergeNub"=1,"com_apple_driver_pm_cstate_reporter"=0,"IO80211PeerMonitor"=6,"AppleGFXHDA8086_9D70Controller"=0,"AIDQueueEventSource"=0,"IOThunderboltSwitchLC"=1,"AMDRadeonX5000_AMDDPPStatusInterface"=0,"PMSettingObject"=5,"AtiEncoderControlInterface_V2"=1,"AppleACPIPCI"=4,"AppleKeyStore"=1,"AppleGPUWrangler_MatchNotificationWorkItem"=0,"IOThunderboltControlPath"=2,"IOPMinformee"=240,"IOUSBCommand"=0,"AppleUSBHostDMABufferMemoryDescriptor"=37,"IOPMPowerSource"=0,"IOSlowAdaptiveClockingManager"=1,"AtiBlankCrtcInterface_V2"=1,"hv_vmx_space_t"=0,"AppleUSBVHCITransferQueue"=1,"AppleBCMWLANWorkOrder"=272,"AppleGFXHDAEngineUserClient"=0,"AtiTransactionCompleteInterrupt"=6,"IOUSBLog"=1,"AMDRadeonX5000_AMDAccelDevice"=44,"CCPipeUserClient"=2,"IOThunderboltWorkLoop"=2,"AtiFirmwareInfoInterface_V2"=1,"AppleSEPManager"=1,"AMDRadeonX5000_AMDDecAppInterface"=1,"AtiSelectCrtcSourceInterface_V2"=1,"IOBluetoothDevice"=2,"AppleBusPowerController"=1,"AppleThunderboltIPTransmitter"=0,"AuxChannelProxy"=1,"IODisplayParameterHandler"=2,"IOAccelSharedNamespace2"=35,"IOBufferMemoryDescriptor"=1835,"AppleUSBXHCILPTH"=0,"AppleACPIButton"=2,"Vega10HwI2cProxy"=1,"IOThunderboltFamilyUserClient"=0,"CCPipe"=2,"IOHIDEventServiceUserClient"=4,"AMDRadeonX5000_AMDRadeonHWServicesSWIP"=1,"IOThunderboltXDomainService"=0,"AppleMultitouchHIDEventDriver"=0,"IOPolledInterface"=3,"IONDRVDevice"=0,"IO80211NetBootNubV2"=0,"IOAccelMemory"=2,"IOTimeSyncTimeLineFilter128"=0,"AtiUpstreamMessageParserV1"=0,"AtiSpreadSpectrumInfoInterface_V1"=0,"AppleUSBDevice"=6,"IOPlatformExpertDevice"=1,"IOBufferCopyEngineUserClientState"=0,"IOUSBHubPolicyMaker"=1,"IOHIPointing"=0,"IOBluetoothHCIController"=1,"IOThunderboltController"=2,"AIDUserClient"=0,"Vega10BandwidthManager"=1,"AMDRadeonX5000_AMDRadeonHWServicesVega10"=1,"AMDRadeonX5000_AMDHWVMContext"=1,"AtiVBiosHelper"=1,"AppleUSBVHCIHostTransferQueue"=2,"AtiFbInterruptReferenceCallback"=0,"AppleAPFSContainerScheme"=1,"IONetworkData"=35,"IOAudioLevelControl"=0,"AppleBCMWLANPCIeLinkChangeEventSource"=1,"AppleUSBXHCISPTLP"=0,"IOBluetoothRFCOMMChannel"=0,"AppleBCMWLANPacketTransmitter"=0,"IOUSBCommandPool"=0,"AtiAdjustDisplayPll_V3"=0,"IOBluetoothHCIPacketLogUserClient"=0,"IOECStateNotifier"=0,"AtiTvPanelInfo"=0,"AppleS1XController"=0,"AppleBCMWLANPCIeIO"=2976,"R700_CHDCP"=0,"AppleUSBVHCICommandQueue"=1,"AppleGFXHDAFunctionGroupATI_RS780"=1,"AppleAPFSVolumeBSDClient"=4,"AppleMultitouchEventServiceWrapper"=0,"Vega10DisplayPortUtilities"=12,"IO80211FlowQueue"=1,"AtiGpioPinLutInterface_V1"=0,"DPTrainingSettingsCalculator"=12,"IOPlatformPluginDevice"=2,"AppleTDMAKSCommand"=0,"IOKernelDebugger"=0,"AMDRadeonX5000_IAMDHWVMContext"=1,"IOBacklightDisplay"=1,"IOThunderboltNHIReceiveRing"=1,"AtiEnableSpreadSpectrumInterface_V1"=0,"AMDRadeonX5000_AMDVega10HardwareSmuDebug"=0,"IONetworkMedium"=51,"IODisplayConnect"=1,"IOHIDResource"=1,"IOTimeSyncTimeLineFilterIIR"=0,"AtiLinkedListIterator"=1,"AGPMHeuristic0"=0,"AppleNVMeTranslationSMARTUserClient"=0,"AtiFbInterruptCallback"=45,"AppleSATLSMARTUserClient"=0,"AppleUSBCDCCompositeDevice"=1,"AMDRadeonX5000_AMDHWRegisters"=1,"IOUSBRootHubDevice"=0,"R700SharedHDCP"=0,"AppleMultitouchInputHIDEventDriver"=1,"AppleUSBVHCIControlRequestPool"=1,"IOSlaveRelayActionCommand"=0,"IOHIDPointingEventDevice"=0,"IOThunderboltXDPropertiesLeafText"=4,"IOHIDDeviceShim"=0,"AppleBCMWLANIOReportingCore"=1,"AppleSCSISubsystemGlobals"=1,"IOBluetoothHostControllerUARTTransport"=1,"IOThunderboltConfigXDomainPathSetupRequestCommand"=0,"AtiProcessAuxTransaction_V1_V2"=0,"AMDRadeonX5000_AMDPM4HWEngine"=1,"IOBluetoothObject"=2,"AppleUSBXHCIARIsochronousRequestPool"=2,"OSMetaClass"=0,"KernelRelayEndpoint"=0,"AppleThunderboltIPPort"=4,"AppleBCMWLANBSSBeacon"=97,"AtiUpstreamStatusInterrupt"=6,"AMDRadeonX5000_AMDVCE4LLQRing"=1,"AppleGraphicsDeviceControl"=4,"IOAccelDisplayPipeGammaTable2"=1,"AtiSetDceClock_V1_V2_1"=0,"AMDRadeonX5000_AMDSMLUVD"=1,"IOUSBControllerV2"=1,"IOHIDPointing"=0,"IOBufferCopyController"=1,"AppleUSBVHCIHostTxRxQueue"=6,"IOAudioSelectorControl"=0,"AtiGetSmuClockInfo_V3_1"=1,"CCDataSession"=0,"AppleBCMWLANPowerManager"=1,"IOBluetoothDeviceUserClient"=1,"IOThunderboltIECSCommandQueue"=2,"IOSKMapper"=1,"AtiBandwidthManager"=1,"IOThunderboltDispatchContext"=4,"IOSCSIProtocolServices"=2,"ATIConnector"=6,"AppleEFINVRAM"=1,"AMDRadeonX5000_AMDStatisticsManager"=1,"AMDRadeonX5000_AMDSIAtomicBlitManager"=1,"IOKitDiagnostics"=1,"AtiSetDceClock_V2_1"=1,"AppleIntelLpssDmacChannel"=0,"IODTNVRAM"=1,"AppleMultitouchDeviceUserClient"=1,"IOHIDEventServiceQueue"=5,"AtiPowerPlayTableInterface_V1_6"=0,"com_apple_driver_pm_reporter"=3,"AppleUSBXHCITDPool"=3,"AppleBCMWLANCallbackEventSource"=1,"AtiPackingConnectorAssignerDynamic"=0,"AMDRadeonX5000_IAMDHWHandler"=1,"AMDRadeonX5000_AMDGFX9SDMAChannel"=2,"AppleACPIEC"=1,"IOAccelDisplayPipeUserClient2"=6,"AppleMultitouchTimestampSync"=0,"hv_vm_t"=0,"IOHDIXCommand"=0,"AppleSSE"=1,"IOPMRequest"=0,"IOECTimeSyncHandler"=0,"AppleBCMWLANLeakyApParser"=1,"IOAccelMemoryMap"=1,"IOHIKeyboard"=0,"IOHIDUserDevice"=0,"AppleGPUWrangler_BusyInterestWorkItem"=0,"AMDRadeonX5000_AMDAccelMemoryMap"=4150,"AMDRadeonX5000_AMDGFX9HWMemory"=1,"AMDRadeonX5000_AMDGFX9VMM"=1,"AppleMCCSControlCello"=0,"AppleBCMWLANDMASlab"=6,"AppleBCMWLANPlatformFunctionMac"=1,"IOService"=163,"AppleBCMWLANTxBuffer"=96,"IORS232SerialStreamSync"=2,"AMD10000ControllerWrangler"=1,"AppleXsanDevice"=0,"IOBluetoothWorkLoop"=0,"IOHIDEventRepairDriver"=0,"AtiHdcp1Lib"=6,"IOAccelBlockFencePort2"=29,"IOSKMemoryBuffer"=12,"BridgeAudioControllerUserClient"=1,"IOAccelSysMemory"=1,"AppleBCMWLANChipBackplane"=1,"AppleSMCFamily"=1,"IOFramebuffer"=1,"HIDAlwaysNotifyingIODataQueue"=1,"AppleMultitouchDevice"=1,"AppleBCMWLANTxItemRing"=1,"AppleGFXHDAFunctionGroupATI_RS710"=0,"AtiAtomBiosParser"=1,"AMDRadeonX5000_AMDAccelLibs"=0,"AppleUSBXHCIIsochronousTransferRing"=0,"AMDRadeonX5000_IAMDSMLCTT"=0,"AppleGFXHDAPathSet"=0,"IOPMCompletionQueue"=1,"AppleSEPCommandPool"=2,"IOTimeSyncUserFilteredService"=0,"AtiSetPixelClock_V1_V6"=0,"AtiAtomFirmwareInterface"=1,"AppleOSXWatchdog"=1,"AppleBCMWLANCoreFirmwareLoader"=0,"AppleHV"=1,"AppleCredentialManagerUserClient"=2,"IOThunderboltNHI"=1,"BroadcomBluetoothHostController"=1,"mDNSOffloadUserClient"=0,"AppleUSBHostPort"=2,"ATIDigitalConnection"=1,"CCDataPipeUserClient"=2,"Vega10ScalerCoeff"=1,"AppleGFXHDAFunctionGroupExternalControlFactory"=0,"IOAccelMemoryInfoUserClient"=0,"IOFDiskPartitionScheme"=0,"com_apple_filesystems_hfs"=1,"AppleMultitouchEventDriverWrapper"=1,"AppleBCMWLANPCIeDoorbell"=1,"AMDRadeonX5000_AMDGFX9ComputeRing"=4,"AMDRadeonX5000_IAMDHWRing"=1,"AppleTDMEffaceableNORDriver"=0,"Vega10BiosDigitalConnection"=6,"BridgeAudioTransportBCESubmissionQueue"=2,"AppleUSBVHCIControlRequest"=5,"AppleUSBXHCIStreamingEndpoint"=0,"AppleSSEUserClient"=0,"IOUSBMassStorageInterfaceNub"=1,"Vega10InterruptManager"=1,"IOBluetoothSerialClient"=1,"KernelRelayHost"=0,"AMDRadeonX5000_AMDAccelPspContext"=1,"AtiUserClient"=0,"IOAccelResource2"=1,"AtiAppServices"=0,"IOPMPowerSourceList"=0,"AtiPowerPlayInfoInterface_V2"=1,"AMDRadeonX5000_AMDAccelSysMemory"=1894,"IOThunderboltNub"=2,"AMDRadeonX5000_AMDHWSemaphorePool"=1,"mDNSHandoff"=0,"AppleVTDDeviceMapper"=0,"AtiUpstreamMessageParser"=1,"IOAccelTraceStream2"=1,"AtiEnableSpreadSpectrumOnPll_V3"=0,"AppleIntelLpssI2C"=0,"IOUSBPipe"=1,"AppleACPICPUInterruptController"=1,"BridgeAudioCommunicationUserClient"=1,"AMDRadeonX5000_AMDAccelStatistics"=1,"AMDRadeonX5000_IAMDHWSemaphorePool"=1,"AppleSEPEndpoint"=4,"AppleBCMWLANProximityInterface"=1,"AppleVTD"=1,"AMDRadeonX5000_IAMDStatisticsGroup"=1,"AMDRadeonX5000_AMDPspDecAppInterface"=1,"AppleEthernetAquantiaAqtionFirmwareInterface"=0,"Vega10SharedAnalogConnection"=0,"IOPlatformExpert"=1,"AtiTransmitterControlInterface_V1"=0,"AMDRadeonX5000_AMDLinkedList"=1,"AtiTransmitterControlInterface_V2"=1,"IOUserEthernetController"=0,"AMDRadeonX5000_AMDVCE4HWEngine"=1,"IOAccelDisplayPipePostCSCGammaVID"=0,"AtiTransmitterControl_V1_V6"=0,"AppleUSBController"=2,"IOTimeSyncUserFilteredServiceUserClient"=0,"IOPartitionScheme"=2,"IOTimeSyncIntervalFilter128"=0,"AtiAdjustDisplayPllInterface_V1"=0,"AppleGFXHDAFunctionGroupExternalControl"=0,"IOSlaveFirmware"=0,"com_apple_driver_AppleUSBCardReaderDriverNub"=1,"IOConditionGate"=4,"AMDRadeonX5000_AMDRTHardware"=1,"AMDRadeonX5000_AmdAddressInterface"=1,"AMDRadeonX5000_VendorGart"=1,"IOHIDUserClient"=1,"AtiProcessAuxTransaction_V1_2"=1,"LogManager"=1,"IOACPIPlatformExpert"=1,"AppleGFXHDAWidget_1002AAA0"=14,"AppleTDMNORFlashDevice"=0,"IOThunderboltSwitchType3"=2,"IOThunderboltUserObjectExporter"=0,"IOThunderboltNHITransmitRing"=1,"AppleOSXWatchdogClient"=1,"Vega10SharedInterrupt"=4,"IOAccelVideoContext2"=1,"com_apple_driver_pm_cpu_mbox"=0,"IOUSBControllerIsochEndpoint"=0,"IOThunderboltConfigResetCommand"=4,"IOUSBPortInterruptEventSource"=27,"AMDRadeonX5000_AMDAccelCommandQueue"=23,"IOBufferCopyEngine"=1,"AppleUSBNCMControl"=1,"AppleBCMWLANBonjourOffload"=1,"AMDRadeonX5000_AMDVCE4LLQChannel"=1,"IOHIDEventService"=3,"IOAudioTimeIntervalFilterFIR"=0,"AtiFirmwareInfoInterface_V2_V3_1"=1,"IOTimeSyncIntervalFilterIIR128"=0,"IOAccelDisplayPipePreCSCLinearizationVID"=3,"IOUserEthernetInterface"=0,"IOThunderboltConfigXDomainLinkChangeRequestCommand"=0,"IOAudioPort"=0,"Vega10HwCursor"=6,"AMDRadeonX5000_AMDHashTable"=0,"IOSkywalkPacketBuffer"=0,"IOHIKeyboardMapper"=0,"AppleUSBBusPowerClient"=8,"AMDRadeonX5000_AMDSMLInterface"=1,"AppleGFXHDAWidgetFactory"=0,"AMDRadeonX5000_AMDUVD7"=1,"KRActionCommandPool"=0,"IOUSBHostInterface"=7,"IOTimeSyncIntervalFilterIIR"=0,"com_apple_driver_pm_msr_limits_reporter"=0,"AppleGPUWrangler"=1,"hv_vmx_vcpu_t"=0,"AtiObjectInfoTableInterface_V2"=1,"IOBufferCopyEngineTestFirmware"=0,"OSArray"=11681,"IOGeneralMemoryDescriptor"=4992,"AMDRadeonX5000_AMDVega10VideoContext"=1,"IOSkywalkBSDClient"=0,"IOThunderboltConfigXDomainLinkStatusRequestCommand"=0,"AMDRadeonX5000_AMDStatisticsGroup"=1,"IOUSBIsocCommand"=0,"AMDRadeonX5000_AMDUVDHWEngine"=1,"STUCWorkLoopLock"=0,"IOThunderboltDispatchQueue"=16,"IOSlaveProcessor"=1,"IO80211FlowQueueLegacy"=0,"IOTimeSyncMachAbsoluteNanoseconds"=0,"Vega10HpdRxInterrupt"=6,"AtiHdcpProxy"=6,"IO80211ControllerMonitor"=1,"IOThunderboltPortMicro"=0,"IOUSBWorkLoop"=2,"IOSurfaceClient"=179,"IOAudioEngineEntry"=0,"AppleThunderboltNHIReceiveRing"=24,"IOGFXHDAStream"=0,"IOThunderboltConfigXDomainCommand"=2,"IOConfigurationDescriptorOrderedSet"=0,"IOThunderboltProtocolListener"=2,"AtiGpuWrangler"=1,"AIDSerialLogger"=0,"com_apple_driver_pm_ltr_reporter"=1,"AppleGraphicsDeviceControlPlugin"=1,"AtiOfflinePanelInfo"=6,"IO80211CommandQueue"=30,"Vega10DisplayEngineClock"=1,"AppleVirtualNORFlashDevice"=1,"AppleUSB20XHCITypeCPort"=4,"IOBootNDRV"=0,"IOHIDElementPrivate"=1736,"AtiSclCoeff"=1,"AppleBCMWLANCommandQueue"=11,"AGDCPluginDisplayMetrics"=1,"AppleSSEInterface"=1,"AppleMultitouchTimestampSyncUC"=0,"IOHITablet"=0,"AtiStaticPllAssigner"=1,"AppleGFXHDANode"=2,"AppleHPMDevice"=4,"AppleACPIEventController"=1,"AppleGFXHDAFunctionGroup"=1,"IOFramebufferUserClient"=6},"IOMalloc allocation"=314685154}
  | }
  | 
  +-o /  <class IOPlatformExpertDevice, id 0x100000114, registered, matched, active, busy 0 (13970 ms), retain 69>
    | {
    |   "IOInterruptSpecifiers" = (<0900000005000000>)
    |   "IOPolledInterface" = "SMCPolledInterface is not serializable"
    |   "system-type" = <01>
    |   "serial-number" = <48583837000000000000000000433032565635524648583837000000000000000000000000000000000000>
    |   "IOPlatformSystemSleepPolicy" = <534c505402000a0020000000200000000000000000000000050000000000000000cd97010000000040060000000000001800000018000000050000000000000000cd97010000000040060000000000001800000018000000020000000100000000cd97010000000040061000000010002040000020400000020000000800000000cd970100000000400610000000100000c0000000c00000020000000800000000cd97010000000040060000000000000880000008800000050000000000000000cd97010000000040060000000000002800000020000000050000000000000000cd97010000000050060000100000000000000000000000050000000000000000cd97010000000040060000000000000000000000000000020000000100000000cd97010000000000000000000000000000000000000000020000000000000000cd970100000000>
    |   "platform-feature" = <2000000000000000>
    |   "IOBusyInterest" = "IOCommand is not serializable"
    |   "target-type" = <"Mac">
    |   "IOInterruptControllers" = ("io-apic-0")
    |   "version" = <"1.0">
    |   "name" = <"/">
    |   "manufacturer" = <"Apple Inc.">
    |   "compatible" = <"iMacPro1,1">
    |   "product-name" = <"iMacPro1,1">
    |   "IOPlatformSerialNumber" = "C02VV5RFHX87"
    |   "clock-frequency" = <00e1f505>
    |   "board-id" = <"Mac-7BA5B2D9E42DDD94">
    |   "model" = <"iMacPro1,1">
    |   "IOGeneralInterest" = "IOCommand is not serializable"
    |   "IOPlatformUUID" = "49554A78-FD54-57B1-BF0C-C66599D3680B"
    | }
    | 
    +-o chosen  <class IOService, id 0x100000101, !registered, !matched, active, busy 0, retain 7>
    | | {
    | |   "boot-args" = <00>
    | |   "boot-uuid" = <"74C55FBE-CCB6-43E2-8A99-54BA6FB80910">
    | |   "IOScreenLockState" = <01000000>
    | |   "boot-file-path" = <04049a005c00370034004300350035004600420045002d0043004300420036002d0034003300450032002d0038004100390039002d003500340042004100360046004200380030003900310030005c00530079007300740065006d005c004c006900620072006100720079005c0043006f0072006500530065007200760069006300650073005c0062006f006f0074002e0065006600690000007fff0400>
    | |   "random-seed" = <00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000>
    | |   "booter-name" = <"boot.efi">
    | |   "boot-file" = <"System\Library\PrelinkedKernels\immutablekernel">
    | |   "booter-version" = <"version:361.37.3">
    | |   "bootroot-active" = <>
    | |   "machine-signature" = <00000000>
    | |   "IOProgressColorTheme" = 1
    | |   "boot-kernelcache-adler32" = <5cefd5f6>
    | |   "boot-signature" = <df8796a8d3325f8f12224170e32216180c83eada>
    | |   "boot-device-path" = <02010c00d041030a0000000001010600001c0101060000000316100001000000000000000000000004012a0002000000062c0100000000001e308e0e00000000f89ce96722eb6245bb06f8d04c961348020204032400f7fc74be7c0bf349914701f4042e684290f493b7b0577d448f6b22f22bb8937d7fff0400>
    | |   "name" = <"chosen">
    | | }
    | | 
    | +-o memory-map  <class IOService, id 0x100000102, !registered, !matched, active, busy 0, retain 4>
    |     {
    |       "name" = <"memory-map">
    |       "FailedCLUT" = <0050002200100000>
    |       "FailedImage" = <0060002220640000>
    |     }
    |     
    +-o efi  <class IOService, id 0x100000103, !registered, !matched, active, busy 0, retain 8>
    | | {
    | |   "firmware-revision" = <00000100>
    | |   "device-properties" = <[encoded data, 142416 characters]>
    | |   "firmware-abi" = <"EFI64">
    | |   "name" = <"efi">
    | |   "firmware-vendor" = <4100700070006c0065000000>
    | | }
    | | 
    | +-o kernel-compatibility  <class IOService, id 0x100000104, !registered, !matched, active, busy 0, retain 4>
    | |   {
    | |     "name" = <"kernel-compatibility">
    | |     "x86_64" = <4470c710>
    | |   }
    | |   
    | +-o runtime-services  <class IOService, id 0x100000105, !registered, !matched, active, busy 0, retain 4>
    | |   {
    | |     "name" = <"runtime-services">
    | |     "table" = <18ee0f4e00000000>
    | |   }
    | |   
    | +-o configuration-table  <class IOService, id 0x100000106, !registered, !matched, active, busy 0, retain 16>
    | | | {
    | | |   "name" = <"configuration-table">
    | | | }
    | | | 
    | | +-o 8868E871-E4F1-11D3-BC22-0080C73C8881  <class IOService, id 0x100000107, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "alias" = <"ACPI_20">
    | | |     "name" = <"8868E871-E4F1-11D3-BC22-0080C73C8881">
    | | |     "table" = <14e0ff4f00000000>
    | | |     "guid" = <71e86888f1e4d311bc220080c73c8881>
    | | |   }
    | | |   
    | | +-o EB9D2D30-2D88-11D3-9A16-0090273FC14D  <class IOService, id 0x100000108, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "alias" = <"ACPI">
    | | |     "name" = <"EB9D2D30-2D88-11D3-9A16-0090273FC14D">
    | | |     "table" = <00e0ff4f00000000>
    | | |     "guid" = <302d9deb882dd3119a160090273fc14d>
    | | |   }
    | | |   
    | | +-o F2FD1544-9794-4A2C-992E-E5BBCF20E394  <class IOService, id 0x100000109, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"F2FD1544-9794-4A2C-992E-E5BBCF20E394">
    | | |     "guid" = <4415fdf294972c4a992ee5bbcf20e394>
    | | |     "table" = <00901f4f00000000>
    | | |   }
    | | |   
    | | +-o EB9D2D31-2D88-11D3-9A16-0090273FC14D  <class IOService, id 0x10000010a, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"EB9D2D31-2D88-11D3-9A16-0090273FC14D">
    | | |     "guid" = <312d9deb882dd3119a160090273fc14d>
    | | |     "table" = <00b01f4f00000000>
    | | |   }
    | | |   
    | | +-o 49152E77-1ADA-4764-B7A2-7AFEFED95E8B  <class IOService, id 0x10000010b, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"49152E77-1ADA-4764-B7A2-7AFEFED95E8B">
    | | |     "guid" = <772e1549da1a6447b7a27afefed95e8b>
    | | |     "table" = <385e474d00000000>
    | | |   }
    | | |   
    | | +-o 4C19049F-4137-4DD3-9C10-8B97A83FFDFA  <class IOService, id 0x10000010c, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"4C19049F-4137-4DD3-9C10-8B97A83FFDFA">
    | | |     "guid" = <9f04194c3741d34d9c108b97a83ffdfa>
    | | |     "table" = <6029474d00000000>
    | | |   }
    | | |   
    | | +-o 7739F24C-93D7-11D4-9A3A-0090273FC14D  <class IOService, id 0x10000010d, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"7739F24C-93D7-11D4-9A3A-0090273FC14D">
    | | |     "guid" = <4cf23977d793d4119a3a0090273fc14d>
    | | |     "table" = <1810e64d00000000>
    | | |   }
    | | |   
    | | +-o 05AD34BA-6F02-4214-952E-4DA0398E2BB9  <class IOService, id 0x10000010e, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"05AD34BA-6F02-4214-952E-4DA0398E2BB9">
    | | |     "guid" = <ba34ad05026f1442952e4da0398e2bb9>
    | | |     "table" = <f831474d00000000>
    | | |   }
    | | |   
    | | +-o EE4E5898-3914-4259-9D6E-DC7BD79403CF  <class IOService, id 0x10000010f, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"EE4E5898-3914-4259-9D6E-DC7BD79403CF">
    | | |     "guid" = <98584eee143959429d6edc7bd79403cf>
    | | |     "table" = <18d8ef4d00000000>
    | | |   }
    | | |   
    | | +-o A31280AD-481E-41B6-95E8-127F4C984779  <class IOService, id 0x100000110, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"A31280AD-481E-41B6-95E8-127F4C984779">
    | | |     "guid" = <ad8012a31e48b64195e8127f4c984779>
    | | |     "table" = <98daef4d00000000>
    | | |   }
    | | |   
    | | +-o 026C0F80-22EC-11E2-AA02-3C07540E73B4  <class IOService, id 0x100000111, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"026C0F80-22EC-11E2-AA02-3C07540E73B4">
    | | |     "guid" = <800f6c02ec22e211aa023c07540e73b4>
    | | |     "table" = <0070ef4d00000000>
    | | |   }
    | | |   
    | | +-o 674ABEA3-0FE5-11E5-988E-B8E8562CBAFA  <class IOService, id 0x100000112, !registered, !matched, active, busy 0, retain 4>
    | |     {
    | |       "name" = <"674ABEA3-0FE5-11E5-988E-B8E8562CBAFA">
    | |       "guid" = <a3be4a67e50fe511988eb8e8562cbafa>
    | |       "table" = <98dbef4d00000000>
    | |     }
    | |     
    | +-o platform  <class IOService, id 0x100000113, !registered, !matched, active, busy 0, retain 7>
    |     {
    |       "SystemSerialNumber" = <"C","0","2","V","V","5","R","F","H","X","8","7">
    |       "system-id" = <88c61abb8f11f15c9473bd049ffb1f73>
    |       "StartupPowerEvents" = <0000000000000000>
    |       "board-rev" = <09>
    |       "InitialTSC" = <26486eee7a2a0000>
    |       "apple-coprocessor-version" = <00000200>
    |       "FSBFrequency" = <00105e5f00000000>
    |       "Model" = <"i","M","a","c","P","r","o","1",",","1">
    |       "DevicePathsSupported" = <01000000>
    |       "name" = <"platform">
    |       "board-id" = <"Mac-7BA5B2D9E42DDD94">
    |     }
    |     
    +-o cpus  <class IOPlatformDevice, id 0x100000129, registered, matched, active, busy 0 (0 ms), retain 42>
    | | {
    | |   "name" = <"cpus">
    | | }
    | | 
    | +-o PR00@0  <class IOACPIPlatformDevice, id 0x10000012a, registered, matched, active, busy 0 (1956 ms), retain 9>
    | |   {
    | |     "processor-lapic" = 0
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 0
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 1
    | |     "bus-frequency" = <00e1f505>
    | |     "plugin-type" = 1
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 0
    | |     "name" = <"PR00">
    | |   }
    | |   
    | +-o PR01@2  <class IOACPIPlatformDevice, id 0x10000012b, registered, matched, active, busy 0 (27 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 2
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 2
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 2
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 1
    | |     "name" = <"PR01">
    | |   }
    | |   
    | +-o PR02@4  <class IOACPIPlatformDevice, id 0x10000012c, registered, matched, active, busy 0 (30 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 4
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 4
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 3
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 2
    | |     "name" = <"PR02">
    | |   }
    | |   
    | +-o PR03@6  <class IOACPIPlatformDevice, id 0x10000012d, registered, matched, active, busy 0 (34 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 6
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 6
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 4
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 3
    | |     "name" = <"PR03">
    | |   }
    | |   
    | +-o PR04@8  <class IOACPIPlatformDevice, id 0x10000012e, registered, matched, active, busy 0 (37 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 8
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 8
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 5
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 4
    | |     "name" = <"PR04">
    | |   }
    | |   
    | +-o PR05@A  <class IOACPIPlatformDevice, id 0x10000012f, registered, matched, active, busy 0 (41 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 10
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 10
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 6
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 5
    | |     "name" = <"PR05">
    | |   }
    | |   
    | +-o PR06@C  <class IOACPIPlatformDevice, id 0x100000130, registered, matched, active, busy 0 (44 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 12
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 12
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 7
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 6
    | |     "name" = <"PR06">
    | |   }
    | |   
    | +-o PR07@E  <class IOACPIPlatformDevice, id 0x100000131, registered, matched, active, busy 0 (47 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 14
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 14
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 8
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 7
    | |     "name" = <"PR07">
    | |   }
    | |   
    | +-o PR08@1  <class IOACPIPlatformDevice, id 0x100000132, registered, matched, active, busy 0 (49 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 1
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 1
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 9
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 8
    | |     "name" = <"PR08">
    | |   }
    | |   
    | +-o PR09@3  <class IOACPIPlatformDevice, id 0x100000133, registered, matched, active, busy 0 (51 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 3
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 3
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 10
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 9
    | |     "name" = <"PR09">
    | |   }
    | |   
    | +-o PR10@5  <class IOACPIPlatformDevice, id 0x100000134, registered, matched, active, busy 0 (53 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 5
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 5
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 11
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 10
    | |     "name" = <"PR10">
    | |   }
    | |   
    | +-o PR11@7  <class IOACPIPlatformDevice, id 0x100000135, registered, matched, active, busy 0 (55 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 7
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 7
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 12
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 11
    | |     "name" = <"PR11">
    | |   }
    | |   
    | +-o PR12@9  <class IOACPIPlatformDevice, id 0x100000136, registered, matched, active, busy 0 (57 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 9
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 9
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 13
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 12
    | |     "name" = <"PR12">
    | |   }
    | |   
    | +-o PR13@B  <class IOACPIPlatformDevice, id 0x100000137, registered, matched, active, busy 0 (59 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 11
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 11
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 14
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 13
    | |     "name" = <"PR13">
    | |   }
    | |   
    | +-o PR14@D  <class IOACPIPlatformDevice, id 0x100000138, registered, matched, active, busy 0 (62 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 13
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 13
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 15
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 14
    | |     "name" = <"PR14">
    | |   }
    | |   
    | +-o PR15@F  <class IOACPIPlatformDevice, id 0x100000139, registered, matched, active, busy 0 (64 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 15
    | |     "clock-frequency" = <0020bcbe>
    | |     "processor-number" = 15
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 16
    | |     "bus-frequency" = <00e1f505>
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 15
    | |     "name" = <"PR15">
    | |   }
    | |   
    | +-o PR16  <class IOACPIPlatformDevice, id 0x10000013a, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 16
    | |     "processor-id" = 17
    | |     "name" = <"PR16">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR17  <class IOACPIPlatformDevice, id 0x10000013b, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 17
    | |     "processor-id" = 18
    | |     "name" = <"PR17">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR18  <class IOACPIPlatformDevice, id 0x10000013c, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 18
    | |     "processor-id" = 19
    | |     "name" = <"PR18">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR19  <class IOACPIPlatformDevice, id 0x10000013d, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 19
    | |     "processor-id" = 20
    | |     "name" = <"PR19">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR20  <class IOACPIPlatformDevice, id 0x10000013e, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 20
    | |     "processor-id" = 21
    | |     "name" = <"PR20">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR21  <class IOACPIPlatformDevice, id 0x10000013f, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 21
    | |     "processor-id" = 22
    | |     "name" = <"PR21">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR22  <class IOACPIPlatformDevice, id 0x100000140, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 22
    | |     "processor-id" = 23
    | |     "name" = <"PR22">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR23  <class IOACPIPlatformDevice, id 0x100000141, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 23
    | |     "processor-id" = 24
    | |     "name" = <"PR23">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR24  <class IOACPIPlatformDevice, id 0x100000142, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 24
    | |     "processor-id" = 25
    | |     "name" = <"PR24">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR25  <class IOACPIPlatformDevice, id 0x100000143, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 25
    | |     "processor-id" = 26
    | |     "name" = <"PR25">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR26  <class IOACPIPlatformDevice, id 0x100000144, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 26
    | |     "processor-id" = 27
    | |     "name" = <"PR26">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR27  <class IOACPIPlatformDevice, id 0x100000145, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 27
    | |     "processor-id" = 28
    | |     "name" = <"PR27">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR28  <class IOACPIPlatformDevice, id 0x100000146, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 28
    | |     "processor-id" = 29
    | |     "name" = <"PR28">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR29  <class IOACPIPlatformDevice, id 0x100000147, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 29
    | |     "processor-id" = 30
    | |     "name" = <"PR29">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR30  <class IOACPIPlatformDevice, id 0x100000148, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 30
    | |     "processor-id" = 31
    | |     "name" = <"PR30">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR31  <class IOACPIPlatformDevice, id 0x100000149, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 31
    | |     "processor-id" = 32
    | |     "name" = <"PR31">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR32  <class IOACPIPlatformDevice, id 0x10000014a, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 32
    | |     "processor-id" = 33
    | |     "name" = <"PR32">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR33  <class IOACPIPlatformDevice, id 0x10000014b, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 33
    | |     "processor-id" = 34
    | |     "name" = <"PR33">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR34  <class IOACPIPlatformDevice, id 0x10000014c, registered, matched, active, busy 0 (64 ms), retain 7>
    | |   {
    | |     "processor-index" = 34
    | |     "processor-id" = 35
    | |     "name" = <"PR34">
    | |     "cpu-type" = <010f>
    | |     "device_type" = <"processor">
    | |   }
    | |   
    | +-o PR35  <class IOACPIPlatformDevice, id 0x10000014d, registered, matched, active, busy 0 (64 ms), retain 7>
    |     {
    |       "processor-index" = 35
    |       "processor-id" = 36
    |       "name" = <"PR35">
    |       "cpu-type" = <010f>
    |       "device_type" = <"processor">
    |     }
    |     
    +-o memory  <class IOService, id 0x100000181, !registered, !matched, active, busy 0, retain 4>
    |   {
    |     "dimm-part-number" = <"HMA81GR7AFR8N-VK HMA81GR7AFR8N-VK HMA81GR7AFR8N-VK HMA81GR7AFR8N-VK ">
    |     "dimm-types" = <"DDR4","DDR4","DDR4","DDR4">
    |     "slot-names" = <"   ","NODE 1/CPU1_DIMM_A0","NODE 1/CPU1_DIMM_B0","NODE 1/CPU1_DIMM_C0","NODE 1/CPU1_DIMM_D0">
    |     "dimm-speeds" = <"2666 MHz","2666 MHz","2666 MHz","2666 MHz">
    |     "dimm-manufacturer" = <"Hynix","Hynix","Hynix","Hynix">
    |     "ecc-enabled" = Yes
    |     "reg" = <0200000000000000020000000000000002000000000000000200000000000000>
    |     "dimm-info" = <0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000>
    |     "dimm-serial-number" = <"079024FA","079024E8","078024F5","073024E7">
    |   }
    |   
    +-o rom@0  <class IOService, id 0x100000182, !registered, !matched, active, busy 0, retain 4>
    |   {
    |     "firmware-features" = 4254070078
    |     "vendor" = <"Apple Inc.">
    |     "fv-main-size" = 7958528
    |     "release-date" = <011b0d00>
    |     "fv-main-address" = 18446744073694253056
    |     "apple-rom-info" = <4170706c6520524f4d2056657273696f6e0a202042494f532049443a202020202020494d5031312e38385a2e303036342e4233302e313731323038313731340a20204275696c742062793a2020202020726f6f74407064623636310a2020446174653a202020202020202020467269204465632020382031373a31343a313420323031370a20205265766973696f6e3a202020202036342e33302e37322028422649290a2020524f4d2056657273696f6e3a2020303036345f4233300a20204275696c6420547970653a2020204f6666696369616c204275696c640a2020436f6d70696c65723a20202020204170706c65204c4c564d2076657273696f6e20392e302e302028636c616e672d3930302e322e3331290a00>
    |     "rom-size" = 16777216
    |   }
    |   
    +-o PCI0@0  <class IOACPIPlatformDevice, id 0x100000184, registered, matched, active, busy 0 (5700 ms), retain 65>
    | | {
    | |   "compatible" = <"PNP0A03">
    | |   "IODTPersist" = 0
    | |   "_STA" = 18446744073709551615
    | |   "IOPCIConfigured" = Yes
    | |   "acpi-address-spaces" = <02000000000000000000000000000000000000000000000000000000000000000200000000000000000000000000000003000000000000000000000000000000000000000000000000000000000000000100000000000000000000000000000000000000000000000000000000000000f70c0000000000000000000000000000f80c0000000000000000000000000000000000000000000000000000000000000100000000000000000000000000000000000000000000000010000000000000ff2f0000000000000000000000000000002000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000400c0000000000ff7f0c000000000000000000000000000040000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001fe00000000ff0f01fe00000000000000000000000000100000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000007000000000ffffff7f00000000000000000000000000000010000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000080000000ffffff3f8000000000000000000000000000004000000000000000000000000000000000000000000000000000000000>
    | |   "IODeviceMemory" = (({"address"=3320,"length"=8}))
    | |   "#size-cells" = <02000000>
    | |   "_UID" = "0"
    | |   "acpi-pci-routing-table" = <1800000000000000ffff00000000000010000000000000001800000000000000ffff04000000000010000000000000001800000001000000ffff04000000000011000000000000001800000002000000ffff04000000000012000000000000001800000003000000ffff04000000000013000000000000001800000000000000ffff05000000000010000000000000001800000001000000ffff05000000000011000000000000001800000002000000ffff05000000000012000000000000001800000003000000ffff05000000000013000000000000001800000000000000ffff08000000000010000000000000001800000001000000ffff08000000000011000000000000001800000002000000ffff08000000000012000000000000001800000003000000ffff08000000000013000000000000001800000000000000ffff1f000000000010000000000000001800000001000000ffff1f000000000011000000000000001800000002000000ffff1f000000000012000000000000001800000003000000ffff1f000000000013000000000000001800000000000000ffff1e000000000014000000000000001800000001000000ffff1e000000000015000000000000001800000002000000ffff1e000000000016000000000000001800000003000000ffff1e000000000017000000000000001800000000000000ffff1d000000000010000000000000001800000001000000ffff1d000000000011000000000000001800000002000000ffff1d000000000012000000000000001800000003000000ffff1d000000000013000000000000001800000000000000ffff1c000000000010000000000000001800000001000000ffff1c000000000011000000000000001800000002000000ffff1c000000000012000000000000001800000003000000ffff1c000000000013000000000000001800000000000000ffff1b000000000010000000000000001800000001000000ffff1b000000000011000000000000001800000002000000ffff1b000000000012000000000000001800000003000000ffff1b000000000013000000000000001800000000000000ffff19000000000015000000000000001800000001000000ffff19000000000016000000000000001800000002000000ffff19000000000017000000000000001800000000000000ffff17000000000010000000000000001800000000000000ffff16000000000010000000000000001800000001000000ffff16000000000011000000000000001800000002000000ffff16000000000012000000000000001800000003000000ffff16000000000013000000000000001800000000000000ffff15000000000010000000000000001800000001000000ffff15000000000011000000000000001800000002000000ffff15000000000012000000000000001800000003000000ffff15000000000013000000000000001800000000000000ffff14000000000010000000000000001800000001000000ffff14000000000011000000000000001800000002000000ffff14000000000012000000000000001800000003000000ffff14000000000013000000000000001800000000000000ffff1300000000001400000000000000000000000000000000000000000000000000000000000000>
    | |   "_ADR" = 0
    | |   "device-properties" = {"acpi-device"="IOACPIPlatformDevice is not serializable","acpi-path"="IOACPIPlane:/_SB/PCI0@0"}
    | |   "#address-cells" = <03000000>
    | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0"
    | |   "name" = <"PNP0A08">
    | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | }
    | | 
    | +-o MHP0@50001  <class IORegistryEntry, id 0x100000274, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/MHP0@50001"
    | |   }
    | |   
    | +-o MHP1@50001  <class IORegistryEntry, id 0x100000275, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/MHP1@50001"
    | |   }
    | |   
    | +-o URT2@190000  <class IORegistryEntry, id 0x100000292, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "uart-channel-number" = <0200000000000000>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/URT2@190000"
    | |   }
    | |   
    | +-o PDRC  <class IOACPIPlatformDevice, id 0x1000001af, registered, matched, active, busy 0 (2 ms), retain 7>
    | |   {
    | |     "_STA" = 18446744073709551615
    | |     "_UID" = "1"
    | |     "IODeviceMemory" = (({"address"=0,"length"=32768}),({"address"=0,"length"=4096}),({"address"=24576,"length"=4096}),({"address"=0,"length"=67108864}),({"address"=4244635648,"length"=25165824}),({"address"=4275175424,"length"=131072}),({"address"=4275634176,"length"=16384}),({"address"=4275326976,"length"=307200}),({"address"=4278190080,"length"=16777216}),({"address"=4276092928,"length"=1048576}))
    | |     "name" = <"PNP0C02">
    | |   }
    | |   
    | +-o PPMC@1f0002  <class IORegistryEntry, id 0x100000293, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PPMC@1f0002"
    | |   }
    | |   
    | +-o DMI0@0  <class IOPCIDevice, id 0x100000276, registered, matched, active, busy 0 (8 ms), retain 9>
    | |   {
    | |     "IOInterruptSpecifiers" = (<1000000007000000>)
    | |     "class-code" = <00000600>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "name" = <"pci8086,2020">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <20200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2020","pciclass,060000","DMI0">
    | |     "IOPCIExpressLinkCapabilities" = 8009795
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/DMI0@0"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 66
    | |     "pcidebug" = "0:0:0"
    | |     "IOName" = "pci8086,2020"
    | |     "reg" = <0000000000000000000000000000000000000000>
    | |   }
    | |   
    | +-o CB0A@4  <class IOPCIDevice, id 0x100000277, registered, matched, active, busy 0 (26 ms), retain 9>
    | |   {
    | |     "assigned-addresses" = <102000828000000000c032010000000000400000>
    | |     "IOInterruptSpecifiers" = (<1000000007000000>,<0300000000000100>)
    | |     "class-code" = <00800800>
    | |     "IODeviceMemory" = (({"address"=549775917056,"length"=16384}))
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,2021">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <21200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2021","pciclass,088000","CB0A">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/CB0A@40000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:4:0"
    | |     "IOName" = "pci8086,2021"
    | |     "reg" = <00200000000000000000000000000000000000001020000200000000000000000000000000400000>
    | |   }
    | |   
    | +-o CB0B@4,1  <class IOPCIDevice, id 0x100000278, registered, matched, active, busy 0 (40 ms), retain 9>
    | |   {
    | |     "assigned-addresses" = <1021008280000000008032010000000000400000>
    | |     "IOInterruptSpecifiers" = (<1100000007000000>,<0400000000000100>)
    | |     "class-code" = <00800800>
    | |     "IODeviceMemory" = (({"address"=549775900672,"length"=16384}))
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,2021">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <21200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2021","pciclass,088000","CB0B">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/CB0B@40001"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:4:1"
    | |     "IOName" = "pci8086,2021"
    | |     "reg" = <00210000000000000000000000000000000000001021000200000000000000000000000000400000>
    | |   }
    | |   
    | +-o CB0C@4,2  <class IOPCIDevice, id 0x100000279, registered, matched, active, busy 0 (23 ms), retain 9>
    | |   {
    | |     "assigned-addresses" = <1022008280000000004032010000000000400000>
    | |     "IOInterruptSpecifiers" = (<1200000007000000>,<0200000000000100>)
    | |     "class-code" = <00800800>
    | |     "IODeviceMemory" = (({"address"=549775884288,"length"=16384}))
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,2021">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <21200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2021","pciclass,088000","CB0C">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/CB0C@40002"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:4:2"
    | |     "IOName" = "pci8086,2021"
    | |     "reg" = <00220000000000000000000000000000000000001022000200000000000000000000000000400000>
    | |   }
    | |   
    | +-o CB0D@4,3  <class IOPCIDevice, id 0x10000027a, registered, matched, active, busy 0 (40 ms), retain 9>
    | |   {
    | |     "assigned-addresses" = <1023008280000000000032010000000000400000>
    | |     "IOInterruptSpecifiers" = (<1300000007000000>,<0700000000000100>)
    | |     "class-code" = <00800800>
    | |     "IODeviceMemory" = (({"address"=549775867904,"length"=16384}))
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,2021">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <21200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2021","pciclass,088000","CB0D">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/CB0D@40003"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:4:3"
    | |     "IOName" = "pci8086,2021"
    | |     "reg" = <00230000000000000000000000000000000000001023000200000000000000000000000000400000>
    | |   }
    | |   
    | +-o CB0E@4,4  <class IOPCIDevice, id 0x10000027b, registered, matched, active, busy 0 (38 ms), retain 9>
    | |   {
    | |     "assigned-addresses" = <102400828000000000c031010000000000400000>
    | |     "IOInterruptSpecifiers" = (<1000000007000000>,<0500000000000100>)
    | |     "class-code" = <00800800>
    | |     "IODeviceMemory" = (({"address"=549775851520,"length"=16384}))
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,2021">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <21200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2021","pciclass,088000","CB0E">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/CB0E@40004"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:4:4"
    | |     "IOName" = "pci8086,2021"
    | |     "reg" = <00240000000000000000000000000000000000001024000200000000000000000000000000400000>
    | |   }
    | |   
    | +-o CB0F@4,5  <class IOPCIDevice, id 0x10000027c, registered, matched, active, busy 0 (38 ms), retain 9>
    | |   {
    | |     "assigned-addresses" = <1025008280000000008031010000000000400000>
    | |     "IOInterruptSpecifiers" = (<1100000007000000>,<0900000000000100>)
    | |     "class-code" = <00800800>
    | |     "IODeviceMemory" = (({"address"=549775835136,"length"=16384}))
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,2021">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <21200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2021","pciclass,088000","CB0F">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/CB0F@40005"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:4:5"
    | |     "IOName" = "pci8086,2021"
    | |     "reg" = <00250000000000000000000000000000000000001025000200000000000000000000000000400000>
    | |   }
    | |   
    | +-o CB0G@4,6  <class IOPCIDevice, id 0x10000027d, registered, matched, active, busy 0 (39 ms), retain 9>
    | |   {
    | |     "assigned-addresses" = <1026008280000000004031010000000000400000>
    | |     "IOInterruptSpecifiers" = (<1200000007000000>,<0600000000000100>)
    | |     "class-code" = <00800800>
    | |     "IODeviceMemory" = (({"address"=549775818752,"length"=16384}))
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,2021">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <21200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2021","pciclass,088000","CB0G">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/CB0G@40006"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:4:6"
    | |     "IOName" = "pci8086,2021"
    | |     "reg" = <00260000000000000000000000000000000000001026000200000000000000000000000000400000>
    | |   }
    | |   
    | +-o CB0H@4,7  <class IOPCIDevice, id 0x10000027e, registered, matched, active, busy 0 (38 ms), retain 9>
    | |   {
    | |     "assigned-addresses" = <1027008280000000000031010000000000400000>
    | |     "IOInterruptSpecifiers" = (<1300000007000000>,<0800000000000100>)
    | |     "class-code" = <00800800>
    | |     "IODeviceMemory" = (({"address"=549775802368,"length"=16384}))
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,2021">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <21200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2021","pciclass,088000","CB0H">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/CB0H@40007"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:4:7"
    | |     "IOName" = "pci8086,2021"
    | |     "reg" = <00270000000000000000000000000000000000001027000200000000000000000000000000400000>
    | |   }
    | |   
    | +-o IIM0@5  <class IOPCIDevice, id 0x10000027f, registered, matched, active, busy 0 (38 ms), retain 9>
    | |   {
    | |     "class-code" = <00800800>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "name" = <"pci8086,2024">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <24200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2024","pciclass,088000","IIM0">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IIM0@50000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:5:0"
    | |     "IOName" = "pci8086,2024"
    | |     "reg" = <0028000000000000000000000000000000000000>
    | |   }
    | |   
    | +-o pci8086,2025@5,2  <class IOPCIDevice, id 0x100000352, registered, matched, active, busy 0 (36 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,2025","pciclass,088000">
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOName" = "pci8086,2025"
    | |     "reg" = <002a000000000000000000000000000000000000>
    | |     "device-id" = <25200000>
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 146
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:5:2"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2025">
    | |   }
    | |   
    | +-o pci8086,2026@5,4  <class IOPCIDevice, id 0x100000353, registered, matched, active, busy 0 (35 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,2026","pciclass,080020">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2026"
    | |     "reg" = <002c000000000000000000000000000000000000102c000200000000000000000000000000100000>
    | |     "device-id" = <26200000>
    | |     "assigned-addresses" = <102c00820000000000c000740000000000100000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIExpressCapabilities" = 145
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "IODeviceMemory" = (({"address"=1946206208,"length"=4096}))
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:5:4"
    | |     "class-code" = <20000800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "subsystem-id" = <26200000>
    | |     "name" = <"pci8086,2026">
    | |   }
    | |   
    | +-o UBX0@8  <class IOPCIDevice, id 0x100000280, registered, matched, active, busy 0 (34 ms), retain 9>
    | |   {
    | |     "class-code" = <00800800>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "name" = <"pci8086,2014">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <14200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2014","pciclass,088000","UBX0">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/UBX0@80000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "0:8:0"
    | |     "IOName" = "pci8086,2014"
    | |     "reg" = <0040000000000000000000000000000000000000>
    | |   }
    | |   
    | +-o pci8086,2015@8,1  <class IOPCIDevice, id 0x100000354, registered, matched, active, busy 0 (32 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2015","pciclass,110100">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2015"
    | |     "reg" = <0041000000000000000000000000000000000000>
    | |     "device-id" = <15200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:8:1"
    | |     "class-code" = <00011100>
    | |     "name" = <"pci8086,2015">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2016@8,2  <class IOPCIDevice, id 0x100000355, registered, matched, active, busy 0 (31 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2016","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2016"
    | |     "reg" = <0042000000000000000000000000000000000000>
    | |     "device-id" = <16200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 146
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:8:2"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2016">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o XHC1@14  <class IOPCIDevice, id 0x100000294, registered, matched, active, busy 0 (1357 ms), retain 15>
    | | | {
    | | |   "assigned-addresses" = <10a0008280000000000030010000000000000100>
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>,<0a00000000000100>)
    | | |   "IODeviceMemory" = (({"address"=549775736832,"length"=65536}))
    | | |   "class-code" = <30030c00>
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <86800000>
    | | |   "built-in" = <00>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOPCIMSIMode" = Yes
    | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | |   "name" = <"pci8086,a2af">
    | | |   "vendor-id" = <86800000>
    | | |   "acpi-pmcap-offset" = 112
    | | |   "device-id" = <afa20000>
    | | |   "IOPCIResourced" = Yes
    | | |   "compatible" = <"pci8086,7270","pci8086,a2af","pciclass,0c0330","XHC1">
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/XHC1@140000"
    | | |   "subsystem-id" = <70720000>
    | | |   "revision-id" = <00000000>
    | | |   "pcidebug" = "0:20:0"
    | | |   "IOName" = "pci8086,a2af"
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="XHC1 1"})
    | | |   "reg" = <00a000000000000000000000000000000000000010a0000200000000000000000000000000000100>
    | | | }
    | | | 
    | | +-o @2:0  <class IOMedia, id 0x10000469f, registered, matched, active, busy 0 (60 ms), retain 11>
    | | |   {
    | | |     "Removable" = Yes
    | | |     "Content" = "GUID_partition_scheme"
    | | |     "Whole" = Yes
    | | |     "Leaf" = No
    | | |     "BSD Name" = "disk2"
    | | |     "Ejectable" = Yes
    | | |     "Preferred Block Size" = 512
    | | |     "IOMediaIcon" = {"IOBundleResourceFile"="Removable.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | | |     "BSD Minor" = 8
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "Writable" = Yes
    | | |     "BSD Major" = 1
    | | |     "Size" = 15552479232
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "Open" = Yes
    | | |     "Content Hint" = ""
    | | |     "BSD Unit" = 2
    | | |   }
    | | |   
    | | +-o @2:1  <class IOMedia, id 0x1000046a5, registered, matched, active, busy 0 (1 ms), retain 9>
    | | |   {
    | | |     "Open" = No
    | | |     "Preferred Block Size" = 512
    | | |     "Base" = 20480
    | | |     "Writable" = Yes
    | | |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     "BSD Minor" = 9
    | | |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |     "Size" = 209715200
    | | |     "Whole" = No
    | | |     "Removable" = Yes
    | | |     "UUID" = "199E3375-262E-451C-B918-C6C4E00E81A6"
    | | |     "BSD Unit" = 2
    | | |     "BSD Major" = 1
    | | |     "BSD Name" = "disk2s1"
    | | |     "Ejectable" = Yes
    | | |     "Partition ID" = 1
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "GPT Attributes" = 0
    | | |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |     "Leaf" = Yes
    | | |   }
    | | |   
    | | +-o @2:2  <class IOMedia, id 0x1000046a6, registered, matched, active, busy 0 (1 ms), retain 10>
    | |     {
    | |       "Open" = Yes
    | |       "Preferred Block Size" = 512
    | |       "Base" = 209735680
    | |       "Writable" = Yes
    | |       "IOBusyInterest" = "IOCommand is not serializable"
    | |       "BSD Minor" = 10
    | |       "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | |       "Size" = 15208505344
    | |       "Whole" = No
    | |       "Removable" = Yes
    | |       "UUID" = "DE9F64FE-9013-454D-98D9-1326EA6DD825"
    | |       "BSD Unit" = 2
    | |       "BSD Major" = 1
    | |       "BSD Name" = "disk2s2"
    | |       "Ejectable" = Yes
    | |       "Partition ID" = 2
    | |       "IOGeneralInterest" = "IOCommand is not serializable"
    | |       "GPT Attributes" = 0
    | |       "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | |       "Leaf" = Yes
    | |     }
    | |     
    | +-o IMEI@16  <class IOPCIDevice, id 0x100000281, registered, matched, active, busy 0 (27 ms), retain 9>
    | |   {
    | |     "assigned-addresses" = <10b0008280000000002033010000000000100000>
    | |     "IOInterruptSpecifiers" = (<1000000007000000>,<0b00000000000100>)
    | |     "IODeviceMemory" = (({"address"=549775941632,"length"=4096}))
    | |     "class-code" = <00800700>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     "name" = <"pci8086,a2ba">
    | |     "vendor-id" = <86800000>
    | |     "acpi-pmcap-offset" = 80
    | |     "device-id" = <baa20000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,7270","pci8086,a2ba","pciclass,078000","IMEI">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/IMEI@160000"
    | |     "subsystem-id" = <70720000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:22:0"
    | |     "IOName" = "pci8086,a2ba"
    | |     "reg" = <00b000000000000000000000000000000000000010b0000200000000000000000000000000100000>
    | |   }
    | |   
    | +-o RP17@1B  <class IOPCIDevice, id 0x100000287, registered, matched, active, busy 0 (3569 ms), retain 12>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 328
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 3
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <eba20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci8086,a2eb","pciclass,060400","RP17">
    | | |   "ranges" = <0000008200000000000040740000008200000000000040740000000000005000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 359812113
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP17@1b0000"
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 28689
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:27:0(1:1)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00d8000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 10793472
    | | | }
    | | | 
    | | +-o ARPT@0  <class IOPCIDevice, id 0x100000288, registered, matched, active, busy 0 (3433 ms), retain 16>
    | |     {
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "built-in" = <00>
    | |       "wlan.tx.ring.size" = 512
    | |       "bcom.oscar.profilestates" = <0000000200200022090d0000>
    | |       "bcom.roam.profiles" = <0c00f6ffb5ff0200b80bb4000200b0041400bfff32001000b5ff80ff02005a001e0001001e000c00bfff3200000000000000000000000000000000000000000000001000b5ff80ff02005a001e0001001e000c0080ff0a0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001400b5ff80ff02005a001e000200b4000c00bfff320000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001400b5ff80ff02005a001e000200b4000c0080ff0a0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000c00f6ffb5ff0200b80bb4000200b0041400bfff32001000b5ff80ff02005a001e000200b4000c00bfff3200000000000000000000000000000000000000000000001000b5ff80ff02005a001e000200b4000c0080ff0a0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000c00f6ffceff0200b004b400020058021400c4ff32000c00ceffbaff0200b004b400020068010f00c4ff32001000baff80ff02005a001e0001001e000c00c4ff32001000baff80ff02005a001e0001001e000c0080ff0a000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000>
    | |       "wlan.awdl.params" = <0000000000000000>
    | |       "wlan.tethering.enabled" = <01000000>
    | |       "IODeviceMemory" = (({"address"=1954545664,"length"=32768}),({"address"=1950351360,"length"=4194304}))
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP17@1b0000/ARPT@0"
    | |       "wlan.listen.interval" = <0a000000>
    | |       "local-mac-address" = <8c859087f4ba>
    | |       "wlan.enhancedlocale.enabled" = <00000000>
    | |       "pci-aspm-default" = 259
    | |       "reg" = <000001000000000000000000000000000000000010000102000000000000000000000000008000001800010200000000000000000000000000004000>
    | |       "acpi-pmcap-offset" = 72
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="ARPT 1"})
    | |       "bcom.btc.params" = <060000000f00000008000000c8af000009000000983a00000a000000204e0000>
    | |       "IOName" = "pci14e4,4464"
    | |       "wlan.autocountry.enabled" = <00000000>
    | |       "wlan.bss.5GHz-preference" = <bfff1e00>
    | |       "IOPCIExpressLinkCapabilities" = 4643857
    | |       "IOChildIndex" = 1
    | |       "wlan.wnm.enabled" = <00000000>
    | |       "wlan.fast_enterprise_nw.enabled" = <00000000>
    | |       "bcom.ps.realtime" = <0300c80000000100a00f0000>
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "bcom.wow.magic-packet" = No
    | |       "bcom.roam.default" = <01005a001e00070002000000b5ff1400b5ff0a00>
    | |       "wlan.vo.blockack" = Yes
    | |       "wlan.dfsproxy.enabled" = <0000000000000000>
    | |       "class-code" = <00800200>
    | |       "WiFiCapability" = {"awdl"=Yes,"ranging"=Yes}
    | |       "IOPCIResourced" = Yes
    | |       "wlan.ocl.enabled" = <>
    | |       "name" = <"pci14e4,4464">
    | |       "module-instance" = "ekans"
    | |       "IOReportLegendPublic" = Yes
    | |       "IOInterruptSpecifiers" = (<1000000007000000>,<0e00000000000100>)
    | |       "compatible" = <"pci106b,7bf","pci14e4,4464","pciclass,028000","ARPT">
    | |       "wlan.enhancedTrgDisc" = <00000000>
    | |       "revision-id" = <03000000>
    | |       "wlan.rx.ring.size" = 512
    | |       "SROM" = <[encoded data, 4096 characters]>
    | |       "IOPCIMSIMode" = Yes
    | |       "subsystem-vendor-id" = <6b100000>
    | |       "assigned-addresses" = <10000182000000000000807400000000008000001800018200000000000040740000000000004000>
    | |       "device-id" = <64440000>
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "wlan.sdb.profile" = <>
    | |       "wlan.mimo_ps.enabled" = <>
    | |       "bcom.roam.enterprise" = <01005a001e00070002000000baff0c00baff0c00>
    | |       "pcidebug" = "1:0:0"
    | |       "IOPCIExpressCapabilities" = 2
    | |       "bcom.ps.default" = <0300c80000000100a00f0000>
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "subsystem-id" = <bf070000>
    | |       "wlan.dfrts" = <>
    | |       "vendor-id" = <e4140000>
    | |       "wifi-module-sn" = <f20008ed30ba>
    | |       "acpi-wake-type" = 2
    | |       "wlan.voice_enterprise_nw.enabled" = <00000000>
    | |       "bcom.roam.enabledenhanced" = <00000000>
    | |     }
    | |     
    | +-o RP01@1C  <class IOPCIDevice, id 0x100000282, registered, matched, active, busy 0 (2528 ms), retain 15>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 64
    | | |   "subsystem-vendor-id" = <80000000>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "built-in" = <00>
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "name" = <"pci-bridge">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <94a20000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci80,0","pci8086,a294","pciclass,060400","RP01">
    | | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c28000000000000000000000c2800000000000000000000000000030010000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 91373635
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000"
    | | |   "subsystem-id" = <00000000>
    | | |   "revision-id" = <f0000000>
    | | |   "IOPCIExpressLinkStatus" = 61507
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:28:0(2:2)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e0000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 2424064
    | | | }
    | | | 
    | | +-o ANS2@0  <class IOPCIDevice, id 0x100000283, registered, matched, active, busy 0 (419 ms), retain 16>
    | | | | {
    | | | |   "assigned-addresses" = <100002c280000000000000000000000000004000180002c280000000000000010000000000000800200002c280000000000020010000000000000100>
    | | | |   "IOInterruptSpecifiers" = (<1600000000000100>)
    | | | |   "class-code" = <02800100>
    | | | |   "IODeviceMemory" = (({"address"=549755813888,"length"=4194304}),({"address"=549772591104,"length"=524288}),({"address"=549774688256,"length"=65536}))
    | | | |   "IOReportLegendPublic" = Yes
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | | |   "subsystem-vendor-id" = <6b100000>
    | | | |   "built-in" = <00>
    | | | |   "pci-aspm-default" = 256
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "IOPCIMSIMode" = Yes
    | | | |   "IOInterruptControllers" = ("IOPCIMessagedInterruptController")
    | | | |   "name" = <"pci106b,2005">
    | | | |   "IOChildIndex" = 1
    | | | |   "device-id" = <05200000>
    | | | |   "vendor-id" = <6b100000>
    | | | |   "acpi-pmcap-offset" = 64
    | | | |   "IOPCIResourced" = Yes
    | | | |   "compatible" = <"pci106b,1800","pci106b,2005","pciclass,018002","ANS2">
    | | | |   "IOPCIExpressLinkCapabilities" = 4683843
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/ANS2@0"
    | | | |   "subsystem-id" = <00180000>
    | | | |   "revision-id" = <01000000>
    | | | |   "IOPCIExpressLinkStatus" = 4163
    | | | |   "IOPCIExpressCapabilities" = 2
    | | | |   "pcidebug" = "2:0:0"
    | | | |   "IOName" = "pci106b,2005"
    | | | |   "pci-functions-dependent" = <0100000000000000>
    | | | |   "reg" = <0000020000000000000000000000000000000000100002420000000000000000000000000000400018000242000000000000000000000000000008002000024200000000000000000000000000000100>
    | | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="ANS2 0"})
    | | | | }
    | | | | 
    | | | +-o AppleANS2Controller  <class AppleANS2Controller, id 0x100000451, registered, matched, active, busy 0 (380 ms), retain 10>
    | | |   | {
    | | |   |   "IOClass" = "AppleANS2Controller"
    | | |   |   "IOPolledInterface" = "IONVMeControllerPolledAdapter is not serializable"
    | | |   |   "IOMaximumSegmentByteCountRead" = 4096
    | | |   |   "IOPlatformPanicAction" = 0
    | | |   |   "IOReportLegendPublic" = Yes
    | | |   |   "IOCommandPoolSize" = 128
    | | |   |   "IOProviderClass" = "IOPCIDevice"
    | | |   |   "Physical Interconnect Location" = "Internal"
    | | |   |   "IOMaximumSegmentByteCountWrite" = 4096
    | | |   |   "IOMaximumSegmentCountRead" = 256
    | | |   |   "Model Number" = "APPLE SSD AP1024M"
    | | |   |   "AppleEffaceableRegistryID" = 4294968444
    | | |   |   "IOProbeScore" = 0
    | | |   |   "IOMaximumSegmentCountWrite" = 256
    | | |   |   "IOMinimumSaturationByteCount" = 8388608
    | | |   |   "NVMe Revision Supported" = "1.10"
    | | |   |   "IOPCIPauseCompatible" = Yes
    | | |   |   "IONameMatch" = ("ANS2")
    | | |   |   "Serial Number" = "C0274830281J803AG"
    | | |   |   "IOPowerManagement" = {"DevicePowerState"=3,"CapabilityFlags"=32768,"CurrentPowerState"=3,"MaxPowerState"=3}
    | | |   |   "Physical Interconnect" = "PCI-Express"
    | | |   |   "Chipset Name" = "SSD Controller"
    | | |   |   "Controller Characteristics" = {"Preferred IO Size"=1048576,"Encryption Type"="AES-XTS"}
    | | |   |   "IOMatchCategory" = "IODefaultMatchCategory"
    | | |   |   "CFBundleIdentifier" = "com.apple.iokit.IONVMeFamily"
    | | |   |   "Vendor Name" = "Apple"
    | | |   |   "IONameMatched" = "ANS2"
    | | |   |   "IOMinimumSegmentAlignmentByteCount" = 4
    | | |   |   "Firmware Revision" = "114.37.2"
    | | |   |   "IOPCITunnelCompatible" = Yes
    | | |   |   "IOReportLegend" = ({"IOReportChannels"=((5644784279684675442,17180000258,"NVMe Power States")),"IOReportGroupName"="NVMe","IOReportChannelInfo"={"IOReportChannelUnit"=72058100844068865}})
    | | |   |   "IOUnitName" = "disk"
    | | |   | }
    | | |   | 
    | | |   +-o IONVMeBlockStorageDevice@1  <class IONVMeBlockStorageDevice, id 0x10000048b, registered, matched, active, busy 0 (380 ms), retain 11>
    | | |     | {
    | | |     |   "IOCFPlugInTypes" = {"AA0FA6F9-C2D6-457F-B10B-59A13253292F"="NVMeSMARTLib.plugin"}
    | | |     |   "NamespaceUUID" = 0
    | | |     |   "Logical Block Size" = 4096
    | | |     |   "NamespaceID" = 1
    | | |     |   "IOUnit" = 1
    | | |     |   "ThermalThrottlingSupported" = Yes
    | | |     |   "IOReportLegend" = ({"IOReportGroupName"="NVMe","IOReportChannels"=((6082504312848663127,6442450945,"Tier0 BW Scale Factor"),(6082504312865440343,6442450945,"Tier1 BW Scale Factor"),(6082504312882217559,6442450945,"Tier2 BW Scale Factor"),(6082504312898994775,6442450945,"Tier3 BW Scale Factor")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="BW Limits"},{"IOReportGroupName"="NVMe","IOReportChannels"=((6084209303804800357,6442450945,"Total time elapsed"),(6082504312848654368,6442450945,"Tier0 Throttle Time"),(6082504312865431584,6442450945,"Tier1 Throttle Time"),(6082504312882208800,6442450945,"Tier2 Throttle Time"),(6082504312898986016,6442450945,"Tier3 Throttle Time")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="Time weighted throttle statistics"})
    | | |     |   "device-type" = "Generic"
    | | |     |   "IOReportLegendPublic" = Yes
    | | |     |   "Physical Block Size" = 4096
    | | |     |   "Protocol Characteristics" = {"Physical Interconnect"="PCI-Express","Physical Interconnect Location"="Internal"}
    | | |     |   "Device Characteristics" = {"Serial Number"="C0274830281J803AG","Medium Type"="Solid State","Product Name"="APPLE SSD AP1024M","Vendor Name"="","Product Revision Level"="114.37.2"}
    | | |     |   "IOStorageFeatures" = {"Unmap"=Yes,"Priority"=Yes,"Barrier"=Yes}
    | | |     |   "NVMe SMART Capable" = Yes
    | | |     | }
    | | |     | 
    | | |     +-o @1:0  <class IOMedia, id 0x10000048d, registered, matched, active, busy 0 (379 ms), retain 11>
    | | |     |   {
    | | |     |     "Removable" = No
    | | |     |     "Content" = "GUID_partition_scheme"
    | | |     |     "Whole" = Yes
    | | |     |     "Leaf" = No
    | | |     |     "BSD Name" = "disk0"
    | | |     |     "Ejectable" = No
    | | |     |     "Preferred Block Size" = 4096
    | | |     |     "IOMediaIcon" = {"IOBundleResourceFile"="Internal.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | | |     |     "BSD Minor" = 0
    | | |     |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     |     "Writable" = Yes
    | | |     |     "BSD Major" = 1
    | | |     |     "Size" = 1000555581440
    | | |     |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     |     "Open" = Yes
    | | |     |     "Content Hint" = ""
    | | |     |     "BSD Unit" = 0
    | | |     |   }
    | | |     |   
    | | |     +-o @1:1  <class IOMedia, id 0x1000004c7, registered, matched, active, busy 0 (4 ms), retain 9>
    | | |     |   {
    | | |     |     "Open" = No
    | | |     |     "Preferred Block Size" = 4096
    | | |     |     "Base" = 24576
    | | |     |     "Writable" = Yes
    | | |     |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |     |     "BSD Minor" = 1
    | | |     |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |     |     "Size" = 314572800
    | | |     |     "Whole" = No
    | | |     |     "Removable" = No
    | | |     |     "UUID" = "E00F0FD5-9EE8-43F3-BDEE-7C9C200A00A8"
    | | |     |     "BSD Unit" = 0
    | | |     |     "BSD Major" = 1
    | | |     |     "BSD Name" = "disk0s1"
    | | |     |     "Ejectable" = No
    | | |     |     "Partition ID" = 1
    | | |     |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     |     "GPT Attributes" = 0
    | | |     |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |     |     "Leaf" = Yes
    | | |     |   }
    | | |     |   
    | | |     +-o @1:2  <class IOMedia, id 0x1000004c8, registered, matched, active, busy 0 (31 ms), retain 11>
    | | |         {
    | | |           "Open" = Yes
    | | |           "Preferred Block Size" = 4096
    | | |           "Base" = 314597376
    | | |           "Writable" = Yes
    | | |           "IOBusyInterest" = "IOCommand is not serializable"
    | | |           "BSD Minor" = 2
    | | |           "Content" = "7C3457EF-0000-11AA-AA11-00306543ECAC"
    | | |           "Size" = 1000240963584
    | | |           "Whole" = No
    | | |           "Removable" = No
    | | |           "UUID" = "67E99CF8-EB22-4562-BB06-F8D04C961348"
    | | |           "BSD Unit" = 0
    | | |           "BSD Major" = 1
    | | |           "BSD Name" = "disk0s2"
    | | |           "Ejectable" = No
    | | |           "Partition ID" = 2
    | | |           "IOGeneralInterest" = "IOCommand is not serializable"
    | | |           "GPT Attributes" = 0
    | | |           "Content Hint" = "7C3457EF-0000-11AA-AA11-00306543ECAC"
    | | |           "Leaf" = No
    | | |           "TierType" = "Main"
    | | |         }
    | | |         
    | | +-o IOBC@0,1  <class IOPCIDevice, id 0x100000284, registered, matched, active, busy 0 (1266 ms), retain 11>
    | | |   {
    | | |     "assigned-addresses" = <100102c280000000000040000000000000004000180102c280000000000008010000000000000800200102c280000000000021010000000000000100>
    | | |     "IOInterruptSpecifiers" = (<1800000000000100>,<1900000000000100>,<1a00000000000100>,<1b00000000000100>,<1c00000000000100>,<1d00000000000100>,<1e00000000000100>,<1f00000000000100>)
    | | |     "class-code" = <00000000>
    | | |     "IODeviceMemory" = (({"address"=549760008192,"length"=4194304}),({"address"=549773115392,"length"=524288}),({"address"=549774753792,"length"=65536}))
    | | |     "IOReportLegendPublic" = Yes
    | | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |     "subsystem-vendor-id" = <6b100000>
    | | |     "built-in" = <00>
    | | |     "pci-aspm-default" = 256
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "IOPCIMSIMode" = Yes
    | | |     "IOInterruptControllers" = ("IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController")
    | | |     "name" = <"pci106b,1801">
    | | |     "IOChildIndex" = 2
    | | |     "device-id" = <01180000>
    | | |     "vendor-id" = <6b100000>
    | | |     "acpi-pmcap-offset" = 64
    | | |     "pci-msi-flags" = <0100000000000000>
    | | |     "compatible" = <"pci106b,1801","pciclass,000000","IOBC">
    | | |     "IOPCIResourced" = Yes
    | | |     "IOPCIExpressLinkCapabilities" = 4683843
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/IOBC@1"
    | | |     "subsystem-id" = <01180000>
    | | |     "revision-id" = <01000000>
    | | |     "IOPCIExpressLinkStatus" = 4163
    | | |     "IOPCIExpressCapabilities" = 2
    | | |     "pcidebug" = "2:0:1"
    | | |     "IOName" = "pci106b,1801"
    | | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="IOBC 0"},{"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182267392,4295098369,"               First Level Interrupt Handler Count"),(5291294645182267393,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182267394,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182267395,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182267396,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="IOBC 4"})
    | | |     "reg" = <0001020000000000000000000000000000000000100102420000000000000000000000000000400018010242000000000000000000000000000008002001024200000000000000000000000000000100>
    | | |   }
    | | |   
    | | +-o SEPM@0,2  <class IOPCIDevice, id 0x100000285, registered, matched, active, busy 0 (11 ms), retain 11>
    | | |   {
    | | |     "assigned-addresses" = <100202c280000000000080000000000000004000180202c280000000000010010000000000000800200202c280000000000022010000000000000100>
    | | |     "IOInterruptSpecifiers" = (<2000000000000100>,<2100000000000100>,<2200000000000100>,<2300000000000100>,<2400000000000100>,<2500000000000100>,<2600000000000100>,<2700000000000100>)
    | | |     "class-code" = <00000000>
    | | |     "IODeviceMemory" = (({"address"=549764202496,"length"=4194304}),({"address"=549773639680,"length"=524288}),({"address"=549774819328,"length"=65536}))
    | | |     "IOReportLegendPublic" = Yes
    | | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |     "subsystem-vendor-id" = <6b100000>
    | | |     "built-in" = <00>
    | | |     "pci-aspm-default" = 256
    | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |     "IOPCIMSIMode" = Yes
    | | |     "IOInterruptControllers" = ("IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController","IOPCIMessagedInterruptController")
    | | |     "name" = <"pci106b,1802">
    | | |     "IOChildIndex" = 3
    | | |     "device-id" = <02180000>
    | | |     "vendor-id" = <6b100000>
    | | |     "acpi-pmcap-offset" = 64
    | | |     "pci-msi-flags" = <0100000000000000>
    | | |     "compatible" = <"pci106b,1802","pciclass,000000","SEPM">
    | | |     "IOPCIResourced" = Yes
    | | |     "IOPCIExpressLinkCapabilities" = 4683843
    | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/SEPM@2"
    | | |     "subsystem-id" = <02180000>
    | | |     "revision-id" = <01000000>
    | | |     "IOPCIExpressLinkStatus" = 4163
    | | |     "IOPCIExpressCapabilities" = 2
    | | |     "pcidebug" = "2:0:2"
    | | |     "IOName" = "pci106b,1802"
    | | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="SEPM 0"},{"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="SEPM 1"})
    | | |     "reg" = <0002020000000000000000000000000000000000100202420000000000000000000000000000400018020242000000000000000000000000000008002002024200000000000000000000000000000100>
    | | |   }
    | | |   
    | | +-o ADIO@0,3  <class IOPCIDevice, id 0x100000286, registered, matched, active, busy 0 (1519 ms), retain 11>
    | |     {
    | |       "assigned-addresses" = <100302c2800000000000c0000000000000004000180302c280000000000018010000000000000800200302c280000000000023010000000000000100>
    | |       "IOInterruptSpecifiers" = (<1700000000000100>)
    | |       "class-code" = <00010400>
    | |       "IODeviceMemory" = (({"address"=549768396800,"length"=4194304}),({"address"=549774163968,"length"=524288}),({"address"=549774884864,"length"=65536}))
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "subsystem-vendor-id" = <6b100000>
    | |       "built-in" = <00>
    | |       "pci-aspm-default" = 256
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "IOInterruptControllers" = ("IOPCIMessagedInterruptController")
    | |       "name" = <"pci106b,1803">
    | |       "IOChildIndex" = 4
    | |       "device-id" = <03180000>
    | |       "vendor-id" = <6b100000>
    | |       "acpi-pmcap-offset" = 64
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci106b,1803","pciclass,040100","ADIO">
    | |       "IOPCIExpressLinkCapabilities" = 4683843
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/ADIO@3"
    | |       "subsystem-id" = <03180000>
    | |       "revision-id" = <01000000>
    | |       "IOPCIExpressLinkStatus" = 4163
    | |       "IOPCIExpressCapabilities" = 2
    | |       "pcidebug" = "2:0:3"
    | |       "IOName" = "pci106b,1803"
    | |       "reg" = <0003020000000000000000000000000000000000100302420000000000000000000000000000400018030242000000000000000000000000000008002003024200000000000000000000000000000100>
    | |     }
    | |     
    | +-o URT0@1E  <class IOPCIDevice, id 0x10000028e, registered, matched, active, busy 0 (945 ms), retain 12>
    | | | {
    | | |   "assigned-addresses" = <10f0008280000000001033010000000000100000>
    | | |   "IOInterruptSpecifiers" = (<1400000007000000>)
    | | |   "class-code" = <00801100>
    | | |   "uart-channel-number" = <0000000000000000>
    | | |   "IODeviceMemory" = (({"address"=549775937536,"length"=4096}))
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <86800000>
    | | |   "built-in" = <00>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "name" = <"pci8086,a2a7">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <a7a20000>
    | | |   "IOPCIResourced" = Yes
    | | |   "compatible" = <"pci8086,7270","pci8086,a2a7","pciclass,118000","URT0">
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/URT0@1e0000"
    | | |   "subsystem-id" = <70720000>
    | | |   "revision-id" = <00000000>
    | | |   "pcidebug" = "0:30:0"
    | | |   "IOName" = "pci8086,a2a7"
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="URT0 0"})
    | | |   "reg" = <00f000000000000000000000000000000000000010f0000200000000000000000000000000100000>
    | | | }
    | | | 
    | | +-o BLTH@0  <class AppleSimpleUARTSync, id 0x10000028f, registered, matched, active, busy 0 (1 ms), retain 9>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "IOTTYBaseName" = "BLTH"
    | |       "serial state" = 18446744073246867559
    | |       "parity" = <0000000000000000>
    | |       "compatible" = <"apple-uart-blth">
    | |       "baud" = <c0c62d0000000000>
    | |       "serial parity" = 1
    | |       "serial baud rate" = 6000000
    | |       "HiddenPort" = Yes
    | |       "stopBits" = <0100000000000000>
    | |       "serial data width" = 16
    | |       "serial flow control" = 36
    | |       "IOTTYSuffix" = ""
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/URT0@1e0000/BLTH@0"
    | |       "serial stop bits" = 2
    | |       "dataBits" = <0800000000000000>
    | |     }
    | |     
    | +-o URT1@1E,1  <class IOPCIDevice, id 0x100000290, registered, matched, active, busy 0 (1103 ms), retain 12>
    | | | {
    | | |   "assigned-addresses" = <10f1008280000000000033010000000000100000>
    | | |   "IOInterruptSpecifiers" = (<1500000007000000>)
    | | |   "class-code" = <00801100>
    | | |   "uart-channel-number" = <0100000000000000>
    | | |   "IODeviceMemory" = (({"address"=549775933440,"length"=4096}))
    | | |   "IOReportLegendPublic" = Yes
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <86800000>
    | | |   "built-in" = <00>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "name" = <"pci8086,a2a8">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <a8a20000>
    | | |   "IOPCIResourced" = Yes
    | | |   "compatible" = <"pci8086,7270","pci8086,a2a8","pciclass,118000","URT1">
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/URT1@1e0001"
    | | |   "subsystem-id" = <70720000>
    | | |   "revision-id" = <00000000>
    | | |   "pcidebug" = "0:30:1"
    | | |   "IOName" = "pci8086,a2a8"
    | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="URT1 0"})
    | | |   "reg" = <00f100000000000000000000000000000000000010f1000200000000000000000000000000100000>
    | | | }
    | | | 
    | | +-o ARPT@0  <class AppleSimpleUARTSync, id 0x100000291, registered, matched, active, busy 0 (164 ms), retain 11>
    | |     {
    | |       "IOTTYBaseName" = "ARPT"
    | |       "serial state" = 18446744073179758695
    | |       "compatible" = <"wlan">
    | |       "serial parity" = 1
    | |       "serial baud rate" = 6000000
    | |       "serial flow control" = 0
    | |       "HiddenPort" = Yes
    | |       "serial data width" = 16
    | |       "IOTTYSuffix" = ""
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/URT1@1e0001/ARPT@0"
    | |       "serial stop bits" = 2
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     }
    | |     
    | +-o LPCB@1F  <class IOPCIDevice, id 0x100000289, registered, matched, active, busy 0 (121 ms), retain 19>
    | | | {
    | | |   "name" = <"pci8086,a2d4">
    | | |   "compatible" = <"pci8086,7270","pci8086,a2d4","pciclass,060100","LPCB">
    | | |   "subsystem-vendor-id" = <86800000>
    | | |   "IOName" = "pci8086,a2d4"
    | | |   "reg" = <00f8000000000000000000000000000000000000>
    | | |   "device-id" = <d4a20000>
    | | |   "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "IOPCIResourced" = Yes
    | | |   "revision-id" = <00000000>
    | | |   "vendor-id" = <86800000>
    | | |   "pcidebug" = "0:31:0"
    | | |   "class-code" = <00010600>
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/LPCB@1f0000"
    | | |   "subsystem-id" = <70720000>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | }
    | | | 
    | | +-o DMAC  <class IOACPIPlatformDevice, id 0x10000019c, registered, matched, active, busy 0 (1 ms), retain 7>
    | | |   {
    | | |     "name" = <"PNP0200">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=0,"length"=32}),({"address"=129,"length"=17}),({"address"=147,"length"=13}),({"address"=192,"length"=32}))
    | | |   }
    | | |   
    | | +-o FWHD  <class IOACPIPlatformDevice, id 0x10000019d, registered, matched, active, busy 0 (1 ms), retain 7>
    | | |   {
    | | |     "name" = <"INT0800">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=4278190080,"length"=16777216}))
    | | |   }
    | | |   
    | | +-o IPIC  <class IOACPIPlatformDevice, id 0x10000019e, registered, matched, active, busy 0 (1 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=32,"length"=2}),({"address"=36,"length"=2}),({"address"=40,"length"=2}),({"address"=44,"length"=2}),({"address"=48,"length"=2}),({"address"=52,"length"=2}),({"address"=56,"length"=2}),({"address"=60,"length"=2}),({"address"=160,"length"=2}),({"address"=164,"length"=2}),({"address"=168,"length"=2}),({"address"=172,"length"=2}),({"address"=176,"length"=2}),({"address"=180,"length"=2}),({"address"=184,"length"=2}),({"address"=188,"length"=2}),({"address"=1232,"length"=2}))
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<0200000000000000>)
    | | |     "name" = <"PNP0000">
    | | |   }
    | | |   
    | | +-o MATH  <class IOACPIPlatformDevice, id 0x10000019f, registered, matched, active, busy 0 (3 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=240,"length"=1}))
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<0d00000000000000>)
    | | |     "name" = <"PNP0C04">
    | | |   }
    | | |   
    | | +-o LDRC  <class IOACPIPlatformDevice, id 0x1000001a0, registered, matched, active, busy 0 (2 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "_UID" = "2"
    | | |     "IODeviceMemory" = (({"address"=46,"length"=2}),({"address"=78,"length"=2}),({"address"=97,"length"=1}),({"address"=99,"length"=1}),({"address"=101,"length"=1}),({"address"=103,"length"=1}),({"address"=128,"length"=1}),({"address"=146,"length"=1}),({"address"=178,"length"=2}),({"address"=65535,"length"=1}),({"address"=6144,"length"=255}),({"address"=2048,"length"=128}))
    | | |     "name" = <"PNP0C02">
    | | |   }
    | | |   
    | | +-o ARTC  <class IOACPIPlatformDevice, id 0x1000001a1, registered, matched, active, busy 0 (17 ms), retain 8>
    | | |   {
    | | |     "name" = <"ACPI000E">
    | | |     "_STA" = 18446744073709551615
    | | |   }
    | | |   
    | | +-o TIMR  <class IOACPIPlatformDevice, id 0x1000001a2, registered, matched, active, busy 0 (2 ms), retain 7>
    | | |   {
    | | |     "name" = <"PNP0100">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=64,"length"=4}),({"address"=80,"length"=4}))
    | | |   }
    | | |   
    | | +-o SMC  <class IOACPIPlatformDevice, id 0x1000001a3, registered, matched, active, busy 0 (646 ms), retain 8>
    | | |   {
    | | |     "IODeviceMemory" = (({"address"=768,"length"=32}),({"address"=4262133760,"length"=65536}))
    | | |     "compatible" = <"smc-huronriver">
    | | |     "IOReportLegendPublic" = Yes
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "_STA" = 11
    | | |     "IOInterruptSpecifiers" = (<0600000000000000>)
    | | |     "name" = <"APP0001">
    | | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="SMC 0"})
    | | |   }
    | | |   
    | | +-o EC  <class IOACPIPlatformDevice, id 0x1000001a4, registered, matched, active, busy 0 (28 ms), retain 10>
    | | |   {
    | | |     "IODeviceMemory" = (({"address"=98,"length"=1}),({"address"=102,"length"=1}))
    | | |     "_STA" = 18446744073709551615
    | | |     "_UID" = "0"
    | | |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |     "name" = <"PNP0C09">
    | | |     "acpi-wake-gpe" = 111
    | | |   }
    | | |   
    | | +-o GPUC  <class IOACPIPlatformDevice, id 0x1000001a5, registered, matched, active, busy 0 (2 ms), retain 7>
    | |     {
    | |       "IODeviceMemory" = (({"address"=4262134272,"length"=8}))
    | |       "_STA" = 11
    | |       "name" = <"APP000B">
    | |       "acpi-wake-gpe" = 19
    | |       "compatible" = <"gpuc">
    | |     }
    | |     
    | +-o PMCR@1F,2  <class IOPCIDevice, id 0x10000028a, registered, matched, active, busy 0 (752 ms), retain 11>
    | |   {
    | |     "name" = <"pci8086,a2a1">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "compatible" = <"pci8086,7270","pci8086,a2a1","pciclass,058000","PMCR">
    | |     "IOName" = "pci8086,a2a1"
    | |     "reg" = <00fa00000000000000000000000000000000000010fa000200000000000000000000000000400000>
    | |     "device-id" = <a1a20000>
    | |     "assigned-addresses" = <10fa008200000000008000740000000000400000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <00000000>
    | |     "IODeviceMemory" = (({"address"=1946189824,"length"=16384}))
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:31:2"
    | |     "class-code" = <00800500>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/PMCR@1f0002"
    | |     "subsystem-id" = <70720000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o SBUS@1F,4  <class IOPCIDevice, id 0x10000028b, registered, matched, active, busy 0 (958 ms), retain 11>
    |   | {
    |   |   "assigned-addresses" = <10fc00828000000000303301000000000001000020fc008100000000002000000000000020000000>
    |   |   "IOInterruptSpecifiers" = (<1000000007000000>)
    |   |   "IODeviceMemory" = (({"address"=549775945728,"length"=256}),"IOSubMemoryDescriptor is not serializable")
    |   |   "class-code" = <00050c00>
    |   |   "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    |   |   "subsystem-vendor-id" = <86800000>
    |   |   "built-in" = <00>
    |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |   |   "IOInterruptControllers" = ("io-apic-0")
    |   |   "name" = <"pci8086,a2a3">
    |   |   "vendor-id" = <86800000>
    |   |   "device-id" = <a3a20000>
    |   |   "IOPCIResourced" = Yes
    |   |   "compatible" = <"pci8086,7270","pci8086,a2a3","pciclass,0c0500","SBUS">
    |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0004"
    |   |   "subsystem-id" = <70720000>
    |   |   "revision-id" = <00000000>
    |   |   "pcidebug" = "0:31:4"
    |   |   "IOName" = "pci8086,a2a3"
    |   |   "reg" = <00fc00000000000000000000000000000000000010fc00020000000000000000000000000001000020fc000100000000000000000000000020000000>
    |   | }
    |   | 
    |   +-o BUS0@0  <class IORegistryEntry, id 0x10000028c, retain 4>
    |   |   {
    |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0004/BUS0@0"
    |   |   }
    |   |   
    |   +-o BUS1@1  <class IORegistryEntry, id 0x10000028d, retain 4>
    |       {
    |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0004/BUS1@1"
    |       }
    |       
    +-o LNKA  <class IOACPIPlatformDevice, id 0x1000001c2, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "1"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKB  <class IOACPIPlatformDevice, id 0x1000001c3, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "2"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKC  <class IOACPIPlatformDevice, id 0x1000001c4, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "3"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKD  <class IOACPIPlatformDevice, id 0x1000001c5, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "4"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKE  <class IOACPIPlatformDevice, id 0x1000001c6, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "5"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKF  <class IOACPIPlatformDevice, id 0x1000001c7, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "6"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKG  <class IOACPIPlatformDevice, id 0x1000001c8, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "7"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKH  <class IOACPIPlatformDevice, id 0x1000001c9, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "8"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o PWRB  <class IOACPIPlatformDevice, id 0x1000001ca, registered, matched, active, busy 0 (5 ms), retain 9>
    |   {
    |     "acpi-wake-type" = 1
    |     "IOReportLegendPublic" = Yes
    |     "IOInterruptControllers" = ("ACPIEventController")
    |     "_STA" = 18446744073709551615
    |     "IOInterruptSpecifiers" = (<0200000000000000>)
    |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="PWRB 0"})
    |     "name" = <"PNP0C0C">
    |   }
    |   
    +-o PC01@0  <class IOACPIPlatformDevice, id 0x1000001cb, registered, matched, active, busy 0 (1085 ms), retain 77>
    | | {
    | |   "compatible" = <"PNP0A03">
    | |   "IODTPersist" = 0
    | |   "_STA" = 15
    | |   "IOPCIConfigured" = Yes
    | |   "acpi-address-spaces" = <02000000000000000000000000000000000000000000000003000000000000000400000000000000000000000000000002000000000000000000000000000000000000000000000000000000000000000100000000000000000000000000000000000000000000000030000000000000ff3f000000000000000000000000000000100000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000008000000000ffffff8f00000000000000000000000000000010000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000004080000000ffffff7f8000000000000000000000000000004000000000000000000000000000000000000000000000000000000000>
    | |   "#size-cells" = <02000000>
    | |   "_UID" = "1"
    | |   "#address-cells" = <03000000>
    | |   "acpi-pci-routing-table" = <1800000000000000ffff00000000000010000000000000001800000000000000ffff01000000000010000000000000001800000000000000ffff02000000000010000000000000001800000000000000ffff03000000000010000000000000001800000000000000ffff08000000000010000000000000001800000001000000ffff08000000000011000000000000001800000002000000ffff08000000000012000000000000001800000003000000ffff08000000000013000000000000001800000000000000ffff09000000000010000000000000001800000001000000ffff09000000000011000000000000001800000002000000ffff09000000000012000000000000001800000003000000ffff09000000000013000000000000001800000000000000ffff0a000000000010000000000000001800000001000000ffff0a000000000011000000000000001800000002000000ffff0a000000000012000000000000001800000003000000ffff0a000000000013000000000000001800000000000000ffff0b000000000010000000000000001800000001000000ffff0b000000000011000000000000001800000002000000ffff0b000000000012000000000000001800000003000000ffff0b000000000013000000000000001800000000000000ffff0e000000000010000000000000001800000001000000ffff0e000000000011000000000000001800000002000000ffff0e000000000012000000000000001800000003000000ffff0e000000000013000000000000001800000000000000ffff0f000000000010000000000000001800000001000000ffff0f000000000011000000000000001800000002000000ffff0f000000000012000000000000001800000003000000ffff0f000000000013000000000000001800000000000000ffff10000000000010000000000000001800000001000000ffff10000000000011000000000000001800000002000000ffff10000000000012000000000000001800000003000000ffff10000000000013000000000000001800000000000000ffff11000000000010000000000000001800000001000000ffff11000000000011000000000000001800000002000000ffff11000000000012000000000000001800000003000000ffff11000000000013000000000000001800000000000000ffff14000000000010000000000000001800000001000000ffff14000000000011000000000000001800000002000000ffff14000000000012000000000000001800000003000000ffff14000000000013000000000000001800000000000000ffff15000000000010000000000000001800000001000000ffff15000000000011000000000000001800000002000000ffff15000000000012000000000000001800000003000000ffff15000000000013000000000000001800000000000000ffff16000000000010000000000000001800000001000000ffff16000000000011000000000000001800000002000000ffff16000000000012000000000000001800000003000000ffff16000000000013000000000000001800000000000000ffff17000000000010000000000000001800000001000000ffff17000000000011000000000000001800000002000000ffff17000000000012000000000000001800000003000000ffff17000000000013000000000000001800000000000000ffff1d000000000010000000000000001800000001000000ffff1d000000000011000000000000001800000002000000ffff1d000000000012000000000000001800000003000000ffff1d000000000013000000000000001800000000000000ffff1e000000000010000000000000001800000001000000ffff1e000000000011000000000000001800000002000000ffff1e000000000012000000000000001800000003000000ffff1e000000000013000000000000001800000000000000ffff1f000000000010000000000000001800000001000000ffff1f000000000011000000000000001800000002000000ffff1f000000000012000000000000001800000003000000ffff1f00000000001300000000000000000000000000000000000000000000000000000000000000>
    | |   "device-properties" = {"acpi-device"="IOACPIPlatformDevice is not serializable","acpi-path"="IOACPIPlane:/_SB/PC01@0"}
    | |   "_ADR" = 0
    | |   "acpi-path" = "IOACPIPlane:/_SB/PC01@0"
    | |   "name" = <"PNP0A08">
    | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | }
    | | 
    | +-o BR1B@10000  <class IORegistryEntry, id 0x1000002a7, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/BR1B@10000"
    | |   }
    | |   
    | +-o BR1C@20000  <class IORegistryEntry, id 0x1000002a8, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/BR1C@20000"
    | |   }
    | |   
    | +-o BR1D@30000  <class IORegistryEntry, id 0x1000002a9, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/BR1D@30000"
    | |   }
    | |   
    | +-o CHA2@a0000  <class IORegistryEntry, id 0x1000002ac, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CHA2@a0000"
    | |   }
    | |   
    | +-o CHA3@b0000  <class IORegistryEntry, id 0x1000002ad, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CHA3@b0000"
    | |   }
    | |   
    | +-o CHA6@100000  <class IORegistryEntry, id 0x1000002b0, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CHA6@100000"
    | |   }
    | |   
    | +-o CHA7@110000  <class IORegistryEntry, id 0x1000002b1, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CHA7@110000"
    | |   }
    | |   
    | +-o CMS0@140000  <class IORegistryEntry, id 0x1000002b2, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CMS0@140000"
    | |   }
    | |   
    | +-o CMS1@150000  <class IORegistryEntry, id 0x1000002b3, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CMS1@150000"
    | |   }
    | |   
    | +-o CMS2@160000  <class IORegistryEntry, id 0x1000002b4, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CMS2@160000"
    | |   }
    | |   
    | +-o CMS3@170000  <class IORegistryEntry, id 0x1000002b5, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CMS3@170000"
    | |   }
    | |   
    | +-o VCU0@1f0000  <class IORegistryEntry, id 0x1000002b8, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/VCU0@1f0000"
    | |   }
    | |   
    | +-o BR1A@0  <class IOPCIDevice, id 0x1000002a5, registered, matched, active, busy 0 (950 ms), retain 12>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 2
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <30200000>
    | | |   "acpi-pmcap-offset" = 224
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci8086,2030","pciclass,060400","BR1A">
    | | |   "ranges" = <0000008200000000000000800000008200000000000000800000000000005000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 24787010
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PC01@0/BR1A@0"
    | | |   "revision-id" = <04000000>
    | | |   "IOPCIExpressLinkStatus" = 12354
    | | |   "IOPCIExpressCapabilities" = 66
    | | |   "pcidebug" = "3:0:0(4:4)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <0000030000000000000000000000000000000000>
    | | | }
    | | | 
    | | +-o XGBE@0  <class IOPCIDevice, id 0x1000002a6, registered, matched, active, busy 0 (805 ms), retain 12>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PC01@0/BR1A@0/XGBE@0"
    | |       "assigned-addresses" = <100004820000000000004080000000000000010018000482000000000000418000000000001000002000048200000000000000800000000000004000>
    | |       "class-code" = <00000200>
    | |       "subsystem-vendor-id" = <6b100000>
    | |       "vendor-id" = <6a1d0000>
    | |       "IOPCIExpressLinkCapabilities" = 4455491
    | |       "IOName" = "ethernet"
    | |       "IOPCIPauseCompatible" = Yes
    | |       "local-mac-address" = <d0817ad3fce5>
    | |       "IOChildIndex" = 1
    | |       "pcidebug" = "4:0:0"
    | |       "IOPCIExpressLinkStatus" = 4162
    | |       "pci-aspm-default" = 0
    | |       "IOPCIExpressCapabilities" = 2
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "built-in" = <00>
    | |       "IOPCIResourced" = Yes
    | |       "IODeviceMemory" = (({"address"=2151677952,"length"=65536}),({"address"=2151743488,"length"=4096}),({"address"=2147483648,"length"=4194304}))
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "acpi-pmcap-offset" = 128
    | |       "name" = <"ethernet">
    | |       "subsystem-id" = <87010000>
    | |       "model" = "Apple AQC107-AFW"
    | |       "compatible" = <"pci106b,187","pci1d6a,7b1","pciclass,020000","XGBE">
    | |       "acpi-wake-type" = 2
    | |       "IOReportLegendPublic" = Yes
    | |       "reg" = <0000040000000000000000000000000000000000100004020000000000000000000000000000010018000402000000000000000000000000001000002000040200000000000000000000000000004000>
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="XGBE 1"})
    | |       "device-id" = <b1070000>
    | |       "revision-id" = <02000000>
    | |       "IOInterruptSpecifiers" = (<1000000007000000>,<1300000000000100>)
    | |       "IOPCIMSIMode" = Yes
    | |     }
    | |     
    | +-o pci8086,2034@5  <class IOPCIDevice, id 0x1000003ab, registered, matched, active, busy 0 (116 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2034","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2034"
    | |     "reg" = <0028030000000000000000000000000000000000>
    | |     "device-id" = <34200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 146
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:5:0"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2034">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2035@5,2  <class IOPCIDevice, id 0x1000003ad, registered, matched, active, busy 0 (124 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,2035","pciclass,088000">
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOName" = "pci8086,2035"
    | |     "reg" = <002a030000000000000000000000000000000000>
    | |     "device-id" = <35200000>
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 146
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:5:2"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2035">
    | |   }
    | |   
    | +-o pci8086,2036@5,4  <class IOPCIDevice, id 0x1000003af, registered, matched, active, busy 0 (119 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,2036","pciclass,080020">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2036"
    | |     "reg" = <002c030000000000000000000000000000000000102c030200000000000000000000000000100000>
    | |     "device-id" = <36200000>
    | |     "assigned-addresses" = <102c038200000000000050800000000000100000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIExpressCapabilities" = 145
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "IODeviceMemory" = (({"address"=2152726528,"length"=4096}))
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:5:4"
    | |     "class-code" = <20000800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "subsystem-id" = <36200000>
    | |     "name" = <"pci8086,2036">
    | |   }
    | |   
    | +-o CHA0@8  <class IOPCIDevice, id 0x1000002aa, registered, matched, active, busy 0 (134 ms), retain 9>
    | |   {
    | |     "name" = <"pci8086,208d">
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000","CHA0">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0040030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:8:0"
    | |     "class-code" = <00800800>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CHA0@80000"
    | |     "subsystem-id" = <00000000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o pci8086,208d@8,1  <class IOPCIDevice, id 0x1000003b4, registered, matched, active, busy 0 (103 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0041030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:8:1"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208d">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208d@8,2  <class IOPCIDevice, id 0x1000003b6, registered, matched, active, busy 0 (130 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0042030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:8:2"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208d">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208d@8,3  <class IOPCIDevice, id 0x1000003b8, registered, matched, active, busy 0 (119 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0043030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:8:3"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208d">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208d@8,4  <class IOPCIDevice, id 0x1000003bb, registered, matched, active, busy 0 (107 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0044030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:8:4"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208d">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208d@8,5  <class IOPCIDevice, id 0x1000003bc, registered, matched, active, busy 0 (124 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0045030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:8:5"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208d">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208d@8,6  <class IOPCIDevice, id 0x1000003be, registered, matched, active, busy 0 (119 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0046030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:8:6"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208d">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208d@8,7  <class IOPCIDevice, id 0x1000003bf, registered, matched, active, busy 0 (132 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0047030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:8:7"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208d">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o CHA1@9  <class IOPCIDevice, id 0x1000002ab, registered, matched, active, busy 0 (129 ms), retain 9>
    | |   {
    | |     "name" = <"pci8086,208d">
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000","CHA1">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0048030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:9:0"
    | |     "class-code" = <00800800>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CHA1@90000"
    | |     "subsystem-id" = <00000000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o pci8086,208d@9,1  <class IOPCIDevice, id 0x1000003c1, registered, matched, active, busy 0 (127 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208d","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208d"
    | |     "reg" = <0049030000000000000000000000000000000000>
    | |     "device-id" = <8d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:9:1"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208d">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o CHA4@E  <class IOPCIDevice, id 0x1000002ae, registered, matched, active, busy 0 (134 ms), retain 9>
    | |   {
    | |     "name" = <"pci8086,208e">
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000","CHA4">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0070030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:14:0"
    | |     "class-code" = <00800800>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CHA4@e0000"
    | |     "subsystem-id" = <00000000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o pci8086,208e@E,1  <class IOPCIDevice, id 0x1000003c4, registered, matched, active, busy 0 (122 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0071030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:14:1"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208e">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208e@E,2  <class IOPCIDevice, id 0x1000003c5, registered, matched, active, busy 0 (127 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0072030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:14:2"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208e">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208e@E,3  <class IOPCIDevice, id 0x1000003c6, registered, matched, active, busy 0 (131 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0073030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:14:3"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208e">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208e@E,4  <class IOPCIDevice, id 0x1000003c9, registered, matched, active, busy 0 (122 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0074030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:14:4"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208e">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208e@E,5  <class IOPCIDevice, id 0x1000003ca, registered, matched, active, busy 0 (126 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0075030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:14:5"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208e">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208e@E,6  <class IOPCIDevice, id 0x1000003cc, registered, matched, active, busy 0 (124 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0076030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:14:6"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208e">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,208e@E,7  <class IOPCIDevice, id 0x1000003ce, registered, matched, active, busy 0 (116 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0077030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:14:7"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208e">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o CHA5@F  <class IOPCIDevice, id 0x1000002af, registered, matched, active, busy 0 (120 ms), retain 9>
    | |   {
    | |     "name" = <"pci8086,208e">
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000","CHA5">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0078030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:15:0"
    | |     "class-code" = <00800800>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CHA5@f0000"
    | |     "subsystem-id" = <00000000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o pci8086,208e@F,1  <class IOPCIDevice, id 0x1000003d1, registered, matched, active, busy 0 (121 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,208e","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,208e"
    | |     "reg" = <0079030000000000000000000000000000000000>
    | |     "device-id" = <8e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:15:1"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,208e">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o CDL0@1D  <class IOPCIDevice, id 0x1000002b6, registered, matched, active, busy 0 (119 ms), retain 9>
    | |   {
    | |     "name" = <"pci8086,2054">
    | |     "compatible" = <"pci8086,0","pci8086,2054","pciclass,088000","CDL0">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2054"
    | |     "reg" = <00e8030000000000000000000000000000000000>
    | |     "device-id" = <54200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:29:0"
    | |     "class-code" = <00800800>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/CDL0@1d0000"
    | |     "subsystem-id" = <00000000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o pci8086,2055@1D,1  <class IOPCIDevice, id 0x1000003d4, registered, matched, active, busy 0 (122 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2055","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2055"
    | |     "reg" = <00e9030000000000000000000000000000000000>
    | |     "device-id" = <55200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:29:1"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,2055">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2056@1D,2  <class IOPCIDevice, id 0x1000003d5, registered, matched, active, busy 0 (112 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2056","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2056"
    | |     "reg" = <00ea030000000000000000000000000000000000>
    | |     "device-id" = <56200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:29:2"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,2056">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2057@1D,3  <class IOPCIDevice, id 0x1000003d6, registered, matched, active, busy 0 (112 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2057","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2057"
    | |     "reg" = <00eb030000000000000000000000000000000000>
    | |     "device-id" = <57200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:29:3"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,2057">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o PCU0@1E  <class IOPCIDevice, id 0x1000002b7, registered, matched, active, busy 0 (107 ms), retain 9>
    | |   {
    | |     "name" = <"pci8086,2080">
    | |     "compatible" = <"pci8086,0","pci8086,2080","pciclass,088000","PCU0">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2080"
    | |     "reg" = <00f0030000000000000000000000000000000000>
    | |     "device-id" = <80200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:30:0"
    | |     "class-code" = <00800800>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC01@0/PCU0@1e0000"
    | |     "subsystem-id" = <00000000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o pci8086,2081@1E,1  <class IOPCIDevice, id 0x1000003d9, registered, matched, active, busy 0 (109 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2081","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2081"
    | |     "reg" = <00f1030000000000000000000000000000000000>
    | |     "device-id" = <81200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:30:1"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,2081">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2082@1E,2  <class IOPCIDevice, id 0x1000003da, registered, matched, active, busy 0 (103 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2082","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2082"
    | |     "reg" = <00f2030000000000000000000000000000000000>
    | |     "device-id" = <82200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:30:2"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,2082">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2083@1E,3  <class IOPCIDevice, id 0x1000003dc, registered, matched, active, busy 0 (104 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2083","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2083"
    | |     "reg" = <00f3030000000000000000000000000000000000>
    | |     "device-id" = <83200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:30:3"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,2083">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2084@1E,4  <class IOPCIDevice, id 0x1000003dd, registered, matched, active, busy 0 (101 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2084","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2084"
    | |     "reg" = <00f4030000000000000000000000000000000000>
    | |     "device-id" = <84200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:30:4"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,2084">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2085@1E,5  <class IOPCIDevice, id 0x1000003df, registered, matched, active, busy 0 (97 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2085","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2085"
    | |     "reg" = <00f5030000000000000000000000000000000000>
    | |     "device-id" = <85200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "3:30:5"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,2085">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2086@1E,6  <class IOPCIDevice, id 0x1000003e0, registered, matched, active, busy 0 (91 ms), retain 9>
    |     {
    |       "compatible" = <"pci8086,0","pci8086,2086","pciclass,088000">
    |       "subsystem-vendor-id" = <86800000>
    |       "IOName" = "pci8086,2086"
    |       "reg" = <00f6030000000000000000000000000000000000>
    |       "device-id" = <86200000>
    |       "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    |       "IOPCIResourced" = Yes
    |       "revision-id" = <04000000>
    |       "vendor-id" = <86800000>
    |       "pcidebug" = "3:30:6"
    |       "class-code" = <00800800>
    |       "name" = <"pci8086,2086">
    |       "subsystem-id" = <00000000>
    |     }
    |     
    +-o PC02@0  <class IOACPIPlatformDevice, id 0x1000001e0, registered, matched, active, busy 0 (1770 ms), retain 54>
    | | {
    | |   "compatible" = <"PNP0A03">
    | |   "IODTPersist" = 0
    | |   "_STA" = 15
    | |   "IOPCIConfigured" = Yes
    | |   "acpi-address-spaces" = <0200000000000000000000000000000000000000000000000500000000000000ef000000000000000000000000000000eb000000000000000000000000000000000000000000000000000000000000000100000000000000000000000000000000000000000000000040000000000000ffdf000000000000000000000000000000a00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009000000000ffbfffdf00000000000000000000000000c0ff4f000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000008080000000ffffffbf8000000000000000000000000000004000000000000000000000000000000000000000000000000000000000>
    | |   "#size-cells" = <02000000>
    | |   "_UID" = "2"
    | |   "#address-cells" = <03000000>
    | |   "acpi-pci-routing-table" = <1800000000000000ffff00000000000010000000000000001800000000000000ffff01000000000010000000000000001800000000000000ffff02000000000010000000000000001800000000000000ffff03000000000010000000000000001800000000000000ffff08000000000010000000000000001800000001000000ffff08000000000011000000000000001800000002000000ffff08000000000012000000000000001800000003000000ffff08000000000013000000000000001800000000000000ffff09000000000010000000000000001800000001000000ffff09000000000011000000000000001800000002000000ffff09000000000012000000000000001800000003000000ffff09000000000013000000000000001800000000000000ffff0a000000000010000000000000001800000001000000ffff0a000000000011000000000000001800000002000000ffff0a000000000012000000000000001800000003000000ffff0a000000000013000000000000001800000000000000ffff0b000000000010000000000000001800000001000000ffff0b000000000011000000000000001800000002000000ffff0b000000000012000000000000001800000003000000ffff0b000000000013000000000000001800000000000000ffff0c000000000010000000000000001800000001000000ffff0c000000000011000000000000001800000002000000ffff0c000000000012000000000000001800000003000000ffff0c000000000013000000000000001800000000000000ffff0d000000000010000000000000001800000001000000ffff0d000000000011000000000000001800000002000000ffff0d000000000012000000000000001800000003000000ffff0d000000000013000000000000001800000000000000ffff16000000000010000000000000001800000001000000ffff16000000000011000000000000001800000002000000ffff16000000000012000000000000001800000003000000ffff16000000000013000000000000001800000000000000ffff17000000000010000000000000001800000001000000ffff17000000000011000000000000001800000002000000ffff17000000000012000000000000001800000003000000ffff1700000000001300000000000000000000000000000000000000000000000000000000000000>
    | |   "device-properties" = {"acpi-device"="IOACPIPlatformDevice is not serializable","acpi-path"="IOACPIPlane:/_SB/PC02@0"}
    | |   "_ADR" = 0
    | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0"
    | |   "name" = <"PNP0A08">
    | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | }
    | | 
    | +-o UMC0@160000  <class IORegistryEntry, id 0x100000339, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/UMC0@160000"
    | |   }
    | |   
    | +-o UMC1@170000  <class IORegistryEntry, id 0x10000033a, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/UMC1@170000"
    | |   }
    | |   
    | +-o BR2C@2  <class IOPCIDevice, id 0x1000002b9, registered, matched, active, busy 0 (1717 ms), retain 12>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <80000000>
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "IOPCIHPType" = 50
    | | |   "name" = <"pci-bridge">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <32200000>
    | | |   "acpi-pmcap-offset" = 224
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci80,0","pci8086,2032","pciclass,060400","BR2C">
    | | |   "ranges" = <000000820000000000001090000000820000000000001090000000000000f027000000c280000000000000a0000000c280000000000000a000000000000000200000008100000000004000000000008100000000004000000000000000500000>
    | | |   "IOPCIExpressLinkCapabilities" = 125450307
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000"
    | | |   "subsystem-id" = <00000000>
    | | |   "revision-id" = <04000000>
    | | |   "IOPCIExpressLinkStatus" = 61507
    | | |   "IOPCIExpressCapabilities" = 66
    | | |   "pcidebug" = "5:2:0(123:239)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <0010050000000000000000000000000000000000>
    | | | }
    | | | 
    | | +-o UPSB@0  <class IOPCIDevice, id 0x1000002ba, registered, matched, active, busy 0 (1679 ms), retain 15>
    | |   | {
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "IOPCIExpressLinkCapabilities" = 4545603
    | |   |   "class-code" = <00040600>
    | |   |   "subsystem-vendor-id" = <80000000>
    | |   |   "vendor-id" = <86800000>
    | |   |   "IOName" = "pci-bridge"
    | |   |   "#size-cells" = <02000000>
    | |   |   "IOPCIHPType" = 49
    | |   |   "IOChildIndex" = 1
    | |   |   "pcidebug" = "123:0:0(124:239)"
    | |   |   "IOPCIExpressLinkStatus" = 4163
    | |   |   "pci-aspm-default" = 0
    | |   |   "IODTPersist" = 0
    | |   |   "IOInterruptControllers" = ("io-apic-0")
    | |   |   "IOPCIConfigured" = Yes
    | |   |   "IOPCIExpressCapabilities" = 82
    | |   |   "built-in" = <00>
    | |   |   "IOPCIResourced" = Yes
    | |   |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |   "ranges" = <000000820000000000001090000000820000000000001090000000000000f027000000c280000000000000a0000000c280000000000000a000000000000000200000008100000000004000000000008100000000004000000000000000500000>
    | |   |   "acpi-pmcap-offset" = 128
    | |   |   "name" = <"pci-bridge">
    | |   |   "subsystem-id" = <00000000>
    | |   |   "USB Cable Attached" = No
    | |   |   "compatible" = <"pci80,0","pci8086,1578","pciclass,060400","UPSB">
    | |   |   "PCI-Thunderbolt" = 1
    | |   |   "reg" = <00007b0000000000000000000000000000000000>
    | |   |   "IOPCITunnelL1Enable" = No
    | |   |   "device-id" = <78150000>
    | |   |   "#address-cells" = <03000000>
    | |   |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | |   |   "revision-id" = <02000000>
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0"
    | |   | }
    | |   | 
    | |   +-o DSB0@0  <class IOPCIDevice, id 0x1000002bb, registered, matched, active, busy 0 (1242 ms), retain 12>
    | |   | | {
    | |   | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "class-code" = <00040600>
    | |   | |   "IOPCIExpressSlotStatus" = 64
    | |   | |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   | |   "built-in" = <00>
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "IOInterruptControllers" = ("io-apic-0")
    | |   | |   "PCIHotplugCapable" = 0
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOChildIndex" = 1
    | |   | |   "device-id" = <d3150000>
    | |   | |   "IOPCIHPType" = 1
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "compatible" = <"pci8086,15d3","pciclass,060400","DSB0">
    | |   | |   "ranges" = <0000008200000000000020900000008200000000000020900000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "IOPCIExpressLinkCapabilities" = 6380609
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "IODTPersist" = 0
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB0@0"
    | |   | |   "IOPCITunnelL1Enable" = Yes
    | |   | |   "revision-id" = <02000000>
    | |   | |   "IOPCIExpressLinkStatus" = 4161
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "pcidebug" = "124:0:0(126:126)"
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "reg" = <00007c0000000000000000000000000000000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 262144
    | |   | | }
    | |   | | 
    | |   | +-o NHI0@0  <class IOPCIDevice, id 0x1000002bc, registered, matched, active, busy 0 (1124 ms), retain 11>
    | |   |     {
    | |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |       "IOPCIMSIMode" = Yes
    | |   |       "assigned-addresses" = <10007e820000000000002090000000000000040014007e8200000000000024900000000000100000>
    | |   |       "class-code" = <00800800>
    | |   |       "subsystem-vendor-id" = <22220000>
    | |   |       "vendor-id" = <86800000>
    | |   |       "IOPCIExpressLinkCapabilities" = 351297
    | |   |       "IOName" = "pci8086,15d2"
    | |   |       "pathcr" = <04000000000000000000070010001000050000000000000000000700100010000100000005000e000e000000000000000200000000000000000002000200010003000000000000000000070002000100>
    | |   |       "TBTDPLowToHigh" = <01000000>
    | |   |       "IOPCIHPType" = 1
    | |   |       "power-save" = 1
    | |   |       "IOChildIndex" = 1
    | |   |       "pcidebug" = "126:0:0"
    | |   |       "IOPCIExpressLinkStatus" = 4161
    | |   |       "TBTFlags" = <03000000>
    | |   |       "pci-aspm-default" = 0
    | |   |       "IOPCIExpressCapabilities" = 2
    | |   |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   |       "linkDetails" = <0800000003000000>
    | |   |       "IOPCITunnelControllerID" = 4294968415
    | |   |       "built-in" = <00>
    | |   |       "IOPCIResourced" = Yes
    | |   |       "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |       "IODeviceMemory" = (({"address"=2418016256,"length"=262144}),({"address"=2418278400,"length"=4096}))
    | |   |       "acpi-pmcap-offset" = 128
    | |   |       "name" = <"pci8086,15d2">
    | |   |       "ThunderboltUUID" = <e8d5b54a0d200951b26086b324bc44f9>
    | |   |       "subsystem-id" = <11110000>
    | |   |       "compatible" = <"pci2222,1111","pci8086,15d2","pciclass,088000","NHI0">
    | |   |       "ThunderboltDROM" = <7e00c549d53e2101000a9b60fa015e0001000c0001000881800280000000088290018000000008838004800100000884900380010000088500000000000003862003878002c80589500000058a50000002cb0d014170706c6520496e632e000c024d6163696e746f736800>
    | |   |       "sscOffset" = <0000>
    | |   |       "IOReportLegendPublic" = Yes
    | |   |       "reg" = <00007e000000000000000000000000000000000010007e020000000000000000000000000000040014007e0200000000000000000000000000100000>
    | |   |       "IOPCITunnelL1Enable" = Yes
    | |   |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="NHI0 1"})
    | |   |       "device-id" = <d2150000>
    | |   |       "ThunderboltConfig" = <0002ffff04000301010004000501020003000301010000000301020002000100>
    | |   |       "revision-id" = <02000000>
    | |   |       "IOInterruptSpecifiers" = (<1000000007000000>,<2800000000000100>)
    | |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB0@0/NHI0@0"
    | |   |     }
    | |   |     
    | |   +-o DSB1@1  <class IOPCIDevice, id 0x1000002bd, registered, matched, active, busy 0 (108 ms), retain 13>
    | |   | | {
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000"
    | |   | |   "IOPCIExpressLinkCapabilities" = 24206401
    | |   | |   "class-code" = <00040600>
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 786528
    | |   | |   "IOPCIHPType" = 48
    | |   | |   "IOChildIndex" = 2
    | |   | |   "pcidebug" = "124:1:0(184:184)"
    | |   | |   "Thunderbolt Path" = "IOService:/AppleACPIPlatformExpert/PC02@0/AppleACPIPCI/BR2C@2/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType3/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType3/IOThunderboltPort@6"
    | |   | |   "IOPCIExpressLinkStatus" = 4161
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "IODTPersist" = 0
    | |   | |   "Thunderbolt Entry ID" = 4294968471
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "AAPL,slot-name" = <"PCI Slot 1">
    | |   | |   "IOPowerManagement" = {"PowerOverrideOn"=Yes,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3,"DevicePowerState"=0,"ChildrenPowerState"=2,"CurrentPowerState"=0}
    | |   | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "IOPCITunnelLinkChange" = Yes
    | |   | |   "compatible" = <"pci8086,15d3","pciclass,060400","DSB1">
    | |   | |   "IOReportLegendPublic" = Yes
    | |   | |   "IOPCIExpressSlotStatus" = 0
    | |   | |   "reg" = <00087c0000000000000000000000000000000000>
    | |   | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="DSB1 1"})
    | |   | |   "device-id" = <d3150000>
    | |   | |   "IOPCITunnelID" = 4294968415
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "IOInterruptSpecifiers" = (<1100000007000000>,<0c00000000000100>)
    | |   | |   "revision-id" = <02000000>
    | |   | |   "IOPCIMSIMode" = Yes
    | |   | | }
    | |   | | 
    | |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000002be, retain 9>
    | |   |   | {
    | |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0"
    | |   |   | }
    | |   |   | 
    | |   |   +-o DSB0@0  <class IORegistryEntry, id 0x1000002bf, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB0@0"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002c0, retain 4>
    | |   |   |     {
    | |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |     }
    | |   |   |     
    | |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000002c1, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000002c2, retain 9>
    | |   |   |   | {
    | |   |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0"
    | |   |   |   | }
    | |   |   |   | 
    | |   |   |   +-o DSB0@0  <class IORegistryEntry, id 0x1000002c3, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002c4, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000002c5, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002c6, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x1000002c7, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002c8, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x1000002c9, retain 4>
    | |   |   |   |   {
    | |   |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB5@50000"
    | |   |   |   |   }
    | |   |   |   |   
    | |   |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x1000002ca, retain 4>
    | |   |   |       {
    | |   |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB6@60000"
    | |   |   |       }
    | |   |   |       
    | |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x1000002cb, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000002cc, retain 9>
    | |   |   |   | {
    | |   |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0"
    | |   |   |   | }
    | |   |   |   | 
    | |   |   |   +-o DSB0@0  <class IORegistryEntry, id 0x1000002cd, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002ce, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000002cf, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002d0, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x1000002d1, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002d2, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x1000002d3, retain 4>
    | |   |   |   |   {
    | |   |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB5@50000"
    | |   |   |   |   }
    | |   |   |   |   
    | |   |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x1000002d4, retain 4>
    | |   |   |       {
    | |   |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB6@60000"
    | |   |   |       }
    | |   |   |       
    | |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x1000002d5, retain 4>
    | |   |   |   {
    | |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB5@50000"
    | |   |   |   }
    | |   |   |   
    | |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x1000002d6, retain 4>
    | |   |       {
    | |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB6@60000"
    | |   |       }
    | |   |       
    | |   +-o DSB2@2  <class IOPCIDevice, id 0x1000002d7, registered, matched, active, busy 0 (486 ms), retain 12>
    | |   | | {
    | |   | |   "IOInterruptSpecifiers" = (<1200000007000000>)
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "class-code" = <00040600>
    | |   | |   "IOPCIExpressSlotStatus" = 64
    | |   | |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   | |   "built-in" = <00>
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "IOInterruptControllers" = ("io-apic-0")
    | |   | |   "PCIHotplugCapable" = 0
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOChildIndex" = 3
    | |   | |   "device-id" = <d3150000>
    | |   | |   "IOPCIHPType" = 2
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "compatible" = <"pci8086,15d3","pciclass,060400","DSB2">
    | |   | |   "ranges" = <0000008200000000000010900000008200000000000010900000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "IOPCIExpressLinkCapabilities" = 40983617
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "IODTPersist" = 0
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB2@20000"
    | |   | |   "IOPCITunnelL1Enable" = No
    | |   | |   "revision-id" = <02000000>
    | |   | |   "IOPCIExpressLinkStatus" = 12353
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "pcidebug" = "124:2:0(125:125)"
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "reg" = <00107c0000000000000000000000000000000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 262240
    | |   | | }
    | |   | | 
    | |   | +-o XHC2@0  <class IOPCIDevice, id 0x1000002d8, registered, matched, active, busy 0 (379 ms), retain 13>
    | |   |   | {
    | |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB2@20000/XHC2@0"
    | |   |   |   "assigned-addresses" = <10007d8200000000000010900000000000000100>
    | |   |   |   "class-code" = <30030c00>
    | |   |   |   "subsystem-vendor-id" = <22220000>
    | |   |   |   "vendor-id" = <86800000>
    | |   |   |   "IOPCIExpressLinkCapabilities" = 4545601
    | |   |   |   "IOName" = "pci8086,15d4"
    | |   |   |   "IOPCIHPType" = 2
    | |   |   |   "IOChildIndex" = 1
    | |   |   |   "pcidebug" = "125:0:0"
    | |   |   |   "IOPCIExpressLinkStatus" = 4161
    | |   |   |   "pci-aspm-default" = 0
    | |   |   |   "IOPCIExpressCapabilities" = 2
    | |   |   |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   |   |   "built-in" = <00>
    | |   |   |   "IOPCIResourced" = Yes
    | |   |   |   "IODeviceMemory" = (({"address"=2416967680,"length"=65536}))
    | |   |   |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |   |   "AAPL,xhci-clock-id" = 1
    | |   |   |   "acpi-pmcap-offset" = 128
    | |   |   |   "name" = <"pci8086,15d4">
    | |   |   |   "subsystem-id" = <11110000>
    | |   |   |   "compatible" = <"pci2222,1111","pci8086,15d4","pciclass,0c0330","XHC2">
    | |   |   |   "IOReportLegendPublic" = Yes
    | |   |   |   "reg" = <00007d000000000000000000000000000000000010007d0200000000000000000000000000000100>
    | |   |   |   "IOPCITunnelL1Enable" = No
    | |   |   |   "USBBusNumber" = 0
    | |   |   |   "device-id" = <d4150000>
    | |   |   |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="XHC2 1"})
    | |   |   |   "revision-id" = <02000000>
    | |   |   |   "IOInterruptSpecifiers" = (<1200000007000000>,<2900000000000100>)
    | |   |   |   "IOPCIMSIMode" = Yes
    | |   |   | }
    | |   |   | 
    | |   |   +-o RHUB@0  <class IORegistryEntry, id 0x1000002d9, retain 6>
    | |   |     | {
    | |   |     |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB2@20000/XHC2@0/RHUB@0"
    | |   |     | }
    | |   |     | 
    | |   |     +-o SSP1@3  <class IORegistryEntry, id 0x1000002da, retain 4>
    | |   |     |   {
    | |   |     |     "UsbCPortNumber" = 2
    | |   |     |     "kUSBWakePortCurrentLimit" = 3000
    | |   |     |     "kUSBSleepPortCurrentLimit" = 3000
    | |   |     |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB2@20000/XHC2@0/RHUB@0/SSP1@3"
    | |   |     |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     |   }
    | |   |     |   
    | |   |     +-o SSP2@4  <class IORegistryEntry, id 0x1000002db, retain 4>
    | |   |         {
    | |   |           "UsbCPortNumber" = 1
    | |   |           "kUSBWakePortCurrentLimit" = 3000
    | |   |           "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |           "kUSBSleepPortCurrentLimit" = 3000
    | |   |           "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB2@20000/XHC2@0/RHUB@0/SSP2@4"
    | |   |           "UsbCompanionPortPresent" = 1
    | |   |         }
    | |   |         
    | |   +-o DSB4@4  <class IOPCIDevice, id 0x1000002dc, registered, matched, active, busy 0 (98 ms), retain 13>
    | |     | {
    | |     |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000"
    | |     |   "IOPCIExpressLinkCapabilities" = 74538049
    | |     |   "class-code" = <00040600>
    | |     |   "vendor-id" = <86800000>
    | |     |   "IOName" = "pci-bridge"
    | |     |   "#size-cells" = <02000000>
    | |     |   "IOPCIExpressSlotCapabilities" = 2359392
    | |     |   "IOPCIHPType" = 48
    | |     |   "IOChildIndex" = 4
    | |     |   "pcidebug" = "124:4:0(127:127)"
    | |     |   "Thunderbolt Path" = "IOService:/AppleACPIPlatformExpert/PC02@0/AppleACPIPCI/BR2C@2/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType3/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType3/IOThunderboltPort@7"
    | |     |   "IOPCIExpressLinkStatus" = 4161
    | |     |   "pci-aspm-default" = 0
    | |     |   "IOPCIExpressCapabilities" = 354
    | |     |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     |   "IOPCIConfigured" = Yes
    | |     |   "IODTPersist" = 0
    | |     |   "Thunderbolt Entry ID" = 4294968472
    | |     |   "IOPCIResourced" = Yes
    | |     |   "AAPL,slot-name" = <"PCI Slot 2">
    | |     |   "IOPowerManagement" = {"PowerOverrideOn"=Yes,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3,"DevicePowerState"=0,"ChildrenPowerState"=2,"CurrentPowerState"=0}
    | |     |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |     |   "acpi-pmcap-offset" = 128
    | |     |   "name" = <"pci-bridge">
    | |     |   "IOPCITunnelLinkChange" = Yes
    | |     |   "compatible" = <"pci8086,15d3","pciclass,060400","DSB4">
    | |     |   "IOReportLegendPublic" = Yes
    | |     |   "IOPCIExpressSlotStatus" = 0
    | |     |   "reg" = <00207c0000000000000000000000000000000000>
    | |     |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="DSB4 1"})
    | |     |   "device-id" = <d3150000>
    | |     |   "IOPCITunnelID" = 4294968415
    | |     |   "#address-cells" = <03000000>
    | |     |   "IOInterruptSpecifiers" = (<1000000007000000>,<0d00000000000100>)
    | |     |   "revision-id" = <02000000>
    | |     |   "IOPCIMSIMode" = Yes
    | |     | }
    | |     | 
    | |     +-o UPS0@0  <class IORegistryEntry, id 0x1000002dd, retain 9>
    | |       | {
    | |       |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0"
    | |       | }
    | |       | 
    | |       +-o DSB0@0  <class IORegistryEntry, id 0x1000002de, retain 5>
    | |       | | {
    | |       | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB0@0"
    | |       | | }
    | |       | | 
    | |       | +-o DEV0@0  <class IORegistryEntry, id 0x1000002df, retain 4>
    | |       |     {
    | |       |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB0@0/DEV0@0"
    | |       |     }
    | |       |     
    | |       +-o DSB3@30000  <class IORegistryEntry, id 0x1000002e0, retain 5>
    | |       | | {
    | |       | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000"
    | |       | | }
    | |       | | 
    | |       | +-o UPS0@0  <class IORegistryEntry, id 0x1000002e1, retain 9>
    | |       |   | {
    | |       |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0"
    | |       |   | }
    | |       |   | 
    | |       |   +-o DSB0@0  <class IORegistryEntry, id 0x1000002e2, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002e3, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000002e4, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002e5, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB4@40000  <class IORegistryEntry, id 0x1000002e6, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002e7, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB5@50000  <class IORegistryEntry, id 0x1000002e8, retain 4>
    | |       |   |   {
    | |       |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB5@50000"
    | |       |   |   }
    | |       |   |   
    | |       |   +-o DSB6@60000  <class IORegistryEntry, id 0x1000002e9, retain 4>
    | |       |       {
    | |       |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB6@60000"
    | |       |       }
    | |       |       
    | |       +-o DSB4@40000  <class IORegistryEntry, id 0x1000002ea, retain 5>
    | |       | | {
    | |       | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000"
    | |       | | }
    | |       | | 
    | |       | +-o UPS0@0  <class IORegistryEntry, id 0x1000002eb, retain 9>
    | |       |   | {
    | |       |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0"
    | |       |   | }
    | |       |   | 
    | |       |   +-o DSB0@0  <class IORegistryEntry, id 0x1000002ec, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002ed, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000002ee, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002ef, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB4@40000  <class IORegistryEntry, id 0x1000002f0, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002f1, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB5@50000  <class IORegistryEntry, id 0x1000002f2, retain 4>
    | |       |   |   {
    | |       |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB5@50000"
    | |       |   |   }
    | |       |   |   
    | |       |   +-o DSB6@60000  <class IORegistryEntry, id 0x1000002f3, retain 4>
    | |       |       {
    | |       |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB6@60000"
    | |       |       }
    | |       |       
    | |       +-o DSB5@50000  <class IORegistryEntry, id 0x1000002f4, retain 4>
    | |       |   {
    | |       |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB5@50000"
    | |       |   }
    | |       |   
    | |       +-o DSB6@60000  <class IORegistryEntry, id 0x1000002f5, retain 4>
    | |           {
    | |             "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |             "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB6@60000"
    | |           }
    | |           
    | +-o BR2D@3  <class IOPCIDevice, id 0x1000002f6, registered, matched, active, busy 0 (1716 ms), retain 12>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <80000000>
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "IOPCIHPType" = 50
    | | |   "name" = <"pci-bridge">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <33200000>
    | | |   "acpi-pmcap-offset" = 224
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci80,0","pci8086,2033","pciclass,060400","BR2D">
    | | |   "ranges" = <0000008200000000000000b80000008200000000000000b8000000000000f027000000c28000000000000080000000c2800000000000008000000000000000200000008100000000009000000000008100000000009000000000000000500000>
    | | |   "IOPCIExpressLinkCapabilities" = 142227523
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000"
    | | |   "subsystem-id" = <00000000>
    | | |   "revision-id" = <04000000>
    | | |   "IOPCIExpressLinkStatus" = 61507
    | | |   "IOPCIExpressCapabilities" = 66
    | | |   "pcidebug" = "5:3:0(6:122)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <0018050000000000000000000000000000000000>
    | | | }
    | | | 
    | | +-o UPSB@0  <class IOPCIDevice, id 0x1000002f7, registered, matched, active, busy 0 (1639 ms), retain 15>
    | |   | {
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "IOPCIExpressLinkCapabilities" = 4545603
    | |   |   "class-code" = <00040600>
    | |   |   "subsystem-vendor-id" = <80000000>
    | |   |   "vendor-id" = <86800000>
    | |   |   "IOName" = "pci-bridge"
    | |   |   "#size-cells" = <02000000>
    | |   |   "IOPCIHPType" = 49
    | |   |   "IOChildIndex" = 1
    | |   |   "pcidebug" = "6:0:0(7:122)"
    | |   |   "IOPCIExpressLinkStatus" = 4163
    | |   |   "pci-aspm-default" = 0
    | |   |   "IODTPersist" = 0
    | |   |   "IOInterruptControllers" = ("io-apic-0")
    | |   |   "IOPCIConfigured" = Yes
    | |   |   "IOPCIExpressCapabilities" = 82
    | |   |   "built-in" = <00>
    | |   |   "IOPCIResourced" = Yes
    | |   |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |   "ranges" = <0000008200000000000000b80000008200000000000000b8000000000000f027000000c28000000000000080000000c2800000000000008000000000000000200000008100000000009000000000008100000000009000000000000000500000>
    | |   |   "acpi-pmcap-offset" = 128
    | |   |   "name" = <"pci-bridge">
    | |   |   "subsystem-id" = <00000000>
    | |   |   "USB Cable Attached" = No
    | |   |   "compatible" = <"pci80,0","pci8086,1578","pciclass,060400","UPSB">
    | |   |   "PCI-Thunderbolt" = 1
    | |   |   "reg" = <0000060000000000000000000000000000000000>
    | |   |   "IOPCITunnelL1Enable" = No
    | |   |   "device-id" = <78150000>
    | |   |   "#address-cells" = <03000000>
    | |   |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | |   |   "revision-id" = <02000000>
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0"
    | |   | }
    | |   | 
    | |   +-o DSB0@0  <class IOPCIDevice, id 0x1000002f8, registered, matched, active, busy 0 (1173 ms), retain 12>
    | |   | | {
    | |   | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "class-code" = <00040600>
    | |   | |   "IOPCIExpressSlotStatus" = 64
    | |   | |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   | |   "built-in" = <00>
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "IOInterruptControllers" = ("io-apic-0")
    | |   | |   "PCIHotplugCapable" = 0
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOChildIndex" = 1
    | |   | |   "device-id" = <d3150000>
    | |   | |   "IOPCIHPType" = 1
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "compatible" = <"pci8086,15d3","pciclass,060400","DSB0">
    | |   | |   "ranges" = <0000008200000000000010b80000008200000000000010b80000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "IOPCIExpressLinkCapabilities" = 6380609
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "IODTPersist" = 0
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB0@0"
    | |   | |   "IOPCITunnelL1Enable" = Yes
    | |   | |   "revision-id" = <02000000>
    | |   | |   "IOPCIExpressLinkStatus" = 4161
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "pcidebug" = "7:0:0(9:9)"
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "reg" = <0000070000000000000000000000000000000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 262144
    | |   | | }
    | |   | | 
    | |   | +-o NHI0@0  <class IOPCIDevice, id 0x1000002f9, registered, matched, active, busy 0 (1111 ms), retain 11>
    | |   |     {
    | |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |       "IOPCIMSIMode" = Yes
    | |   |       "assigned-addresses" = <1000098200000000000010b800000000000004001400098200000000000014b80000000000100000>
    | |   |       "class-code" = <00800800>
    | |   |       "subsystem-vendor-id" = <22220000>
    | |   |       "vendor-id" = <86800000>
    | |   |       "IOPCIExpressLinkCapabilities" = 351297
    | |   |       "IOName" = "pci8086,15d2"
    | |   |       "pathcr" = <04000000000000000000070010001000050000000000000000000700100010000100000005000e000e000000000000000200000000000000000002000200010003000000000000000000070002000100>
    | |   |       "TBTDPLowToHigh" = <01000000>
    | |   |       "IOPCIHPType" = 1
    | |   |       "power-save" = 1
    | |   |       "IOChildIndex" = 1
    | |   |       "pcidebug" = "9:0:0"
    | |   |       "IOPCIExpressLinkStatus" = 4161
    | |   |       "TBTFlags" = <03000000>
    | |   |       "pci-aspm-default" = 0
    | |   |       "IOPCIExpressCapabilities" = 2
    | |   |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   |       "linkDetails" = <0800000003000000>
    | |   |       "IOPCITunnelControllerID" = 4294968446
    | |   |       "built-in" = <00>
    | |   |       "IOPCIResourced" = Yes
    | |   |       "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |       "IODeviceMemory" = (({"address"=3088056320,"length"=262144}),({"address"=3088318464,"length"=4096}))
    | |   |       "acpi-pmcap-offset" = 128
    | |   |       "name" = <"pci8086,15d2">
    | |   |       "ThunderboltUUID" = <937622ae6882b95398aa13417513c10c>
    | |   |       "subsystem-id" = <11110000>
    | |   |       "compatible" = <"pci2222,1111","pci8086,15d2","pciclass,088000","NHI0">
    | |   |       "ThunderboltDROM" = <6d01c549d53e21010004ce8d61015e0001000c0001000881810281000000088291018100000008838104810100000884910381010000088500000000000003862003878002c80589500000058a50000002cb0d014170706c6520496e632e000c024d6163696e746f736800>
    | |   |       "sscOffset" = <0000>
    | |   |       "IOReportLegendPublic" = Yes
    | |   |       "reg" = <000009000000000000000000000000000000000010000902000000000000000000000000000004001400090200000000000000000000000000100000>
    | |   |       "IOPCITunnelL1Enable" = Yes
    | |   |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="NHI0 1"})
    | |   |       "device-id" = <d2150000>
    | |   |       "ThunderboltConfig" = <0102ffff04000301010004000501020003000301010001000301020004000300>
    | |   |       "revision-id" = <02000000>
    | |   |       "IOInterruptSpecifiers" = (<1000000007000000>,<2d00000000000100>)
    | |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB0@0/NHI0@0"
    | |   |     }
    | |   |     
    | |   +-o DSB1@1  <class IOPCIDevice, id 0x1000002fa, registered, matched, active, busy 0 (53 ms), retain 13>
    | |   | | {
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000"
    | |   | |   "IOPCIExpressLinkCapabilities" = 24206401
    | |   | |   "class-code" = <00040600>
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 786528
    | |   | |   "IOPCIHPType" = 48
    | |   | |   "IOChildIndex" = 2
    | |   | |   "pcidebug" = "7:1:0(67:67)"
    | |   | |   "Thunderbolt Path" = "IOService:/AppleACPIPlatformExpert/PC02@0/AppleACPIPCI/BR2D@3/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType3/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType3/IOThunderboltPort@6"
    | |   | |   "IOPCIExpressLinkStatus" = 4161
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "IODTPersist" = 0
    | |   | |   "Thunderbolt Entry ID" = 4294968479
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "AAPL,slot-name" = <"PCI Slot 1">
    | |   | |   "IOPowerManagement" = {"PowerOverrideOn"=Yes,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3,"DevicePowerState"=0,"ChildrenPowerState"=2,"CurrentPowerState"=0}
    | |   | |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "IOPCITunnelLinkChange" = Yes
    | |   | |   "compatible" = <"pci8086,15d3","pciclass,060400","DSB1">
    | |   | |   "IOReportLegendPublic" = Yes
    | |   | |   "IOPCIExpressSlotStatus" = 0
    | |   | |   "reg" = <0008070000000000000000000000000000000000>
    | |   | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="DSB1 1"})
    | |   | |   "device-id" = <d3150000>
    | |   | |   "IOPCITunnelID" = 4294968446
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "IOInterruptSpecifiers" = (<1100000007000000>,<1400000000000100>)
    | |   | |   "revision-id" = <02000000>
    | |   | |   "IOPCIMSIMode" = Yes
    | |   | | }
    | |   | | 
    | |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000002fb, retain 9>
    | |   |   | {
    | |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0"
    | |   |   | }
    | |   |   | 
    | |   |   +-o DSB0@0  <class IORegistryEntry, id 0x1000002fc, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB0@0"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x1000002fd, retain 4>
    | |   |   |     {
    | |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |     }
    | |   |   |     
    | |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x1000002fe, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o UPS0@0  <class IORegistryEntry, id 0x1000002ff, retain 9>
    | |   |   |   | {
    | |   |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0"
    | |   |   |   | }
    | |   |   |   | 
    | |   |   |   +-o DSB0@0  <class IORegistryEntry, id 0x100000300, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x100000301, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x100000302, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x100000303, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x100000304, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x100000305, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x100000306, retain 4>
    | |   |   |   |   {
    | |   |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB5@50000"
    | |   |   |   |   }
    | |   |   |   |   
    | |   |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x100000307, retain 4>
    | |   |   |       {
    | |   |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB6@60000"
    | |   |   |       }
    | |   |   |       
    | |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x100000308, retain 5>
    | |   |   | | {
    | |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000"
    | |   |   | | }
    | |   |   | | 
    | |   |   | +-o UPS0@0  <class IORegistryEntry, id 0x100000309, retain 9>
    | |   |   |   | {
    | |   |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0"
    | |   |   |   | }
    | |   |   |   | 
    | |   |   |   +-o DSB0@0  <class IORegistryEntry, id 0x10000030a, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x10000030b, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB3@30000  <class IORegistryEntry, id 0x10000030c, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x10000030d, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB4@40000  <class IORegistryEntry, id 0x10000030e, retain 5>
    | |   |   |   | | {
    | |   |   |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000"
    | |   |   |   | | }
    | |   |   |   | | 
    | |   |   |   | +-o DEV0@0  <class IORegistryEntry, id 0x10000030f, retain 4>
    | |   |   |   |     {
    | |   |   |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000/DEV0@0"
    | |   |   |   |     }
    | |   |   |   |     
    | |   |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x100000310, retain 4>
    | |   |   |   |   {
    | |   |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB5@50000"
    | |   |   |   |   }
    | |   |   |   |   
    | |   |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x100000311, retain 4>
    | |   |   |       {
    | |   |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB6@60000"
    | |   |   |       }
    | |   |   |       
    | |   |   +-o DSB5@50000  <class IORegistryEntry, id 0x100000312, retain 4>
    | |   |   |   {
    | |   |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB5@50000"
    | |   |   |   }
    | |   |   |   
    | |   |   +-o DSB6@60000  <class IORegistryEntry, id 0x100000313, retain 4>
    | |   |       {
    | |   |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB6@60000"
    | |   |       }
    | |   |       
    | |   +-o DSB2@2  <class IOPCIDevice, id 0x100000314, registered, matched, active, busy 0 (418 ms), retain 12>
    | |   | | {
    | |   | |   "IOInterruptSpecifiers" = (<1200000007000000>)
    | |   | |   "#address-cells" = <03000000>
    | |   | |   "class-code" = <00040600>
    | |   | |   "IOPCIExpressSlotStatus" = 64
    | |   | |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   | |   "built-in" = <00>
    | |   | |   "pci-aspm-default" = 0
    | |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   | |   "IOInterruptControllers" = ("io-apic-0")
    | |   | |   "PCIHotplugCapable" = 0
    | |   | |   "vendor-id" = <86800000>
    | |   | |   "IOChildIndex" = 3
    | |   | |   "device-id" = <d3150000>
    | |   | |   "IOPCIHPType" = 2
    | |   | |   "name" = <"pci-bridge">
    | |   | |   "acpi-pmcap-offset" = 128
    | |   | |   "compatible" = <"pci8086,15d3","pciclass,060400","DSB2">
    | |   | |   "ranges" = <0000008200000000000000b80000008200000000000000b80000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |   | |   "IOPCIExpressLinkCapabilities" = 40983617
    | |   | |   "IOPCIResourced" = Yes
    | |   | |   "IODTPersist" = 0
    | |   | |   "IOPCIConfigured" = Yes
    | |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB2@20000"
    | |   | |   "IOPCITunnelL1Enable" = No
    | |   | |   "revision-id" = <02000000>
    | |   | |   "IOPCIExpressLinkStatus" = 12353
    | |   | |   "IOPCIExpressCapabilities" = 354
    | |   | |   "pcidebug" = "7:2:0(8:8)"
    | |   | |   "IOName" = "pci-bridge"
    | |   | |   "#size-cells" = <02000000>
    | |   | |   "reg" = <0010070000000000000000000000000000000000>
    | |   | |   "IOPCIExpressSlotCapabilities" = 262240
    | |   | | }
    | |   | | 
    | |   | +-o XHC3@0  <class IOPCIDevice, id 0x100000315, registered, matched, active, busy 0 (366 ms), retain 13>
    | |   |   | {
    | |   |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB2@20000/XHC3@0"
    | |   |   |   "assigned-addresses" = <1000088200000000000000b80000000000000100>
    | |   |   |   "class-code" = <30030c00>
    | |   |   |   "subsystem-vendor-id" = <22220000>
    | |   |   |   "vendor-id" = <86800000>
    | |   |   |   "IOPCIExpressLinkCapabilities" = 4545601
    | |   |   |   "IOName" = "pci8086,15d4"
    | |   |   |   "IOPCIHPType" = 2
    | |   |   |   "IOChildIndex" = 1
    | |   |   |   "pcidebug" = "8:0:0"
    | |   |   |   "IOPCIExpressLinkStatus" = 4161
    | |   |   |   "pci-aspm-default" = 0
    | |   |   |   "IOPCIExpressCapabilities" = 2
    | |   |   |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |   |   |   "built-in" = <00>
    | |   |   |   "IOPCIResourced" = Yes
    | |   |   |   "IODeviceMemory" = (({"address"=3087007744,"length"=65536}))
    | |   |   |   "IOPowerManagement" = {"ChildrenPowerState"=0,"CurrentPowerState"=0,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |   |   "AAPL,xhci-clock-id" = 1
    | |   |   |   "acpi-pmcap-offset" = 128
    | |   |   |   "name" = <"pci8086,15d4">
    | |   |   |   "subsystem-id" = <11110000>
    | |   |   |   "compatible" = <"pci2222,1111","pci8086,15d4","pciclass,0c0330","XHC3">
    | |   |   |   "IOReportLegendPublic" = Yes
    | |   |   |   "reg" = <00000800000000000000000000000000000000001000080200000000000000000000000000000100>
    | |   |   |   "IOPCITunnelL1Enable" = No
    | |   |   |   "USBBusNumber" = 1
    | |   |   |   "device-id" = <d4150000>
    | |   |   |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="XHC3 1"})
    | |   |   |   "revision-id" = <02000000>
    | |   |   |   "IOInterruptSpecifiers" = (<1200000007000000>,<2c00000000000100>)
    | |   |   |   "IOPCIMSIMode" = Yes
    | |   |   | }
    | |   |   | 
    | |   |   +-o RHUB@0  <class IORegistryEntry, id 0x100000316, retain 6>
    | |   |     | {
    | |   |     |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB2@20000/XHC3@0/RHUB@0"
    | |   |     | }
    | |   |     | 
    | |   |     +-o SSP1@3  <class IORegistryEntry, id 0x100000317, retain 4>
    | |   |     |   {
    | |   |     |     "UsbCPortNumber" = 4
    | |   |     |     "kUSBWakePortCurrentLimit" = 3000
    | |   |     |     "kUSBSleepPortCurrentLimit" = 3000
    | |   |     |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB2@20000/XHC3@0/RHUB@0/SSP1@3"
    | |   |     |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     |   }
    | |   |     |   
    | |   |     +-o SSP2@4  <class IORegistryEntry, id 0x100000318, retain 4>
    | |   |         {
    | |   |           "UsbCPortNumber" = 3
    | |   |           "kUSBWakePortCurrentLimit" = 3000
    | |   |           "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |           "kUSBSleepPortCurrentLimit" = 3000
    | |   |           "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB2@20000/XHC3@0/RHUB@0/SSP2@4"
    | |   |           "UsbCompanionPortPresent" = 1
    | |   |         }
    | |   |         
    | |   +-o DSB4@4  <class IOPCIDevice, id 0x100000319, registered, matched, active, busy 0 (44 ms), retain 13>
    | |     | {
    | |     |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000"
    | |     |   "IOPCIExpressLinkCapabilities" = 74538049
    | |     |   "class-code" = <00040600>
    | |     |   "vendor-id" = <86800000>
    | |     |   "IOName" = "pci-bridge"
    | |     |   "#size-cells" = <02000000>
    | |     |   "IOPCIExpressSlotCapabilities" = 2359392
    | |     |   "IOPCIHPType" = 48
    | |     |   "IOChildIndex" = 4
    | |     |   "pcidebug" = "7:4:0(10:10)"
    | |     |   "Thunderbolt Path" = "IOService:/AppleACPIPlatformExpert/PC02@0/AppleACPIPCI/BR2D@3/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType3/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType3/IOThunderboltPort@7"
    | |     |   "IOPCIExpressLinkStatus" = 4161
    | |     |   "pci-aspm-default" = 0
    | |     |   "IOPCIExpressCapabilities" = 354
    | |     |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     |   "IOPCIConfigured" = Yes
    | |     |   "IODTPersist" = 0
    | |     |   "Thunderbolt Entry ID" = 4294968480
    | |     |   "IOPCIResourced" = Yes
    | |     |   "AAPL,slot-name" = <"PCI Slot 2">
    | |     |   "IOPowerManagement" = {"PowerOverrideOn"=Yes,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3,"DevicePowerState"=0,"ChildrenPowerState"=2,"CurrentPowerState"=0}
    | |     |   "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |     |   "acpi-pmcap-offset" = 128
    | |     |   "name" = <"pci-bridge">
    | |     |   "IOPCITunnelLinkChange" = Yes
    | |     |   "compatible" = <"pci8086,15d3","pciclass,060400","DSB4">
    | |     |   "IOReportLegendPublic" = Yes
    | |     |   "IOPCIExpressSlotStatus" = 0
    | |     |   "reg" = <0020070000000000000000000000000000000000>
    | |     |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="DSB4 1"})
    | |     |   "device-id" = <d3150000>
    | |     |   "IOPCITunnelID" = 4294968446
    | |     |   "#address-cells" = <03000000>
    | |     |   "IOInterruptSpecifiers" = (<1000000007000000>,<1500000000000100>)
    | |     |   "revision-id" = <02000000>
    | |     |   "IOPCIMSIMode" = Yes
    | |     | }
    | |     | 
    | |     +-o UPS0@0  <class IORegistryEntry, id 0x10000031a, retain 9>
    | |       | {
    | |       |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0"
    | |       | }
    | |       | 
    | |       +-o DSB0@0  <class IORegistryEntry, id 0x10000031b, retain 5>
    | |       | | {
    | |       | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB0@0"
    | |       | | }
    | |       | | 
    | |       | +-o DEV0@0  <class IORegistryEntry, id 0x10000031c, retain 4>
    | |       |     {
    | |       |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB0@0/DEV0@0"
    | |       |     }
    | |       |     
    | |       +-o DSB3@30000  <class IORegistryEntry, id 0x10000031d, retain 5>
    | |       | | {
    | |       | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000"
    | |       | | }
    | |       | | 
    | |       | +-o UPS0@0  <class IORegistryEntry, id 0x10000031e, retain 9>
    | |       |   | {
    | |       |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0"
    | |       |   | }
    | |       |   | 
    | |       |   +-o DSB0@0  <class IORegistryEntry, id 0x10000031f, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x100000320, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB0@0/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB3@30000  <class IORegistryEntry, id 0x100000321, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x100000322, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB3@30000/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB4@40000  <class IORegistryEntry, id 0x100000323, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x100000324, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB5@50000  <class IORegistryEntry, id 0x100000325, retain 4>
    | |       |   |   {
    | |       |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB5@50000"
    | |       |   |   }
    | |       |   |   
    | |       |   +-o DSB6@60000  <class IORegistryEntry, id 0x100000326, retain 4>
    | |       |       {
    | |       |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000/UPS0@0/DSB6@60000"
    | |       |       }
    | |       |       
    | |       +-o DSB4@40000  <class IORegistryEntry, id 0x100000327, retain 5>
    | |       | | {
    | |       | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000"
    | |       | | }
    | |       | | 
    | |       | +-o UPS0@0  <class IORegistryEntry, id 0x100000328, retain 9>
    | |       |   | {
    | |       |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0"
    | |       |   | }
    | |       |   | 
    | |       |   +-o DSB0@0  <class IORegistryEntry, id 0x100000329, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x10000032a, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB0@0/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB3@30000  <class IORegistryEntry, id 0x10000032b, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x10000032c, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB4@40000  <class IORegistryEntry, id 0x10000032d, retain 5>
    | |       |   | | {
    | |       |   | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   | |   "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000"
    | |       |   | | }
    | |       |   | | 
    | |       |   | +-o DEV0@0  <class IORegistryEntry, id 0x10000032e, retain 4>
    | |       |   |     {
    | |       |   |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |       "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB4@40000/DEV0@0"
    | |       |   |     }
    | |       |   |     
    | |       |   +-o DSB5@50000  <class IORegistryEntry, id 0x10000032f, retain 4>
    | |       |   |   {
    | |       |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |   |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB5@50000"
    | |       |   |   }
    | |       |   |   
    | |       |   +-o DSB6@60000  <class IORegistryEntry, id 0x100000330, retain 4>
    | |       |       {
    | |       |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |         "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB4@40000/UPS0@0/DSB6@60000"
    | |       |       }
    | |       |       
    | |       +-o DSB5@50000  <class IORegistryEntry, id 0x100000331, retain 4>
    | |       |   {
    | |       |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB5@50000"
    | |       |   }
    | |       |   
    | |       +-o DSB6@60000  <class IORegistryEntry, id 0x100000332, retain 4>
    | |           {
    | |             "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |             "acpi-path" = "IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB4@40000/UPS0@0/DSB6@60000"
    | |           }
    | |           
    | +-o pci8086,2034@5  <class IOPCIDevice, id 0x100000373, registered, matched, active, busy 0 (66 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2034","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2034"
    | |     "reg" = <0028050000000000000000000000000000000000>
    | |     "device-id" = <34200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 146
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:5:0"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2034">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2035@5,2  <class IOPCIDevice, id 0x100000374, registered, matched, active, busy 0 (75 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,2035","pciclass,088000">
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOName" = "pci8086,2035"
    | |     "reg" = <002a050000000000000000000000000000000000>
    | |     "device-id" = <35200000>
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 146
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:5:2"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2035">
    | |   }
    | |   
    | +-o pci8086,2036@5,4  <class IOPCIDevice, id 0x100000376, registered, matched, active, busy 0 (71 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,2036","pciclass,080020">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2036"
    | |     "reg" = <002c050000000000000000000000000000000000102c050200000000000000000000000000100000>
    | |     "device-id" = <36200000>
    | |     "assigned-addresses" = <102c058200000000000000900000000000100000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIExpressCapabilities" = 145
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "IODeviceMemory" = (({"address"=2415919104,"length"=4096}))
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:5:4"
    | |     "class-code" = <20000800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "subsystem-id" = <36200000>
    | |     "name" = <"pci8086,2036">
    | |   }
    | |   
    | +-o M2M0@8  <class IOPCIDevice, id 0x100000333, registered, matched, active, busy 0 (88 ms), retain 9>
    | |   {
    | |     "class-code" = <00800800>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "name" = <"pci8086,2066">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <66200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2066","pciclass,088000","M2M0">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/M2M0@80000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 145
    | |     "pcidebug" = "5:8:0"
    | |     "IOName" = "pci8086,2066"
    | |     "reg" = <0040050000000000000000000000000000000000>
    | |   }
    | |   
    | +-o M2M1@9  <class IOPCIDevice, id 0x100000334, registered, matched, active, busy 0 (78 ms), retain 9>
    | |   {
    | |     "class-code" = <00800800>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "name" = <"pci8086,2066">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <66200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2066","pciclass,088000","M2M1">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/M2M1@90000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 145
    | |     "pcidebug" = "5:9:0"
    | |     "IOName" = "pci8086,2066"
    | |     "reg" = <0048050000000000000000000000000000000000>
    | |   }
    | |   
    | +-o MCM0@A  <class IOPCIDevice, id 0x100000335, registered, matched, active, busy 0 (87 ms), retain 9>
    | |   {
    | |     "class-code" = <00800800>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "name" = <"pci8086,2040">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <40200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2040","pciclass,088000","MCM0">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/MCM0@a0000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 145
    | |     "pcidebug" = "5:10:0"
    | |     "IOName" = "pci8086,2040"
    | |     "reg" = <0050050000000000000000000000000000000000>
    | |   }
    | |   
    | +-o pci8086,2041@A,1  <class IOPCIDevice, id 0x100000379, registered, matched, active, busy 0 (84 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2041","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2041"
    | |     "reg" = <0051050000000000000000000000000000000000>
    | |     "device-id" = <41200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:10:1"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2041">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2042@A,2  <class IOPCIDevice, id 0x10000037a, registered, matched, active, busy 0 (100 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2042","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2042"
    | |     "reg" = <0052050000000000000000000000000000000000>
    | |     "device-id" = <42200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:10:2"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2042">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2043@A,3  <class IOPCIDevice, id 0x10000037b, registered, matched, active, busy 0 (96 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2043","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2043"
    | |     "reg" = <0053050000000000000000000000000000000000>
    | |     "device-id" = <43200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:10:3"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2043">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2044@A,4  <class IOPCIDevice, id 0x10000037c, registered, matched, active, busy 0 (91 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2044","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2044"
    | |     "reg" = <0054050000000000000000000000000000000000>
    | |     "device-id" = <44200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:10:4"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2044">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2045@A,5  <class IOPCIDevice, id 0x10000037d, registered, matched, active, busy 0 (93 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2045","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2045"
    | |     "reg" = <0055050000000000000000000000000000000000>
    | |     "device-id" = <45200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:10:5"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2045">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2046@A,6  <class IOPCIDevice, id 0x10000037e, registered, matched, active, busy 0 (106 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2046","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2046"
    | |     "reg" = <0056050000000000000000000000000000000000>
    | |     "device-id" = <46200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:10:6"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2046">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2047@A,7  <class IOPCIDevice, id 0x10000037f, registered, matched, active, busy 0 (102 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2047","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2047"
    | |     "reg" = <0057050000000000000000000000000000000000>
    | |     "device-id" = <47200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:10:7"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2047">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o MCD0@B  <class IOPCIDevice, id 0x100000336, registered, matched, active, busy 0 (103 ms), retain 9>
    | |   {
    | |     "class-code" = <00800800>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "name" = <"pci8086,2048">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <48200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2048","pciclass,088000","MCD0">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/MCD0@b0000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 145
    | |     "pcidebug" = "5:11:0"
    | |     "IOName" = "pci8086,2048"
    | |     "reg" = <0058050000000000000000000000000000000000>
    | |   }
    | |   
    | +-o pci8086,2049@B,1  <class IOPCIDevice, id 0x100000380, registered, matched, active, busy 0 (103 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2049","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2049"
    | |     "reg" = <0059050000000000000000000000000000000000>
    | |     "device-id" = <49200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:11:1"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2049">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,204a@B,2  <class IOPCIDevice, id 0x100000381, registered, matched, active, busy 0 (95 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,204a","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,204a"
    | |     "reg" = <005a050000000000000000000000000000000000>
    | |     "device-id" = <4a200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:11:2"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,204a">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,204b@B,3  <class IOPCIDevice, id 0x100000382, registered, matched, active, busy 0 (104 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,204b","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,204b"
    | |     "reg" = <005b050000000000000000000000000000000000>
    | |     "device-id" = <4b200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:11:3"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,204b">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o MCM1@C  <class IOPCIDevice, id 0x100000337, registered, matched, active, busy 0 (97 ms), retain 9>
    | |   {
    | |     "class-code" = <00800800>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "name" = <"pci8086,2040">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <40200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2040","pciclass,088000","MCM1">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/MCM1@c0000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 145
    | |     "pcidebug" = "5:12:0"
    | |     "IOName" = "pci8086,2040"
    | |     "reg" = <0060050000000000000000000000000000000000>
    | |   }
    | |   
    | +-o pci8086,2041@C,1  <class IOPCIDevice, id 0x100000383, registered, matched, active, busy 0 (127 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2041","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2041"
    | |     "reg" = <0061050000000000000000000000000000000000>
    | |     "device-id" = <41200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:12:1"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2041">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2042@C,2  <class IOPCIDevice, id 0x100000384, registered, matched, active, busy 0 (105 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2042","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2042"
    | |     "reg" = <0062050000000000000000000000000000000000>
    | |     "device-id" = <42200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:12:2"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2042">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2043@C,3  <class IOPCIDevice, id 0x100000385, registered, matched, active, busy 0 (114 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2043","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2043"
    | |     "reg" = <0063050000000000000000000000000000000000>
    | |     "device-id" = <43200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:12:3"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2043">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2044@C,4  <class IOPCIDevice, id 0x100000386, registered, matched, active, busy 0 (113 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2044","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2044"
    | |     "reg" = <0064050000000000000000000000000000000000>
    | |     "device-id" = <44200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:12:4"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2044">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2045@C,5  <class IOPCIDevice, id 0x100000387, registered, matched, active, busy 0 (102 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2045","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2045"
    | |     "reg" = <0065050000000000000000000000000000000000>
    | |     "device-id" = <45200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:12:5"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2045">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2046@C,6  <class IOPCIDevice, id 0x100000388, registered, matched, active, busy 0 (113 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2046","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2046"
    | |     "reg" = <0066050000000000000000000000000000000000>
    | |     "device-id" = <46200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:12:6"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2046">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2047@C,7  <class IOPCIDevice, id 0x100000389, registered, matched, active, busy 0 (109 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2047","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2047"
    | |     "reg" = <0067050000000000000000000000000000000000>
    | |     "device-id" = <47200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:12:7"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2047">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o MCD1@D  <class IOPCIDevice, id 0x100000338, registered, matched, active, busy 0 (113 ms), retain 9>
    | |   {
    | |     "class-code" = <00800800>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "name" = <"pci8086,2048">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <48200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,2048","pciclass,088000","MCD1">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC02@0/MCD1@d0000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 145
    | |     "pcidebug" = "5:13:0"
    | |     "IOName" = "pci8086,2048"
    | |     "reg" = <0068050000000000000000000000000000000000>
    | |   }
    | |   
    | +-o pci8086,2049@D,1  <class IOPCIDevice, id 0x10000038a, registered, matched, active, busy 0 (116 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2049","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2049"
    | |     "reg" = <0069050000000000000000000000000000000000>
    | |     "device-id" = <49200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:13:1"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2049">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,204a@D,2  <class IOPCIDevice, id 0x10000038b, registered, matched, active, busy 0 (114 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,204a","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,204a"
    | |     "reg" = <006a050000000000000000000000000000000000>
    | |     "device-id" = <4a200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 145
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "5:13:2"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,204a">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,204b@D,3  <class IOPCIDevice, id 0x10000038c, registered, matched, active, busy 0 (126 ms), retain 9>
    |     {
    |       "pci-aspm-default" = 0
    |       "compatible" = <"pci8086,0","pci8086,204b","pciclass,088000">
    |       "subsystem-vendor-id" = <86800000>
    |       "IOName" = "pci8086,204b"
    |       "reg" = <006b050000000000000000000000000000000000>
    |       "device-id" = <4b200000>
    |       "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    |       "IOPCIResourced" = Yes
    |       "IOPCIExpressCapabilities" = 145
    |       "revision-id" = <04000000>
    |       "vendor-id" = <86800000>
    |       "pcidebug" = "5:13:3"
    |       "class-code" = <00800800>
    |       "IOPCIExpressLinkCapabilities" = 0
    |       "IOPCIExpressLinkStatus" = 0
    |       "name" = <"pci8086,204b">
    |       "subsystem-id" = <00000000>
    |     }
    |     
    +-o PC03@0  <class IOACPIPlatformDevice, id 0x100000263, registered, matched, active, busy 0 (6039 ms), retain 33>
    | | {
    | |   "compatible" = <"PNP0A03">
    | |   "IODTPersist" = 0
    | |   "_STA" = 15
    | |   "IOPCIConfigured" = Yes
    | |   "acpi-address-spaces" = <020000000000000000000000000000000000000000000000f000000000000000f5000000000000000000000000000000060000000000000000000000000000000000000000000000000000000000000001000000000000000000000000000000000000000000000000e0000000000000ffff00000000000000000000000000000020000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000e000000000fffffffb0000000000000000000000000000001c00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000c080000000ffffffff8000000000000000000000000000004000000000000000000000000000000000000000000000000000000000>
    | |   "#size-cells" = <02000000>
    | |   "_UID" = "3"
    | |   "#address-cells" = <03000000>
    | |   "acpi-pci-routing-table" = <1800000000000000ffff00000000000010000000000000001800000000000000ffff01000000000010000000000000001800000000000000ffff02000000000010000000000000001800000000000000ffff03000000000010000000000000001800000000000000ffff0e000000000010000000000000001800000001000000ffff0e000000000011000000000000001800000002000000ffff0e000000000012000000000000001800000003000000ffff0e000000000013000000000000001800000000000000ffff0f000000000010000000000000001800000001000000ffff0f000000000011000000000000001800000002000000ffff0f000000000012000000000000001800000003000000ffff0f000000000013000000000000001800000000000000ffff10000000000010000000000000001800000001000000ffff10000000000011000000000000001800000002000000ffff10000000000012000000000000001800000003000000ffff10000000000013000000000000001800000000000000ffff12000000000010000000000000001800000001000000ffff12000000000011000000000000001800000002000000ffff12000000000012000000000000001800000003000000ffff12000000000013000000000000001800000000000000ffff15000000000010000000000000001800000001000000ffff15000000000011000000000000001800000002000000ffff15000000000012000000000000001800000003000000ffff15000000000013000000000000001800000000000000ffff16000000000010000000000000001800000001000000ffff16000000000011000000000000001800000002000000ffff16000000000012000000000000001800000003000000ffff16000000000013000000000000001800000000000000ffff17000000000010000000000000001800000001000000ffff17000000000011000000000000001800000002000000ffff17000000000012000000000000001800000003000000ffff1700000000001300000000000000000000000000000000000000000000000000000000000000>
    | |   "device-properties" = {"acpi-device"="IOACPIPlatformDevice is not serializable","acpi-path"="IOACPIPlane:/_SB/PC03@0"}
    | |   "_ADR" = 0
    | |   "acpi-path" = "IOACPIPlane:/_SB/PC03@0"
    | |   "name" = <"PNP0A08">
    | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | }
    | | 
    | +-o KTI0@e0000  <class IORegistryEntry, id 0x100000341, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC03@0/KTI0@e0000"
    | |   }
    | |   
    | +-o KTI1@f0000  <class IORegistryEntry, id 0x100000342, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC03@0/KTI1@f0000"
    | |   }
    | |   
    | +-o KTI2@100000  <class IORegistryEntry, id 0x100000343, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC03@0/KTI2@100000"
    | |   }
    | |   
    | +-o BR3A@0  <class IOPCIDevice, id 0x10000033b, registered, matched, active, busy 0 (5987 ms), retain 12>
    | | | {
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <80000000>
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "name" = <"pci-bridge">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <30200000>
    | | |   "acpi-pmcap-offset" = 224
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci80,0","pci8086,2030","pciclass,060400","BR3A">
    | | |   "ranges" = <0000008200000000000020f00000008200000000000020f00000000000002000000000c280000000000000c0000000c280000000000000c00000000000002010000000810000000000e00000000000810000000000e000000000000000100000>
    | | |   "IOPCIExpressLinkCapabilities" = 159004931
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PC03@0/BR3A@0"
    | | |   "subsystem-id" = <00000000>
    | | |   "revision-id" = <04000000>
    | | |   "IOPCIExpressLinkStatus" = 12547
    | | |   "IOPCIExpressCapabilities" = 66
    | | |   "pcidebug" = "240:0:0(241:243)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <0000f00000000000000000000000000000000000>
    | | | }
    | | | 
    | | +-o EGP0@0  <class IOPCIDevice, id 0x10000033c, registered, matched, active, busy 0 (5904 ms), retain 12>
    | |   | {
    | |   |   "assigned-addresses" = <1000f18200000000000030f00000000000400000>
    | |   |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | |   |   "#address-cells" = <03000000>
    | |   |   "class-code" = <00040600>
    | |   |   "IODeviceMemory" = (({"address"=4029677568,"length"=16384}))
    | |   |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |   |   "subsystem-vendor-id" = <80000000>
    | |   |   "built-in" = <00>
    | |   |   "pci-aspm-default" = 0
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "IOInterruptControllers" = ("io-apic-0")
    | |   |   "name" = <"pci-bridge">
    | |   |   "vendor-id" = <22100000>
    | |   |   "device-id" = <70140000>
    | |   |   "IOChildIndex" = 1
    | |   |   "acpi-pmcap-offset" = 80
    | |   |   "IOPCIResourced" = Yes
    | |   |   "compatible" = <"pci80,0","pci1022,1470","pciclass,060400","EGP0">
    | |   |   "ranges" = <0000008200000000000020f00000008200000000000020f00000000000001000000000c280000000000000c0000000c280000000000000c00000000000002010000000810000000000e00000000000810000000000e000000000000000100000>
    | |   |   "IOPCIExpressLinkCapabilities" = 4667651
    | |   |   "IODTPersist" = 0
    | |   |   "IOPCIConfigured" = Yes
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PC03@0/BR3A@0/EGP0@0"
    | |   |   "subsystem-id" = <00000000>
    | |   |   "revision-id" = <00000000>
    | |   |   "IOPCIExpressLinkStatus" = 4355
    | |   |   "IOPCIExpressCapabilities" = 82
    | |   |   "pcidebug" = "241:0:0(242:243)"
    | |   |   "IOName" = "pci-bridge"
    | |   |   "#size-cells" = <02000000>
    | |   |   "reg" = <0000f100000000000000000000000000000000001000f10200000000000000000000000000400000>
    | |   | }
    | |   | 
    | |   +-o EGP1@0  <class IOPCIDevice, id 0x10000033d, registered, matched, active, busy 0 (5769 ms), retain 13>
    | |     | {
    | |     |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | |     |   "#address-cells" = <03000000>
    | |     |   "class-code" = <00040600>
    | |     |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     |   "subsystem-vendor-id" = <80000000>
    | |     |   "built-in" = <00>
    | |     |   "pci-aspm-default" = 0
    | |     |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     |   "IOInterruptControllers" = ("io-apic-0")
    | |     |   "name" = <"pci-bridge">
    | |     |   "IOChildIndex" = 1
    | |     |   "device-id" = <71140000>
    | |     |   "vendor-id" = <22100000>
    | |     |   "acpi-pmcap-offset" = 80
    | |     |   "IOPCIResourced" = Yes
    | |     |   "compatible" = <"pci80,0","pci1022,1471","pciclass,060400","EGP1">
    | |     |   "ranges" = <0000008200000000000020f00000008200000000000020f00000000000001000000000c280000000000000c0000000c280000000000000c00000000000002010000000810000000000e00000000000810000000000e000000000000000100000>
    | |     |   "IOPCIExpressLinkCapabilities" = 7343363
    | |     |   "IODTPersist" = 0
    | |     |   "IOPCIConfigured" = Yes
    | |     |   "acpi-path" = "IOACPIPlane:/_SB/PC03@0/BR3A@0/EGP0@0/EGP1@0"
    | |     |   "subsystem-id" = <00000000>
    | |     |   "revision-id" = <00000000>
    | |     |   "IOPCIExpressLinkStatus" = 12547
    | |     |   "IOPCIExpressCapabilities" = 98
    | |     |   "pcidebug" = "242:0:0(243:243)"
    | |     |   "IOName" = "pci-bridge"
    | |     |   "#size-cells" = <02000000>
    | |     |   "reg" = <0000f20000000000000000000000000000000000>
    | |     | }
    | |     | 
    | |     +-o GFX0@0  <class IOPCIDevice, id 0x10000033e, registered, matched, active, busy 0 (5710 ms), retain 64>
    | |     | | {
    | |     | |   "IOPCIMSIMode" = Yes
    | |     | |   "CFG_USE_STUTTER" = Yes
    | |     | |   "PP_StaticMappingInfo14" = <a0000000>
    | |     | |   "CFG_NO_MST" = No
    | |     | |   "PP_DiDtSQStallPatternOverride" = 16383
    | |     | |   "ATY,SCLK" = 851990
    | |     | |   "device-id" = <67680000>
    | |     | |   "compatible" = <"pci106b,17b","pci1002,6867","pciclass,030000","GFX0">
    | |     | |   "ATY,RevID" = 18446744073709551615
    | |     | |   "CFG_USE_FBC" = No
    | |     | |   "DALReadDelayStutterOff" = 4
    | |     | |   "CFG_GEN_FLAGS" = 0
    | |     | |   "IOPCIExpressLinkStatus" = 4355
    | |     | |   "CFG_FORCE_MAX_DPS" = No
    | |     | |   "PP_StaticMappingInfo28" = <00a0b6d3>
    | |     | |   "IOName" = "display"
    | |     | |   "ATY,EFIVersionROMBL" = <000b0d00>
    | |     | |   "CFG_FB_LIMIT" = 0
    | |     | |   "ATY,vram_base" = <00000000f4000000>
    | |     | |   "revision-id" = <00000000>
    | |     | |   "IOPCIExpressCapabilities" = 18
    | |     | |   "PP_StaticMappingInfo7" = <01000000>
    | |     | |   "ATY,EFI-dpcd-DPPreferBitRate" = <f0d20000>
    | |     | |   "IOPCIResourced" = Yes
    | |     | |   "CFG_USE_SRRB" = No
    | |     | |   "pci-bus-number" = 243
    | |     | |   "ATY,PlatformInfo" = <>
    | |     | |   "CAIL_EnableXdmaSupport" = 0
    | |     | |   "PP_StaticMappingInfo2" = <20030000>
    | |     | |   "ATY,MemVendorID" = <0100>
    | |     | |   "subsystem-vendor-id" = <6b100000>
    | |     | |   "CFG_CAA" = 0
    | |     | |   "PP_StaticMappingInfo23" = <f4000000>
    | |     | |   "reg" = <0000f300000000000000000000000000000000001000f342000000000000000000000000000000101800f342000000000000000000000000000020002000f301000000000000000000000000000100002400f302000000000000000000000000000008003000f30200000000000000000000000000000200>
    | |     | |   "ATY,MCLK" = 785990
    | |     | |   "PP_ACDCGpioDisabled" = 0
    | |     | |   "IOBusyInterest" = "IOCommand is not serializable"
    | |     | |   "ATY,EFIVersionE" = <"113-D0500D-981">
    | |     | |   "ATY,EFIBootMode" = <00000100020000000000010001000000000000000000000000000000000000000000000000000000000000010000000000010000000300000050cfcd1c00000000000a0000400b0000a00000000000000000000000520000000000000000000000300000002000000000030000000a000000000000000100020000000000000000000000000000000000000000000a0000000000000000010000000000010000000300000050cfcd1c00000000000a0000400b0000a00000000000000000000000520000000000000000000000300000002000000000030000000a000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000100000000000100000003000000108fec370000000000140000400b0000a0000000000000000000000052000000000000000000000030000000200000000003000000050000000000>
    | |     | |   "PP_StaticMappingInfo15" = <a3ffffff>
    | |     | |   "CAIL_EnableLBPWSupport" = 0
    | |     | |   "iofb_no_regptr" = Yes
    | |     | |   "ATY,EFIBKM" = <03>
    | |     | |   "ATY,EFIVersion" = <"01.00.981">
    | |     | |   "ATY,EFICompileDate" = <"Sep 26 2017">
    | |     | |   "CFG_PULSE_INT" = Yes
    | |     | |   "PP_StaticMappingInfo10" = <0050aed3>
    | |     | |   "PP_StaticMappingInfo29" = <f4000000>
    | |     | |   "ATY,AsicSubSystemID" = <7b01>
    | |     | |   "CFG_NON_ZERO_MC_LOC" = Yes
    | |     | |   "acpi-pmcap-offset" = 80
    | |     | |   "ATY,EFIOrientation" = <0001>
    | |     | |   "IOInterruptSpecifiers" = (<1000000007000000>,<2a00000000000100>)
    | |     | |   "PP_StaticMappingInfo9" = <a3ffffff>
    | |     | |   "PP_RefreshRate" = <3c000000>
    | |     | |   "ATY,EFIEnabledMode" = <04>
    | |     | |   "pci-aspm-default" = 0
    | |     | |   "PP_StaticMappingInfo4" = <0030aed3>
    | |     | |   "PP_StaticMappingInfo24" = <00602000>
    | |     | |   "ATY,RefCLK" = <8c0a0000>
    | |     | |   "StartupDisplay" = <474e02000000000000140000400b0000108fec370000000000140000400b0000a0000000000000000000000052000000000000000000000030000000200000000300000005000000000000000000000000000002000000000000000010061eae0100000000000000000a0000400b000050cfcd1c00000000000a0000400b0000a000000000000000000000005200000000000000000000003000000020000000030000000a0000000000000000000000000a00000000000010061eae0200000000000000000a0000400b000050cfcd1c00000000000a0000400b0000a000000000000000000000005200000000000000000000003000000020000000030000000a0000000000000000000000>
    | |     | |   "name" = <"ATY,JapuraParent">
    | |     | |   "CFG_USE_CP2" = Yes
    | |     | |   "built-in" = <00>
    | |     | |   "PP_StaticMappingInfo16" = <0070aed3>
    | |     | |   "ATY,Card#" = <"102-D05001-00">
    | |     | |   "ATY,EFIFBSize" = <0000840300000000>
    | |     | |   "acpi-path" = "IOACPIPlane:/_SB/PC03@0/BR3A@0/EGP0@0/EGP1@0/GFX0@0"
    | |     | |   "vendor-id" = <02100000>
    | |     | |   "CFG_USE_SWIP" = Yes
    | |     | |   "PP_DisableClockStretcher" = 1
    | |     | |   "model" = <"Radeon Pro Vega 56">
    | |     | |   "PP_StaticMappingInfo11" = <f4000000>
    | |     | |   "ATY,EFI-dpcd-training-result" = <148400000000001001>
    | |     | |   "ATY,EFILinebytes" = <00500000>
    | |     | |   "subsystem-id" = <7b010000>
    | |     | |   "assigned-addresses" = <1000f3c280000000000000c000000000000000101800f3c280000000000000d000000000000020002000f3810000000000e0000000000000000100002400f38200000000000020f000000000000008003000f38200000000000028f00000000000000200>
    | |     | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     | |   "ATY,EFIVersionROMMC" = <"02.30.09.02">
    | |     | |   "PP_PhmUseDummyBackEnd" = 0
    | |     | |   "hda-gfx" = <"onboard-1">
    | |     | |   "PP_StaticMappingInfo6" = <00002000>
    | |     | |   "PP_StaticMappingInfo25" = <01000000>
    | |     | |   "ATY,EFIVersionB" = <"113-D05001A1XL-017">
    | |     | |   "CFG_TRANS_WSRV" = Yes
    | |     | |   "PP_StaticMappingInfo1" = <01000000>
    | |     | |   "CFG_INT_SSPC" = 25
    | |     | |   "IODeviceMemory" = (({"address"=552977039360,"length"=268435456}),({"address"=553245474816,"length"=2097152}),"IOSubMemoryDescriptor is not serializable",({"address"=4028628992,"length"=524288}),({"address"=4029153280,"length"=131072}))
    | |     | |   "E" = <00000000>
    | |     | |   "ATY,AsicRevID" = <00000000>
    | |     | |   "ATY,PageFlipEnable" = <01000000>
    | |     | |   "pcidebug" = "243:0:0"
    | |     | |   "PP_StaticMappingInfo17" = <f4000000>
    | |     | |   "CFG_NO_MSI" = No
    | |     | |   "PP_StaticMappingInfo20" = <00000800>
    | |     | |   "LoadAMDSupport" = Yes
    | |     | |   "VRAM,totalMB" = 8176
    | |     | |   "CFG_PAA" = 0
    | |     | |   "PP_PhmSoftWTTable" = <5802cf02a700170200000000d0028813a7001702010000005802cf021802881302000000d002881318028813030000005802ac02a700170200000000ad028813a7001702010000005802ac021802881302000000ad028813180288130300000000000000000000000000000000000000000000000000000000000000>
    | |     | |   "PP_BootupDisplayState" = <01000000>
    | |     | |   "ATY,DeviceID" = <"gh">
    | |     | |   "PP_StaticMappingInfo12" = <00202000>
    | |     | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     | |   "IOChildIndex" = 1
    | |     | |   "PP_DisablePPTuning" = 1
    | |     | |   "IOPMIsPowerManaged" = Yes
    | |     | |   "PP_DisableAVFS" = 0
    | |     | |   "PP_StaticMappingInfo8" = <7c000000>
    | |     | |   "PP_StaticMappingInfo26" = <80000000>
    | |     | |   "CFG_USE_REGAMMA" = Yes
    | |     | |   "pci-function-number" = 0
    | |     | |   "CFG_NO_SLS" = No
    | |     | |   "PP_StaticMappingInfo3" = <a3ffffff>
    | |     | |   "PP_ToolsLogSpaceSize" = 524288
    | |     | |   "ATY,Copyright" = <"Copyright AMD Inc. All Rights Reserved. 2005-2017">
    | |     | |   "device_type" = <"ATY,JapuraParent">
    | |     | |   "ATY,Rom#" = <"113-D0500D-981">
    | |     | |   "CFG_NO_PP" = No
    | |     | |   "PP_DisableDIDT" = 0
    | |     | |   "ATY,EFIFBOffset" = <0000300000000000>
    | |     | |   "class-code" = <00000300>
    | |     | |   "PP_DisableULV" = 1
    | |     | |   "IOPCIExpressLinkCapabilities" = 4459779
    | |     | |   "ATY,bin_image" = <[encoded data, 131072 characters]>
    | |     | |   "PP_StaticMappingInfo21" = <a3ffffff>
    | |     | |   "PP_StaticMappingInfo18" = <00402000>
    | |     | |   "CFG_USE_DPT" = Yes
    | |     | |   "CFG_USE_FEDS" = Yes
    | |     | |   "ATY,memsize" = 8573157376
    | |     | |   "IOHibernateState" = <00000000>
    | |     | |   "PP_DiDtSQPatternWidthOverride" = 14
    | |     | |   "CFG_PTPL2_TBL" = <d2000000cc000000c6000000c0000000ba000000b4000000aa000000a0000000960000008c00000082000000780000006e000000640000005a0000001e000000>
    | |     | |   "CFG_USE_AGDC" = Yes
    | |     | |   "ATY,remap-size" = 2097152
    | |     | |   "PP_StaticMappingInfo13" = <01000000>
    | |     | |   "pci-device-number" = 0
    | |     | |   "CFG_APER_MODE" = 1
    | |     | |   "ATY,MemRevisionID" = <0000>
    | |     | |   "PP_VBlankTime" = <cd010000>
    | |     | |   "AsicOnLowPower" = <00000000>
    | |     | |   "LoadController" = Yes
    | |     | |   "PP_StaticMappingInfo30" = <00702800>
    | |     | |   "PP_StaticMappingInfo27" = <a3ffffff>
    | |     | |   "CAIL_EnableSecureMmFwLoading" = 1
    | |     | |   "CAIL_DisableCailLoadUcode" = 1
    | |     | |   "LoadAccelerator" = Yes
    | |     | |   "PP_Falcon_QuickTransition_Enable" = 1
    | |     | |   "PP_StaticMappingInfo5" = <f4000000>
    | |     | |   "PP_DisableACG" = 1
    | |     | |   "CFG_NODM" = Yes
    | |     | |   "CFG_NO_HDCP" = No
    | |     | |   "CFG_FORCEMAXDPM" = No
    | |     | |   "ATY,EFI-dpcd-post-training" = <777781000000>
    | |     | |   "CFG_NVV" = 2
    | |     | |   "CAIL_EnablePeerDataAperture" = 0
    | |     | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |     | |   "attached-gpu-control-path" = "IOService:/AppleACPIPlatformExpert/PC03@0/AppleACPIPCI/BR3A@0/IOPP/EGP0@0/IOPP/EGP1@0/IOPP/GFX0@0/ATY,Japura@0/AMDFramebufferVega10/AGPM"
    | |     | |   "ATY,VendorID" = <0210>
    | |     | |   "PP_StaticMappingInfo22" = <0090aed3>
    | |     | |   "PP_StaticMappingInfo19" = <01000000>
    | |     | |   "DALUseUrgencyWaterMarkOffset" = 0
    | |     | |   "ATY,EFIVersionROMB" = <"113-D05001A1XL-017">
    | |     | |   "ATY,EFIDriverType" = <02>
    | |     | |   "CFG_USE_LPT" = No
    | |     | |   "CAIL_DisableJpegEngine" = 0
    | |     | | }
    | |     | | 
    | |     | +-o LCD@110  <class IORegistryEntry, id 0x10000033f, retain 4>
    | |     | |   {
    | |     | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     | |     "acpi-path" = "IOACPIPlane:/_SB/PC03@0/BR3A@0/EGP0@0/EGP1@0/GFX0@0/LCD@110"
    | |     | |   }
    | |     | |   
    | |     | +-o ATY,Japura@0  <class AtiFbStub, id 0x100000642, registered, matched, active, busy 0 (86 ms), retain 8>
    | |     | |   {
    | |     | |     "DPLinkRate" = <f0d20000>
    | |     | |     "AAPL,boot-display" = <01000000>
    | |     | |     "ATY,ActiveFlags" = 256
    | |     | |     "audio-codec-info" = <00010d00>
    | |     | |     "AAPL,gray-page" = <01000000>
    | |     | |     "connector-type" = 2
    | |     | |     "dpcd-post-training" = <777701010000>
    | |     | |     "IOFBDependentID" = 4294968126
    | |     | |     "name" = "ATY,Japura"
    | |     | |     "ATY,ControlFlags" = 256
    | |     | |     "DPLinkBit" = <1e000000>
    | |     | |     "display-connect-flags" = <04000000>
    | |     | |     "display-pixel-component-bits" = <0a000000>
    | |     | |     "compatible" = <"ATY,Japura">
    | |     | |     "DPLanes" = <04000000>
    | |     | |     "av-signal-type" = <10000000>
    | |     | |     "IOFBDependentIndex" = 0
    | |     | |     "AAPL,gray-value" = <00000000>
    | |     | |     "display-bpc" = <0a000000>
    | |     | |     "display-type" = "LCD"
    | |     | |     "port-number" = 0
    | |     | |     "dpcd-registers" = <1214c40101000180020104010f00010000000000000000000000000000000000000001000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000014840000000000100108000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000410077770101000000000000000000000d800e800e800f80000a000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001a415449774c00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010fa4d4e32376831100102520200000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000>
    | |     | |     "device_type" = "display"
    | |     | |     "ATY,EFIDisplay" = <"DP1">
    | |     | |     "display-link-component-bits" = <0a000000>
    | |     | |   }
    | |     | |   
    | |     | +-o ATY,Japura@1  <class AtiFbStub, id 0x100000643, registered, matched, active, busy 0 (0 ms), retain 8>
    | |     | |   {
    | |     | |     "DPLinkRate" = <f0d20000>
    | |     | |     "ATY,ActiveFlags" = 256
    | |     | |     "audio-codec-info" = <00010b00>
    | |     | |     "AAPL,gray-page" = <01000000>
    | |     | |     "connector-type" = 2
    | |     | |     "dpcd-post-training" = <777701010000>
    | |     | |     "IOFBDependentID" = 4294968126
    | |     | |     "name" = "ATY,Japura"
    | |     | |     "ATY,ControlFlags" = 256
    | |     | |     "DPLinkBit" = <1e000000>
    | |     | |     "display-connect-flags" = <00000000>
    | |     | |     "display-pixel-component-bits" = <0a000000>
    | |     | |     "compatible" = <"ATY,Japura">
    | |     | |     "DPLanes" = <04000000>
    | |     | |     "av-signal-type" = <10000000>
    | |     | |     "IOFBDependentIndex" = 1
    | |     | |     "AAPL,gray-value" = <00000000>
    | |     | |     "display-bpc" = <0a000000>
    | |     | |     "display-type" = "LCD"
    | |     | |     "port-number" = 1
    | |     | |     "dpcd-registers" = <1214c40101000180020104010f0001000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001484000000000010010800000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000041007777010100000000000000000000108010800f800c80000a000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001a415449774c00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010fa4d4e32376831100102520000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000>
    | |     | |     "device_type" = "display"
    | |     | |     "display-link-component-bits" = <0a000000>
    | |     | |   }
    | |     | |   
    | |     | +-o ATY,Japura@2  <class AtiFbStub, id 0x100000644, registered, matched, active, busy 0 (0 ms), retain 8>
    | |     | |   {
    | |     | |     "display-type" = "NONE"
    | |     | |     "compatible" = <"ATY,Japura">
    | |     | |     "connector-type" = 1024
    | |     | |     "ATY,ActiveFlags" = 1
    | |     | |     "IOFBDependentIndex" = 2
    | |     | |     "audio-codec-info" = <00010500>
    | |     | |     "IOFBDependentID" = 4294968126
    | |     | |     "ATY,ControlFlags" = 772
    | |     | |     "AAPL,gray-page" = <01000000>
    | |     | |     "device_type" = "display"
    | |     | |     "av-signal-type" = <00000000>
    | |     | |     "AAPL,gray-value" = <00000000>
    | |     | |     "display-connect-flags" = <00000000>
    | |     | |     "name" = "ATY,Japura"
    | |     | |     "port-number" = 2
    | |     | |   }
    | |     | |   
    | |     | +-o ATY,Japura@3  <class AtiFbStub, id 0x100000645, registered, matched, active, busy 0 (0 ms), retain 8>
    | |     | |   {
    | |     | |     "display-type" = "NONE"
    | |     | |     "compatible" = <"ATY,Japura">
    | |     | |     "connector-type" = 1024
    | |     | |     "ATY,ActiveFlags" = 1
    | |     | |     "IOFBDependentIndex" = 3
    | |     | |     "audio-codec-info" = <00010300>
    | |     | |     "IOFBDependentID" = 4294968126
    | |     | |     "ATY,ControlFlags" = 772
    | |     | |     "AAPL,gray-page" = <01000000>
    | |     | |     "device_type" = "display"
    | |     | |     "av-signal-type" = <00000000>
    | |     | |     "AAPL,gray-value" = <00000000>
    | |     | |     "display-connect-flags" = <00000000>
    | |     | |     "name" = "ATY,Japura"
    | |     | |     "port-number" = 3
    | |     | |   }
    | |     | |   
    | |     | +-o ATY,Japura@4  <class AtiFbStub, id 0x100000646, registered, matched, active, busy 0 (0 ms), retain 8>
    | |     | |   {
    | |     | |     "display-type" = "NONE"
    | |     | |     "compatible" = <"ATY,Japura">
    | |     | |     "connector-type" = 1024
    | |     | |     "ATY,ActiveFlags" = 1
    | |     | |     "IOFBDependentIndex" = 4
    | |     | |     "audio-codec-info" = <00010700>
    | |     | |     "IOFBDependentID" = 4294968126
    | |     | |     "ATY,ControlFlags" = 772
    | |     | |     "AAPL,gray-page" = <01000000>
    | |     | |     "device_type" = "display"
    | |     | |     "av-signal-type" = <00000000>
    | |     | |     "AAPL,gray-value" = <00000000>
    | |     | |     "display-connect-flags" = <00000000>
    | |     | |     "name" = "ATY,Japura"
    | |     | |     "port-number" = 4
    | |     | |   }
    | |     | |   
    | |     | +-o ATY,Japura@5  <class AtiFbStub, id 0x100000647, registered, matched, active, busy 0 (0 ms), retain 8>
    | |     |     {
    | |     |       "display-type" = "NONE"
    | |     |       "compatible" = <"ATY,Japura">
    | |     |       "connector-type" = 1024
    | |     |       "ATY,ActiveFlags" = 1
    | |     |       "IOFBDependentIndex" = 5
    | |     |       "audio-codec-info" = <00010900>
    | |     |       "IOFBDependentID" = 4294968126
    | |     |       "ATY,ControlFlags" = 772
    | |     |       "AAPL,gray-page" = <01000000>
    | |     |       "device_type" = "display"
    | |     |       "av-signal-type" = <00000000>
    | |     |       "AAPL,gray-value" = <00000000>
    | |     |       "display-connect-flags" = <00000000>
    | |     |       "name" = "ATY,Japura"
    | |     |       "port-number" = 5
    | |     |     }
    | |     |     
    | |     +-o HDAU@0,1  <class IOPCIDevice, id 0x100000340, registered, matched, active, busy 0 (1513 ms), retain 11>
    | |         {
    | |           "assigned-addresses" = <1001f3820000000000002af00000000000400000>
    | |           "IOInterruptSpecifiers" = (<1100000007000000>,<2b00000000000100>)
    | |           "class-code" = <00030400>
    | |           "IODeviceMemory" = (({"address"=4029284352,"length"=16384}))
    | |           "IOReportLegendPublic" = Yes
    | |           "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |           "subsystem-vendor-id" = <02100000>
    | |           "built-in" = <00>
    | |           "pci-aspm-default" = 0
    | |           "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |           "hda-gfx" = <"onboard-1">
    | |           "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |           "IOPCIMSIMode" = Yes
    | |           "name" = <"pci1002,aaf8">
    | |           "IOChildIndex" = 2
    | |           "device-id" = <f8aa0000>
    | |           "vendor-id" = <02100000>
    | |           "acpi-pmcap-offset" = 80
    | |           "IOPCIResourced" = Yes
    | |           "compatible" = <"pci1002,aaf8","pciclass,040300","HDAU">
    | |           "layout-id" = <00000000>
    | |           "IOPCIExpressLinkCapabilities" = 4459779
    | |           "acpi-path" = "IOACPIPlane:/_SB/PC03@0/BR3A@0/EGP0@0/EGP1@0/HDAU@1"
    | |           "subsystem-id" = <f8aa0000>
    | |           "revision-id" = <00000000>
    | |           "IOPCIExpressLinkStatus" = 4355
    | |           "IOPCIExpressCapabilities" = 2
    | |           "pcidebug" = "243:0:1"
    | |           "IOName" = "pci1002,aaf8"
    | |           "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="HDAU 1"})
    | |           "reg" = <0001f300000000000000000000000000000000001001f30200000000000000000000000000400000>
    | |         }
    | |         
    | +-o pci8086,2034@5  <class IOPCIDevice, id 0x100000394, registered, matched, active, busy 0 (79 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,0","pci8086,2034","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2034"
    | |     "reg" = <0028f00000000000000000000000000000000000>
    | |     "device-id" = <34200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 146
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "240:5:0"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2034">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,2035@5,2  <class IOPCIDevice, id 0x100000395, registered, matched, active, busy 0 (84 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,2035","pciclass,088000">
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOName" = "pci8086,2035"
    | |     "reg" = <002af00000000000000000000000000000000000>
    | |     "device-id" = <35200000>
    | |     "IOPCIResourced" = Yes
    | |     "IOPCIExpressCapabilities" = 146
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "240:5:2"
    | |     "class-code" = <00800800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "name" = <"pci8086,2035">
    | |   }
    | |   
    | +-o pci8086,2036@5,4  <class IOPCIDevice, id 0x100000396, registered, matched, active, busy 0 (94 ms), retain 9>
    | |   {
    | |     "pci-aspm-default" = 0
    | |     "compatible" = <"pci8086,2036","pciclass,080020">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2036"
    | |     "reg" = <002cf00000000000000000000000000000000000102cf00200000000000000000000000000100000>
    | |     "device-id" = <36200000>
    | |     "assigned-addresses" = <102cf08200000000000040f00000000000100000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIExpressCapabilities" = 145
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "IODeviceMemory" = (({"address"=4030726144,"length"=4096}))
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "240:5:4"
    | |     "class-code" = <20000800>
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "subsystem-id" = <36200000>
    | |     "name" = <"pci8086,2036">
    | |   }
    | |   
    | +-o M3K0@12  <class IOPCIDevice, id 0x100000344, registered, matched, active, busy 0 (90 ms), retain 9>
    | |   {
    | |     "class-code" = <00011100>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "subsystem-vendor-id" = <86800000>
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "name" = <"pci8086,204c">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <4c200000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci8086,0","pci8086,204c","pciclass,110100","M3K0">
    | |     "IOPCIExpressLinkCapabilities" = 0
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC03@0/M3K0@120000"
    | |     "subsystem-id" = <00000000>
    | |     "revision-id" = <04000000>
    | |     "IOPCIExpressLinkStatus" = 0
    | |     "IOPCIExpressCapabilities" = 146
    | |     "pcidebug" = "240:18:0"
    | |     "IOName" = "pci8086,204c"
    | |     "reg" = <0090f00000000000000000000000000000000000>
    | |   }
    | |   
    | +-o pci8086,204d@12,1  <class IOPCIDevice, id 0x100000398, registered, matched, active, busy 0 (104 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,204d","pciclass,110100">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,204d"
    | |     "reg" = <0091f00000000000000000000000000000000000>
    | |     "device-id" = <4d200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "240:18:1"
    | |     "class-code" = <00011100>
    | |     "name" = <"pci8086,204d">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o pci8086,204e@12,2  <class IOPCIDevice, id 0x100000399, registered, matched, active, busy 0 (98 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,204e","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,204e"
    | |     "reg" = <0092f00000000000000000000000000000000000>
    | |     "device-id" = <4e200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "240:18:2"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,204e">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o M2U0@15  <class IOPCIDevice, id 0x100000345, registered, matched, active, busy 0 (99 ms), retain 9>
    | |   {
    | |     "name" = <"pci8086,2018">
    | |     "compatible" = <"pci8086,0","pci8086,2018","pciclass,088000","M2U0">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2018"
    | |     "reg" = <00a8f00000000000000000000000000000000000>
    | |     "device-id" = <18200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "240:21:0"
    | |     "class-code" = <00800800>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC03@0/M2U0@150000"
    | |     "subsystem-id" = <00000000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o M2D0@16  <class IOPCIDevice, id 0x100000346, registered, matched, active, busy 0 (92 ms), retain 9>
    | |   {
    | |     "name" = <"pci8086,2018">
    | |     "compatible" = <"pci8086,0","pci8086,2018","pciclass,088000","M2D0">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2018"
    | |     "reg" = <00b0f00000000000000000000000000000000000>
    | |     "device-id" = <18200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "240:22:0"
    | |     "class-code" = <00800800>
    | |     "acpi-path" = "IOACPIPlane:/_SB/PC03@0/M2D0@160000"
    | |     "subsystem-id" = <00000000>
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   }
    | |   
    | +-o pci8086,2018@16,4  <class IOPCIDevice, id 0x10000039a, registered, matched, active, busy 0 (100 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci8086,0","pci8086,2018","pciclass,088000">
    | |     "subsystem-vendor-id" = <86800000>
    | |     "IOName" = "pci8086,2018"
    | |     "reg" = <00b4f00000000000000000000000000000000000>
    | |     "device-id" = <18200000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <04000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "240:22:4"
    | |     "class-code" = <00800800>
    | |     "name" = <"pci8086,2018">
    | |     "subsystem-id" = <00000000>
    | |   }
    | |   
    | +-o M20@17  <class IOPCIDevice, id 0x100000347, registered, matched, active, busy 0 (105 ms), retain 9>
    |     {
    |       "compatible" = <"pci8086,2018","pciclass,088000","M20">
    |       "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    |       "IOName" = "pci8086,2018"
    |       "reg" = <00b8f00000000000000000000000000000000000>
    |       "device-id" = <18200000>
    |       "built-in" = <00>
    |       "IOPCIResourced" = Yes
    |       "revision-id" = <04000000>
    |       "vendor-id" = <86800000>
    |       "pcidebug" = "240:23:0"
    |       "class-code" = <00800800>
    |       "acpi-path" = "IOACPIPlane:/_SB/PC03@0/M20@170000"
    |       "name" = <"pci8086,2018">
    |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |     }
    |     
    +-o PNLF@0  <class IOACPIPlatformDevice, id 0x100000272, registered, matched, active, busy 0 (1694 ms), retain 10>
    |   {
    |     "refnum" = 0
    |     "compatible" = <"backlight">
    |     "acpi-path" = "IOACPIPlane:/_SB/PNLF@0"
    |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |     "_UID" = "16"
    |     "device-properties" = {"acpi-path"="IOACPIPlane:/_SB/PNLF@0","acpi-device"="IOACPIPlatformDevice is not serializable","type"=1228030720,"refnum"=0,"version"=3}
    |     "version" = 3
    |     "_STA" = 11
    |     "type" = 1228030720
    |     "_ADR" = 0
    |     "name" = <"APP0002">
    |   }
    |   
    +-o SLPB  <class IOACPIPlatformDevice, id 0x100000273, registered, matched, active, busy 0 (3 ms), retain 8>
    |   {
    |     "name" = <"PNP0C0E">
    |     "_STA" = 11
    |   }
    |   
    +-o options  <class AppleEFINVRAM, id 0x10000035f, registered, matched, active, busy 0 (0 ms), retain 8>
        {
          "display-config" = <000025017308ffff0100>
          "bluetoothInternalControllerInfo" = <7b00ac05000000008c859094532b>
          "fmm-computer-name" = <"iMac Pro - C02VV5RFHX87 - ars180.21">
          "fmm-mobileme-token-FMM" = <62706c6973743030dc0102030405060708090a0b0c0d0e100d110d12131415161d5f100f756e726567697374657253746174655f1012656e61626c656444617461636c61737365735961757468546f6b656e5e64697361626c65436f6e74657874567573657269645d656e61626c65436f6e7465787458757365726e616d6558706572736f6e49445761646454696d6554677569645875736572496e666f5f101364617461636c61737350726f706572746965731000a10f5f1021636f6d2e6170706c652e44617461636c6173732e4465766963654c6f6361746f725f1028415141414141426152442d327a586b49576365615650392d754842637262386c50514d4e67436b7e1101f65f10116172733138302e3231406d61632e636f6d593136373333363733362341d6910fef17f45e5f102436444442394243362d384535322d344431322d383346442d314136363846454532303941d31718191a1b1c5f1015496e5573654f776e6572446973706c61794e616d655f1013496e5573654f776e657246697273744e616d655f1012496e5573654f776e65724c6173744e616d655e4a6f686e204170706c6573656564544a6f686e594170706c6573656564d10f1ed41f2021222324252656617073456e7658686f73746e616d655d617574684d656368616e69736d56736368656d655a50726f64756374696f6e5f10137033392d666d69702e69636c6f75642e636f6d55746f6b656e55687474707300080021003300480052006100680076007f008800900095009e00b400b600b800dc0107010a011e012801310158015f0177018d01a201b101b601c001c301cc01d301dc01ea01f101fc02120218000000000000020100000000000000270000000000000000000000000000021e>
          "bluetoothActiveControllerInfo" = <7b00ac050000000000008c859094532b>
          "backlight-level" = <ffff>
          "BridgeOSVersion" = <"15.16.2064.0.0,0">
          "enable-remap-mode" = <"true">
          "LocationServicesEnabled" = <01>
          "usb-cr-rec" = <01000000>
          "EFIBluetoothDelay" = <b80b>
        }
        
