[
{"data":{"title":"assigned-addresses"},"attr":{"id":"38046","ColType":"Data","ColValue":"&lt;1000088200000000000000b80000000000000100&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"38048","ColType":"String","ColValue":"8:0:0"}},
{"data":{"title":"IOPCITunnelL1Enable"},"attr":{"id":"38050","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"38052","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"38054","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38055","ColType":"Data","ColValue":"&lt;1200000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"38056","ColType":"Data","ColValue":"&lt;2c00000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"38058","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB2@20000/XHC3@0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"38060","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"38062","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38063","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"38064","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"USBBusNumber"},"attr":{"id":"38066","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"38068","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"38070","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"38072","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"38074","ColType":"Data","ColValue":"&lt;22220000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"38076","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"38078","ColType":"Data","ColValue":"&lt;\"pci8086,15d4\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"38080","ColType":"Number","ColValue":"2"}},
{"data":{"title":"compatible"},"attr":{"id":"38082","ColType":"Data","ColValue":"&lt;\"pci2222,1111\",\"pci8086,15d4\",\"pciclass,0c0330\",\"XHC3\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"38084","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"38086","ColType":"Number","ColValue":"0"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"38088","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"38090","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"38092","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"38094","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"38096","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"38098","ColType":"Number","ColValue":"4545601"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"38100","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AAPL,xhci-clock-id"},"attr":{"id":"38102","ColType":"Number","ColValue":"1"}},
{"data":{"title":"built-in"},"attr":{"id":"38104","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"38106","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"38108","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38109","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38110","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"38112","ColType":"Number","ColValue":"3087007744"}},{"data":{"title":"length"},"attr":{"id":"38114","ColType":"Number","ColValue":"65536"}}]}]}]},
{"data":{"title":"IOName"},"attr":{"id":"38116","ColType":"String","ColValue":"pci8086,15d4"}},
{"data":{"title":"acpi-device"},"attr":{"id":"38118","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"38120","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"38122","ColType":"Data","ColValue":"&lt;11110000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"38124","ColType":"Data","ColValue":"&lt;00000800000000000000000000000000000000001000080200000000000000000000000000000100&gt;"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"38126","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38127","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"38129","ColType":"String","ColValue":"XHC3 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"38131","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38132","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38133","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"38134","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38135","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"38136","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38137","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"38138","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38139","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"38140","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38141","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"38142","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38143","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"38144","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38145","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"38146","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38147","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"38148","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"38149","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"38150","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"38151","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"38153","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"38155","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"38157","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"38159","ColType":"Data","ColValue":"&lt;30030c00&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"38161","ColType":"Data","ColValue":"&lt;d4150000&gt;"}}
]
