[
{"data":{"title":"_STA"},"attr":{"id":"5550","ColType":"Number","ColValue":"15"}},
{"data":{"title":"_ADR"},"attr":{"id":"5552","ColType":"Number","ColValue":"0"}},
{"data":{"title":"device-properties"},"attr":{"id":"5554","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-path"},"attr":{"id":"5556","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000/UPS0@0/DSB4@40000/UPS0@0/DSB3@30000/DEV0@0"}},{"data":{"title":"acpi-device"},"attr":{"id":"5558","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}}]}
]
