[
{"data":{"title":"built-in"},"attr":{"id":"31023","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"31025","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31026","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31027","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"31029","ColType":"Number","ColValue":"549775937536"}},{"data":{"title":"length"},"attr":{"id":"31031","ColType":"Number","ColValue":"4096"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"31033","ColType":"Data","ColValue":"&lt;a7a20000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"31035","ColType":"Data","ColValue":"&lt;\"pci8086,a2a7\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"31037","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/URT0@1e0000"}},
{"data":{"title":"IOName"},"attr":{"id":"31039","ColType":"String","ColValue":"pci8086,a2a7"}},
{"data":{"title":"vendor-id"},"attr":{"id":"31041","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"31043","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"31045","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"acpi-device"},"attr":{"id":"31047","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"31049","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"31051","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31052","ColType":"String","ColValue":"io-apic-0"}}]},
{"data":{"title":"IOReportLegend"},"attr":{"id":"31054","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31055","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"31057","ColType":"String","ColValue":"URT0 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"31059","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31060","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31061","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"31062","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"31063","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"31064","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31065","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"31066","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"31067","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"31068","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31069","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"31070","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"31071","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"31072","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31073","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"31074","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"31075","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"31076","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31077","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"31078","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"31079","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"31081","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"31083","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"31085","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pcidebug"},"attr":{"id":"31087","ColType":"String","ColValue":"0:30:0"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"31089","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"31091","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"31093","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"31095","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"31097","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"31099","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"31101","ColType":"Data","ColValue":"&lt;00801100&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"31103","ColType":"Data","ColValue":"&lt;\"pci8086,7270\",\"pci8086,a2a7\",\"pciclass,118000\",\"URT0\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"31105","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"uart-channel-number"},"attr":{"id":"31107","ColType":"Data","ColValue":"&lt;0000000000000000&gt;"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"31109","ColType":"Data","ColValue":"&lt;70720000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"31111","ColType":"Data","ColValue":"&lt;10f0008280000000001033010000000000100000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"31113","ColType":"Data","ColValue":"&lt;00f000000000000000000000000000000000000010f0000200000000000000000000000000100000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"31115","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"31116","ColType":"Data","ColValue":"&lt;1400000007000000&gt;"}}]}
]
