[
{"data":{"title":"IOPCITunnelLinkChange"},"attr":{"id":"36500","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"ranges"},"attr":{"id":"36502","ColType":"Data","ColValue":"&lt;0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"36504","ColType":"String","ColValue":"124:4:0(127:127)"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"36506","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"36508","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36509","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"36510","ColType":"Data","ColValue":"&lt;0d00000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"36512","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000"}},
{"data":{"title":"Thunderbolt Path"},"attr":{"id":"36514","ColType":"String","ColValue":"IOService:/AppleACPIPlatformExpert/PC02@0/AppleACPIPCI/BR2C@2/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType3/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType3/IOThunderboltPort@7"}},
{"data":{"title":"IOPCIExpressSlotCapabilities"},"attr":{"id":"36516","ColType":"Number","ColValue":"2359392"}},
{"data":{"title":"IOPCIExpressSlotStatus"},"attr":{"id":"36518","ColType":"Number","ColValue":"0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"36520","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"36522","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36523","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"36524","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"36526","ColType":"Number","ColValue":"354"}},
{"data":{"title":"AAPL,slot-name"},"attr":{"id":"36528","ColType":"Data","ColValue":"&lt;\"PCI Slot 2\"&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"36530","ColType":"Number","ColValue":"4"}},
{"data":{"title":"IOPCITunnelID"},"attr":{"id":"36532","ColType":"Number","ColValue":"4294968415"}},
{"data":{"title":"IOPCIConfigured"},"attr":{"id":"36534","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"36536","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IODTPersist"},"attr":{"id":"36538","ColType":"Number","ColValue":"0"}},
{"data":{"title":"#size-cells"},"attr":{"id":"36540","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"36542","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"36544","ColType":"Data","ColValue":"&lt;\"pci-bridge\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"36546","ColType":"Number","ColValue":"48"}},
{"data":{"title":"compatible"},"attr":{"id":"36548","ColType":"Data","ColValue":"&lt;\"pci8086,15d3\",\"pciclass,060400\",\"DSB4\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"36550","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"DevicePowerState"},"attr":{"id":"36552","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"36554","ColType":"Number","ColValue":"0"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"36556","ColType":"Number","ColValue":"0"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"36558","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"36560","ColType":"Number","ColValue":"2"}},{"data":{"title":"PowerOverrideOn"},"attr":{"id":"36562","ColType":"Boolean","ColValue":"Yes"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"36564","ColType":"Number","ColValue":"2"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"36566","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"36568","ColType":"Number","ColValue":"74538049"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"36570","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"36572","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"#address-cells"},"attr":{"id":"36574","ColType":"Data","ColValue":"&lt;03000000&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"36576","ColType":"String","ColValue":"pci-bridge"}},
{"data":{"title":"acpi-device"},"attr":{"id":"36578","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"36580","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"reg"},"attr":{"id":"36582","ColType":"Data","ColValue":"&lt;00207c0000000000000000000000000000000000&gt;"}},
{"data":{"title":"Thunderbolt Entry ID"},"attr":{"id":"36584","ColType":"Number","ColValue":"4294968472"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"36586","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36587","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"36589","ColType":"String","ColValue":"DSB4 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"36591","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36592","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36593","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"36594","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36595","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"36596","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36597","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"36598","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36599","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"36600","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36601","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"36602","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36603","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"36604","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36605","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"36606","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36607","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"36608","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36609","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"36610","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36611","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"36613","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"36615","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"36617","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"36619","ColType":"Data","ColValue":"&lt;00040600&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"36621","ColType":"Data","ColValue":"&lt;d3150000&gt;"}}
]
