[
{"data":{"title":"IOPCITunnelLinkChange"},"attr":{"id":"35730","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"ranges"},"attr":{"id":"35732","ColType":"Data","ColValue":"&lt;0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"35734","ColType":"String","ColValue":"124:1:0(184:184)"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"35736","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"35738","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35739","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"35740","ColType":"Data","ColValue":"&lt;0c00000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"35742","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB1@10000"}},
{"data":{"title":"Thunderbolt Path"},"attr":{"id":"35744","ColType":"String","ColValue":"IOService:/AppleACPIPlatformExpert/PC02@0/AppleACPIPCI/BR2C@2/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType3/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType3/IOThunderboltPort@6"}},
{"data":{"title":"IOPCIExpressSlotCapabilities"},"attr":{"id":"35746","ColType":"Number","ColValue":"786528"}},
{"data":{"title":"IOPCIExpressSlotStatus"},"attr":{"id":"35748","ColType":"Number","ColValue":"0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"35750","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"35752","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35753","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"35754","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"35756","ColType":"Number","ColValue":"354"}},
{"data":{"title":"AAPL,slot-name"},"attr":{"id":"35758","ColType":"Data","ColValue":"&lt;\"PCI Slot 1\"&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"35760","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCITunnelID"},"attr":{"id":"35762","ColType":"Number","ColValue":"4294968415"}},
{"data":{"title":"IOPCIConfigured"},"attr":{"id":"35764","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"35766","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IODTPersist"},"attr":{"id":"35768","ColType":"Number","ColValue":"0"}},
{"data":{"title":"#size-cells"},"attr":{"id":"35770","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"35772","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"35774","ColType":"Data","ColValue":"&lt;\"pci-bridge\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"35776","ColType":"Number","ColValue":"48"}},
{"data":{"title":"compatible"},"attr":{"id":"35778","ColType":"Data","ColValue":"&lt;\"pci8086,15d3\",\"pciclass,060400\",\"DSB1\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"35780","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"DevicePowerState"},"attr":{"id":"35782","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"35784","ColType":"Number","ColValue":"0"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"35786","ColType":"Number","ColValue":"0"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"35788","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"35790","ColType":"Number","ColValue":"2"}},{"data":{"title":"PowerOverrideOn"},"attr":{"id":"35792","ColType":"Boolean","ColValue":"Yes"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"35794","ColType":"Number","ColValue":"2"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"35796","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"35798","ColType":"Number","ColValue":"24206401"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"35800","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"35802","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"#address-cells"},"attr":{"id":"35804","ColType":"Data","ColValue":"&lt;03000000&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"35806","ColType":"String","ColValue":"pci-bridge"}},
{"data":{"title":"acpi-device"},"attr":{"id":"35808","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"35810","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"reg"},"attr":{"id":"35812","ColType":"Data","ColValue":"&lt;00087c0000000000000000000000000000000000&gt;"}},
{"data":{"title":"Thunderbolt Entry ID"},"attr":{"id":"35814","ColType":"Number","ColValue":"4294968471"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"35816","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35817","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"35819","ColType":"String","ColValue":"DSB1 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"35821","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35822","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35823","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"35824","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35825","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"35826","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35827","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"35828","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35829","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"35830","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35831","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"35832","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35833","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"35834","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35835","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"35836","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35837","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"35838","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35839","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"35840","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"35841","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"35843","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"35845","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"35847","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"35849","ColType":"Data","ColValue":"&lt;00040600&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"35851","ColType":"Data","ColValue":"&lt;d3150000&gt;"}}
]
