[
{"data":{"title":"IOReportLegend"},"attr":{"id":"4913","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4914","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"4916","ColType":"String","ColValue":"PWRB 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"4918","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4919","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4920","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"4921","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4922","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"4923","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4924","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"4925","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4926","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"4927","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4928","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"4929","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4930","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"4931","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4932","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"4933","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4934","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"4935","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4936","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"4937","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4938","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"4940","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"4942","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"4944","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"4946","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4947","ColType":"Data","ColValue":"&lt;0200000000000000&gt;"}}]},
{"data":{"title":"acpi-wake-type"},"attr":{"id":"4949","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"4951","ColType":"Data","ColValue":"&lt;\"PNP0C0C\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"4953","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"4955","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4956","ColType":"String","ColValue":"ACPIEventController"}}]},
{"data":{"title":"_STA"},"attr":{"id":"4958","ColType":"Number","ColValue":"18446744073709551615"}}
]
