[
{"data":{"title":"_STA"},"attr":{"id":"6196","ColType":"Number","ColValue":"15"}},
{"data":{"title":"_ADR"},"attr":{"id":"6198","ColType":"Number","ColValue":"0"}},
{"data":{"title":"device-properties"},"attr":{"id":"6200","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-path"},"attr":{"id":"6202","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000/UPS0@0/DSB3@30000/UPS0@0/DSB4@40000/DEV0@0"}},{"data":{"title":"acpi-device"},"attr":{"id":"6204","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}}]}
]
