[
{"data":{"title":"_STA"},"attr":{"id":"5620","ColType":"Number","ColValue":"15"}},
{"data":{"title":"_ADR"},"attr":{"id":"5622","ColType":"Number","ColValue":"131072"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5624","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"MaxPowerState"},"attr":{"id":"5626","ColType":"Number","ColValue":"2"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"5628","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5630","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"device-properties"},"attr":{"id":"5632","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-device"},"attr":{"id":"5634","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},{"data":{"title":"acpi-path"},"attr":{"id":"5636","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB2@20000"}},{"data":{"title":"PCIHotplugCapable"},"attr":{"id":"5638","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"acpi-pci-pm"},"attr":{"id":"5640","ColType":"Boolean","ColValue":"Yes"}}
]
