[
{"data":{"title":"assigned-addresses"},"attr":{"id":"36100","ColType":"Data","ColValue":"&lt;10007d8200000000000010900000000000000100&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"36102","ColType":"String","ColValue":"125:0:0"}},
{"data":{"title":"IOPCITunnelL1Enable"},"attr":{"id":"36104","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"36106","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"36108","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36109","ColType":"Data","ColValue":"&lt;1200000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"36110","ColType":"Data","ColValue":"&lt;2900000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"36112","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB2@20000/XHC2@0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"36114","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"36116","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36117","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"36118","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"USBBusNumber"},"attr":{"id":"36120","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"36122","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"36124","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"36126","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"36128","ColType":"Data","ColValue":"&lt;22220000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"36130","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"36132","ColType":"Data","ColValue":"&lt;\"pci8086,15d4\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"36134","ColType":"Number","ColValue":"2"}},
{"data":{"title":"compatible"},"attr":{"id":"36136","ColType":"Data","ColValue":"&lt;\"pci2222,1111\",\"pci8086,15d4\",\"pciclass,0c0330\",\"XHC2\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"36138","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"36140","ColType":"Number","ColValue":"0"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"36142","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"36144","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"36146","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"36148","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"36150","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"36152","ColType":"Number","ColValue":"4545601"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"36154","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AAPL,xhci-clock-id"},"attr":{"id":"36156","ColType":"Number","ColValue":"1"}},
{"data":{"title":"built-in"},"attr":{"id":"36158","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"36160","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"36162","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36163","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36164","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"36166","ColType":"Number","ColValue":"2416967680"}},{"data":{"title":"length"},"attr":{"id":"36168","ColType":"Number","ColValue":"65536"}}]}]}]},
{"data":{"title":"IOName"},"attr":{"id":"36170","ColType":"String","ColValue":"pci8086,15d4"}},
{"data":{"title":"acpi-device"},"attr":{"id":"36172","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"36174","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"36176","ColType":"Data","ColValue":"&lt;11110000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"36178","ColType":"Data","ColValue":"&lt;00007d000000000000000000000000000000000010007d0200000000000000000000000000000100&gt;"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"36180","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36181","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"36183","ColType":"String","ColValue":"XHC2 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"36185","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36186","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36187","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"36188","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36189","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"36190","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36191","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"36192","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36193","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"36194","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36195","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"36196","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36197","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"36198","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36199","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"36200","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36201","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"36202","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36203","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"36204","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36205","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"36207","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"36209","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"36211","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"36213","ColType":"Data","ColValue":"&lt;30030c00&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"36215","ColType":"Data","ColValue":"&lt;d4150000&gt;"}}
]
