[
{"data":{"title":"built-in"},"attr":{"id":"4403","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"4405","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4406","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4407","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"4409","ColType":"Number","ColValue":"549775736832"}},{"data":{"title":"length"},"attr":{"id":"4411","ColType":"Number","ColValue":"65536"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"4413","ColType":"Number","ColValue":"112"}},
{"data":{"title":"device-id"},"attr":{"id":"4415","ColType":"Data","ColValue":"&lt;afa20000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"4417","ColType":"Data","ColValue":"&lt;\"pci8086,a2af\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"4419","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/XHC1@140000"}},
{"data":{"title":"IOName"},"attr":{"id":"4421","ColType":"String","ColValue":"pci8086,a2af"}},
{"data":{"title":"vendor-id"},"attr":{"id":"4423","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"4425","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"4427","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"acpi-device"},"attr":{"id":"4429","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"4431","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"4433","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4434","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"4435","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOReportLegend"},"attr":{"id":"4437","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4438","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"4440","ColType":"String","ColValue":"XHC1 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"4442","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4443","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4444","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"4445","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4446","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"4447","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4448","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"4449","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4450","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"4451","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4452","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"4453","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4454","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"4455","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4456","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"4457","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4458","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"4459","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4460","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"4461","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"4462","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"4464","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"4466","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"4468","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pcidebug"},"attr":{"id":"4470","ColType":"String","ColValue":"0:20:0"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"4472","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"4474","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"4476","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"4478","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"4480","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"4482","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"4484","ColType":"Data","ColValue":"&lt;30030c00&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"4486","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"4488","ColType":"Data","ColValue":"&lt;\"pci8086,7270\",\"pci8086,a2af\",\"pciclass,0c0330\",\"XHC1\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"4490","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"4492","ColType":"Data","ColValue":"&lt;70720000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"4494","ColType":"Data","ColValue":"&lt;10a0008280000000000030010000000000000100&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"4496","ColType":"Data","ColValue":"&lt;00a000000000000000000000000000000000000010a0000200000000000000000000000000000100&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"4498","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4499","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"4500","ColType":"Data","ColValue":"&lt;0a00000000000100&gt;"}}]}
]
