[
{"data":{"title":"_STA"},"attr":{"id":"5756","ColType":"Number","ColValue":"15"}},
{"data":{"title":"_ADR"},"attr":{"id":"5758","ColType":"Number","ColValue":"196608"}},
{"data":{"title":"device-properties"},"attr":{"id":"5760","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-path"},"attr":{"id":"5762","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB4@40000/UPS0@0/DSB3@30000"}},{"data":{"title":"acpi-device"},"attr":{"id":"5764","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}}]}
]
