[
{"data":{"title":"assigned-addresses"},"attr":{"id":"10419","ColType":"Data","ColValue":"&lt;1000088200000000000000b80000000000000100&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"10421","ColType":"String","ColValue":"8:0:0"}},
{"data":{"title":"IOPCITunnelL1Enable"},"attr":{"id":"10423","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"10425","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"10427","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10428","ColType":"Data","ColValue":"&lt;1200000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"10429","ColType":"Data","ColValue":"&lt;2c00000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"10431","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB2@20000/XHC3@0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"10433","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"10435","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10436","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"10437","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"USBBusNumber"},"attr":{"id":"10439","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"10441","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"10443","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"10445","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"10447","ColType":"Data","ColValue":"&lt;22220000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"10449","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"10451","ColType":"Data","ColValue":"&lt;\"pci8086,15d4\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"10453","ColType":"Number","ColValue":"2"}},
{"data":{"title":"compatible"},"attr":{"id":"10455","ColType":"Data","ColValue":"&lt;\"pci2222,1111\",\"pci8086,15d4\",\"pciclass,0c0330\",\"XHC3\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"10457","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"10459","ColType":"Number","ColValue":"0"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"10461","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"10463","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"10465","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"10467","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"10469","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"10471","ColType":"Number","ColValue":"4545601"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"10473","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AAPL,xhci-clock-id"},"attr":{"id":"10475","ColType":"Number","ColValue":"1"}},
{"data":{"title":"built-in"},"attr":{"id":"10477","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"10479","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"10481","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10482","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10483","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"10485","ColType":"Number","ColValue":"3087007744"}},{"data":{"title":"length"},"attr":{"id":"10487","ColType":"Number","ColValue":"65536"}}]}]}]},
{"data":{"title":"IOName"},"attr":{"id":"10489","ColType":"String","ColValue":"pci8086,15d4"}},
{"data":{"title":"acpi-device"},"attr":{"id":"10491","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"10493","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"10495","ColType":"Data","ColValue":"&lt;11110000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"10497","ColType":"Data","ColValue":"&lt;00000800000000000000000000000000000000001000080200000000000000000000000000000100&gt;"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"10499","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10500","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"10502","ColType":"String","ColValue":"XHC3 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"10504","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10505","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10506","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"10507","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10508","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"10509","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10510","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"10511","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10512","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"10513","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10514","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"10515","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10516","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"10517","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10518","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"10519","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10520","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"10521","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10522","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"10523","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10524","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"10526","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"10528","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"10530","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"10532","ColType":"Data","ColValue":"&lt;30030c00&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"10534","ColType":"Data","ColValue":"&lt;d4150000&gt;"}}
]
