[
{"data":{"title":"_STA"},"attr":{"id":"4487","ColType":"Number","ColValue":"15"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"4489","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4490","ColType":"Data","ColValue":"&lt;1400000007000000&gt;"}}]},
{"data":{"title":"_ADR"},"attr":{"id":"4492","ColType":"Number","ColValue":"1966080"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"4494","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"4495","ColType":"String","ColValue":"io-apic-0"}}]},
{"data":{"title":"device-properties"},"attr":{"id":"4497","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"acpi-device"},"attr":{"id":"4499","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},{"data":{"title":"uart-channel-number"},"attr":{"id":"4501","ColType":"Data","ColValue":"&lt;0000000000000000&gt;"}},{"data":{"title":"acpi-path"},"attr":{"id":"4503","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/URT0@1e0000"}}]}
]
