[
{"data":{"title":"built-in"},"attr":{"id":"5767","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"5769","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5770","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5771","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5773","ColType":"Number","ColValue":"549775900672"}},{"data":{"title":"length"},"attr":{"id":"5775","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"5777","ColType":"Data","ColValue":"&lt;21200000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"5779","ColType":"Data","ColValue":"&lt;\"pci8086,2021\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"5781","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/CB0B@40001"}},
{"data":{"title":"IOName"},"attr":{"id":"5783","ColType":"String","ColValue":"pci8086,2021"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5785","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5787","ColType":"Data","ColValue":"&lt;04000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"5789","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5791","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5793","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5795","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5796","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"5797","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5799","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5801","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"5803","ColType":"String","ColValue":"0:4:1"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"5805","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"5807","ColType":"Number","ColValue":"146"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5809","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5811","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5813","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5815","ColType":"Number","ColValue":"3"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5817","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"5819","ColType":"Data","ColValue":"&lt;00800800&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"5821","ColType":"Data","ColValue":"&lt;\"pci8086,0\",\"pci8086,2021\",\"pciclass,088000\",\"CB0B\"&gt;"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"5823","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"5825","ColType":"Data","ColValue":"&lt;1021008280000000008032010000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"5827","ColType":"Data","ColValue":"&lt;00210000000000000000000000000000000000001021000200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"5829","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5830","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"5831","ColType":"Data","ColValue":"&lt;0400000000000100&gt;"}}]}
]
