[
{"data":{"title":"built-in"},"attr":{"id":"12896","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"12898","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12899","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12900","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"12902","ColType":"Number","ColValue":"4029284352"}},{"data":{"title":"length"},"attr":{"id":"12904","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"12906","ColType":"Number","ColValue":"80"}},
{"data":{"title":"layout-id"},"attr":{"id":"12908","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"hda-gfx"},"attr":{"id":"12910","ColType":"Data","ColValue":"&lt;\"onboard-1\"&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"12912","ColType":"Data","ColValue":"&lt;f8aa0000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"12914","ColType":"Number","ColValue":"2"}},
{"data":{"title":"name"},"attr":{"id":"12916","ColType":"Data","ColValue":"&lt;\"pci1002,aaf8\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"12918","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC03@0/BR3A@0/EGP0@0/EGP1@0/HDAU@1"}},
{"data":{"title":"IOName"},"attr":{"id":"12920","ColType":"String","ColValue":"pci1002,aaf8"}},
{"data":{"title":"vendor-id"},"attr":{"id":"12922","ColType":"Data","ColValue":"&lt;02100000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"12924","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"12926","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"12928","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"12930","ColType":"Data","ColValue":"&lt;02100000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"12932","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12933","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"12934","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"12936","ColType":"Number","ColValue":"4459779"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"12938","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12939","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"12941","ColType":"String","ColValue":"HDAU 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"12943","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12944","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12945","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"12946","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"12947","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"12948","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12949","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"12950","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"12951","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"12952","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12953","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"12954","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"12955","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"12956","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12957","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"12958","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"12959","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"12960","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"12961","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"12962","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"12963","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"12965","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"12967","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"12969","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"12971","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"12973","ColType":"String","ColValue":"243:0:1"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"12975","ColType":"Number","ColValue":"4355"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"12977","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"12979","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"12981","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"12983","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"12985","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"12987","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"12989","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"12991","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"12993","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"12995","ColType":"Data","ColValue":"&lt;\"pci1002,aaf8\",\"pciclass,040300\",\"HDAU\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"12997","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"12999","ColType":"Data","ColValue":"&lt;f8aa0000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"13001","ColType":"Data","ColValue":"&lt;1001f3820000000000002af00000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"13003","ColType":"Data","ColValue":"&lt;0001f300000000000000000000000000000000001001f30200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"13005","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"13006","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"13007","ColType":"Data","ColValue":"&lt;2b00000000000100&gt;"}}]}
]
