[
{"data":{"title":"built-in"},"attr":{"id":"5468","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"5470","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5471","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5472","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5474","ColType":"Number","ColValue":"549755813888"}},{"data":{"title":"length"},"attr":{"id":"5476","ColType":"Number","ColValue":"4194304"}}]}]},{"data":{"title":"1"},"attr":{"id":"5477","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5478","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5480","ColType":"Number","ColValue":"549772591104"}},{"data":{"title":"length"},"attr":{"id":"5482","ColType":"Number","ColValue":"524288"}}]}]},{"data":{"title":"1"},"attr":{"id":"5483","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5484","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5486","ColType":"Number","ColValue":"549774688256"}},{"data":{"title":"length"},"attr":{"id":"5488","ColType":"Number","ColValue":"65536"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"5490","ColType":"Number","ColValue":"64"}},
{"data":{"title":"device-id"},"attr":{"id":"5492","ColType":"Data","ColValue":"&lt;05200000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"5494","ColType":"Number","ColValue":"1"}},
{"data":{"title":"name"},"attr":{"id":"5496","ColType":"Data","ColValue":"&lt;\"pci106b,2005\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"5498","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/ANS2@0"}},
{"data":{"title":"IOName"},"attr":{"id":"5500","ColType":"String","ColValue":"pci106b,2005"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5502","ColType":"Data","ColValue":"&lt;6b100000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5504","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"5506","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"pci-functions-dependent"},"attr":{"id":"5508","ColType":"Data","ColValue":"&lt;0100000000000000&gt;"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5510","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5512","ColType":"Data","ColValue":"&lt;6b100000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5514","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5515","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5517","ColType":"Number","ColValue":"4683843"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"5519","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5520","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"5522","ColType":"String","ColValue":"ANS2 0"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"5524","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5525","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5526","ColType":"Number","ColValue":"5291294645182005248"}},{"data":{"title":"1"},"attr":{"id":"5527","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5528","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5529","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5530","ColType":"Number","ColValue":"5291294645182005249"}},{"data":{"title":"1"},"attr":{"id":"5531","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5532","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"5533","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5534","ColType":"Number","ColValue":"5291294645182005250"}},{"data":{"title":"1"},"attr":{"id":"5535","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5536","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5537","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5538","ColType":"Number","ColValue":"5291294645182005251"}},{"data":{"title":"1"},"attr":{"id":"5539","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5540","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"5541","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5542","ColType":"Number","ColValue":"5291294645182005252"}},{"data":{"title":"1"},"attr":{"id":"5543","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"5544","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"5546","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"5548","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"5550","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5552","ColType":"Number","ColValue":"256"}},
{"data":{"title":"pcidebug"},"attr":{"id":"5554","ColType":"String","ColValue":"2:0:0"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"5556","ColType":"Number","ColValue":"4163"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"5558","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"5560","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"5562","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"5564","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"5566","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"5568","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"5570","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"5572","ColType":"Data","ColValue":"&lt;02800100&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"5574","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"5576","ColType":"Data","ColValue":"&lt;\"pci106b,1800\",\"pci106b,2005\",\"pciclass,018002\",\"ANS2\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"5578","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"5580","ColType":"Data","ColValue":"&lt;00180000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"5582","ColType":"Data","ColValue":"&lt;100002c280000000000000000000000000004000180002c280000000000000010000000000000800200002c280000000000020010000000000000100&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"5584","ColType":"Data","ColValue":"&lt;0000020000000000000000000000000000000000100002420000000000000000000000000000400018000242000000000000000000000000000008002000024200000000000000000000000000000100&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"5586","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5587","ColType":"Data","ColValue":"&lt;1600000000000100&gt;"}}]}
]
