[
{"data":{"title":"built-in"},"attr":{"id":"5965","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"5967","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5968","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5969","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"5971","ColType":"Number","ColValue":"549775851520"}},{"data":{"title":"length"},"attr":{"id":"5973","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"device-id"},"attr":{"id":"5975","ColType":"Data","ColValue":"&lt;21200000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"5977","ColType":"Data","ColValue":"&lt;\"pci8086,2021\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"5979","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/CB0E@40004"}},
{"data":{"title":"IOName"},"attr":{"id":"5981","ColType":"String","ColValue":"pci8086,2021"}},
{"data":{"title":"vendor-id"},"attr":{"id":"5983","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"5985","ColType":"Data","ColValue":"&lt;04000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"5987","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"5989","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"5991","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"5993","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"5994","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"5995","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"5997","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"5999","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"6001","ColType":"String","ColValue":"0:4:4"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"6003","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"6005","ColType":"Number","ColValue":"146"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"6007","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"6009","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"6011","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"6013","ColType":"Number","ColValue":"3"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"6015","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"6017","ColType":"Data","ColValue":"&lt;00800800&gt;"}},
{"data":{"title":"compatible"},"attr":{"id":"6019","ColType":"Data","ColValue":"&lt;\"pci8086,0\",\"pci8086,2021\",\"pciclass,088000\",\"CB0E\"&gt;"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"6021","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"6023","ColType":"Data","ColValue":"&lt;102400828000000000c031010000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"6025","ColType":"Data","ColValue":"&lt;00240000000000000000000000000000000000001024000200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"6027","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"6028","ColType":"Data","ColValue":"&lt;1000000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"6029","ColType":"Data","ColValue":"&lt;0500000000000100&gt;"}}]}
]
