[
{"data":{"title":"IOPCITunnelLinkChange"},"attr":{"id":"10120","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"ranges"},"attr":{"id":"10122","ColType":"Data","ColValue":"&lt;0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"10124","ColType":"String","ColValue":"7:1:0(67:67)"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"10126","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"10128","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10129","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"10130","ColType":"Data","ColValue":"&lt;1400000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"10132","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2D@30000/UPSB@0/DSB1@10000"}},
{"data":{"title":"Thunderbolt Path"},"attr":{"id":"10134","ColType":"String","ColValue":"IOService:/AppleACPIPlatformExpert/PC02@0/AppleACPIPCI/BR2D@3/IOPP/UPSB@0/IOPP/DSB0@0/IOPP/NHI0@0/AppleThunderboltHAL/AppleThunderboltNHIType3/IOThunderboltController/IOThunderboltPort@5/IOThunderboltSwitchType3/IOThunderboltPort@6"}},
{"data":{"title":"IOPCIExpressSlotCapabilities"},"attr":{"id":"10136","ColType":"Number","ColValue":"786528"}},
{"data":{"title":"IOPCIExpressSlotStatus"},"attr":{"id":"10138","ColType":"Number","ColValue":"0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"10140","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"10142","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10143","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"10144","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"10146","ColType":"Number","ColValue":"354"}},
{"data":{"title":"AAPL,slot-name"},"attr":{"id":"10148","ColType":"Data","ColValue":"&lt;\"PCI Slot 1\"&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"10150","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPCITunnelID"},"attr":{"id":"10152","ColType":"Number","ColValue":"4294968446"}},
{"data":{"title":"IOPCIConfigured"},"attr":{"id":"10154","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"10156","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IODTPersist"},"attr":{"id":"10158","ColType":"Number","ColValue":"0"}},
{"data":{"title":"#size-cells"},"attr":{"id":"10160","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"10162","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"10164","ColType":"Data","ColValue":"&lt;\"pci-bridge\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"10166","ColType":"Number","ColValue":"48"}},
{"data":{"title":"compatible"},"attr":{"id":"10168","ColType":"Data","ColValue":"&lt;\"pci8086,15d3\",\"pciclass,060400\",\"DSB1\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"10170","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"DevicePowerState"},"attr":{"id":"10172","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"10174","ColType":"Number","ColValue":"0"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"10176","ColType":"Number","ColValue":"0"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"10178","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"10180","ColType":"Number","ColValue":"2"}},{"data":{"title":"PowerOverrideOn"},"attr":{"id":"10182","ColType":"Boolean","ColValue":"Yes"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"10184","ColType":"Number","ColValue":"2"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"10186","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"10188","ColType":"Number","ColValue":"24206401"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"10190","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"10192","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"#address-cells"},"attr":{"id":"10194","ColType":"Data","ColValue":"&lt;03000000&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"10196","ColType":"String","ColValue":"pci-bridge"}},
{"data":{"title":"acpi-device"},"attr":{"id":"10198","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"10200","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"reg"},"attr":{"id":"10202","ColType":"Data","ColValue":"&lt;0008070000000000000000000000000000000000&gt;"}},
{"data":{"title":"Thunderbolt Entry ID"},"attr":{"id":"10204","ColType":"Number","ColValue":"4294968479"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"10206","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10207","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"10209","ColType":"String","ColValue":"DSB1 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"10211","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10212","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10213","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"10214","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10215","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"10216","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10217","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"10218","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10219","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"10220","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10221","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"10222","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10223","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"10224","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10225","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"10226","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10227","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"10228","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"10229","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"10230","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"10231","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"10233","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"10235","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"10237","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"10239","ColType":"Data","ColValue":"&lt;00040600&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"10241","ColType":"Data","ColValue":"&lt;d3150000&gt;"}}
]
