[
{"data":{"title":"built-in"},"attr":{"id":"41492","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"41494","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41495","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41496","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"41498","ColType":"Number","ColValue":"4029284352"}},{"data":{"title":"length"},"attr":{"id":"41500","ColType":"Number","ColValue":"16384"}}]}]}]},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"41502","ColType":"Number","ColValue":"80"}},
{"data":{"title":"layout-id"},"attr":{"id":"41504","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"hda-gfx"},"attr":{"id":"41506","ColType":"Data","ColValue":"&lt;\"onboard-1\"&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"41508","ColType":"Data","ColValue":"&lt;f8aa0000&gt;"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"41510","ColType":"Number","ColValue":"2"}},
{"data":{"title":"name"},"attr":{"id":"41512","ColType":"Data","ColValue":"&lt;\"pci1002,aaf8\"&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"41514","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC03@0/BR3A@0/EGP0@0/EGP1@0/HDAU@1"}},
{"data":{"title":"IOName"},"attr":{"id":"41516","ColType":"String","ColValue":"pci1002,aaf8"}},
{"data":{"title":"vendor-id"},"attr":{"id":"41518","ColType":"Data","ColValue":"&lt;02100000&gt;"}},
{"data":{"title":"revision-id"},"attr":{"id":"41520","ColType":"Data","ColValue":"&lt;00000000&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"41522","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"41524","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"41526","ColType":"Data","ColValue":"&lt;02100000&gt;"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"41528","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41529","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"41530","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"41532","ColType":"Number","ColValue":"4459779"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"41534","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41535","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"41537","ColType":"String","ColValue":"HDAU 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"41539","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41540","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41541","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"41542","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"41543","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"41544","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41545","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"41546","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"41547","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"41548","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41549","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"41550","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"41551","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"41552","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41553","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"41554","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"41555","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"41556","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41557","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"41558","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"41559","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"41561","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"41563","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"41565","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"41567","ColType":"Number","ColValue":"0"}},
{"data":{"title":"pcidebug"},"attr":{"id":"41569","ColType":"String","ColValue":"243:0:1"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"41571","ColType":"Number","ColValue":"4355"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"41573","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"41575","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"41577","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"41579","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"41581","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"41583","ColType":"Number","ColValue":"2"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"41585","ColType":"Number","ColValue":"258"}}]},
{"data":{"title":"class-code"},"attr":{"id":"41587","ColType":"Data","ColValue":"&lt;00030400&gt;"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"41589","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"compatible"},"attr":{"id":"41591","ColType":"Data","ColValue":"&lt;\"pci1002,aaf8\",\"pciclass,040300\",\"HDAU\"&gt;"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"41593","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"41595","ColType":"Data","ColValue":"&lt;f8aa0000&gt;"}},
{"data":{"title":"assigned-addresses"},"attr":{"id":"41597","ColType":"Data","ColValue":"&lt;1001f3820000000000002af00000000000400000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"41599","ColType":"Data","ColValue":"&lt;0001f300000000000000000000000000000000001001f30200000000000000000000000000400000&gt;"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"41601","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"41602","ColType":"Data","ColValue":"&lt;1100000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"41603","ColType":"Data","ColValue":"&lt;2b00000000000100&gt;"}}]}
]
