[
{"data":{"title":"device-id"},"attr":{"id":"44364","ColType":"Data","ColValue":"&lt;18200000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"44366","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"IOName"},"attr":{"id":"44368","ColType":"String","ColValue":"pci8086,2018"}},
{"data":{"title":"pcidebug"},"attr":{"id":"44370","ColType":"String","ColValue":"240:23:0"}},
{"data":{"title":"built-in"},"attr":{"id":"44372","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"acpi-path"},"attr":{"id":"44374","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC03@0/M20@170000"}},
{"data":{"title":"revision-id"},"attr":{"id":"44376","ColType":"Data","ColValue":"&lt;04000000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"44378","ColType":"Data","ColValue":"&lt;00b8f00000000000000000000000000000000000&gt;"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"44380","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"class-code"},"attr":{"id":"44382","ColType":"Data","ColValue":"&lt;00800800&gt;"}},
{"data":{"title":"acpi-device"},"attr":{"id":"44384","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"compatible"},"attr":{"id":"44386","ColType":"Data","ColValue":"&lt;\"pci8086,2018\",\"pciclass,088000\",\"M20\"&gt;"}},
{"data":{"title":"name"},"attr":{"id":"44388","ColType":"Data","ColValue":"&lt;\"pci8086,2018\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"44390","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"44392","ColType":"Number","ColValue":"2"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"44394","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"44396","ColType":"Number","ColValue":"3"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"44398","ColType":"Number","ColValue":"258"}}]}
]
