[
{"data":{"title":"assigned-addresses"},"attr":{"id":"35975","ColType":"Data","ColValue":"&lt;10007d8200000000000010900000000000000100&gt;"}},
{"data":{"title":"pcidebug"},"attr":{"id":"35977","ColType":"String","ColValue":"125:0:0"}},
{"data":{"title":"IOPCITunnelL1Enable"},"attr":{"id":"35979","ColType":"Boolean","ColValue":"No"}},
{"data":{"title":"pci-aspm-default"},"attr":{"id":"35981","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOInterruptSpecifiers"},"attr":{"id":"35983","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35984","ColType":"Data","ColValue":"&lt;1200000007000000&gt;"}},{"data":{"title":"1"},"attr":{"id":"35985","ColType":"Data","ColValue":"&lt;2900000000000100&gt;"}}]},
{"data":{"title":"acpi-path"},"attr":{"id":"35987","ColType":"String","ColValue":"IOACPIPlane:/_SB/PC02@0/BR2C@20000/UPSB@0/DSB2@20000/XHC2@0"}},
{"data":{"title":"acpi-pmcap-offset"},"attr":{"id":"35989","ColType":"Number","ColValue":"128"}},
{"data":{"title":"IOInterruptControllers"},"attr":{"id":"35991","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"35992","ColType":"String","ColValue":"io-apic-0"}},{"data":{"title":"1"},"attr":{"id":"35993","ColType":"String","ColValue":"IOPCIMessagedInterruptController"}}]},
{"data":{"title":"USBBusNumber"},"attr":{"id":"35995","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPCIExpressCapabilities"},"attr":{"id":"35997","ColType":"Number","ColValue":"2"}},
{"data":{"title":"IOChildIndex"},"attr":{"id":"35999","ColType":"Number","ColValue":"1"}},
{"data":{"title":"IOPCIResourced"},"attr":{"id":"36001","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-vendor-id"},"attr":{"id":"36003","ColType":"Data","ColValue":"&lt;22220000&gt;"}},
{"data":{"title":"vendor-id"},"attr":{"id":"36005","ColType":"Data","ColValue":"&lt;86800000&gt;"}},
{"data":{"title":"name"},"attr":{"id":"36007","ColType":"Data","ColValue":"&lt;\"pci8086,15d4\"&gt;"}},
{"data":{"title":"IOPCIHPType"},"attr":{"id":"36009","ColType":"Number","ColValue":"2"}},
{"data":{"title":"compatible"},"attr":{"id":"36011","ColType":"Data","ColValue":"&lt;\"pci2222,1111\",\"pci8086,15d4\",\"pciclass,0c0330\",\"XHC2\"&gt;"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"36013","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"36015","ColType":"Number","ColValue":"0"}},{"data":{"title":"ChildProxyPowerState"},"attr":{"id":"36017","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"36019","ColType":"Number","ColValue":"3"}},{"data":{"title":"ChildrenPowerState"},"attr":{"id":"36021","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"36023","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"revision-id"},"attr":{"id":"36025","ColType":"Data","ColValue":"&lt;02000000&gt;"}},
{"data":{"title":"IOPCIExpressLinkCapabilities"},"attr":{"id":"36027","ColType":"Number","ColValue":"4545601"}},
{"data":{"title":"IOPCIMSIMode"},"attr":{"id":"36029","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"AAPL,xhci-clock-id"},"attr":{"id":"36031","ColType":"Number","ColValue":"1"}},
{"data":{"title":"built-in"},"attr":{"id":"36033","ColType":"Data","ColValue":"&lt;00&gt;"}},
{"data":{"title":"IOPCIExpressLinkStatus"},"attr":{"id":"36035","ColType":"Number","ColValue":"4161"}},
{"data":{"title":"IODeviceMemory"},"attr":{"id":"36037","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36038","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36039","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"address"},"attr":{"id":"36041","ColType":"Number","ColValue":"2416967680"}},{"data":{"title":"length"},"attr":{"id":"36043","ColType":"Number","ColValue":"65536"}}]}]}]},
{"data":{"title":"IOName"},"attr":{"id":"36045","ColType":"String","ColValue":"pci8086,15d4"}},
{"data":{"title":"acpi-device"},"attr":{"id":"36047","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}},
{"data":{"title":"IOReportLegendPublic"},"attr":{"id":"36049","ColType":"Boolean","ColValue":"Yes"}},
{"data":{"title":"subsystem-id"},"attr":{"id":"36051","ColType":"Data","ColValue":"&lt;11110000&gt;"}},
{"data":{"title":"reg"},"attr":{"id":"36053","ColType":"Data","ColValue":"&lt;00007d000000000000000000000000000000000010007d0200000000000000000000000000000100&gt;"}},
{"data":{"title":"IOReportLegend"},"attr":{"id":"36055","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36056","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportSubGroupName"},"attr":{"id":"36058","ColType":"String","ColValue":"XHC2 1"}},{"data":{"title":"IOReportChannels"},"attr":{"id":"36060","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36061","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36062","ColType":"Number","ColValue":"5291294645182070784"}},{"data":{"title":"1"},"attr":{"id":"36063","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36064","ColType":"String","ColValue":"               First Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"36065","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36066","ColType":"Number","ColValue":"5291294645182070785"}},{"data":{"title":"1"},"attr":{"id":"36067","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36068","ColType":"String","ColValue":"              Second Level Interrupt Handler Count"}}]},{"data":{"title":"3"},"attr":{"id":"36069","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36070","ColType":"Number","ColValue":"5291294645182070786"}},{"data":{"title":"1"},"attr":{"id":"36071","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36072","ColType":"String","ColValue":"        First Level Interrupt Handler Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"36073","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36074","ColType":"Number","ColValue":"5291294645182070787"}},{"data":{"title":"1"},"attr":{"id":"36075","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36076","ColType":"String","ColValue":"   Second Level Interrupt Handler CPU Time (MATUs)"}}]},{"data":{"title":"3"},"attr":{"id":"36077","ColType":"Array","ColValue":"0_values"},"children":[{"data":{"title":"0"},"attr":{"id":"36078","ColType":"Number","ColValue":"5291294645182070788"}},{"data":{"title":"1"},"attr":{"id":"36079","ColType":"Number","ColValue":"4295098369"}},{"data":{"title":"2"},"attr":{"id":"36080","ColType":"String","ColValue":"Second Level Interrupt Handler System Time (MATUs)"}}]}]},{"data":{"title":"IOReportGroupName"},"attr":{"id":"36082","ColType":"String","ColValue":"Interrupt Statistics (by index)"}},{"data":{"title":"IOReportChannelInfo"},"attr":{"id":"36084","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"IOReportChannelUnit"},"attr":{"id":"36086","ColType":"Number","ColValue":"0"}}]}]}]},
{"data":{"title":"class-code"},"attr":{"id":"36088","ColType":"Data","ColValue":"&lt;30030c00&gt;"}},
{"data":{"title":"device-id"},"attr":{"id":"36090","ColType":"Data","ColValue":"&lt;d4150000&gt;"}}
]
