[
{"data":{"title":"_STA"},"attr":{"id":"3920","ColType":"Number","ColValue":"15"}},
{"data":{"title":"_ADR"},"attr":{"id":"3922","ColType":"Number","ColValue":"0"}},
{"data":{"title":"IOPowerManagement"},"attr":{"id":"3924","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"MaxPowerState"},"attr":{"id":"3926","ColType":"Number","ColValue":"2"}},{"data":{"title":"CurrentPowerState"},"attr":{"id":"3928","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"3930","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"device-properties"},"attr":{"id":"3932","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"pci-functions-dependent"},"attr":{"id":"3934","ColType":"Data","ColValue":"&lt;0100000000000000&gt;"}},{"data":{"title":"acpi-path"},"attr":{"id":"3936","ColType":"String","ColValue":"IOACPIPlane:/_SB/PCI0@0/RP01@1c0000/ANS2@0"}},{"data":{"title":"acpi-device"},"attr":{"id":"3938","ColType":"String","ColValue":"IOACPIPlatformDevice is not serializable"}}]},
{"data":{"title":"acpi-pci-pm"},"attr":{"id":"3940","ColType":"Boolean","ColValue":"Yes"}}
]
